<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="31.42" x2="0" y2="0.635" width="0" layer="20"/>
<wire x1="0" y1="0.635" x2="0.635" y2="0" width="0" layer="20" curve="90"/>
<wire x1="0.635" y1="0" x2="23.38" y2="0" width="0" layer="20"/>
<wire x1="23.38" y1="0" x2="25.38" y2="2" width="0" layer="20" curve="90"/>
<wire x1="25.38" y1="2" x2="25.38" y2="30.055" width="0" layer="20"/>
<wire x1="25.38" y1="30.055" x2="23.38" y2="32.055" width="0" layer="20" curve="90"/>
<wire x1="23.38" y1="32.055" x2="0.635" y2="32.055" width="0" layer="20"/>
<wire x1="0.635" y1="32.055" x2="0" y2="31.42" width="0" layer="20" curve="90"/>
<text>R1</text>
<text>POWER</text>
<text>CD1</text>
<text>CD2</text>
<text>syncchannel.blogspot.com
D.W. 4/25/18</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="HDF15H">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="SMA_EDGELAUNCH">
</package>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PAD-JUMPER-2-NO_YES_SILK">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="X1" library="adafruit" package="HDF15H" value="">
<attribute name="VALUE"/>
</element>
<element name="X2" library="adafruit" package="SMA_EDGELAUNCH" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="SparkFun-Passives" package="PAD-JUMPER-2-NO_YES_SILK" value="JUMPER-PAD-2-NOYES_SILK"/>
<element name="SJ2" library="SparkFun-Passives" package="PAD-JUMPER-2-NO_YES_SILK" value="JUMPER-PAD-2-NOYES_SILK"/>
<element name="LED1" library="adafruit" package="CHIPLED_0805" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="R0805" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="RF">
<contactref element="X1" pad="1"/>
<contactref element="X2" pad="P"/>
</signal>
<signal name="GND">
<contactref element="X1" pad="6"/>
<contactref element="X1" pad="7"/>
<contactref element="X1" pad="8"/>
<contactref element="X2" pad="GND@2"/>
<contactref element="X2" pad="GND@1"/>
<contactref element="X2" pad="GND@4"/>
<contactref element="X2" pad="GND@3"/>
<contactref element="SJ1" pad="2"/>
<contactref element="SJ2" pad="2"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="5V">
<contactref element="X1" pad="9"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="CD2">
<contactref element="X1" pad="10"/>
<contactref element="SJ2" pad="1"/>
</signal>
<signal name="CD1">
<contactref element="X1" pad="5"/>
<contactref element="SJ1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
