(kicad_pcb (version 20171130) (host pcbnew 5.1.5-52549c5~84~ubuntu19.04.1)
  (general
    (thickness 1.6)
    (drawings 12)
    (tracks 55)
    (zones 0)
    (modules 5)
    (nets 4)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(D1-Pad2)")
  (net 3 +3V3)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
  )
  (module touch:TestPoint_Pad_4.0x4.0mm (layer B.Cu) (tedit 5DF7CA08)
    (at 181.2925 53.975)
    (descr "SMD rectangular pad as test Point, square 4.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference J2 (at 0 2.898) (layer B.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 -3.1) (layer B.Fab))
    (fp_text user %R (at 0 2.9) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 10 10) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
  )
  (module touch:TestPoint_Pad_4.0x4.0mm (layer B.Cu) (tedit 5DF7C9E5)
    (at 125.73 53.7464)
    (descr "SMD rectangular pad as test Point, square 4.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference J1 (at 0 2.898) (layer B.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 -3.1) (layer B.Fab))
    (fp_text user %R (at 0 2.9) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 10 10) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5DF7C9BB)
    (at 153.4795 43.4975 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 1.43 270) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(D1-Pad2)"))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5DF7C974)
    (at 153.4795 54.751 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D1 (at 0.014 -1.43 90) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.43 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module afterdark:OSH_small_copper-mask (layer F.Cu) (tedit 5DF3FF89)
    (at 153.5684 56.2864)
    (descr "Imported from OSHPARK.svg")
    (tags svg2mod)
    (attr smd)
    (fp_text reference OSH_small (at 0 -11.457835) (layer F.Cu) hide)
    (fp_text value G*** (at 0 11.457835) (layer F.Cu) hide)
  )
  (gr_text "OSH Park\n2 layer flexible PCB" (at 153.21788 49.97704) (layer B.Cu))
  (gr_text "Drew Fustini" (at 153.0985 58.039) (layer B.Cu))
  (gr_line (start 120.8405 40.64) (end 187.198 40.64) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 118.0465 43.434) (end 118.11 64.3255) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 187.198 67.056) (end 120.904 67.1195) (layer Edge.Cuts) (width 0.12))
  (gr_arc (start 120.904 64.3255) (end 118.11 64.3255) (angle -90) (layer Edge.Cuts) (width 0.12))
  (gr_arc (start 120.8405 43.434) (end 120.8405 40.64) (angle -90) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 189.992 43.434) (end 189.992 64.262) (layer Edge.Cuts) (width 0.12))
  (gr_arc (start 187.198 43.434) (end 189.992 43.434) (angle -90) (layer Edge.Cuts) (width 0.12))
  (gr_arc (start 187.198 64.262) (end 187.198 67.056) (angle -90) (layer Edge.Cuts) (width 0.12))
  (gr_text "Drew Fustini" (at 153.0985 58.039) (layer B.Mask))
  (gr_text drew@oshpark.com (at 153.2636 62.5856) (layer B.SilkS))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 168.917322 54.1) (xy 169.770985 54.13375) (xy 170.604434 54.235) (xy 171.417669 54.40375) (xy 172.210691 54.64)
        (xy 172.983499 54.94375) (xy 173.736093 55.315) (xy 174.468474 55.75375) (xy 175.180641 56.26) (xy 175.872593 56.83375)
        (xy 176.544333 57.475) (xy 182.615047 53.975) (xy 176.544333 50.475) (xy 175.872593 51.11625) (xy 175.180641 51.69)
        (xy 174.468474 52.19625) (xy 173.736093 52.635) (xy 172.983499 53.00625) (xy 172.210691 53.31) (xy 171.417669 53.54625)
        (xy 170.604434 53.715) (xy 169.770985 53.81625) (xy 168.917322 53.85)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.32447 55.501) (xy 154.264987 55.498925) (xy 154.207484 55.4927) (xy 154.15196 55.482325) (xy 154.098415 55.4678)
        (xy 154.04685 55.449125) (xy 153.997265 55.4263) (xy 153.949658 55.399325) (xy 153.904032 55.3682) (xy 153.860384 55.332925)
        (xy 153.818717 55.2935) (xy 153.242 55.626) (xy 153.818717 55.9585) (xy 153.860384 55.919074) (xy 153.904032 55.883799)
        (xy 153.949658 55.852674) (xy 153.997265 55.825699) (xy 154.04685 55.802874) (xy 154.098415 55.784199) (xy 154.15196 55.769674)
        (xy 154.207484 55.759299) (xy 154.264987 55.753074) (xy 154.32447 55.751)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.938 55.464404) (xy 154.939549 55.419884) (xy 154.944199 55.376852) (xy 154.951949 55.335308) (xy 154.962799 55.295252)
        (xy 154.976749 55.256683) (xy 154.993799 55.219602) (xy 155.013949 55.184009) (xy 155.037199 55.149904) (xy 155.063549 55.117286)
        (xy 155.093 55.086157) (xy 154.813 54.6005) (xy 154.533 55.086157) (xy 154.56245 55.117286) (xy 154.5888 55.149904)
        (xy 154.61205 55.184009) (xy 154.6322 55.219602) (xy 154.64925 55.256683) (xy 154.6632 55.295252) (xy 154.67405 55.335308)
        (xy 154.6818 55.376852) (xy 154.68645 55.419884) (xy 154.688 55.464404)
      )
    )
  )
  (zone (net 2) (net_name "Net-(D1-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.3545 45.881596) (xy 153.35295 45.926115) (xy 153.3483 45.969147) (xy 153.34055 46.010691) (xy 153.3297 46.050747)
        (xy 153.31575 46.089316) (xy 153.2987 46.126397) (xy 153.27855 46.16199) (xy 153.2553 46.196095) (xy 153.22895 46.228713)
        (xy 153.1995 46.259843) (xy 153.4795 46.7455) (xy 153.7595 46.259843) (xy 153.730049 46.228713) (xy 153.703699 46.196095)
        (xy 153.680449 46.16199) (xy 153.660299 46.126397) (xy 153.643249 46.089316) (xy 153.629299 46.050747) (xy 153.618449 46.010691)
        (xy 153.610699 45.969147) (xy 153.606049 45.926115) (xy 153.6045 45.881596)
      )
    )
  )
  (zone (net 2) (net_name "Net-(D1-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.6045 45.21747) (xy 153.606574 45.157987) (xy 153.612799 45.100484) (xy 153.623174 45.04496) (xy 153.637699 44.991415)
        (xy 153.656374 44.93985) (xy 153.679199 44.890265) (xy 153.706174 44.842658) (xy 153.737299 44.797032) (xy 153.772574 44.753384)
        (xy 153.812 44.711717) (xy 153.4795 44.135) (xy 153.147 44.711717) (xy 153.186425 44.753384) (xy 153.2217 44.797032)
        (xy 153.252825 44.842658) (xy 153.2798 44.890265) (xy 153.302625 44.93985) (xy 153.3213 44.991415) (xy 153.335825 45.04496)
        (xy 153.3462 45.100484) (xy 153.352425 45.157987) (xy 153.3545 45.21747)
      )
    )
  )
  (zone (net 2) (net_name "Net-(D1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.6045 47.209404) (xy 153.606049 47.164884) (xy 153.610699 47.121852) (xy 153.618449 47.080308) (xy 153.629299 47.040252)
        (xy 153.643249 47.001683) (xy 153.660299 46.964602) (xy 153.680449 46.929009) (xy 153.703699 46.894904) (xy 153.730049 46.862286)
        (xy 153.7595 46.831157) (xy 153.4795 46.3455) (xy 153.1995 46.831157) (xy 153.22895 46.862286) (xy 153.2553 46.894904)
        (xy 153.27855 46.929009) (xy 153.2987 46.964602) (xy 153.31575 47.001683) (xy 153.3297 47.040252) (xy 153.34055 47.080308)
        (xy 153.3483 47.121852) (xy 153.35295 47.164884) (xy 153.3545 47.209404)
      )
    )
  )
  (zone (net 2) (net_name "Net-(D1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.3545 53.00303) (xy 153.352425 53.067832) (xy 153.3462 53.130095) (xy 153.335825 53.189819) (xy 153.3213 53.247004)
        (xy 153.302625 53.301649) (xy 153.2798 53.353754) (xy 153.252825 53.403321) (xy 153.2217 53.450347) (xy 153.186425 53.494835)
        (xy 153.147 53.536783) (xy 153.4795 54.1135) (xy 153.812 53.536783) (xy 153.772574 53.494835) (xy 153.737299 53.450347)
        (xy 153.706174 53.403321) (xy 153.679199 53.353754) (xy 153.656374 53.301649) (xy 153.637699 53.247004) (xy 153.623174 53.189819)
        (xy 153.612799 53.130095) (xy 153.606574 53.067832) (xy 153.6045 53.00303)
      )
    )
  )
  (zone (net 3) (net_name +3V3) (layer B.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 138.70146 53.595) (xy 137.739211 53.56125) (xy 136.808607 53.46) (xy 135.909647 53.29125) (xy 135.04233 53.055)
        (xy 134.206657 52.75125) (xy 133.402628 52.38) (xy 132.630242 51.94125) (xy 131.8895 51.435) (xy 131.180403 50.86125)
        (xy 130.502949 50.22) (xy 124.432235 53.72) (xy 130.502949 57.22) (xy 131.180403 56.57875) (xy 131.8895 56.005)
        (xy 132.630242 55.49875) (xy 133.402628 55.06) (xy 134.206657 54.68875) (xy 135.04233 54.385) (xy 135.909647 54.14875)
        (xy 136.808607 53.98) (xy 137.739211 53.87875) (xy 138.70146 53.845)
      )
    )
  )
  (zone (net 3) (net_name +3V3) (layer B.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 152.63453 42.7475) (xy 152.694012 42.749574) (xy 152.751515 42.755799) (xy 152.807039 42.766174) (xy 152.860584 42.780699)
        (xy 152.912149 42.799374) (xy 152.961734 42.822199) (xy 153.009341 42.849174) (xy 153.054967 42.880299) (xy 153.098615 42.915574)
        (xy 153.140283 42.955) (xy 153.717 42.6225) (xy 153.140283 42.29) (xy 153.098615 42.329425) (xy 153.054967 42.3647)
        (xy 153.009341 42.395825) (xy 152.961734 42.4228) (xy 152.912149 42.445625) (xy 152.860584 42.4643) (xy 152.807039 42.478825)
        (xy 152.751515 42.4892) (xy 152.694012 42.495425) (xy 152.63453 42.4975)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.476626 54.674033) (xy 155.432103 54.672581) (xy 155.389061 54.668026) (xy 155.3475 54.660368) (xy 155.30742 54.649606)
        (xy 155.26882 54.635742) (xy 155.231702 54.618774) (xy 155.196064 54.598703) (xy 155.161907 54.575528) (xy 155.129232 54.54925)
        (xy 155.098037 54.51987) (xy 154.613001 54.800942) (xy 155.099275 55.079867) (xy 155.130339 55.050348) (xy 155.162899 55.023926)
        (xy 155.196952 55.000601) (xy 155.232501 54.980372) (xy 155.269544 54.96324) (xy 155.308082 54.949205) (xy 155.348114 54.938266)
        (xy 155.389641 54.930424) (xy 155.432662 54.925679) (xy 155.477179 54.924031)
      )
    )
  )
)
