(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 13)
    (tracks 816)
    (zones 0)
    (modules 39)
    (nets 62)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.254000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 5V)
  (net 3 VCC)
  (net 4 SRCLK)
  (net 5 RCLK)
  (net 6 OE)
  (net 7 SER)
  (net 8 10)
  (net 9 11)
  (net 10 "Net-(J1-Pad10)")
  (net 11 14)
  (net 12 15)
  (net 13 16)
  (net 14 17)
  (net 15 18)
  (net 16 19)
  (net 17 20)
  (net 18 21)
  (net 19 22)
  (net 20 23)
  (net 21 LA)
  (net 22 "Net-(R2-Pad2)")
  (net 23 "Net-(R3-Pad2)")
  (net 24 LB)
  (net 25 LC)
  (net 26 "Net-(R4-Pad2)")
  (net 27 "Net-(R5-Pad2)")
  (net 28 LD)
  (net 29 LE)
  (net 30 "Net-(R6-Pad2)")
  (net 31 "Net-(R7-Pad2)")
  (net 32 LF)
  (net 33 LG)
  (net 34 "Net-(R8-Pad2)")
  (net 35 "Net-(R9-Pad2)")
  (net 36 LH)
  (net 37 D6)
  (net 38 BG)
  (net 39 BE)
  (net 40 D5)
  (net 41 BH)
  (net 42 BF)
  (net 43 BD)
  (net 44 BC)
  (net 45 BB)
  (net 46 BA)
  (net 47 "Net-(U1-Pad9)")
  (net 48 "Net-(U2-Pad9)")
  (net 49 "Net-(U3-Pad1)")
  (net 50 D0)
  (net 51 D1)
  (net 52 D2)
  (net 53 D3)
  (net 54 D4)
  (net 55 D7)
  (net 56 "Net-(U3-Pad18)")
  (net 57 "Net-(U3-Pad20)")
  (net 58 "Net-(R10-Pad2)")
  (net 59 "Net-(R11-Pad2)")
  (net 60 "Net-(R12-Pad2)")
  (net 61 "Net-(R13-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 10)
    (add_net 11)
    (add_net 14)
    (add_net 15)
    (add_net 16)
    (add_net 17)
    (add_net 18)
    (add_net 19)
    (add_net 20)
    (add_net 21)
    (add_net 22)
    (add_net 23)
    (add_net 5V)
    (add_net BA)
    (add_net BB)
    (add_net BC)
    (add_net BD)
    (add_net BE)
    (add_net BF)
    (add_net BG)
    (add_net BH)
    (add_net D0)
    (add_net D1)
    (add_net D2)
    (add_net D3)
    (add_net D4)
    (add_net D5)
    (add_net D6)
    (add_net D7)
    (add_net GND)
    (add_net LA)
    (add_net LB)
    (add_net LC)
    (add_net LD)
    (add_net LE)
    (add_net LF)
    (add_net LG)
    (add_net LH)
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R13-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U2-Pad9)")
    (add_net "Net-(U3-Pad1)")
    (add_net "Net-(U3-Pad18)")
    (add_net "Net-(U3-Pad20)")
    (add_net OE)
    (add_net RCLK)
    (add_net SER)
    (add_net SRCLK)
    (add_net VCC)
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 90.17 39.6494)
    (fp_text reference SW1 (at 4.572 6.3246) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 9 11) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 58 "Net-(R10-Pad2)"))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 38 BG) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
  )
  (module AOR_custom:AOR_LOGO (layer F.Cu) (tedit 5C26ADAA)
    (at 121.666 106.934 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value AOR_LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5CF08A7E)
    (at 88.265 50.165)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5CF08A7E)
    (at 122.555 50.165)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5CF08A7E)
    (at 122.555 153.67)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Connector_IDC:IDC-Header_2x10_P2.54mm_Vertical (layer B.Cu) (tedit 59DE0251)
    (at 99.06 93.98)
    (descr "Through hole straight IDC box header, 2x10, 2.54mm pitch, double rows")
    (tags "Through hole IDC box header THT 2x10 2.54mm double row")
    (fp_text reference J1 (at 1.27 6.604) (layer B.SilkS))
    (fp_text value Conn_01x20 (at 1.27 -29.464) (layer B.Fab))
    (fp_text user %R (at 1.27 -11.43) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 5V))
    (pad 3 thru_hole oval (at 0 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 4 thru_hole oval (at 2.54 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 SRCLK))
    (pad 5 thru_hole oval (at 0 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 RCLK))
    (pad 6 thru_hole oval (at 2.54 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 OE))
    (pad 7 thru_hole oval (at 0 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 SER))
    (pad 8 thru_hole oval (at 2.54 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 10))
    (pad 9 thru_hole oval (at 0 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 11))
    (pad 10 thru_hole oval (at 2.54 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad10)"))
    (pad 11 thru_hole oval (at 0 -12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 14))
    (pad 12 thru_hole oval (at 2.54 -12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 15))
    (pad 13 thru_hole oval (at 0 -15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 16))
    (pad 14 thru_hole oval (at 2.54 -15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 17))
    (pad 15 thru_hole oval (at 0 -17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 18))
    (pad 16 thru_hole oval (at 2.54 -17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 19))
    (pad 17 thru_hole oval (at 0 -20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 20))
    (pad 18 thru_hole oval (at 2.54 -20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 21))
    (pad 19 thru_hole oval (at 0 -22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 22))
    (pad 20 thru_hole oval (at 2.54 -22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 23))
    (model ${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 87.884 102.616 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J2 (at 0 2.33 180) (layer B.SilkS))
    (fp_text value Conn_01x02 (at 0 -4.87 180) (layer B.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 91.44 102.616 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J3 (at 0 2.33 180) (layer B.SilkS))
    (fp_text value Conn_01x02 (at 0 -4.87 180) (layer B.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 94.996 102.616 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J4 (at 0 2.33 180) (layer B.SilkS))
    (fp_text value Conn_01x02 (at 0 -4.87 180) (layer B.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer B.Fab))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 5V))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5B391E66)
    (at 92.71 86.614 90)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 0 1.8 90) (layer B.SilkS))
    (fp_text value SolderJumper_2_Open (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd custom (at -0.65 0 90) (size 1 0.5) (layers B.Cu B.Mask)
      (net 3 VCC) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0 90) (size 1 0.5) (layers B.Cu B.Mask)
      (net 10 "Net-(J1-Pad10)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 92.964 90.932 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value R_US (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 17 20))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 121.158 57.912 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 -1.82 270) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 21 LA))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 22 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 117.348 57.912 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 -1.82 270) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 23 "Net-(R3-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 24 LB))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 113.538 57.912 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 -1.82 270) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 25 LC))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 26 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 109.728 57.912 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0 -1.82 270) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 27 "Net-(R5-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 28 LD))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 105.918 57.912 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0 -1.82 270) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 29 LE))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 30 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 102.108 57.912 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0 -1.82 270) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 31 "Net-(R7-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 32 LF))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 98.298 57.912 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0 -1.82 270) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 33 LG))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 34 "Net-(R8-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 94.488 57.912 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 0 -1.82 270) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 35 "Net-(R9-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 36 LH))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 90.17 79.9592)
    (fp_text reference SW2 (at -0.1 -6.35) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 9 11) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 59 "Net-(R11-Pad2)"))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 39 BE) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 97.2058 115.7732)
    (fp_text reference SW3 (at -0.1 -6.35) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 17 20) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 36 LH))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 40 D5))
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 41 BH) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 97.2058 130.793066)
    (fp_text reference SW4 (at -0.1 -6.35) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 17 20) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 LG))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 40 D5))
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 38 BG) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 97.2058 145.812932)
    (fp_text reference SW5 (at -0.1 -6.35) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 17 20) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 32 LF))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 40 D5))
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 42 BF) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 97.2058 160.8328)
    (fp_text reference SW6 (at -0.1 -6.35) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 17 20) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 29 LE))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 40 D5))
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 39 BE) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 120.1928 39.6494)
    (fp_text reference SW7 (at 3.2512 6.3246) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 42 BF) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 60 "Net-(R12-Pad2)"))
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 9 11) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 120.1928 79.9592)
    (fp_text reference SW8 (at -0.1 -6.35) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 43 BD) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 61 "Net-(R13-Pad2)"))
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 9 11) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 112.2426 115.7732)
    (fp_text reference SW9 (at -0.1 -6.35) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 43 BD) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 40 D5))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 LD))
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 17 20) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 112.2426 130.793066)
    (fp_text reference SW10 (at -0.1 -6.35) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 44 BC) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 40 D5))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 25 LC))
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 17 20) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 112.2426 145.812932)
    (fp_text reference SW11 (at -0.1 -6.35) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 45 BB) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 40 D5))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 24 LB))
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 17 20) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 112.2426 160.8328)
    (fp_text reference SW12 (at -0.1 -6.35) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 46 BA) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 40 D5))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 21 LA))
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 17 20) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
  )
  (module Package_SO:SOIC-16_3.9x9.9mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 111.76 91.948 270)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 -6 270) (layer F.SilkS))
    (fp_text value 74HC595 (at 0 6 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 16 smd rect (at 2.7 -4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 15 smd rect (at 2.7 -3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 46 BA))
    (pad 14 smd rect (at 2.7 -1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 SER))
    (pad 13 smd rect (at 2.7 -0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 OE))
    (pad 12 smd rect (at 2.7 0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 RCLK))
    (pad 11 smd rect (at 2.7 1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 SRCLK))
    (pad 10 smd rect (at 2.7 3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 9 smd rect (at 2.7 4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U1-Pad9)"))
    (pad 8 smd rect (at -2.7 4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -2.7 3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 BH))
    (pad 6 smd rect (at -2.7 1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 BG))
    (pad 5 smd rect (at -2.7 0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 BF))
    (pad 4 smd rect (at -2.7 -0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 BE))
    (pad 3 smd rect (at -2.7 -1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 BD))
    (pad 2 smd rect (at -2.7 -3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 BC))
    (pad 1 smd rect (at -2.7 -4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 BB))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-16_3.9x9.9mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 112.522 67.564 270)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at 0 -6 270) (layer F.SilkS))
    (fp_text value 74HC595 (at 0 6 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R3-Pad2)"))
    (pad 2 smd rect (at -2.7 -3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R4-Pad2)"))
    (pad 3 smd rect (at -2.7 -1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R5-Pad2)"))
    (pad 4 smd rect (at -2.7 -0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R6-Pad2)"))
    (pad 5 smd rect (at -2.7 0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R7-Pad2)"))
    (pad 6 smd rect (at -2.7 1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R8-Pad2)"))
    (pad 7 smd rect (at -2.7 3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R9-Pad2)"))
    (pad 8 smd rect (at -2.7 4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 2.7 4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U2-Pad9)"))
    (pad 10 smd rect (at 2.7 3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 11 smd rect (at 2.7 1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 SRCLK))
    (pad 12 smd rect (at 2.7 0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 RCLK))
    (pad 13 smd rect (at 2.7 -0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 OE))
    (pad 14 smd rect (at 2.7 -1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U1-Pad9)"))
    (pad 15 smd rect (at 2.7 -3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R2-Pad2)"))
    (pad 16 smd rect (at 2.7 -4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 105.156 43.18 90)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U3 (at 0 -7.5 90) (layer F.SilkS))
    (fp_text value TPIC6595 (at 0 7.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -4.7 -5.715 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(U3-Pad1)"))
    (pad 2 smd rect (at -4.7 -4.445 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 3 smd rect (at -4.7 -3.175 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U2-Pad9)"))
    (pad 4 smd rect (at -4.7 -1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 D0))
    (pad 5 smd rect (at -4.7 -0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 D1))
    (pad 6 smd rect (at -4.7 0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 52 D2))
    (pad 7 smd rect (at -4.7 1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 53 D3))
    (pad 8 smd rect (at -4.7 3.175 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 9 smd rect (at -4.7 4.445 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 OE))
    (pad 10 smd rect (at -4.7 5.715 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 4.7 5.715 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd rect (at 4.7 4.445 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 RCLK))
    (pad 13 smd rect (at 4.7 3.175 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 SRCLK))
    (pad 14 smd rect (at 4.7 1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 54 D4))
    (pad 15 smd rect (at 4.7 0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 D5))
    (pad 16 smd rect (at 4.7 -0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 D6))
    (pad 17 smd rect (at 4.7 -1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 55 D7))
    (pad 18 smd rect (at 4.7 -3.175 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U3-Pad18)"))
    (pad 19 smd rect (at 4.7 -4.445 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 20 smd rect (at 4.7 -5.715 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(U3-Pad20)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-20W_7.5x12.8mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5CF08A7E)
    (at 88.265 153.67)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module AOR_custom:AOR_LOGO (layer B.Cu) (tedit 5C26ADAA)
    (at 104.394 148.336 270)
    (fp_text reference G*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value AOR_LOGO (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 95.25 49.022 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 0 -1.82 180) (layer F.SilkS))
    (fp_text value R_US (at 0 1.82 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 VCC))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 58 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 87.376 89.408 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value R_US (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 59 "Net-(R11-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 115.062 48.006)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R_US (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 60 "Net-(R12-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 120.396 70.866)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R_US (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 VCC))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 61 "Net-(R13-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "ACP3-W-PR1-PCB\nREV A, 5-30-2019" (at 121.666 124.46 90) (layer F.SilkS))
  (gr_text "ACP3-W-PR1-PCB\nREV A, 5-30-2019" (at 104.394 130.81 90) (layer B.SilkS))
  (gr_text GND (at 94.742 98.806) (layer B.SilkS))
  (gr_text GND (at 91.186 98.806) (layer B.SilkS))
  (gr_text GND (at 87.884 98.806) (layer B.SilkS))
  (gr_text 5V (at 94.996 107.442) (layer B.SilkS))
  (gr_text 5V (at 91.44 107.442) (layer B.SilkS))
  (gr_text 5V (at 87.884 107.442) (layer B.SilkS))
  (gr_text "PIN 12 HIGH" (at 90.17 86.614 90) (layer B.SilkS))
  (gr_line (start 84.455 167.005) (end 126.365 167.005) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 84.455 33.655) (end 84.455 167.005) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 126.365 33.655) (end 126.365 167.005) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 84.455 33.655) (end 126.365 33.655) (layer Edge.Cuts) (width 0.2))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 84.455 33.655) (xy 126.365 33.655) (xy 126.365 167.005) (xy 84.455 167.005)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 84.455 33.655) (xy 126.365 33.655) (xy 126.365 167.005) (xy 84.455 167.005)
      )
    )
  )
)
