(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 25)
    (tracks 149)
    (zones 0)
    (modules 3)
    (nets 37)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.762)
    (via_drill 0.4064)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad18)")
  (net 2 "Net-(J1-Pad17)")
  (net 3 "Net-(J1-Pad16)")
  (net 4 "Net-(J1-Pad15)")
  (net 5 "Net-(J1-Pad14)")
  (net 6 "Net-(J1-Pad13)")
  (net 7 "Net-(J1-Pad12)")
  (net 8 "Net-(J1-Pad11)")
  (net 9 "Net-(J1-Pad10)")
  (net 10 "Net-(J1-Pad9)")
  (net 11 "Net-(J1-Pad8)")
  (net 12 "Net-(J1-Pad7)")
  (net 13 "Net-(J1-Pad6)")
  (net 14 "Net-(J1-Pad5)")
  (net 15 "Net-(J1-Pad4)")
  (net 16 "Net-(J1-Pad3)")
  (net 17 "Net-(J1-Pad2)")
  (net 18 "Net-(J1-Pad1)")
  (net 19 "Net-(J2-Pad1)")
  (net 20 "Net-(J2-Pad2)")
  (net 21 "Net-(J2-Pad3)")
  (net 22 "Net-(J2-Pad4)")
  (net 23 "Net-(J2-Pad5)")
  (net 24 "Net-(J2-Pad6)")
  (net 25 "Net-(J2-Pad7)")
  (net 26 "Net-(J2-Pad8)")
  (net 27 "Net-(J2-Pad9)")
  (net 28 "Net-(J2-Pad10)")
  (net 29 "Net-(J2-Pad11)")
  (net 30 "Net-(J2-Pad12)")
  (net 31 "Net-(J2-Pad13)")
  (net 32 "Net-(J2-Pad14)")
  (net 33 "Net-(J2-Pad15)")
  (net 34 "Net-(J2-Pad16)")
  (net 35 "Net-(J2-Pad17)")
  (net 36 "Net-(J2-Pad18)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.762)
    (via_drill 0.4064)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad14)")
    (add_net "Net-(J2-Pad15)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad17)")
    (add_net "Net-(J2-Pad18)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J2-Pad9)")
  )
  (module NRFmodules:NRF5xmodule (layer F.Cu) (tedit 5B97477C)
    (at 148.84 105.735001)
    (descr "Through hole straight pin header, 2x09, 2.00mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.00mm double row")
    (fp_text reference U1 (at 2.5 -19.9) (layer F.SilkS))
    (fp_text value NRF51822 (at 9.1226 -0.960001) (layer F.Fab))
    (pad 18 thru_hole oval (at 1.5 -17.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad18)"))
    (pad 17 thru_hole oval (at 3.5 -17.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad17)"))
    (pad 16 thru_hole oval (at 1.5 -15.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad16)"))
    (pad 15 thru_hole oval (at 3.5 -15.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad15)"))
    (pad 14 thru_hole oval (at 1.5 -13.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad14)"))
    (pad 13 thru_hole oval (at 3.5 -13.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad13)"))
    (pad 12 thru_hole oval (at 1.5 -11.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad12)"))
    (pad 11 thru_hole oval (at 3.5 -11.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad11)"))
    (pad 10 thru_hole oval (at 1.5 -9.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad10)"))
    (pad 9 thru_hole oval (at 3.5 -9.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad9)"))
    (pad 8 thru_hole oval (at 1.5 -7.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad8)"))
    (pad 7 thru_hole oval (at 3.5 -7.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 1.5 -5.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 3.5 -5.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at 1.5 -3.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 3.5 -3.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 1.5 -1.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 3.5 -1.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad1)"))
    (pad 20 thru_hole oval (at 21.48 -1.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad2)"))
    (pad 24 thru_hole oval (at 21.48 -5.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad6)"))
    (pad 19 thru_hole rect (at 23.48 -1.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad1)"))
    (pad 31 thru_hole oval (at 23.48 -13.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(J2-Pad13)"))
    (pad 26 thru_hole oval (at 21.48 -7.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(J2-Pad8)"))
    (pad 35 thru_hole oval (at 23.48 -17.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad17)"))
    (pad 33 thru_hole oval (at 23.48 -15.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(J2-Pad15)"))
    (pad 25 thru_hole oval (at 23.48 -7.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad7)"))
    (pad 32 thru_hole oval (at 21.48 -13.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad14)"))
    (pad 34 thru_hole oval (at 21.48 -15.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(J2-Pad16)"))
    (pad 30 thru_hole oval (at 21.48 -11.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad12)"))
    (pad 29 thru_hole oval (at 23.48 -11.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad11)"))
    (pad 27 thru_hole oval (at 23.48 -9.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(J2-Pad9)"))
    (pad 36 thru_hole oval (at 21.48 -17.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(J2-Pad18)"))
    (pad 28 thru_hole oval (at 21.48 -9.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad10)"))
    (pad 23 thru_hole oval (at 23.48 -5.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad5)"))
    (pad 22 thru_hole oval (at 21.48 -3.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad4)"))
    (pad 21 thru_hole oval (at 23.48 -3.5 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad3)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x09_Pitch2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x09_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 144.78 104.14 180)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference J1 (at -2.8702 -0.2032 180) (layer F.SilkS))
    (fp_text value Conn_02x09_Odd_Even (at 1.27 22.65 180) (layer F.Fab))
    (fp_text user %R (at 1.27 10.16 270) (layer F.Fab))
    (pad 18 thru_hole oval (at 2.54 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad18)"))
    (pad 17 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad17)"))
    (pad 16 thru_hole oval (at 2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad16)"))
    (pad 15 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad15)"))
    (pad 14 thru_hole oval (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad14)"))
    (pad 13 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad13)"))
    (pad 12 thru_hole oval (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad12)"))
    (pad 11 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad11)"))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad10)"))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad9)"))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad8)"))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x09_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x09_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 180.34 104.14 180)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference J2 (at 5.3086 -0.4318 180) (layer F.SilkS))
    (fp_text value Conn_02x09_Odd_Even (at 1.27 22.65 180) (layer F.Fab))
    (fp_text user %R (at 1.27 10.16 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J2-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J2-Pad9)"))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad11)"))
    (pad 12 thru_hole oval (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J2-Pad13)"))
    (pad 14 thru_hole oval (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad14)"))
    (pad 15 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J2-Pad15)"))
    (pad 16 thru_hole oval (at 2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J2-Pad16)"))
    (pad 17 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad17)"))
    (pad 18 thru_hole oval (at 2.54 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J2-Pad18)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x09_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 182.9308 106.6546) (end 139.5222 106.6546) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.9308 79.4512) (end 182.9308 106.6546) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.5222 79.4512) (end 182.9562 79.4512) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.5222 106.6546) (end 139.5222 79.4512) (layer Edge.Cuts) (width 0.1))
  (gr_text "Adapter for NRF5x HolyIoT\n2mm to 2.54mm\n" (at 161.7726 82.4484) (layer B.SilkS))
  (gr_text "VDD GND  P09 P10" (at 161.5186 104.3178) (layer B.SilkS))
  (gr_text "P12 P11  P07 P08" (at 161.5186 102.1842) (layer B.SilkS))
  (gr_text "P14 P13  P05 P06" (at 161.5948 100.2538) (layer B.SilkS))
  (gr_text "P16 P15  P03 P04" (at 161.5186 98.2218) (layer B.SilkS))
  (gr_text "P18 P17  P01 P02" (at 161.5186 96.1136) (layer B.SilkS))
  (gr_text "P20 P19  P31 P00" (at 161.544 94.107) (layer B.SilkS))
  (gr_text "SCLK P21 P29 P30" (at 161.4932 92.1512) (layer B.SilkS))
  (gr_text "P22 SDO  P27 P28" (at 161.3916 90.1954) (layer B.SilkS))
  (gr_text "P24 P23  P25 P26" (at 161.4424 88.1634) (layer B.SilkS))
  (gr_text NRF52832 (at 161.1376 85.852) (layer B.SilkS))
  (gr_text NRF51822 (at 157.3784 85.8774) (layer F.SilkS))
  (gr_text "P03 P04  P05 P06" (at 154.2288 104.3178) (layer F.SilkS))
  (gr_text "P01 P02  P07 P08" (at 154.2288 102.3874) (layer F.SilkS))
  (gr_text "P30 P00  P09 P10" (at 154.2288 100.3554) (layer F.SilkS))
  (gr_text "VDD GND  P11 P12" (at 154.2288 98.2726) (layer F.SilkS))
  (gr_text "P28 P29  P13 P14" (at 154.2288 96.2406) (layer F.SilkS))
  (gr_text "NC  NC   P15 P16" (at 154.2288 94.361) (layer F.SilkS))
  (gr_text "P24 P25 SDO SCLK" (at 154.2288 92.4306) (layer F.SilkS))
  (gr_text "P22 P23  P17 P19" (at 154.2288 90.2208) (layer F.SilkS))
  (gr_text "GND P21  P18 P20" (at 154.2288 88.1634) (layer F.SilkS))
)
