(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 128)
    (no_connects 0)
    (area 75.588999 72.426759 199.889001 95.467001)
    (thickness 1.6)
    (drawings 56)
    (tracks 753)
    (zones 0)
    (modules 37)
    (nets 84)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.03)
    (pcb_text_size 0.635 0.635)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(ANT1-Pad1)")
  (net 2 GND)
  (net 3 3v3)
  (net 4 ARFF)
  (net 5 VBAT)
  (net 6 VBUS)
  (net 7 "Net-(D2-Pad1)")
  (net 8 "Net-(D3-Pad2)")
  (net 9 "Net-(D4-Pad2)")
  (net 10 /1)
  (net 11 /0)
  (net 12 /MISO)
  (net 13 /MOSI)
  (net 14 /SCK)
  (net 15 /A5)
  (net 16 /A4)
  (net 17 /A3)
  (net 18 /A2)
  (net 19 /A1)
  (net 20 /A0)
  (net 21 RST)
  (net 22 /6)
  (net 23 /TEST1)
  (net 24 /TEST0)
  (net 25 "Net-(JP2-Pad6)")
  (net 26 /EN)
  (net 27 /13)
  (net 28 /12)
  (net 29 /11)
  (net 30 /10)
  (net 31 9)
  (net 32 /5)
  (net 33 /3)
  (net 34 /2)
  (net 35 "Net-(P1-Pad2)")
  (net 36 "Net-(P1-Pad3)")
  (net 37 "Net-(P1-Pad4)")
  (net 38 "Net-(P1-Pad6)")
  (net 39 "Net-(R1-Pad1)")
  (net 40 "Net-(R2-Pad1)")
  (net 41 "Net-(R4-Pad1)")
  (net 42 "Net-(R5-Pad2)")
  (net 43 "Net-(R8-Pad1)")
  (net 44 "Net-(U1-Pad2)")
  (net 45 "Net-(U1-Pad4)")
  (net 46 "Net-(U1-Pad5)")
  (net 47 "Net-(U1-Pad6)")
  (net 48 "Net-(U1-Pad7)")
  (net 49 "Net-(U1-Pad11)")
  (net 50 "Net-(U1-Pad13)")
  (net 51 "Net-(U1-Pad14)")
  (net 52 "Net-(U1-Pad15)")
  (net 53 "Net-(U1-Pad16)")
  (net 54 "Net-(U1-Pad17)")
  (net 55 "Net-(U1-Pad18)")
  (net 56 "Net-(U1-Pad20)")
  (net 57 /D7)
  (net 58 "Net-(U2-Pad2)")
  (net 59 "Net-(U2-Pad8)")
  (net 60 "Net-(U2-Pad22)")
  (net 61 /D4)
  (net 62 /D8)
  (net 63 "Net-(U3-Pad2)")
  (net 64 "Net-(U3-Pad3)")
  (net 65 "Net-(U3-Pad4)")
  (net 66 "Net-(U3-Pad5)")
  (net 67 "Net-(U3-Pad9)")
  (net 68 "Net-(U3-Pad10)")
  (net 69 "Net-(U3-Pad13)")
  (net 70 "Net-(U3-Pad35)")
  (net 71 "Net-(U3-Pad36)")
  (net 72 "Net-(U3-Pad37)")
  (net 73 "Net-(U3-Pad38)")
  (net 74 "Net-(U3-Pad39)")
  (net 75 "Net-(U3-Pad40)")
  (net 76 "Net-(U3-Pad43)")
  (net 77 "Net-(U3-Pad44)")
  (net 78 "Net-(U3-Pad45)")
  (net 79 "Net-(U3-Pad46)")
  (net 80 "Net-(U4-Pad5)")
  (net 81 "Net-(U1-Pad8)")
  (net 82 "Net-(8MHz1-Pad1)")
  (net 83 "Net-(8MHz1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /0)
    (add_net /1)
    (add_net /10)
    (add_net /11)
    (add_net /12)
    (add_net /13)
    (add_net /2)
    (add_net /3)
    (add_net /5)
    (add_net /6)
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /D4)
    (add_net /D7)
    (add_net /D8)
    (add_net /EN)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /SCK)
    (add_net /TEST0)
    (add_net /TEST1)
    (add_net 3v3)
    (add_net 9)
    (add_net ARFF)
    (add_net GND)
    (add_net "Net-(8MHz1-Pad1)")
    (add_net "Net-(8MHz1-Pad2)")
    (add_net "Net-(ANT1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(JP2-Pad6)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad22)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U3-Pad10)")
    (add_net "Net-(U3-Pad13)")
    (add_net "Net-(U3-Pad2)")
    (add_net "Net-(U3-Pad3)")
    (add_net "Net-(U3-Pad35)")
    (add_net "Net-(U3-Pad36)")
    (add_net "Net-(U3-Pad37)")
    (add_net "Net-(U3-Pad38)")
    (add_net "Net-(U3-Pad39)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U3-Pad40)")
    (add_net "Net-(U3-Pad43)")
    (add_net "Net-(U3-Pad44)")
    (add_net "Net-(U3-Pad45)")
    (add_net "Net-(U3-Pad46)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U3-Pad9)")
    (add_net "Net-(U4-Pad5)")
    (add_net RST)
    (add_net VBAT)
    (add_net VBUS)
  )
  (module misc:Mounting-Hole (layer F.Cu) (tedit 58759305)
    (at 196.596 75.438)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference REF** (at 117.348 42.672) (layer F.SilkS))
    (fp_text value Measurement_Point_Round-SMD-Pad_Big (at -27.432 14.986) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module misc:Mounting-Hole (layer F.Cu) (tedit 587592FF)
    (at 196.596 92.456)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference REF** (at 124.206 8.382) (layer F.SilkS))
    (fp_text value Measurement_Point_Round-SMD-Pad_Big (at 126.492 16.51) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module misc:CON-SMA-EDGE (layer F.Cu) (tedit 58758C49)
    (at 197.554 83.902 270)
    (fp_text reference ANT1 (at -4.908 0.45 360) (layer F.SilkS))
    (fp_text value CON-SMA (at 0.172 4.26 270) (layer F.SilkS))
    (pad 1 smd rect (at 0 0 270) (size 1.524 4.064) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(ANT1-Pad1)"))
    (pad 2 smd rect (at -2.54 0 270) (size 1.524 4.064) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.54 0 270) (size 1.524 4.064) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -2.54 0 270) (size 1.524 4.064) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2.54 0 270) (size 1.524 4.064) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x16 (layer F.Cu) (tedit 58758912)
    (at 144.87652 93.83776 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP1 (at -0.36576 -2.44348 270) (layer F.SilkS))
    (fp_text value CONN_01X16 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 /1))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 /0))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 /MISO))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 /MOSI))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 /SCK))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 /A5))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 /A4))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 /A3))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 /A2))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 /A1))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /A0))
    (pad 13 thru_hole oval (at 0 30.48 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 14 thru_hole oval (at 0 33.02 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 ARFF))
    (pad 15 thru_hole oval (at 0 35.56 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 3v3))
    (pad 16 thru_hole oval (at 0 38.1 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 RST))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x16.wrl
      (at (xyz 0 -0.75 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module adafruit:adafruit-1X06 (layer F.Cu) (tedit 58759313)
    (at 154.104 83.702 270)
    (descr "PIN HEADER")
    (tags "PIN HEADER")
    (attr virtual)
    (fp_text reference JP2 (at 36.44 -171.27 270) (layer B.SilkS))
    (fp_text value PINHD-1X6 (at 22.724 -164.412 360) (layer B.SilkS))
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 3.048) (drill 1.016) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 22 /6))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 3.048) (drill 1.016) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 3 3v3))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 3.048) (drill 1.016) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 3.048) (drill 1.016) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 23 /TEST1))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 3.048) (drill 1.016) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 24 /TEST0))
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 3.048) (drill 1.016) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 25 "Net-(JP2-Pad6)"))
  )
  (module open-project:SW_PUSH_SMD (layer F.Cu) (tedit 58758A70)
    (at 90.854 92.102 180)
    (fp_text reference SW1 (at -6.428 -1.116 180) (layer F.SilkS))
    (fp_text value SPST (at -0.078 -0.608 180) (layer F.SilkS))
    (pad 1 smd rect (at -3.99796 -2.2479 180) (size 1.5494 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 21 RST))
    (pad 1 smd rect (at 3.99796 -2.2479 180) (size 1.5494 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 21 RST))
    (pad 2 smd rect (at 3.99796 2.2479 180) (size 1.5494 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -3.99796 2.2479 180) (size 1.5494 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module FGPMMOPA6H:FGPMMOPA6H (layer F.Cu) (tedit 50BDFD05)
    (at 104.648 82.042 90)
    (fp_text reference U1 (at -1.00076 8.99922 90) (layer F.SilkS))
    (fp_text value FGPMMOPA6H (at 0 -8.99922 90) (layer F.SilkS))
    (fp_text user 1 (at -5.3848 -6.5024 90) (layer F.SilkS))
    (pad 1 smd rect (at -8.001 -6.74878 90) (size 1.99898 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 3 3v3))
    (pad 2 smd rect (at -8.001 -5.25018 90) (size 1.99898 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(U1-Pad2)"))
    (pad 3 smd rect (at -8.001 -3.74904 90) (size 1.99898 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -8.001 -2.25044 90) (size 1.99898 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(U1-Pad4)"))
    (pad 5 smd rect (at -8.001 -0.7493 90) (size 1.99898 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at -8.001 0.7493 90) (size 1.99898 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U1-Pad6)"))
    (pad 7 smd rect (at -8.001 2.25044 90) (size 1.99898 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U1-Pad7)"))
    (pad 8 smd rect (at -8.001 3.74904 90) (size 1.99898 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(U1-Pad8)"))
    (pad 9 smd rect (at -8.001 5.25018 90) (size 1.99898 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 11 /0))
    (pad 10 smd rect (at -8.001 6.74878 90) (size 1.99898 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 10 /1))
    (pad 11 smd rect (at 8.001 6.74878 90) (size 1.99898 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(U1-Pad11)"))
    (pad 12 smd rect (at 8.001 5.25018 90) (size 1.99898 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 13 smd rect (at 8.001 3.74904 90) (size 1.99898 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(U1-Pad13)"))
    (pad 14 smd rect (at 8.001 2.25044 90) (size 1.99898 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U1-Pad14)"))
    (pad 15 smd rect (at 8.001 0.7493 90) (size 1.99898 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U1-Pad15)"))
    (pad 16 smd rect (at 8.001 -0.7493 90) (size 1.99898 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(U1-Pad16)"))
    (pad 17 smd rect (at 8.001 -2.25044 90) (size 1.99898 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(U1-Pad17)"))
    (pad 18 smd rect (at 8.001 -3.74904 90) (size 1.99898 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(U1-Pad18)"))
    (pad 19 smd rect (at 8.001 -5.25018 90) (size 1.99898 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 20 smd rect (at 8.001 -6.74878 90) (size 1.99898 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U1-Pad20)"))
  )
  (module Housings_QFP:TQFP-44_10x10mm_Pitch0.8mm (layer F.Cu) (tedit 54130A77)
    (at 134.112 84.074 90)
    (descr "44-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1.0 mm Body [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U2 (at 0 -7.45 90) (layer F.SilkS))
    (fp_text value ATmega32U4-AU (at 0 7.45 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -5.7 -4 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 57 /D7))
    (pad 2 smd rect (at -5.7 -3.2 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(U2-Pad2)"))
    (pad 3 smd rect (at -5.7 -2.4 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R2-Pad1)"))
    (pad 4 smd rect (at -5.7 -1.6 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R1-Pad1)"))
    (pad 5 smd rect (at -5.7 -0.8 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -5.7 0 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 3v3))
    (pad 7 smd rect (at -5.7 0.8 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 VBUS))
    (pad 8 smd rect (at -5.7 1.6 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(U2-Pad8)"))
    (pad 9 smd rect (at -5.7 2.4 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 /SCK))
    (pad 10 smd rect (at -5.7 3.2 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 13 /MOSI))
    (pad 11 smd rect (at -5.7 4 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 /MISO))
    (pad 12 smd rect (at -4 5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 29 /11))
    (pad 13 smd rect (at -3.2 5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 21 RST))
    (pad 14 smd rect (at -2.4 5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 3v3))
    (pad 15 smd rect (at -1.6 5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 16 smd rect (at -0.8 5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(8MHz1-Pad2)"))
    (pad 17 smd rect (at 0 5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(8MHz1-Pad1)"))
    (pad 18 smd rect (at 0.8 5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 33 /3))
    (pad 19 smd rect (at 1.6 5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 34 /2))
    (pad 20 smd rect (at 2.4 5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 /0))
    (pad 21 smd rect (at 3.2 5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 /1))
    (pad 22 smd rect (at 4 5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(U2-Pad22)"))
    (pad 23 smd rect (at 5.7 4 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 24 smd rect (at 5.7 3.2 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 3v3))
    (pad 25 smd rect (at 5.7 2.4 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 61 /D4))
    (pad 26 smd rect (at 5.7 1.6 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 28 /12))
    (pad 27 smd rect (at 5.7 0.8 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 22 /6))
    (pad 28 smd rect (at 5.7 0 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 62 /D8))
    (pad 29 smd rect (at 5.7 -0.8 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 31 9))
    (pad 30 smd rect (at 5.7 -1.6 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 30 /10))
    (pad 31 smd rect (at 5.7 -2.4 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 32 /5))
    (pad 32 smd rect (at 5.7 -3.2 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 27 /13))
    (pad 33 smd rect (at 5.7 -4 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 3v3))
    (pad 34 smd rect (at 4 -5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 3v3))
    (pad 35 smd rect (at 3.2 -5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 36 smd rect (at 2.4 -5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 20 /A0))
    (pad 37 smd rect (at 1.6 -5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 19 /A1))
    (pad 38 smd rect (at 0.8 -5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 /A2))
    (pad 39 smd rect (at 0 -5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 /A3))
    (pad 40 smd rect (at -0.8 -5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 /A4))
    (pad 41 smd rect (at -1.6 -5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 /A5))
    (pad 42 smd rect (at -2.4 -5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 ARFF))
    (pad 43 smd rect (at -3.2 -5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 44 smd rect (at -4 -5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 3v3))
    (model Housings_QFP.3dshapes/TQFP-44_10x10mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RN2903-I_RM095:XCVR_RN2903-I%2fRM095 (layer F.Cu) (tedit 58758C52)
    (at 170.5864 83.6422 270)
    (solder_mask_margin 0.1)
    (attr smd)
    (fp_text reference U3 (at -0.0762 -0.6096 270) (layer F.SilkS))
    (fp_text value RN2903-I/RM095 (at -1.0922 14.3764 270) (layer F.SilkS))
    (pad 1 smd rect (at 8.89 12.065) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.2))
    (pad 2 smd rect (at 8.89 10.795) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(U3-Pad2)") (solder_mask_margin 0.2))
    (pad 3 smd rect (at 8.89 9.525) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(U3-Pad3)") (solder_mask_margin 0.2))
    (pad 4 smd rect (at 8.89 8.255) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(U3-Pad4)") (solder_mask_margin 0.2))
    (pad 5 smd rect (at 8.89 6.985) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(U3-Pad5)") (solder_mask_margin 0.2))
    (pad 6 smd rect (at 8.89 5.715) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 30 /10) (solder_mask_margin 0.2))
    (pad 7 smd rect (at 8.89 4.445) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 32 /5) (solder_mask_margin 0.2))
    (pad 8 smd rect (at 8.89 3.175) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.2))
    (pad 9 smd rect (at 8.89 1.905) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(U3-Pad9)") (solder_mask_margin 0.2))
    (pad 10 smd rect (at 8.89 0.635) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(U3-Pad10)") (solder_mask_margin 0.2))
    (pad 11 smd rect (at 8.89 -0.635) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.2))
    (pad 12 smd rect (at 8.89 -1.905) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 3 3v3) (solder_mask_margin 0.2))
    (pad 13 smd rect (at 8.89 -3.175) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(U3-Pad13)") (solder_mask_margin 0.2))
    (pad 14 smd rect (at 8.89 -4.445) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R8-Pad1)") (solder_mask_margin 0.2))
    (pad 15 smd rect (at 8.89 -5.715) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.2))
    (pad 16 smd rect (at 8.89 -6.985) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.2))
    (pad 17 smd rect (at 8.89 -8.255) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.2))
    (pad 18 smd rect (at 8.89 -9.525) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.2))
    (pad 19 smd rect (at 8.89 -10.795) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.2))
    (pad 20 smd rect (at 8.89 -12.065) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.2))
    (pad 21 smd rect (at 3.81 -13.335 90) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.2))
    (pad 22 smd rect (at 2.54 -13.335 90) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.2))
    (pad 23 smd rect (at 1.27 -13.335 90) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(ANT1-Pad1)") (solder_mask_margin 0.2))
    (pad 24 smd rect (at 0 -13.335 90) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.2))
    (pad 25 smd rect (at -1.27 -13.335 90) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.2))
    (pad 26 smd rect (at -2.54 -13.335 90) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.2))
    (pad 27 smd rect (at -3.81 -13.335 90) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.2))
    (pad 28 smd rect (at -8.89 -12.065 180) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.2))
    (pad 29 smd rect (at -8.89 -10.795 180) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.2))
    (pad 30 smd rect (at -8.89 -9.525 180) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 24 /TEST0) (solder_mask_margin 0.2))
    (pad 31 smd rect (at -8.89 -8.255 180) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 23 /TEST1) (solder_mask_margin 0.2))
    (pad 32 smd rect (at -8.89 -6.985 180) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 22 /6) (solder_mask_margin 0.2))
    (pad 33 smd rect (at -8.89 -5.715 180) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.2))
    (pad 34 smd rect (at -8.89 -4.445 180) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 3 3v3) (solder_mask_margin 0.2))
    (pad 35 smd rect (at -8.89 -3.175 180) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(U3-Pad35)") (solder_mask_margin 0.2))
    (pad 36 smd rect (at -8.89 -1.905 180) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(U3-Pad36)") (solder_mask_margin 0.2))
    (pad 37 smd rect (at -8.89 -0.635 180) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(U3-Pad37)") (solder_mask_margin 0.2))
    (pad 38 smd rect (at -8.89 0.635 180) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(U3-Pad38)") (solder_mask_margin 0.2))
    (pad 39 smd rect (at -8.89 1.905 180) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(U3-Pad39)") (solder_mask_margin 0.2))
    (pad 40 smd rect (at -8.89 3.175 180) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(U3-Pad40)") (solder_mask_margin 0.2))
    (pad 41 smd rect (at -8.89 4.445 180) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.2))
    (pad 42 smd rect (at -8.89 5.715 180) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.2))
    (pad 43 smd rect (at -8.89 6.985 180) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(U3-Pad43)") (solder_mask_margin 0.2))
    (pad 44 smd rect (at -8.89 8.255 180) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U3-Pad44)") (solder_mask_margin 0.2))
    (pad 45 smd rect (at -8.89 9.525 180) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U3-Pad45)") (solder_mask_margin 0.2))
    (pad 46 smd rect (at -8.89 10.795 180) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(U3-Pad46)") (solder_mask_margin 0.2))
    (pad 47 smd rect (at -8.89 12.065 180) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.2))
  )
  (module Connect:USB_Mini-B (layer F.Cu) (tedit 58759303)
    (at 80.654 84.102)
    (descr "USB Mini-B 5-pin SMD connector")
    (tags "USB USB_B USB_Mini connector")
    (attr smd)
    (fp_text reference P1 (at 234.56 36.294) (layer F.SilkS) hide)
    (fp_text value USB_OTG (at 0 -7.0993) (layer F.Fab))
    (pad 1 smd rect (at 3.44932 -1.6002) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 6 VBUS))
    (pad 2 smd rect (at 3.44932 -0.8001) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(P1-Pad2)"))
    (pad 3 smd rect (at 3.44932 0) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(P1-Pad3)"))
    (pad 4 smd rect (at 3.44932 0.8001) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(P1-Pad4)"))
    (pad 5 smd rect (at 3.44932 1.6002) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 3.35026 -4.45008) (size 2.49936 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(P1-Pad6)"))
    (pad 6 smd rect (at -2.14884 -4.45008) (size 2.49936 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(P1-Pad6)"))
    (pad 6 smd rect (at 3.35026 4.45008) (size 2.49936 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(P1-Pad6)"))
    (pad 6 smd rect (at -2.14884 4.45008) (size 2.49936 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(P1-Pad6)"))
    (pad "" np_thru_hole circle (at 0.8509 -2.19964) (size 0.89916 0.89916) (drill 0.89916) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.8509 2.19964) (size 0.89916 0.89916) (drill 0.89916) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58642191)
    (at 119.888 85.344 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 3v3))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 541A9B4D)
    (at 147.066 84.582 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 -1.9 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 3v3))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58642199)
    (at 122.428 85.344 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 1uF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 ARFF))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58758B1C)
    (at 81.788 76.962 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0 -1.27 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 VBAT))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 587589D4)
    (at 92.71 82.55 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 2.286 -1.016 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 3v3))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module adafruit:adafruit-JST-PH-2-SMT (layer F.Cu) (tedit 5875936B)
    (at 90.854 77.302 180)
    (attr smd)
    (fp_text reference CN1 (at 0.635 -4.445 180) (layer B.SilkS))
    (fp_text value JST_2PIN-SMT (at -225.376 -52.746 180) (layer B.SilkS))
    (fp_text user + (at -220.042 -48.682 180) (layer B.SilkS))
    (fp_text user - (at -225.122 -48.936 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.99822 1.79832 180) (size 0.99822 5.4991) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.99822 1.79832 180) (size 0.99822 5.4991) (layers F.Cu F.Paste F.Mask)
      (net 5 VBAT))
    (pad NC1 smd rect (at -3.39852 0 180) (size 3.39852 1.59766) (layers F.Cu F.Paste F.Mask))
    (pad NC2 smd rect (at 3.39852 0 180) (size 3.39852 1.59766) (layers F.Cu F.Paste F.Mask))
  )
  (module Diodes_SMD:D_0805 (layer F.Cu) (tedit 58758D1E)
    (at 117.602 79.248 270)
    (descr "Diode SMD in 0805 package")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D1 (at 0.762 -1.27 270) (layer F.SilkS))
    (fp_text value DIODESCH (at 0 -1.6 270) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 270) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 VBAT))
    (pad 2 smd rect (at 1.05 0 270) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 VBUS))
  )
  (module Diodes_SMD:D_0805 (layer F.Cu) (tedit 5875930C)
    (at 77.47 73.406)
    (descr "Diode SMD in 0805 package")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D2 (at 244.348 29.21) (layer F.SilkS) hide)
    (fp_text value LED-BAT (at 235.458 29.21) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 1.05 0) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 VBUS))
  )
  (module Diodes_SMD:D_0805 (layer F.Cu) (tedit 587588E7)
    (at 191.516 94.234)
    (descr "Diode SMD in 0805 package")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D3 (at -0.254 3.048) (layer F.SilkS) hide)
    (fp_text value LED-RED (at 0 -1.6) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.05 0) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D3-Pad2)"))
  )
  (module Diodes_SMD:D_0805 (layer F.Cu) (tedit 58759312)
    (at 83.312 93.98 180)
    (descr "Diode SMD in 0805 package")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D4 (at -226.06 -23.622 180) (layer F.SilkS) hide)
    (fp_text value LED-POW (at 0 -1.6 180) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 180) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.05 0 180) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D4-Pad2)"))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5875930F)
    (at 89.154 87.122 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -230.632 -25.146 180) (layer F.SilkS))
    (fp_text value 22 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(P1-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58758A55)
    (at 89.154 85.344 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -2.54 -1.778 180) (layer F.SilkS))
    (fp_text value 22 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(P1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5864205B)
    (at 120.65 77.724)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 100k (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 /EN))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 VBUS))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5875930A)
    (at 77.47 77.47 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -233.68 -22.352 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5864212C)
    (at 77.47 75.184)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R5-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58758D2D)
    (at 114.554 79.248 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -1.016 1.27 90) (layer F.SilkS))
    (fp_text value 100k (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 9))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 VBAT))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58307AEF)
    (at 147.066 80.264 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 0 -1.9 90) (layer F.SilkS))
    (fp_text value 100k (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 9))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 587588DD)
    (at 191.77 91.694)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at -0.254 -1.27) (layer F.SilkS))
    (fp_text value 1k (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R8-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5875930D)
    (at 83.566 91.694 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at -224.79 -22.098 180) (layer F.SilkS) hide)
    (fp_text value 1k (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 3v3))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5864219C)
    (at 117.602 83.82 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.9 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 VBUS))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module misc:SPX3819 (layer F.Cu) (tedit 5863EF37)
    (at 88.654 82.502 270)
    (descr "SMALL OUTLINE TRANSISTOR")
    (tags "SMALL OUTLINE TRANSISTOR")
    (attr smd)
    (fp_text reference U4 (at 1.27 -2.54 270) (layer B.SilkS))
    (fp_text value SPX3819 (at 1.905 2.794 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.94996 1.29794 270) (size 0.54864 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 6 VBUS))
    (pad 2 smd rect (at 0 1.29794 270) (size 0.54864 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0.94996 1.29794 270) (size 0.54864 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 26 /EN))
    (pad 5 smd rect (at 0.94996 -1.29794 270) (size 0.54864 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(U4-Pad5)"))
    (pad 4 smd rect (at -0.94996 -1.29794 270) (size 0.54864 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 3 3v3))
  )
  (module Pin_Headers:Pin_Header_Straight_1x12 (layer F.Cu) (tedit 0)
    (at 116.84 74.168 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP3 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value PINHD-1X12 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 VBAT))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 /EN))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 VBUS))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 /13))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 /12))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 /11))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 /10))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 9))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 /6))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 /5))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 /3))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 /2))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x12.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module arthurc:SOT23-5 (layer F.Cu) (tedit 58758B29)
    (at 82.296 74.422 90)
    (descr SOT23-5)
    (attr smd)
    (fp_text reference U5 (at 0 3.048 90) (layer F.SilkS))
    (fp_text value MCP73831 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 1.3335 90) (size 0.59944 1.15062) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R4-Pad1)"))
    (pad 3 smd rect (at 0.9525 1.3335 90) (size 0.59944 1.15062) (layers F.Cu F.Paste F.Mask)
      (net 5 VBAT))
    (pad 2 smd rect (at 0 1.3335 90) (size 0.59944 1.15062) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0.9525 -1.3335 90) (size 0.59944 1.15062) (layers F.Cu F.Paste F.Mask)
      (net 6 VBUS))
    (pad 5 smd rect (at -0.9525 -1.3335 90) (size 0.59944 1.15062) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R5-Pad2)"))
    (model libs/3D_Modules/SOT23_3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 180))
    )
  )
  (module misc:Mounting-Hole (layer F.Cu) (tedit 58759302)
    (at 78.486 92.456)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference REF** (at 236.474 19.812) (layer F.SilkS))
    (fp_text value Measurement_Point_Round-SMD-Pad_Big (at 248.92 23.368) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Crystals:ABM3 (layer F.Cu) (tedit 58764C5C)
    (at 152.654 93.472 180)
    (descr "Abracon Miniature Ceramic Smd Crystal http://www.abracon.com/Resonators/abm3.pdf")
    (tags "smd crystal")
    (attr smd)
    (fp_text reference 8MHz1 (at -0.254 0 180) (layer F.SilkS))
    (fp_text value CRYSTAL_2 (at 0 3 180) (layer F.Fab))
    (pad 2 smd rect (at 2.05 0 180) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(8MHz1-Pad2)"))
    (pad 1 smd rect (at -2.05 0 180) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(8MHz1-Pad1)"))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58764D8A)
    (at 150.114 87.376)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at -2.54 1.778) (layer F.SilkS))
    (fp_text value C (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(8MHz1-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58764D99)
    (at 150.114 89.154)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at -2.286 -2.286) (layer F.SilkS))
    (fp_text value C (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(8MHz1-Pad2)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text VBAT (at 89.154 78.994) (layer F.SilkS))
  (gr_text GND (at 91.948 78.994) (layer F.SilkS))
  (gr_text R4 (at 77.47 77.724) (layer F.SilkS))
  (gr_text R5 (at 77.47 76.2) (layer F.SilkS))
  (gr_text D2 (at 77.47 73.66) (layer F.SilkS))
  (gr_text D4 (at 81.28 92.964) (layer F.SilkS))
  (gr_text R9 (at 86.106 91.694) (layer F.SilkS))
  (gr_text R1 (at 91.694 85.598) (layer F.SilkS))
  (gr_text SPX3819 (at 88.9 80.518) (layer F.SilkS))
  (gr_text "LoRaWAN Stick - Rev2\nGPS   - MTK3339 \nLoRa - RN2903\nuC     - 32u4\n1/10/2017" (at 184.15 75.438) (layer F.SilkS))
  (gr_text D3 (at 191.516 92.964) (layer F.SilkS))
  (gr_text C4 (at 123.698 84.328 90) (layer F.SilkS))
  (gr_text C2 (at 118.618 86.36 90) (layer F.SilkS))
  (gr_text C1 (at 116.332 84.836 90) (layer F.SilkS))
  (gr_text R3 (at 120.65 78.994) (layer F.SilkS))
  (gr_text BAT (at 79.502 73.406 90) (layer F.SilkS))
  (gr_text POW (at 80.518 94.742) (layer F.SilkS))
  (gr_text GPIO10 (at 188.214 94.742) (layer F.SilkS))
  (gr_text RST (at 151.384 77.47) (layer F.SilkS))
  (gr_text TEST0 (at 151.384 87.122) (layer F.SilkS))
  (gr_text TEST1 (at 151.384 84.836) (layer F.SilkS))
  (gr_text GND (at 151.638 82.55) (layer F.SilkS))
  (gr_text 3v (at 151.13 79.756) (layer F.SilkS))
  (gr_text 2 (at 144.78 75.946) (layer F.SilkS))
  (gr_text 3 (at 142.24 75.946) (layer F.SilkS))
  (gr_text 5 (at 139.7 75.946) (layer F.SilkS))
  (gr_text 6 (at 137.16 75.946) (layer F.SilkS))
  (gr_text 9 (at 134.62 75.946) (layer F.SilkS))
  (gr_text 10 (at 132.08 75.946) (layer F.SilkS))
  (gr_text 11 (at 129.54 75.946) (layer F.SilkS))
  (gr_text 12 (at 127 75.946) (layer F.SilkS))
  (gr_text 13 (at 124.46 75.946) (layer F.SilkS))
  (gr_text VBUS (at 121.92 75.946) (layer F.SilkS))
  (gr_text EN (at 119.38 75.946) (layer F.SilkS))
  (gr_text VBAT (at 116.84 76.2) (layer F.SilkS))
  (gr_text GND (at 144.78 91.948) (layer F.SilkS))
  (gr_text TX (at 142.24 91.948) (layer F.SilkS))
  (gr_text RX (at 139.7 91.948) (layer F.SilkS))
  (gr_text MISO (at 137.16 91.948) (layer F.SilkS))
  (gr_text MOSI (at 134.62 91.948) (layer F.SilkS))
  (gr_text SCK (at 132.08 91.948) (layer F.SilkS))
  (gr_text A5 (at 129.54 91.948) (layer F.SilkS))
  (gr_text A4 (at 127 91.948) (layer F.SilkS))
  (gr_text A3 (at 124.46 91.948) (layer F.SilkS))
  (gr_text A2 (at 121.92 91.948) (layer F.SilkS))
  (gr_text A1 (at 119.38 91.948) (layer F.SilkS))
  (gr_text A0 (at 116.84 91.948) (layer F.SilkS))
  (gr_text GND (at 114.3 91.948) (layer F.SilkS))
  (gr_text ARFF (at 112.014 91.948) (layer F.SilkS))
  (gr_text 3v (at 109.22 91.948) (layer F.SilkS))
  (gr_text RST (at 106.68 91.948) (layer F.SilkS))
  (gr_line (start 199.814 72.502) (end 75.664 72.502) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 199.814 95.392) (end 75.664 95.392) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 199.81164 95.38462) (end 199.81164 72.57288) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 75.66406 95.36684) (end 75.68438 95.34652) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 75.66406 72.50176) (end 75.66406 95.36176) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75.692 72.39) (xy 199.898 72.39) (xy 199.644 95.504) (xy 75.692 95.504)
      )
    )
  )
)
