(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 1.6)
    (drawings 4312)
    (tracks 740)
    (zones 0)
    (modules 77)
    (nets 111)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 0.762)
    (user_trace_width 0.889)
    (user_trace_width 1.016)
    (user_trace_width 1.143)
    (trace_clearance 0.2032)
    (zone_clearance 0.127)
    (zone_45_only no)
    (trace_min 0.000152)
    (via_size 0.635)
    (via_drill 0.381)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3048)
    (uvia_drill 0.1016)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.25 1.75)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 154.432 88.646)
    (grid_origin 111.125 121.92)
    (visible_elements 7FFDFFFF)
    (pcbplotparams
      (layerselection 0x00010_7ffffffe)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C5-Pad1)")
  (net 3 "Net-(C6-Pad1)")
  (net 4 RESET)
  (net 5 "Net-(C8-Pad1)")
  (net 6 "Net-(C9-Pad1)")
  (net 7 IGNITION)
  (net 8 "Net-(C15-Pad1)")
  (net 9 DIAL_Tx)
  (net 10 DIAL_Rx)
  (net 11 CAN_H)
  (net 12 CAN_L)
  (net 13 ILL+)
  (net 14 ILL-)
  (net 15 "Net-(J2-Pad10)")
  (net 16 "Net-(J2-Pad16)")
  (net 17 "Net-(J2-Pad1)")
  (net 18 "Net-(J2-Pad2)")
  (net 19 "Net-(J2-Pad3)")
  (net 20 "Net-(J2-Pad6)")
  (net 21 "Net-(J2-Pad7)")
  (net 22 "Net-(J2-Pad8)")
  (net 23 "Net-(J2-Pad9)")
  (net 24 "Net-(J2-Pad11)")
  (net 25 "Net-(J2-Pad12)")
  (net 26 "Net-(J2-Pad13)")
  (net 27 "Net-(J2-Pad14)")
  (net 28 "Net-(J2-Pad15)")
  (net 29 BATTERY)
  (net 30 ACC)
  (net 31 MIC_VCC)
  (net 32 MIC_GND)
  (net 33 MIC_SIG)
  (net 34 PARK_BREAK)
  (net 35 REVERSE)
  (net 36 SPEED)
  (net 37 "Net-(R2-Pad1)")
  (net 38 "Net-(R7-Pad2)")
  (net 39 CAN_INT)
  (net 40 TxCAN)
  (net 41 RxCAN)
  (net 42 "Net-(U5-Pad4)")
  (net 43 "Net-(U6-Pad4)")
  (net 44 "Net-(C11-Pad1)")
  (net 45 STRG_SW_A)
  (net 46 STRG_SW_B)
  (net 47 +3V3)
  (net 48 "Net-(U12-Pad5)")
  (net 49 "Net-(U12-Pad4)")
  (net 50 "Net-(U12-Pad3)")
  (net 51 "Net-(U12-Pad1)")
  (net 52 "Net-(U12-Pad12)")
  (net 53 "Net-(U12-Pad15)")
  (net 54 "Net-(U12-Pad6)")
  (net 55 "Net-(U12-Pad9)")
  (net 56 "Net-(U12-Pad11)")
  (net 57 "Net-(R3-Pad1)")
  (net 58 "Net-(R4-Pad1)")
  (net 59 SPI1_MOSI)
  (net 60 SPI1_MISO)
  (net 61 SPI1_SCLK)
  (net 62 SPI1_CS)
  (net 63 SCL2)
  (net 64 SDA2)
  (net 65 BT_Tx->UART1_Rx)
  (net 66 BT_Rx->UART1_Tx)
  (net 67 DIAL_TTL_Tx->UART2_Rx)
  (net 68 DIAL_TTL_Rx->UART2_Tx)
  (net 69 +5V)
  (net 70 "Net-(U1-Pad4)")
  (net 71 "Net-(U2-Pad15)")
  (net 72 "Net-(U2-Pad12)")
  (net 73 "Net-(U2-Pad11)")
  (net 74 "Net-(U2-Pad7)")
  (net 75 "Net-(U2-Pad6)")
  (net 76 "Net-(U2-Pad5)")
  (net 77 "Net-(U2-Pad4)")
  (net 78 "Net-(U2-Pad3)")
  (net 79 USB_P)
  (net 80 USB_N)
  (net 81 /D_P)
  (net 82 /D_N)
  (net 83 DEBUG_CLK)
  (net 84 DEBUG_DIO)
  (net 85 "Net-(D4-Pad2)")
  (net 86 PB9)
  (net 87 PB8)
  (net 88 PB7)
  (net 89 PB6)
  (net 90 PB5)
  (net 91 PB4)
  (net 92 PB3)
  (net 93 PA15)
  (net 94 PB13)
  (net 95 PB12)
  (net 96 PB1)
  (net 97 PC15)
  (net 98 PC14)
  (net 99 PC13)
  (net 100 "Net-(J7-Pad1)")
  (net 101 "Net-(J7-Pad4)")
  (net 102 BT_CFG)
  (net 103 "Net-(SW1-Pad1)")
  (net 104 "Net-(R20-Pad1)")
  (net 105 "Net-(C21-Pad2)")
  (net 106 "Net-(C21-Pad1)")
  (net 107 "Net-(R21-Pad1)")
  (net 108 "Net-(C20-Pad1)")
  (net 109 BT_nRESET)
  (net 110 "Net-(U9-Pad27)")
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.254)
    (via_dia 0.635)
    (via_drill 0.381)
    (uvia_dia 0.3048)
    (uvia_drill 0.1016)
    (add_net +5V)
    (add_net BT_CFG)
    (add_net BT_Rx->UART1_Tx)
    (add_net BT_Tx->UART1_Rx)
    (add_net BT_nRESET)
    (add_net CAN_H)
    (add_net CAN_INT)
    (add_net CAN_L)
    (add_net DEBUG_CLK)
    (add_net DEBUG_DIO)
    (add_net DIAL_Rx)
    (add_net DIAL_TTL_Rx->UART2_Tx)
    (add_net DIAL_TTL_Tx->UART2_Rx)
    (add_net DIAL_Tx)
    (add_net GND)
    (add_net MIC_GND)
    (add_net MIC_SIG)
    (add_net MIC_VCC)
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C20-Pad1)")
    (add_net "Net-(C21-Pad1)")
    (add_net "Net-(C21-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad14)")
    (add_net "Net-(J2-Pad15)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J2-Pad9)")
    (add_net "Net-(J7-Pad1)")
    (add_net "Net-(J7-Pad4)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R20-Pad1)")
    (add_net "Net-(R21-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(SW1-Pad1)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U12-Pad1)")
    (add_net "Net-(U12-Pad11)")
    (add_net "Net-(U12-Pad12)")
    (add_net "Net-(U12-Pad15)")
    (add_net "Net-(U12-Pad3)")
    (add_net "Net-(U12-Pad4)")
    (add_net "Net-(U12-Pad5)")
    (add_net "Net-(U12-Pad6)")
    (add_net "Net-(U12-Pad9)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U5-Pad4)")
    (add_net "Net-(U6-Pad4)")
    (add_net "Net-(U9-Pad27)")
    (add_net PA15)
    (add_net PARK_BREAK)
    (add_net PB1)
    (add_net PB12)
    (add_net PB13)
    (add_net PB3)
    (add_net PB4)
    (add_net PB5)
    (add_net PB6)
    (add_net PB7)
    (add_net PB8)
    (add_net PB9)
    (add_net PC13)
    (add_net PC14)
    (add_net PC15)
    (add_net RESET)
    (add_net REVERSE)
    (add_net RxCAN)
    (add_net SCL2)
    (add_net SDA2)
    (add_net SPEED)
    (add_net SPI1_CS)
    (add_net SPI1_MISO)
    (add_net SPI1_MOSI)
    (add_net SPI1_SCLK)
    (add_net STRG_SW_A)
    (add_net STRG_SW_B)
    (add_net TxCAN)
  )
  (net_class 12V_PWR ""
    (clearance 0.2032)
    (trace_width 1.27)
    (via_dia 1.27)
    (via_drill 0.635)
    (uvia_dia 0.3048)
    (uvia_drill 0.1016)
    (add_net ACC)
    (add_net IGNITION)
    (add_net ILL+)
    (add_net ILL-)
  )
  (net_class 3.3V_PWR ""
    (clearance 0.2032)
    (trace_width 0.381)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.3048)
    (uvia_drill 0.1016)
    (add_net +3V3)
  )
  (net_class 5V_PWR ""
    (clearance 0.2032)
    (trace_width 0.381)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.3048)
    (uvia_drill 0.1016)
  )
  (net_class BATT_PWR ""
    (clearance 0.2032)
    (trace_width 0.635)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.3048)
    (uvia_drill 0.1016)
    (add_net BATTERY)
  )
  (net_class USB_Diff ""
    (clearance 0.0508)
    (trace_width 0.1524)
    (via_dia 0.635)
    (via_drill 0.381)
    (uvia_dia 0.3048)
    (uvia_drill 0.1016)
    (diff_pair_width 0.2032)
    (diff_pair_gap 0.1524)
    (add_net /D_N)
    (add_net /D_P)
    (add_net USB_N)
    (add_net USB_P)
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5FEA6433)
    (at 131.2926 66.9909 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C20 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND) (zone_connect 1) (thermal_width 0.762))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 108 "Net-(C20-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.00mm:PinHeader_1x05_P2.00mm_Vertical (layer F.Cu) (tedit 5FEA5579)
    (at 133.223 97.282)
    (descr "Through hole straight pin header, 1x05, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.00mm single row")
    (fp_text reference J4 (at 0 -1.4732) (layer F.SilkS))
    (fp_text value Debug (at 0 10.06) (layer F.Fab))
    (fp_text user %R (at 0 4 90) (layer F.Fab))
    (pad 5 thru_hole oval (at 0 8) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 +3V3) (zone_connect 2) (thermal_width 0.508))
    (pad 4 thru_hole oval (at 0 6) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 RESET))
    (pad 3 thru_hole oval (at 0 4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole oval (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 83 DEBUG_CLK))
    (pad 1 thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 84 DEBUG_DIO))
  )
  (module Capacitor_SMD:C_1210_3225Metric (layer F.Cu) (tedit 5B301BBE)
    (at 121.793 68.072)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C24 (at 0 -2.159) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.28) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 47 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 136.525 70.2564)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C22 (at 0 1.1176) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 108 "Net-(C20-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_Murata:LQH3NPZ100MMEL (layer F.Cu) (tedit 5F5EECDF)
    (at 127.8382 68.7705 180)
    (attr smd)
    (fp_text reference L1 (at 0 2.0193 180) (layer F.SilkS))
    (fp_text value 10uH (at 0 2.4) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 0.8 2.7) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C11-Pad1)"))
    (pad 1 smd rect (at -1.1 0 180) (size 0.8 2.7) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(C21-Pad2)"))
    (model ${KIPRJMOD}/3D_CAD/LQH3NPZ100MMEL.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 133.858 67.056 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D3 (at 2.6924 0 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 30 ACC))
    (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 108 "Net-(C20-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1210_3225Metric (layer F.Cu) (tedit 5B301BBE)
    (at 135.4582 77.1144 270)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 2.6924 0 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.28 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 44 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 5A02FF57)
    (at 133.1595 71.4375 90)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U3 (at -2.2733 0) (layer F.SilkS))
    (fp_text value TPS560430 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 108 "Net-(C20-Pad1)"))
    (pad 6 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(C21-Pad2)"))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 108 "Net-(C20-Pad1)"))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 107 "Net-(R21-Pad1)"))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 106 "Net-(C21-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F5A82D5)
    (at 128.905 73.533 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R22 (at 2.2352 0) (layer F.SilkS))
    (fp_text value 22.1K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 107 "Net-(R21-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND) (thermal_gap 0.127))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 127.508 71.4375 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R21 (at 2.2098 0.0127) (layer F.SilkS))
    (fp_text value 113K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 "Net-(C11-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 107 "Net-(R21-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 130.4925 70.993 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C21 (at -0.381 -0.9525 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 105 "Net-(C21-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 106 "Net-(C21-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-252-3_TabPin4 (layer F.Cu) (tedit 5F5543D9)
    (at 148.752 76.199)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (attr smd)
    (fp_text reference U4 (at 2.0478 -3.809) (layer F.SilkS))
    (fp_text value UA78M33IKVURG3 (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd rect (at 0.425 1.525) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 3.775 -1.525) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 0.425 -1.525) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 3.775 1.525) (size 3.05 2.75) (layers F.Paste))
    (pad 4 smd rect (at 2.1 0) (size 6.4 5.800001) (layers F.Cu F.Mask)
      (net 1 GND) (thermal_width 2.54) (thermal_gap 0.254))
    (pad 3 smd rect (at -4.2 2.28) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 47 +3V3) (zone_connect 2))
    (pad "" connect rect (at -4.2 0) (size 2.2 1.2) (layers Dwgs.User)
      (solder_paste_margin -2.54) (clearance 0.000127) (thermal_width 1.27) (thermal_gap 0.000127))
    (pad 1 smd rect (at -4.2 -2.28) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-252-3_TabPin4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 141.986 74.8665 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C18 (at 2.0955 -0.0254 180) (layer F.SilkS))
    (fp_text value 0.33uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:PCM12SMTR (layer F.Cu) (tedit 5F3B4AB9)
    (at 122.7582 59.055 180)
    (attr smd)
    (fp_text reference SW1 (at 4.1148 -2.159) (layer F.SilkS))
    (fp_text value PCM12SMTR (at 0 4.3) (layer F.Fab))
    (pad 0 smd rect (at 3.5 -0.965 270) (size 0.8 1) (layers F.Cu F.Paste F.Mask))
    (pad 0 smd rect (at 3.5 0.965 270) (size 0.8 1) (layers F.Cu F.Paste F.Mask))
    (pad 0 smd rect (at -3.5 -0.965 270) (size 0.8 1) (layers F.Cu F.Paste F.Mask))
    (pad 0 smd rect (at -3.5 0.965 270) (size 0.8 1) (layers F.Cu F.Paste F.Mask))
    (pad "" np_thru_hole circle (at 1.5 0 270) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.5 0 270) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
    (pad 3 smd rect (at -2.25 -1.75 270) (size 1.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(R20-Pad1)"))
    (pad 2 smd rect (at 0.75 -1.75 270) (size 1.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 102 BT_CFG))
    (pad 1 smd rect (at 2.25 -1.75 270) (size 1.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(SW1-Pad1)"))
    (model ${KIPRJMOD}/3D_CAD/PCM12SMTR_c_.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -180))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 128.0922 60.0075 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R20 (at 0 1.1176 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 104 "Net-(R20-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Conn-2x10_3.0mm_pitch (layer F.Cu) (tedit 5F554303)
    (at 150.622 66.294 180)
    (fp_text reference J3 (at -0.0254 -3.4544) (layer F.SilkS))
    (fp_text value "Universal Interface" (at 0.05 9.48) (layer F.Fab))
    (pad 6 thru_hole oval (at -1.5 1.5 180) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 11 CAN_H))
    (pad 16 thru_hole oval (at -1.5 -1.5 180) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 12 CAN_L))
    (pad 5 thru_hole oval (at 1.5 1.5 180) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND) (thermal_gap 0.254))
    (pad 15 thru_hole oval (at 1.5 -1.5 180) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND) (thermal_gap 0.254))
    (pad 9 thru_hole oval (at -10.5 1.5 180) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 19 thru_hole oval (at -10.5 -1.5 180) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 29 BATTERY))
    (pad 8 thru_hole oval (at -7.5 1.5 180) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 32 MIC_GND))
    (pad 18 thru_hole oval (at -7.5 -1.5 180) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 33 MIC_SIG))
    (pad 7 thru_hole oval (at -4.5 1.5 180) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 34 PARK_BREAK))
    (pad 17 thru_hole oval (at -4.5 -1.5 180) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 36 SPEED))
    (pad 4 thru_hole oval (at 4.5 1.5 180) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND) (thermal_gap 0.254))
    (pad 14 thru_hole oval (at 4.5 -1.5 180) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND) (thermal_gap 0.254))
    (pad 2 thru_hole oval (at 10.5 1.5 180) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND) (thermal_gap 0.254))
    (pad 12 thru_hole oval (at 10.5 -1.5 180) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND) (thermal_gap 0.254))
    (pad 0 thru_hole oval (at 15.65 5.82 180) (size 3.5 4) (drill 2.4) (layers *.Cu *.Mask))
    (pad 0 thru_hole oval (at -15.65 5.82 180) (size 3.5 4) (drill 2.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at 13.5 1.5 180) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 7 IGNITION))
    (pad 3 thru_hole oval (at 7.5 1.5 180) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND) (thermal_gap 0.254))
    (pad 10 thru_hole oval (at -13.5 1.5 180) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 31 MIC_VCC))
    (pad 20 thru_hole oval (at -13.5 -1.5 180) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 35 REVERSE))
    (pad 13 thru_hole oval (at 7.5 -1.5 180) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND) (thermal_gap 0.254))
    (pad 11 thru_hole oval (at 13.5 -1.5 180) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 30 ACC))
    (model ${KIPRJMOD}/3D_CAD/5-794677-0.stp
      (offset (xyz 0 -10.4394 4.0132))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module footprints:Conn-2x8_3.0mm_pitch locked (layer F.Cu) (tedit 5F3851C5)
    (at 180.745 73.128 90)
    (fp_text reference J5 (at 14.073 -1.675 180) (layer F.SilkS))
    (fp_text value User_Out (at 0.05 9.48 90) (layer F.Fab))
    (pad 7 thru_hole oval (at -7.5 1.5 90) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 64 SDA2))
    (pad 15 thru_hole oval (at -7.5 -1.5 90) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 63 SCL2))
    (pad 6 thru_hole oval (at -4.5 1.5 90) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND) (thermal_width 0.889))
    (pad 14 thru_hole oval (at -4.5 -1.5 90) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 12 CAN_L))
    (pad 5 thru_hole oval (at -1.5 1.5 90) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 36 SPEED))
    (pad 13 thru_hole oval (at -1.5 -1.5 90) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 11 CAN_H))
    (pad 4 thru_hole oval (at 1.5 1.5 90) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 34 PARK_BREAK))
    (pad 12 thru_hole oval (at 1.5 -1.5 90) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 33 MIC_SIG))
    (pad 2 thru_hole oval (at 7.5 1.5 90) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 31 MIC_VCC))
    (pad 10 thru_hole oval (at 7.5 -1.5 90) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 35 REVERSE))
    (pad 0 thru_hole oval (at 12.66 5.82 90) (size 3.5 4) (drill 2.4) (layers *.Cu *.Mask))
    (pad 0 thru_hole oval (at -12.66 5.82 90) (size 3.5 4) (drill 2.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at 10.5 1.5 90) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 7 IGNITION))
    (pad 3 thru_hole oval (at 4.5 1.5 90) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 32 MIC_GND))
    (pad 8 thru_hole oval (at -10.5 1.5 90) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 14 ILL-))
    (pad 16 thru_hole oval (at -10.5 -1.5 90) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 13 ILL+))
    (pad 11 thru_hole oval (at 4.5 -1.5 90) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 29 BATTERY))
    (pad 9 thru_hole oval (at 10.5 -1.5 90) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 30 ACC))
    (model ${KIPRJMOD}/3D_CAD/4-794677-6.stp
      (offset (xyz 0 -10.4394 4.0132))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module footprints:Conn-2x3_3.0mm_pitch (layer F.Cu) (tedit 5EF8F09F)
    (at 120.444 111.482)
    (fp_text reference J6 (at -6.3345 -2.135) (layer F.SilkS))
    (fp_text value "Dial Control" (at 0.1524 9.4742) (layer F.Fab))
    (pad 0 thru_hole oval (at 5.16 5.82) (size 3.5 4) (drill 2.4) (layers *.Cu *.Mask))
    (pad 0 thru_hole oval (at -5.16 5.82) (size 3.5 4) (drill 2.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at 3 1.5) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 14 ILL-))
    (pad 2 thru_hole oval (at 0 1.5) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at -3 1.5) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 7 IGNITION))
    (pad 6 thru_hole oval (at -3 -1.5) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 9 DIAL_Tx))
    (pad 4 thru_hole oval (at 3 -1.5) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 13 ILL+))
    (pad 5 thru_hole oval (at 0 -1.5) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 10 DIAL_Rx))
    (model ${KIPRJMOD}/3D_CAD/3-794677-6.stp
      (offset (xyz 0 -10.4394 4.0132))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module footprints:Conn-2x2_3.0mm_pitch (layer F.Cu) (tedit 5EF8F036)
    (at 137.414 111.506)
    (fp_text reference J1 (at -4.7625 -2.159) (layer F.SilkS))
    (fp_text value "STRG Switch" (at 0.11 9.42) (layer F.Fab))
    (pad 0 thru_hole oval (at 3.66 5.82) (size 3.5 4) (drill 2.4) (layers *.Cu *.Mask))
    (pad 0 thru_hole oval (at -3.66 5.82) (size 3.5 4) (drill 2.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at 1.5 1.5) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at -1.5 1.5) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at -1.5 -1.5) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 46 STRG_SW_B))
    (pad 3 thru_hole oval (at 1.5 -1.5) (size 1.5 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 45 STRG_SW_A))
    (model ${KIPRJMOD}/3D_CAD/3-794677-4.stp
      (offset (xyz 0 -10.4394 4.0132))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module _my_TE_Connectivity_Connectors:USB_Mini_B-2172034-1 (layer F.Cu) (tedit 5EEFBF21)
    (at 111.125 88.519 270)
    (fp_text reference J7 (at 4.3434 -7.2136 180) (layer F.SilkS))
    (fp_text value "USB MiniB" (at 0 0.9525 90) (layer F.Fab))
    (fp_text user "Board Edge" (at 0 -0.25 90) (layer F.Fab))
    (fp_text user ID (at 0.8 -4.2 90) (layer F.Fab))
    (fp_text user D- (at -0.8 -4.2 90) (layer F.Fab))
    (fp_text user VBUS (at -1.6 -8.1 90) (layer F.Fab))
    (fp_text user D+ (at 0 -8.1 90) (layer F.Fab))
    (fp_text user GND (at 1.6 -8.1 90) (layer F.Fab))
    (pad 1 thru_hole oval (at -1.6 -6.8 270) (size 1.1 1.65) (drill 0.7 (offset 0 -0.275)) (layers *.Cu *.Mask)
      (net 100 "Net-(J7-Pad1)"))
    (pad 5 thru_hole oval (at 1.6 -6.8 270) (size 1.1 1.65) (drill 0.7 (offset 0 -0.275)) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 -6.8 270) (size 1.1 1.65) (drill 0.7 (offset 0 -0.275)) (layers *.Cu *.Mask)
      (net 79 USB_P))
    (pad 2 thru_hole oval (at -0.8 -5.6 270) (size 1.1 1.65) (drill 0.7 (offset 0 0.275)) (layers *.Cu *.Mask)
      (net 80 USB_N))
    (pad 4 thru_hole oval (at 0.8 -5.6 270) (size 1.1 1.65) (drill 0.7 (offset 0 0.275)) (layers *.Cu *.Mask)
      (net 101 "Net-(J7-Pad4)"))
    (pad 0 thru_hole oval (at -3.65 -1.75 270) (size 1.7 2.7) (drill oval 0.7 1.9) (layers *.Cu *.Mask))
    (pad 0 thru_hole oval (at 3.65 -1.75 270) (size 1.7 2.7) (drill oval 0.7 1.9) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/3D_CAD/2172034-1--3DModel-STEP-56544.STEP
      (offset (xyz 0 -1.9812 2.032))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module "footprints:D0-219AB_(SMF)" (layer F.Cu) (tedit 5EEFBBB9)
    (at 140.97 70.485)
    (attr smd)
    (fp_text reference D5 (at -0.0254 1.4478) (layer F.SilkS))
    (fp_text value VTVS19ASMF-HM3-08 (at 0.3 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0) (size 1.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 30 ACC))
    (pad 2 smd rect (at 1.45 0) (size 1.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducial:Fiducial_1mm_Mask2mm (layer F.Cu) (tedit 5C18CB26)
    (at 114.554 64.643)
    (descr "Circular Fiducial, 1mm bare copper, 2mm soldermask opening (Level A)")
    (tags fiducial)
    (attr smd)
    (fp_text reference FID2 (at -0.0254 1.7018) (layer F.SilkS))
    (fp_text value Fiducial (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.5) (clearance 0.5))
  )
  (module Fiducial:Fiducial_1mm_Mask2mm (layer F.Cu) (tedit 5C18CB26)
    (at 154.432 88.646)
    (descr "Circular Fiducial, 1mm bare copper, 2mm soldermask opening (Level A)")
    (tags fiducial)
    (attr smd)
    (fp_text reference FID1 (at 1.2446 -1.4732) (layer F.SilkS))
    (fp_text value Fiducial (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.5) (clearance 0.5))
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 144.526 111.4045 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R19 (at -1.8795 0 180) (layer F.SilkS))
    (fp_text value 470 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 +3V3))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 STRG_SW_A))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 146.177 111.4045 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at -1.8795 0 180) (layer F.SilkS))
    (fp_text value 470 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 +3V3))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 STRG_SW_B))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 179.07 89.154 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at 0 -1.1176) (layer F.SilkS))
    (fp_text value 499 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 +3V3))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 85 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 182.753 89.154 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D4 (at 0 -1.1176) (layer F.SilkS))
    (fp_text value "Power LED" (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 85 "Net-(D4-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 121.539 88.9)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at 2.3368 0) (layer F.SilkS))
    (fp_text value 22 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 81 /D_P))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 USB_P))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 121.539 87.376)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at 2.3368 0) (layer F.SilkS))
    (fp_text value 22 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 82 /D_N))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 USB_N))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 121.539 90.551 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at -2.1336 0.0254) (layer F.SilkS))
    (fp_text value 1.5K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 +3V3))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 81 /D_P))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 118.364 68.834 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C19 (at 0 -1.0414 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm (layer F.Cu) (tedit 5A02F25C)
    (at 161.036 90.932 180)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (solder_paste_ratio -0.15)
    (clearance 0.0889)
    (attr smd)
    (fp_text reference U2 (at -3.2258 -4.0132) (layer F.SilkS))
    (fp_text value MCP2515-E_ST (at 0 4.3) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 20 smd rect (at 2.95 -2.925 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 47 +3V3))
    (pad 19 smd rect (at 2.95 -2.275 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 RESET))
    (pad 18 smd rect (at 2.95 -1.625 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 62 SPI1_CS))
    (pad 17 smd rect (at 2.95 -0.975 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 60 SPI1_MISO))
    (pad 16 smd rect (at 2.95 -0.325 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 59 SPI1_MOSI))
    (pad 15 smd rect (at 2.95 0.325 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(U2-Pad15)"))
    (pad 14 smd rect (at 2.95 0.975 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 61 SPI1_SCLK))
    (pad 13 smd rect (at 2.95 1.625 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 39 CAN_INT))
    (pad 12 smd rect (at 2.95 2.275 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(U2-Pad12)"))
    (pad 11 smd rect (at 2.95 2.925 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(U2-Pad11)"))
    (pad 10 smd rect (at -2.95 2.925 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -2.95 2.275 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C9-Pad1)"))
    (pad 8 smd rect (at -2.95 1.625 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C8-Pad1)"))
    (pad 7 smd rect (at -2.95 0.975 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(U2-Pad7)"))
    (pad 6 smd rect (at -2.95 0.325 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(U2-Pad6)"))
    (pad 5 smd rect (at -2.95 -0.325 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(U2-Pad5)"))
    (pad 4 smd rect (at -2.95 -0.975 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U2-Pad4)"))
    (pad 3 smd rect (at -2.95 -1.625 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U2-Pad3)"))
    (pad 2 smd rect (at -2.95 -2.275 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 41 RxCAN))
    (pad 1 smd rect (at -2.95 -2.925 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 40 TxCAN))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_HC49-U_Vertical (layer F.Cu) (tedit 5A1AD3B8)
    (at 171.069 86.179 270)
    (descr "Crystal THT HC-49/U http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-49/U")
    (fp_text reference Y2 (at 8.6138 0 180) (layer F.SilkS))
    (fp_text value 16MHz (at 2.44 3.525 90) (layer F.Fab))
    (fp_text user %R (at 2.44 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 4.88 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C8-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_HC49-U_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_HC49-U_Vertical (layer F.Cu) (tedit 5A1AD3B8)
    (at 147.1295 105.029 45)
    (descr "Crystal THT HC-49/U http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-49/U")
    (fp_text reference Y1 (at 2.685097 3.15207 45) (layer F.SilkS))
    (fp_text value 8MHz (at 2.44 3.525 45) (layer F.Fab))
    (fp_text user %R (at 2.44 0 45) (layer F.Fab))
    (pad 2 thru_hole circle (at 4.88 0 45) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C6-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 45) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_HC49-U_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5C97300E)
    (at 165.608 78.486 90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U7 (at -1.778 3.2258 180) (layer F.SilkS))
    (fp_text value MCP2562-H/SN (at 0 3.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 8 smd roundrect (at 2.475 -1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(R2-Pad1)"))
    (pad 7 smd roundrect (at 2.475 -0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 CAN_H))
    (pad 6 smd roundrect (at 2.475 0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 CAN_L))
    (pad 5 smd roundrect (at 2.475 1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 +3V3))
    (pad 4 smd roundrect (at -2.475 1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 RxCAN))
    (pad 3 smd roundrect (at -2.475 0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 +5V))
    (pad 2 smd roundrect (at -2.475 -0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -2.475 -1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 TxCAN))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 125.857 80.391)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at 2.286 0) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 109 BT_nRESET))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 172.212 79.756 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at 1.8288 -0.0254 180) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 SDA2))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 175.26 79.756 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at 1.8288 -0.0254 180) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 SCL2))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 125.349 104.013 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 0 -1.0922) (layer F.SilkS))
    (fp_text value DNI (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 DIAL_Rx))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 DIAL_TTL_Rx->UART2_Tx))
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 119.38 104.8385 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 0 -1.1303) (layer F.SilkS))
    (fp_text value DNI (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 DIAL_Tx))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 DIAL_TTL_Tx->UART2_Rx))
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 171.704 74.93 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 0 1.0922 90) (layer F.SilkS))
    (fp_text value DNI (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 CAN_L))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 CAN_H))
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 125.415 100.076)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 1.966 0) (layer F.SilkS))
    (fp_text value 220 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(R7-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 DIAL_Rx))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 121.031 97.348 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at -2.0472 0 180) (layer F.SilkS))
    (fp_text value 1K (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(C15-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 118.049 95.25)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at -0.0152 -1.0668) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 DIAL_TTL_Tx->UART2_Rx))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 161.671 75.184 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 1.8288 0 180) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 151.384 93.98 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -1.8796 0.0254 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 RESET))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 174.625 74.93)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D2 (at 0 -2.032) (layer F.SilkS))
    (fp_text value PESD1CAN (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 12 CAN_L))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 11 CAN_H))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 114.173 98.426 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at 2.668 0 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C15-Pad1)"))
    (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 9 DIAL_Tx))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 125.9586 78.8416)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C23 (at 2.1844 0) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 109 BT_nRESET))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 125.415 102.108)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C17 (at 2.22 0) (layer F.SilkS))
    (fp_text value 560pF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 DIAL_Rx))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 114.869 101.854)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at 0.0152 1.1176) (layer F.SilkS))
    (fp_text value 560pF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 DIAL_Tx))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 119.949 101.854 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at -0.0152 -1.0668) (layer F.SilkS))
    (fp_text value 4.7nF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 +3V3))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(C15-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 169.291 77.47 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at 0 1.1176 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1210_3225Metric (layer F.Cu) (tedit 5D758A7C)
    (at 149.352 84.582)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at 0 1.9304) (layer F.SilkS))
    (fp_text value 22uF (at 0 2.28) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 47 +3V3) (zone_connect 2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5D758A6E)
    (at 148.6155 81.788)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at 2.2351 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 +3V3) (zone_connect 2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 157.33268 95.54464 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 0 -1.12776) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 167.132 87.249 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at 0 -1.0922 90) (layer F.SilkS))
    (fp_text value 22pF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 167.132 90.64 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at -0.0128 1.0922 90) (layer F.SilkS))
    (fp_text value 22pF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C8-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 153.162 93.98 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 1.8796 0.0254 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 RESET))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 147.5105 99.1235 45)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 0 -1.023749 45) (layer F.SilkS))
    (fp_text value 22pF (at 0 1.43 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 145.175653 101.521847 225)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at -0.006218 1.032729 45) (layer F.SilkS))
    (fp_text value 22pF (at 0 1.43 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 225) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 225) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 134.4675 94.361 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 1.0414) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 141.351 101.4731 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 1.8541 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1210_3225Metric (layer F.Cu) (tedit 5B301BBE)
    (at 157.988 81.026 180)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0 -1.9304) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 2.28) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 69 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 161.544 80.772 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 1.8288 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 157.6705 77.1525)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U1 (at 0.0381 -2.1209) (layer F.SilkS))
    (fp_text value NCP718 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 69 +5V))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(U1-Pad4)"))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 138.952653 86.311153 135)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at -0.006218 1.086611 135) (layer F.SilkS))
    (fp_text value 100K (at 0 1.43 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 135) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 135) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(R4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_QFP:LQFP-48_7x7mm_P0.5mm (layer F.Cu) (tedit 5C18330E)
    (at 141.351 94.488 135)
    (descr "LQFP, 48 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ltc2358-16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "LQFP QFP")
    (solder_paste_ratio -0.2)
    (clearance 0.0889)
    (attr smd)
    (fp_text reference U9 (at -4.310523 3.663944 180) (layer F.SilkS))
    (fp_text value STM32F103C8T6 (at 0 5.85 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 48 smd roundrect (at -2.75 -4.1625 135) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 +3V3))
    (pad 47 smd roundrect (at -2.25 -4.1625 135) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 46 smd roundrect (at -1.75 -4.1625 135) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 PB9))
    (pad 45 smd roundrect (at -1.25 -4.1625 135) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 87 PB8))
    (pad 44 smd roundrect (at -0.75 -4.1625 135) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(R3-Pad1)"))
    (pad 43 smd roundrect (at -0.25 -4.1625 135) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 88 PB7))
    (pad 42 smd roundrect (at 0.25 -4.1625 135) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 89 PB6))
    (pad 41 smd roundrect (at 0.75 -4.1625 135) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 90 PB5))
    (pad 40 smd roundrect (at 1.25 -4.1625 135) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 91 PB4))
    (pad 39 smd roundrect (at 1.75 -4.1625 135) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 92 PB3))
    (pad 38 smd roundrect (at 2.25 -4.1625 135) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 93 PA15))
    (pad 37 smd roundrect (at 2.75 -4.1625 135) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 DEBUG_CLK))
    (pad 36 smd roundrect (at 4.1625 -2.75 135) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 +3V3))
    (pad 35 smd roundrect (at 4.1625 -2.25 135) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 34 smd roundrect (at 4.1625 -1.75 135) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 DEBUG_DIO))
    (pad 33 smd roundrect (at 4.1625 -1.25 135) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 81 /D_P))
    (pad 32 smd roundrect (at 4.1625 -0.75 135) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 82 /D_N))
    (pad 31 smd roundrect (at 4.1625 -0.25 135) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 BT_Tx->UART1_Rx))
    (pad 30 smd roundrect (at 4.1625 0.25 135) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 BT_Rx->UART1_Tx))
    (pad 29 smd roundrect (at 4.1625 0.75 135) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 BT_CFG))
    (pad 28 smd roundrect (at 4.1625 1.25 135) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 109 BT_nRESET))
    (pad 27 smd roundrect (at 4.1625 1.75 135) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 110 "Net-(U9-Pad27)"))
    (pad 26 smd roundrect (at 4.1625 2.25 135) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 PB13))
    (pad 25 smd roundrect (at 4.1625 2.75 135) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 95 PB12))
    (pad 24 smd roundrect (at 2.75 4.1625 135) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 +3V3))
    (pad 23 smd roundrect (at 2.25 4.1625 135) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 22 smd roundrect (at 1.75 4.1625 135) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 SDA2))
    (pad 21 smd roundrect (at 1.25 4.1625 135) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 SCL2))
    (pad 20 smd roundrect (at 0.75 4.1625 135) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(R4-Pad1)"))
    (pad 19 smd roundrect (at 0.25 4.1625 135) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 PB1))
    (pad 18 smd roundrect (at -0.25 4.1625 135) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 CAN_INT))
    (pad 17 smd roundrect (at -0.75 4.1625 135) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 SPI1_MOSI))
    (pad 16 smd roundrect (at -1.25 4.1625 135) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 SPI1_MISO))
    (pad 15 smd roundrect (at -1.75 4.1625 135) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 SPI1_SCLK))
    (pad 14 smd roundrect (at -2.25 4.1625 135) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 SPI1_CS))
    (pad 13 smd roundrect (at -2.75 4.1625 135) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 DIAL_TTL_Tx->UART2_Rx))
    (pad 12 smd roundrect (at -4.1625 2.75 135) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 DIAL_TTL_Rx->UART2_Tx))
    (pad 11 smd roundrect (at -4.1625 2.25 135) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 STRG_SW_A))
    (pad 10 smd roundrect (at -4.1625 1.75 135) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 STRG_SW_B))
    (pad 9 smd roundrect (at -4.1625 1.25 135) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 +3V3))
    (pad 8 smd roundrect (at -4.1625 0.75 135) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 7 smd roundrect (at -4.1625 0.25 135) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 RESET))
    (pad 6 smd roundrect (at -4.1625 -0.25 135) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(C6-Pad1)"))
    (pad 5 smd roundrect (at -4.1625 -0.75 135) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(C5-Pad1)"))
    (pad 4 smd roundrect (at -4.1625 -1.25 135) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 97 PC15))
    (pad 3 smd roundrect (at -4.1625 -1.75 135) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 98 PC14))
    (pad 2 smd roundrect (at -4.1625 -2.25 135) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 PC13))
    (pad 1 smd roundrect (at -4.1625 -2.75 135) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 +3V3))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/LQFP-48_7x7mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 136.8425 98.933 135)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at -0.00898 -1.104572 135) (layer F.SilkS))
    (fp_text value 100K (at 0 1.43 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 135) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 135) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Conn-2x8_2.2mmx3.0mm_RA (layer F.Cu) (tedit 5C85AB2C)
    (at 171.97 109.616 90)
    (fp_text reference J2 (at 10.429 -2.679) (layer F.SilkS))
    (fp_text value "M72 MF Switch" (at 0.2 19.4 90) (layer F.Fab))
    (pad 10 thru_hole oval (at 1.1 -1.5 90) (size 1.3 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad10)"))
    (pad 16 thru_hole oval (at 7.7 -1.5 90) (size 1.3 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad16)"))
    (pad 1 thru_hole oval (at -7.7 1.5 90) (size 1.3 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at -7.7 -1.5 90) (size 1.3 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at -5.5 1.5 90) (size 1.3 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at -5.5 -1.5 90) (size 1.3 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 ILL+))
    (pad 5 thru_hole oval (at -3.3 1.5 90) (size 1.3 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 ILL-))
    (pad 6 thru_hole oval (at -3.3 -1.5 90) (size 1.3 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad6)"))
    (pad 7 thru_hole oval (at -1.1 1.5 90) (size 1.3 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad7)"))
    (pad 8 thru_hole oval (at -1.1 -1.5 90) (size 1.3 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad8)"))
    (pad 9 thru_hole oval (at 1.1 1.5 90) (size 1.3 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad9)"))
    (pad 11 thru_hole oval (at 3.3 1.5 90) (size 1.3 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad11)"))
    (pad 12 thru_hole oval (at 3.3 -1.5 90) (size 1.3 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad12)"))
    (pad 13 thru_hole oval (at 5.5 1.5 90) (size 1.3 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 26 "Net-(J2-Pad13)"))
    (pad 14 thru_hole oval (at 5.5 -1.5 90) (size 1.3 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 27 "Net-(J2-Pad14)"))
    (pad 15 thru_hole oval (at 7.7 1.5 90) (size 1.3 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad15)"))
    (pad "" np_thru_hole circle (at 7 7.1 90) (size 3.6 3.6) (drill 3.6) (layers *.Cu *.Mask)
      (clearance 1.27))
    (pad "" np_thru_hole circle (at -7 7 90) (size 3.6 3.6) (drill 3.6) (layers *.Cu *.Mask)
      (clearance 1.27))
    (model ${KIPRJMOD}/3D_CAD/1318382-2.stp
      (offset (xyz -0.0508 -22.5298 7.9502))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module footprints:SOT-457 (layer F.Cu) (tedit 5C84BB7E)
    (at 126.365 97.348 90)
    (attr smd)
    (fp_text reference U6 (at 1.8948 0 180) (layer F.SilkS))
    (fp_text value IMD3A (at 0 2.921 90) (layer F.Fab))
    (pad 6 smd rect (at 0.95 -1.05 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0 -1.05 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U6-Pad4)"))
    (pad 4 smd rect (at -0.95 -1.05 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U6-Pad4)"))
    (pad 3 smd rect (at -0.95 1.05 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 +3V3))
    (pad 2 smd rect (at 0 1.05 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 68 DIAL_TTL_Rx->UART2_Tx))
    (pad 1 smd rect (at 0.95 1.05 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module footprints:SOT-457 (layer F.Cu) (tedit 5C84BB7E)
    (at 117.949 99.126 90)
    (attr smd)
    (fp_text reference U5 (at 1.8948 -0.0168 180) (layer F.SilkS))
    (fp_text value IMD3A (at 0.127 2.921 90) (layer F.Fab))
    (pad 6 smd rect (at 0.95 -1.05 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0 -1.05 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U5-Pad4)"))
    (pad 4 smd rect (at -0.95 -1.05 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U5-Pad4)"))
    (pad 3 smd rect (at -0.95 1.05 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 +3V3))
    (pad 2 smd rect (at 0 1.05 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C15-Pad1)"))
    (pad 1 smd rect (at 0.95 1.05 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 67 DIAL_TTL_Tx->UART2_Rx))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module footprints:RN4871 (layer F.Cu) (tedit 5C933224)
    (at 118.364 75.946 90)
    (attr smd)
    (fp_text reference U12 (at -5.9055 -1.5875 180) (layer F.SilkS))
    (fp_text value RN4871 (at 0 -4.05 90) (layer F.Fab))
    (pad 5 smd rect (at -4.25 2.4 90) (size 1.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U12-Pad5)"))
    (pad 4 smd rect (at -4.25 1.2 90) (size 1.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(U12-Pad4)"))
    (pad 3 smd rect (at -4.25 0 90) (size 1.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(U12-Pad3)"))
    (pad 2 smd rect (at -4.25 -1.2 90) (size 1.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -4.25 -2.4 90) (size 1.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U12-Pad1)"))
    (pad 12 smd rect (at 4.25 2.4 90) (size 1.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U12-Pad12)"))
    (pad 13 smd rect (at 4.25 1.2 90) (size 1.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 14 smd rect (at 4.25 0 90) (size 1.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 47 +3V3))
    (pad 15 smd rect (at 4.25 -1.2 90) (size 1.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(U12-Pad15)"))
    (pad 16 smd rect (at 4.25 -2.4 90) (size 1.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 102 BT_CFG))
    (pad 6 smd rect (at -3 4.05 180) (size 1.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(U12-Pad6)"))
    (pad 7 smd rect (at -1.8 4.05 180) (size 1.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 66 BT_Rx->UART1_Tx))
    (pad 8 smd rect (at -0.6 4.05 180) (size 1.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 65 BT_Tx->UART1_Rx))
    (pad 9 smd rect (at 0.6 4.05 180) (size 1.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(U12-Pad9)"))
    (pad 10 smd rect (at 1.8 4.05 180) (size 1.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 109 BT_nRESET))
    (pad 11 smd rect (at 3 4.05 180) (size 1.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U12-Pad11)"))
    (model ${KIPRJMOD}/3D_CAD/Module_Microchip_RN4871_.stp
      (offset (xyz 0 1.4478 0.635))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 180))
    )
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 5CA01637)
    (at 114.935 59.69)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr virtual)
    (fp_text reference M1 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value Mount_Hole_1 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask)
      (clearance 1.27))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 5CA01642)
    (at 172.72 64.77)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr virtual)
    (fp_text reference M2 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value Mount_Hole_2 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask)
      (clearance 1.27))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 5CA01648)
    (at 187.325 92.71)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr virtual)
    (fp_text reference M3 (at -4.191 0) (layer F.SilkS) hide)
    (fp_text value Mount_Hole_3 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask)
      (clearance 1.27))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 5CA0164D)
    (at 149.225 115.57)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr virtual)
    (fp_text reference M4 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text value Mount_Hole_4 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask)
      (clearance 1.27))
  )
  (gr_text RST (at 131.2418 103.2764) (layer F.SilkS))
  (gr_text "eZ Navi-Delete\nNissan 370Z (Universal)\nHW v1.0b" (at 158.496 111.252) (layer B.Cu))
  (gr_arc (start 112.395 83.185) (end 112.395 81.915) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 112.395 68.707) (end 111.125 68.707) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 113.7285 71.247) (end 114.9985 71.247) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 113.7285 80.645) (end 113.7285 81.915) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 111.125 83.185) (end 111.125 120.65) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 113.7285 69.977) (end 112.395 69.977) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114.9985 80.645) (end 114.9985 71.247) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 112.395 81.915) (end 113.7285 81.915) (layer Edge.Cuts) (width 0.15))
  (gr_text BT-MODE (at 122.7074 62.3824) (layer F.SilkS))
  (gr_text APP (at 119.5197 56.8325) (layer F.SilkS))
  (gr_text TEST (at 125.9332 56.769) (layer F.SilkS))
  (gr_text GND (at 161.2265 62.357 90) (layer B.SilkS))
  (gr_text "Mic GND" (at 158.1785 61.341 90) (layer B.SilkS))
  (gr_text "Park Break" (at 155.1305 60.7695 90) (layer B.SilkS))
  (gr_text CAN-H (at 152.146 61.7855 90) (layer B.SilkS))
  (gr_text Reverse (at 166.9415 67.7545) (layer B.SilkS))
  (gr_text Battery (at 162.56 61.595 90) (layer B.SilkS))
  (gr_text "Mic Vcc" (at 167.005 64.77) (layer B.SilkS))
  (gr_text "Mic Sig" (at 159.5755 61.595 90) (layer B.SilkS))
  (gr_text Speed (at 156.6545 61.976 90) (layer B.SilkS))
  (gr_text CAN-L (at 153.5811 61.7855 90) (layer B.SilkS))
  (gr_text GND (at 144.5895 66.294) (layer B.SilkS))
  (gr_text Ignition (at 134.239 64.897) (layer B.SilkS))
  (gr_text ACC (at 135.001 67.8815) (layer B.SilkS))
  (gr_text Universal (at 163.6014 70.0024) (layer F.SilkS))
  (gr_text USB (at 117.6655 83.6295) (layer F.SilkS))
  (gr_text GND (at 131.2418 101.346) (layer F.SilkS))
  (gr_text 3.3V (at 131.1402 105.2576) (layer F.SilkS))
  (gr_text ST-LINK (at 133.223 107.061) (layer F.SilkS))
  (gr_text POWER (at 180.848 91.948) (layer F.SilkS))
  (gr_text DIO (at 131.3942 97.3328) (layer F.SilkS))
  (gr_text CLK (at 131.2926 99.2632) (layer F.SilkS))
  (gr_text "eZ Navi-Delete\n370Z" (at 158.623 113.284) (layer F.SilkS))
  (gr_arc (start 189.865 120.65) (end 191.135 120.65) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 189.865 57.15) (end 189.865 55.88) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 112.395 57.15) (end 111.125 57.15) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 112.395 120.65) (end 112.395 121.92) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "I2C CLK" (at 185.928 79.1464) (layer B.SilkS))
  (gr_text "I2C DATA" (at 186.182 80.645) (layer B.SilkS))
  (gr_text "Dial Control" (at 124.079 107.696) (layer F.SilkS))
  (gr_text "STRG SW" (at 139.954 107.823) (layer F.SilkS))
  (gr_text "User I/O" (at 184.6326 57.2516) (layer F.SilkS))
  (gr_text M72 (at 187.452 97.028) (layer F.SilkS))
  (gr_text Ignition (at 115.824 106.172 90) (layer B.SilkS))
  (gr_text "Dial Tx" (at 117.602 106.172 90) (layer B.SilkS))
  (gr_text GND (at 118.872 106.934 90) (layer B.SilkS))
  (gr_text "Dial RX" (at 120.396 106.172 90) (layer B.SilkS))
  (gr_text ILL- (at 121.92 106.934 90) (layer B.SilkS))
  (gr_text ILL+ (at 123.444 106.934 90) (layer B.SilkS))
  (gr_text GND (at 137.414 106.934 90) (layer B.SilkS))
  (gr_text STRG-B (at 135.89 106.172 90) (layer B.SilkS))
  (gr_text STRG-A (at 139.065 106.172 90) (layer B.SilkS))
  (gr_line (start 111.125 68.707) (end 111.125 57.15) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 189.865 121.92) (end 112.395 121.92) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 191.135 57.15) (end 191.135 120.65) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 112.395 55.88) (end 189.865 55.88) (layer Edge.Cuts) (width 0.15))
  (gr_text ILL- (at 184.912 83.439) (layer B.SilkS))
  (gr_text ILL+ (at 184.912 82.042) (layer B.SilkS))
  (gr_text GND (at 184.912 77.597) (layer B.SilkS))
  (gr_text CAN-L (at 185.547 76.0984) (layer B.SilkS))
  (gr_text Reverse (at 185.6105 64.0715) (layer B.SilkS))
  (gr_text CAN-H (at 185.547 73.152) (layer B.SilkS))
  (gr_text Speed (at 185.293 74.676) (layer B.SilkS))
  (gr_text "Park Brake" (at 186.4995 71.5645) (layer B.SilkS))
  (gr_text "Mic Sig" (at 185.6105 70.0659) (layer B.SilkS))
  (gr_text "Mic GND" (at 185.8645 68.707) (layer B.SilkS))
  (gr_text "Mic Vcc" (at 185.674 65.532) (layer B.SilkS))
  (gr_text Battery (at 185.547 67.0306) (layer B.SilkS))
  (gr_text Ignition (at 182.245 60.3885) (layer B.SilkS))
  (gr_text ACC (at 182.3085 58.928) (layer B.SilkS))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.254))
    (polygon
      (pts
        (xy 111.125 55.88) (xy 191.135 55.88) (xy 191.135 121.92) (xy 111.125 121.92)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (mode segment) (arc_segments 32) (thermal_gap 0.381) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 191.0969 98.1456) (xy 168.1099 98.1456) (xy 168.148 121.92) (xy 191.135 121.92)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (mode segment) (arc_segments 32) (thermal_gap 0.381) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 191.135 98.933) (xy 168.148 98.933) (xy 168.148 121.92) (xy 191.135 121.92)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.125 108.331) (xy 143.256 108.331) (xy 143.51 108.585) (xy 143.51 110.744) (xy 147.193 110.744)
        (xy 147.193 108.585) (xy 147.447 108.331) (xy 168.402 108.331) (xy 168.402 121.92) (xy 111.125 121.92)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.125 55.88) (xy 111.125 78.74) (xy 111.125 81.915) (xy 123.698 81.915) (xy 123.698 78.2955)
        (xy 123.063 78.2955) (xy 123.063 72.7075) (xy 122.047 71.628) (xy 117.7925 71.628) (xy 117.7925 69.7484)
        (xy 116.89715 69.7484) (xy 116.9035 61.595) (xy 135.763 61.595) (xy 135.763 55.88)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (mode segment) (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 111.125 72.136) (xy 111.125 55.88) (xy 120.142152 55.879391) (xy 133.35 55.88) (xy 133.38175 58.7375)
        (xy 127.635 58.73115) (xy 127.635 60.766325) (xy 122.682 60.7695) (xy 115.316 68.199) (xy 115.316 72.39)
        (xy 123.327853 72.39) (xy 123.306148 79.502) (xy 115.27259 79.502) (xy 115.27259 83.312) (xy 111.125 83.312)
        (xy 111.125 78.994)
      )
    )
  )
  (zone (net 47) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148.59 81.28) (xy 145.669 81.28) (xy 145.669 78.105) (xy 143.637 78.105) (xy 143.637 83.947)
        (xy 143.637 85.979) (xy 148.59 85.979)
      )
    )
  )
  (zone (net 47) (net_name +3V3) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.381) (smoothing chamfer) (radius 0.254))
    (polygon
      (pts
        (xy 111.125 55.88) (xy 191.135 55.88) (xy 191.135 121.92) (xy 111.125 121.92)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115.3795 86.868) (xy 122.428 86.868) (xy 122.428 87.122) (xy 134.112 87.122) (xy 137.9855 91.1225)
        (xy 136.525 92.583) (xy 133.096 89.154) (xy 124.46 89.154) (xy 124.30125 89.154) (xy 119.53875 89.154)
        (xy 119.38 89.2175) (xy 115.3795 89.2175)
      )
    )
  )
  (zone (net 69) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.254))
    (polygon
      (pts
        (xy 158.115 75.057) (xy 158.115 80.137) (xy 160.401 80.137) (xy 166.878 80.137) (xy 166.878 79.121)
        (xy 169.164 79.121) (xy 169.164 77.851) (xy 160.02 77.851) (xy 160.02 75.057)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 191.135 85.09) (xy 178.435 85.09) (xy 177.673 84.201) (xy 177.673 55.88) (xy 191.135 55.88)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.08 71.501) (xy 134.239 71.501) (xy 134.239 73.533) (xy 132.08 73.533)
      )
    )
  )
  (zone (net 108) (net_name "Net-(C20-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.254))
    (polygon
      (pts
        (xy 133.2865 68.25488) (xy 132.1054 67.7672) (xy 130.3782 67.7672) (xy 130.3782 69.1896) (xy 132.842 69.1896)
        (xy 132.842 70.866) (xy 136.2202 70.866) (xy 136.2202 69.6722) (xy 134.4422 69.6722) (xy 134.4422 68.25615)
      )
    )
  )
  (zone (net 105) (net_name "Net-(C21-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.254))
    (polygon
      (pts
        (xy 132.5245 69.7865) (xy 129.667 69.7865) (xy 129.667 67.4116) (xy 128.4986 67.4116) (xy 128.4986 70.612)
        (xy 131.0005 70.612) (xy 131.8895 70.612) (xy 131.8895 70.866) (xy 132.5245 70.866)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.254))
    (polygon
      (pts
        (xy 150.6855 62.738) (xy 164.0205 62.738) (xy 164.0205 58.42) (xy 138.557 58.42) (xy 138.557 69.342)
        (xy 135.4455 69.342) (xy 135.4455 61.595) (xy 116.9035 61.595) (xy 116.9035 69.342) (xy 120.142 69.342)
        (xy 120.142 66.4845) (xy 122.3645 66.4845) (xy 122.3645 69.342) (xy 125.2855 69.342) (xy 125.2855 73.533)
        (xy 125.2855 74.422) (xy 131.572 80.137) (xy 151.511 80.137) (xy 157.734 80.137) (xy 157.734 75.311)
        (xy 156.083 74.295) (xy 150.6855 69.0245)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.08 58.2295) (xy 138.557 58.2295) (xy 138.557 69.2785) (xy 135.4455 69.2785) (xy 135.43915 63.5508)
        (xy 132.07365 63.5508)
      )
    )
  )
  (zone (net 47) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.127))
    (polygon
      (pts
        (xy 136.2964 93.1418) (xy 135.0264 94.4118) (xy 134.8105 94.8055) (xy 135.68045 94.67215) (xy 136.75995 93.59265)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.8166 65.532) (xy 134.8994 65.532) (xy 134.8994 68.072) (xy 132.8166 68.072)
      )
    )
  )
)
