(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 1.6)
    (drawings 5)
    (tracks 664)
    (zones 0)
    (modules 64)
    (nets 113)
  )
  (page A4)
  (title_block
    (title Thermometry)
    (rev v1.0)
    (comment 4 "Eric Cheng")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user hide)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.508)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 1.27)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.762)
    (via_drill 0.381)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.762)
    (uvia_drill 0.381)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 0.5)
    (pad_drill 2)
    (pad_to_mask_clearance 0.000051)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(0.1uF1-Pad1)")
  (net 2 "Net-(0.1uF1-Pad2)")
  (net 3 +3V3)
  (net 4 GND)
  (net 5 "Net-(ADC1-Pad5)")
  (net 6 /CLK)
  (net 7 "Net-(ADC1-Pad3)")
  (net 8 /SDI)
  (net 9 /CS_1)
  (net 10 "Net-(ADC1-Pad8)")
  (net 11 "Net-(ADC1-Pad11)")
  (net 12 "Net-(ADC1-Pad10)")
  (net 13 "Net-(ADC1-Pad9)")
  (net 14 "Net-(ADC1-Pad12)")
  (net 15 "Net-(ADC2-Pad12)")
  (net 16 "Net-(ADC2-Pad9)")
  (net 17 "Net-(ADC2-Pad10)")
  (net 18 "Net-(ADC2-Pad11)")
  (net 19 "Net-(ADC2-Pad8)")
  (net 20 /CS_2)
  (net 21 "Net-(ADC2-Pad3)")
  (net 22 "Net-(ADC2-Pad5)")
  (net 23 "Net-(ADC3-Pad5)")
  (net 24 "Net-(ADC3-Pad3)")
  (net 25 /CS_3)
  (net 26 "Net-(ADC3-Pad8)")
  (net 27 "Net-(ADC3-Pad11)")
  (net 28 "Net-(ADC3-Pad10)")
  (net 29 "Net-(ADC3-Pad9)")
  (net 30 "Net-(ADC3-Pad12)")
  (net 31 "Net-(ADC4-Pad12)")
  (net 32 "Net-(ADC4-Pad9)")
  (net 33 "Net-(ADC4-Pad10)")
  (net 34 "Net-(ADC4-Pad11)")
  (net 35 "Net-(ADC4-Pad8)")
  (net 36 /CS_4)
  (net 37 "Net-(ADC4-Pad3)")
  (net 38 "Net-(ADC4-Pad5)")
  (net 39 "Net-(ADC5-Pad5)")
  (net 40 "Net-(ADC5-Pad3)")
  (net 41 /CS_5)
  (net 42 "Net-(ADC5-Pad8)")
  (net 43 "Net-(ADC5-Pad11)")
  (net 44 "Net-(ADC5-Pad10)")
  (net 45 "Net-(ADC5-Pad9)")
  (net 46 "Net-(ADC5-Pad12)")
  (net 47 "Net-(ADC6-Pad5)")
  (net 48 "Net-(ADC6-Pad2)")
  (net 49 /CS_6)
  (net 50 "Net-(ADC6-Pad8)")
  (net 51 "Net-(ADC6-Pad9)")
  (net 52 "Net-(ADC6-Pad10)")
  (net 53 "Net-(ADC6-Pad11)")
  (net 54 "Net-(ADC7-Pad11)")
  (net 55 "Net-(ADC7-Pad10)")
  (net 56 "Net-(ADC7-Pad9)")
  (net 57 "Net-(ADC7-Pad8)")
  (net 58 /CS_7)
  (net 59 "Net-(ADC7-Pad2)")
  (net 60 "Net-(ADC7-Pad5)")
  (net 61 "Net-(CP1-Pad1)")
  (net 62 /5V)
  (net 63 /TFT_DC)
  (net 64 /TFT_CS)
  (net 65 /SDO)
  (net 66 /T_CS)
  (net 67 /T_IRQ)
  (net 68 "Net-(MCU1-Pad45)")
  (net 69 "Net-(MCU1-Pad44)")
  (net 70 "Net-(MCU1-Pad43)")
  (net 71 "Net-(MCU1-Pad42)")
  (net 72 "Net-(MCU1-Pad41)")
  (net 73 "Net-(MCU1-Pad39)")
  (net 74 "Net-(MCU1-Pad38)")
  (net 75 "Net-(MCU1-Pad37)")
  (net 76 "Net-(MCU1-Pad36)")
  (net 77 "Net-(MCU1-Pad35)")
  (net 78 "Net-(MCU1-Pad1)")
  (net 79 "Net-(MCU1-Pad2)")
  (net 80 "Net-(MCU1-Pad3)")
  (net 81 "Net-(MCU1-Pad4)")
  (net 82 "Net-(MCU1-Pad5)")
  (net 83 "Net-(MCU1-Pad6)")
  (net 84 "Net-(MCU1-Pad13)")
  (net 85 "Net-(MCU1-Pad24)")
  (net 86 "Net-(MCU1-Pad23)")
  (net 87 "Net-(MCU1-Pad22)")
  (net 88 "Net-(MCU1-Pad15)")
  (net 89 "Net-(MCU1-Pad20)")
  (net 90 "Net-(MCU1-Pad18)")
  (net 91 "Net-(MCU1-Pad17)")
  (net 92 "Net-(MCU1-Pad60)")
  (net 93 "Net-(MCU1-Pad65)")
  (net 94 "Net-(MCU1-Pad61)")
  (net 95 "Net-(MCU1-Pad63)")
  (net 96 "Net-(MCU1-Pad62)")
  (net 97 "Net-(R10-Pad2)")
  (net 98 "Net-(Teensy_Ethernet1-Pad7)")
  (net 99 "Net-(Teensy_Ethernet1-Pad12)")
  (net 100 "Net-(Teensy_Ethernet1-Pad11)")
  (net 101 "Net-(U1-Pad2)")
  (net 102 /CS_8)
  (net 103 "Net-(J1-Pad0)")
  (net 104 "Net-(ILI9341TFT3-Pad9)")
  (net 105 "Net-(ILI9341TFT3-Pad13)")
  (net 106 "Net-(MCU1-Pad7)")
  (net 107 "Net-(MCU1-Pad8)")
  (net 108 "Net-(MCU1-Pad9)")
  (net 109 "Net-(MCU1-Pad10)")
  (net 110 "Net-(MCU1-Pad11)")
  (net 111 "Net-(MCU1-Pad12)")
  (net 112 "Net-(MCU1-Pad30)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.762)
    (uvia_drill 0.381)
    (add_net +3V3)
    (add_net /5V)
    (add_net /CLK)
    (add_net /CS_1)
    (add_net /CS_2)
    (add_net /CS_3)
    (add_net /CS_4)
    (add_net /CS_5)
    (add_net /CS_6)
    (add_net /CS_7)
    (add_net /CS_8)
    (add_net /SDI)
    (add_net /SDO)
    (add_net /TFT_CS)
    (add_net /TFT_DC)
    (add_net /T_CS)
    (add_net /T_IRQ)
    (add_net GND)
    (add_net "Net-(0.1uF1-Pad1)")
    (add_net "Net-(0.1uF1-Pad2)")
    (add_net "Net-(ADC1-Pad10)")
    (add_net "Net-(ADC1-Pad11)")
    (add_net "Net-(ADC1-Pad12)")
    (add_net "Net-(ADC1-Pad3)")
    (add_net "Net-(ADC1-Pad5)")
    (add_net "Net-(ADC1-Pad8)")
    (add_net "Net-(ADC1-Pad9)")
    (add_net "Net-(ADC2-Pad10)")
    (add_net "Net-(ADC2-Pad11)")
    (add_net "Net-(ADC2-Pad12)")
    (add_net "Net-(ADC2-Pad3)")
    (add_net "Net-(ADC2-Pad5)")
    (add_net "Net-(ADC2-Pad8)")
    (add_net "Net-(ADC2-Pad9)")
    (add_net "Net-(ADC3-Pad10)")
    (add_net "Net-(ADC3-Pad11)")
    (add_net "Net-(ADC3-Pad12)")
    (add_net "Net-(ADC3-Pad3)")
    (add_net "Net-(ADC3-Pad5)")
    (add_net "Net-(ADC3-Pad8)")
    (add_net "Net-(ADC3-Pad9)")
    (add_net "Net-(ADC4-Pad10)")
    (add_net "Net-(ADC4-Pad11)")
    (add_net "Net-(ADC4-Pad12)")
    (add_net "Net-(ADC4-Pad3)")
    (add_net "Net-(ADC4-Pad5)")
    (add_net "Net-(ADC4-Pad8)")
    (add_net "Net-(ADC4-Pad9)")
    (add_net "Net-(ADC5-Pad10)")
    (add_net "Net-(ADC5-Pad11)")
    (add_net "Net-(ADC5-Pad12)")
    (add_net "Net-(ADC5-Pad3)")
    (add_net "Net-(ADC5-Pad5)")
    (add_net "Net-(ADC5-Pad8)")
    (add_net "Net-(ADC5-Pad9)")
    (add_net "Net-(ADC6-Pad10)")
    (add_net "Net-(ADC6-Pad11)")
    (add_net "Net-(ADC6-Pad2)")
    (add_net "Net-(ADC6-Pad5)")
    (add_net "Net-(ADC6-Pad8)")
    (add_net "Net-(ADC6-Pad9)")
    (add_net "Net-(ADC7-Pad10)")
    (add_net "Net-(ADC7-Pad11)")
    (add_net "Net-(ADC7-Pad2)")
    (add_net "Net-(ADC7-Pad5)")
    (add_net "Net-(ADC7-Pad8)")
    (add_net "Net-(ADC7-Pad9)")
    (add_net "Net-(CP1-Pad1)")
    (add_net "Net-(ILI9341TFT3-Pad13)")
    (add_net "Net-(ILI9341TFT3-Pad9)")
    (add_net "Net-(J1-Pad0)")
    (add_net "Net-(MCU1-Pad1)")
    (add_net "Net-(MCU1-Pad10)")
    (add_net "Net-(MCU1-Pad11)")
    (add_net "Net-(MCU1-Pad12)")
    (add_net "Net-(MCU1-Pad13)")
    (add_net "Net-(MCU1-Pad15)")
    (add_net "Net-(MCU1-Pad17)")
    (add_net "Net-(MCU1-Pad18)")
    (add_net "Net-(MCU1-Pad2)")
    (add_net "Net-(MCU1-Pad20)")
    (add_net "Net-(MCU1-Pad22)")
    (add_net "Net-(MCU1-Pad23)")
    (add_net "Net-(MCU1-Pad24)")
    (add_net "Net-(MCU1-Pad3)")
    (add_net "Net-(MCU1-Pad30)")
    (add_net "Net-(MCU1-Pad35)")
    (add_net "Net-(MCU1-Pad36)")
    (add_net "Net-(MCU1-Pad37)")
    (add_net "Net-(MCU1-Pad38)")
    (add_net "Net-(MCU1-Pad39)")
    (add_net "Net-(MCU1-Pad4)")
    (add_net "Net-(MCU1-Pad41)")
    (add_net "Net-(MCU1-Pad42)")
    (add_net "Net-(MCU1-Pad43)")
    (add_net "Net-(MCU1-Pad44)")
    (add_net "Net-(MCU1-Pad45)")
    (add_net "Net-(MCU1-Pad5)")
    (add_net "Net-(MCU1-Pad6)")
    (add_net "Net-(MCU1-Pad60)")
    (add_net "Net-(MCU1-Pad61)")
    (add_net "Net-(MCU1-Pad62)")
    (add_net "Net-(MCU1-Pad63)")
    (add_net "Net-(MCU1-Pad65)")
    (add_net "Net-(MCU1-Pad7)")
    (add_net "Net-(MCU1-Pad8)")
    (add_net "Net-(MCU1-Pad9)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(Teensy_Ethernet1-Pad11)")
    (add_net "Net-(Teensy_Ethernet1-Pad12)")
    (add_net "Net-(Teensy_Ethernet1-Pad7)")
    (add_net "Net-(U1-Pad2)")
  )
  (module Thermometry:breakoff (layer F.Cu) (tedit 6206E601)
    (at 121.031 151.257 90)
    (fp_text reference REF** (at 0 1.27 90) (layer Dwgs.User) hide)
    (fp_text value breakoff (at 0 -1.27 90) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0 90) (size 2 0.5) (drill oval 2 0.5) (layers *.Cu *.Mask))
  )
  (module Thermometry:breakoff (layer F.Cu) (tedit 6206E601)
    (at 121.031 149.225 90)
    (fp_text reference REF** (at 0 1.27 90) (layer Dwgs.User) hide)
    (fp_text value breakoff (at 0 -1.27 90) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0 90) (size 2 0.5) (drill oval 2 0.5) (layers *.Cu *.Mask))
  )
  (module Thermometry:breakoff (layer F.Cu) (tedit 6206E601)
    (at 121.031 147.066 90)
    (fp_text reference REF** (at 0 1.27 90) (layer Dwgs.User) hide)
    (fp_text value breakoff (at 0 -1.27 90) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0 90) (size 2 0.5) (drill oval 2 0.5) (layers *.Cu *.Mask))
  )
  (module Thermometry:breakoff (layer F.Cu) (tedit 6206E601)
    (at 121.031 145.034 90)
    (fp_text reference REF** (at 0 1.27 90) (layer Dwgs.User) hide)
    (fp_text value breakoff (at 0 -1.27 90) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0 90) (size 2 0.5) (drill oval 2 0.5) (layers *.Cu *.Mask))
  )
  (module Thermometry:breakoff (layer F.Cu) (tedit 6206E601)
    (at 121.031 142.875 90)
    (fp_text reference REF** (at 0 1.27 90) (layer Dwgs.User) hide)
    (fp_text value breakoff (at 0 -1.27 90) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0 90) (size 2 0.5) (drill oval 2 0.5) (layers *.Cu *.Mask))
  )
  (module Thermometry:breakoff (layer F.Cu) (tedit 6206E601)
    (at 121.031 140.843 90)
    (fp_text reference REF** (at 0 1.27 90) (layer Dwgs.User) hide)
    (fp_text value breakoff (at 0 -1.27 90) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0 90) (size 2 0.5) (drill oval 2 0.5) (layers *.Cu *.Mask))
  )
  (module Thermometry:breakoff (layer F.Cu) (tedit 6206E601)
    (at 121.031 138.684 90)
    (fp_text reference REF** (at 0 1.27 90) (layer Dwgs.User) hide)
    (fp_text value breakoff (at 0 -1.27 90) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0 90) (size 2 0.5) (drill oval 2 0.5) (layers *.Cu *.Mask))
  )
  (module Thermometry:breakoff (layer F.Cu) (tedit 6206E601)
    (at 121.031 136.652 90)
    (fp_text reference REF** (at 0 1.27 90) (layer Dwgs.User) hide)
    (fp_text value breakoff (at 0 -1.27 90) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0 90) (size 2 0.5) (drill oval 2 0.5) (layers *.Cu *.Mask))
  )
  (module Thermometry:breakoff (layer F.Cu) (tedit 6206E601)
    (at 121.031 134.493 90)
    (fp_text reference REF** (at 0 1.27 90) (layer Dwgs.User) hide)
    (fp_text value breakoff (at 0 -1.27 90) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0 90) (size 2 0.5) (drill oval 2 0.5) (layers *.Cu *.Mask))
  )
  (module Thermometry:breakoff (layer F.Cu) (tedit 6206E601)
    (at 121.031 132.461 90)
    (fp_text reference REF** (at 0 1.27 90) (layer Dwgs.User) hide)
    (fp_text value breakoff (at 0 -1.27 90) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0 90) (size 2 0.5) (drill oval 2 0.5) (layers *.Cu *.Mask))
  )
  (module Thermometry:breakoff (layer F.Cu) (tedit 6206E601)
    (at 121.031 130.302 90)
    (fp_text reference REF** (at 0 1.27 90) (layer Dwgs.User) hide)
    (fp_text value breakoff (at 0 -1.27 90) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0 90) (size 2 0.5) (drill oval 2 0.5) (layers *.Cu *.Mask))
  )
  (module Thermometry:breakoff (layer F.Cu) (tedit 6206E601)
    (at 121.031 128.27 90)
    (fp_text reference REF** (at 0 1.27 90) (layer Dwgs.User) hide)
    (fp_text value breakoff (at 0 -1.27 90) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0 90) (size 2 0.5) (drill oval 2 0.5) (layers *.Cu *.Mask))
  )
  (module Thermometry:breakoff (layer F.Cu) (tedit 6206E601)
    (at 121.031 126.111 90)
    (fp_text reference REF** (at 0 1.27 90) (layer Dwgs.User) hide)
    (fp_text value breakoff (at 0 -1.27 90) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0 90) (size 2 0.5) (drill oval 2 0.5) (layers *.Cu *.Mask))
  )
  (module Thermometry:breakoff (layer F.Cu) (tedit 6206E601)
    (at 121.031 124.079 90)
    (fp_text reference REF** (at 0 1.27 90) (layer Dwgs.User) hide)
    (fp_text value breakoff (at 0 -1.27 90) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0 90) (size 2 0.5) (drill oval 2 0.5) (layers *.Cu *.Mask))
  )
  (module Thermometry:breakoff (layer F.Cu) (tedit 6206E601)
    (at 121.031 121.92 90)
    (fp_text reference REF** (at 0 1.27 90) (layer Dwgs.User) hide)
    (fp_text value breakoff (at 0 -1.27 90) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0 90) (size 2 0.5) (drill oval 2 0.5) (layers *.Cu *.Mask))
  )
  (module Thermometry:breakoff (layer F.Cu) (tedit 6206E601)
    (at 121.031 119.888 90)
    (fp_text reference REF** (at 0 1.27 90) (layer Dwgs.User) hide)
    (fp_text value breakoff (at 0 -1.27 90) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0 90) (size 2 0.5) (drill oval 2 0.5) (layers *.Cu *.Mask))
  )
  (module Thermometry:breakoff (layer F.Cu) (tedit 6206E601)
    (at 121.031 117.729 90)
    (fp_text reference REF** (at 0 1.27 90) (layer Dwgs.User) hide)
    (fp_text value breakoff (at 0 -1.27 90) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0 90) (size 2 0.5) (drill oval 2 0.5) (layers *.Cu *.Mask))
  )
  (module Thermometry:breakoff (layer F.Cu) (tedit 6206E601)
    (at 121.031 115.697 90)
    (fp_text reference REF** (at 0 1.27 90) (layer Dwgs.User) hide)
    (fp_text value breakoff (at 0 -1.27 90) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0 90) (size 2 0.5) (drill oval 2 0.5) (layers *.Cu *.Mask))
  )
  (module Thermometry:breakoff (layer F.Cu) (tedit 6206E601)
    (at 121.031 113.538 90)
    (fp_text reference REF** (at 0 1.27 90) (layer Dwgs.User) hide)
    (fp_text value breakoff (at 0 -1.27 90) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0 90) (size 2 0.5) (drill oval 2 0.5) (layers *.Cu *.Mask))
  )
  (module Thermometry:breakoff (layer F.Cu) (tedit 6206E601)
    (at 121.031 111.506 90)
    (fp_text reference REF** (at 0 1.27 90) (layer Dwgs.User) hide)
    (fp_text value breakoff (at 0 -1.27 90) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0 90) (size 2 0.5) (drill oval 2 0.5) (layers *.Cu *.Mask))
  )
  (module Thermometry:breakoff (layer F.Cu) (tedit 6206E601)
    (at 121.031 109.347 90)
    (fp_text reference REF** (at 0 1.27 90) (layer Dwgs.User) hide)
    (fp_text value breakoff (at 0 -1.27 90) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0 90) (size 2 0.5) (drill oval 2 0.5) (layers *.Cu *.Mask))
  )
  (module Thermometry:breakoff (layer F.Cu) (tedit 6206E601)
    (at 121.031 107.315 90)
    (fp_text reference REF** (at 0 1.27 90) (layer Dwgs.User) hide)
    (fp_text value breakoff (at 0 -1.27 90) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0 90) (size 2 0.5) (drill oval 2 0.5) (layers *.Cu *.Mask))
  )
  (module Thermometry:breakoff (layer F.Cu) (tedit 6206E601)
    (at 121.031 105.156 90)
    (fp_text reference REF** (at 0 1.27 90) (layer Dwgs.User) hide)
    (fp_text value breakoff (at 0 -1.27 90) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0 90) (size 2 0.5) (drill oval 2 0.5) (layers *.Cu *.Mask))
  )
  (module Thermometry:breakoff (layer F.Cu) (tedit 6206E601)
    (at 139.446 104.013)
    (fp_text reference REF** (at 0 1.27) (layer Dwgs.User) hide)
    (fp_text value breakoff (at 0 -1.27) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0) (size 2 0.5) (drill oval 2 0.5) (layers *.Cu *.Mask))
  )
  (module Thermometry:breakoff (layer F.Cu) (tedit 6206E601)
    (at 137.16 104.013)
    (fp_text reference REF** (at 0 1.27) (layer Dwgs.User) hide)
    (fp_text value breakoff (at 0 -1.27) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0) (size 2 0.5) (drill oval 2 0.5) (layers *.Cu *.Mask))
  )
  (module Thermometry:breakoff (layer F.Cu) (tedit 6206E601)
    (at 135.001 104.013)
    (fp_text reference REF** (at 0 1.27) (layer Dwgs.User) hide)
    (fp_text value breakoff (at 0 -1.27) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0) (size 2 0.5) (drill oval 2 0.5) (layers *.Cu *.Mask))
  )
  (module Thermometry:breakoff (layer F.Cu) (tedit 6206E601)
    (at 132.842 104.013)
    (fp_text reference REF** (at 0 1.27) (layer Dwgs.User) hide)
    (fp_text value breakoff (at 0 -1.27) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0) (size 2 0.5) (drill oval 2 0.5) (layers *.Cu *.Mask))
  )
  (module Thermometry:breakoff (layer F.Cu) (tedit 6206E601)
    (at 130.81 104.013)
    (fp_text reference REF** (at 0 1.27) (layer Dwgs.User) hide)
    (fp_text value breakoff (at 0 -1.27) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0) (size 2 0.5) (drill oval 2 0.5) (layers *.Cu *.Mask))
  )
  (module Thermometry:breakoff (layer F.Cu) (tedit 6206E601)
    (at 128.651 104.013)
    (fp_text reference REF** (at 0 1.27) (layer Dwgs.User) hide)
    (fp_text value breakoff (at 0 -1.27) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0) (size 2 0.5) (drill oval 2 0.5) (layers *.Cu *.Mask))
  )
  (module Thermometry:breakoff (layer F.Cu) (tedit 6206E601)
    (at 126.619 104.013)
    (fp_text reference REF** (at 0 1.27) (layer Dwgs.User) hide)
    (fp_text value breakoff (at 0 -1.27) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0) (size 2 0.5) (drill oval 2 0.5) (layers *.Cu *.Mask))
  )
  (module Thermometry:breakoff (layer F.Cu) (tedit 6206E601)
    (at 124.46 104.013)
    (fp_text reference REF** (at 0 1.27) (layer Dwgs.User) hide)
    (fp_text value breakoff (at 0 -1.27) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0) (size 2 0.5) (drill oval 2 0.5) (layers *.Cu *.Mask))
  )
  (module Thermometry:breakoff (layer F.Cu) (tedit 6206E601)
    (at 122.301 104.013)
    (fp_text reference REF** (at 0 1.27) (layer Dwgs.User) hide)
    (fp_text value breakoff (at 0 -1.27) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0) (size 2 0.5) (drill oval 2 0.5) (layers *.Cu *.Mask))
  )
  (module Thermometry:thermo_fuse (layer F.Cu) (tedit 6206E31A)
    (at 42.418 95.504 180)
    (fp_text reference F1 (at 0 -3.556 180) (layer F.SilkS))
    (fp_text value 1A (at 0 3.556 180) (layer F.Fab))
    (pad 1 smd rect (at -3.5 0 180) (size 4.24 3.81) (layers F.Cu F.Paste F.Mask)
      (net 62 /5V))
    (pad 2 smd rect (at 3.5 0 180) (size 4.24 3.81) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(CP1-Pad1)"))
  )
  (module Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 41.021 103.378 180)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference REF** (at 0 -2.3) (layer F.SilkS))
    (fp_text value C_1210_3225Metric_Pad1.33x2.70mm_HandSolder (at 0 2.3) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.5625 0 180) (size 1.325 2.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.188679))
    (pad 1 smd roundrect (at -1.5625 0 180) (size 1.325 2.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.188679))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Thermometry:MAX31865 (layer F.Cu) (tedit 6206DE05)
    (at 112.522 77.724)
    (fp_text reference ADC4 (at 0 -14.732) (layer F.SilkS))
    (fp_text value PT100 (at 0 14.986) (layer F.Fab))
    (fp_text user VIN (at -8.89 9.652) (layer F.SilkS))
    (fp_text user GND (at -6.35 12.7) (layer F.SilkS))
    (fp_text user 3V3 (at -3.81 9.652) (layer F.SilkS))
    (fp_text user CLK (at -1.27 12.7) (layer F.SilkS))
    (fp_text user SDO (at 1.27 9.652) (layer F.SilkS))
    (fp_text user SDI (at 3.81 12.7) (layer F.SilkS))
    (fp_text user CS (at 6.35 9.652) (layer F.SilkS))
    (fp_text user RDY (at 8.89 12.7) (layer F.SilkS))
    (fp_text user F- (at -5.334 -8.636) (layer F.SilkS))
    (fp_text user F+ (at 5.334 -12.192) (layer F.SilkS))
    (fp_text user RTD+ (at 1.778 -8.636 180) (layer F.SilkS))
    (fp_text user RTD- (at -1.524 -12.192 180) (layer F.SilkS))
    (fp_text user MAX31865 (at -0.1 -0.1) (layer F.SilkS))
    (pad 1 thru_hole circle (at -8.89 11.176) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole circle (at -6.35 11.176) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 5 thru_hole circle (at 1.27 11.176) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(ADC4-Pad5)"))
    (pad 4 thru_hole circle (at -1.27 11.176) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 6 /CLK))
    (pad 3 thru_hole circle (at -3.81 11.176) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(ADC4-Pad3)"))
    (pad 6 thru_hole circle (at 3.81 11.176) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 8 /SDI))
    (pad 7 thru_hole circle (at 6.35 11.176) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 36 /CS_4))
    (pad 8 thru_hole circle (at 8.89 11.176) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(ADC4-Pad8)"))
    (pad 11 thru_hole circle (at -1.778 -10.414) (size 2.184 2.184) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(ADC4-Pad11)"))
    (pad 10 thru_hole circle (at 1.778 -10.414) (size 2.184 2.184) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(ADC4-Pad10)"))
    (pad 9 thru_hole circle (at 5.334 -10.414) (size 2.184 2.184) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(ADC4-Pad9)"))
    (pad 12 thru_hole circle (at -5.334 -10.414) (size 2.184 2.184) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(ADC4-Pad12)"))
  )
  (module Thermometry:MAX31865 (layer F.Cu) (tedit 6206DE05)
    (at 100.076 107.95 270)
    (fp_text reference ADC5 (at 0 -14.732 90) (layer F.SilkS))
    (fp_text value PT100 (at 0 14.986 90) (layer F.Fab))
    (fp_text user VIN (at -8.89 9.652 90) (layer F.SilkS))
    (fp_text user GND (at -6.35 12.7 90) (layer F.SilkS))
    (fp_text user 3V3 (at -3.81 9.652 90) (layer F.SilkS))
    (fp_text user CLK (at -1.27 12.7 90) (layer F.SilkS))
    (fp_text user SDO (at 1.27 9.652 90) (layer F.SilkS))
    (fp_text user SDI (at 3.81 12.7 90) (layer F.SilkS))
    (fp_text user CS (at 6.35 9.652 90) (layer F.SilkS))
    (fp_text user RDY (at 8.89 12.7 90) (layer F.SilkS))
    (fp_text user F- (at -5.334 -8.636 90) (layer F.SilkS))
    (fp_text user F+ (at 5.334 -12.192 90) (layer F.SilkS))
    (fp_text user RTD+ (at 1.778 -8.636 270) (layer F.SilkS))
    (fp_text user RTD- (at -1.524 -12.192 270) (layer F.SilkS))
    (fp_text user MAX31865 (at -0.1 -0.1 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -8.89 11.176 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole circle (at -6.35 11.176 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 5 thru_hole circle (at 1.27 11.176 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(ADC5-Pad5)"))
    (pad 4 thru_hole circle (at -1.27 11.176 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 6 /CLK))
    (pad 3 thru_hole circle (at -3.81 11.176 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(ADC5-Pad3)"))
    (pad 6 thru_hole circle (at 3.81 11.176 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 8 /SDI))
    (pad 7 thru_hole circle (at 6.35 11.176 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 41 /CS_5))
    (pad 8 thru_hole circle (at 8.89 11.176 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(ADC5-Pad8)"))
    (pad 11 thru_hole circle (at -1.778 -10.414 270) (size 2.184 2.184) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(ADC5-Pad11)"))
    (pad 10 thru_hole circle (at 1.778 -10.414 270) (size 2.184 2.184) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(ADC5-Pad10)"))
    (pad 9 thru_hole circle (at 5.334 -10.414 270) (size 2.184 2.184) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(ADC5-Pad9)"))
    (pad 12 thru_hole circle (at -5.334 -10.414 270) (size 2.184 2.184) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(ADC5-Pad12)"))
  )
  (module Thermometry:MAX31865 (layer F.Cu) (tedit 6206DE05)
    (at 59.69 77.724)
    (fp_text reference ADC2 (at 0 -14.732) (layer F.SilkS))
    (fp_text value PT100 (at 0 14.986) (layer F.Fab))
    (fp_text user VIN (at -8.89 9.652) (layer F.SilkS))
    (fp_text user GND (at -6.35 12.7) (layer F.SilkS))
    (fp_text user 3V3 (at -3.81 9.652) (layer F.SilkS))
    (fp_text user CLK (at -1.27 12.7) (layer F.SilkS))
    (fp_text user SDO (at 1.27 9.652) (layer F.SilkS))
    (fp_text user SDI (at 3.81 12.7) (layer F.SilkS))
    (fp_text user CS (at 6.35 9.652) (layer F.SilkS))
    (fp_text user RDY (at 8.89 12.7) (layer F.SilkS))
    (fp_text user F- (at -5.334 -8.636) (layer F.SilkS))
    (fp_text user F+ (at 5.334 -12.192) (layer F.SilkS))
    (fp_text user RTD+ (at 1.778 -8.636 180) (layer F.SilkS))
    (fp_text user RTD- (at -1.524 -12.192 180) (layer F.SilkS))
    (fp_text user MAX31865 (at -0.1 -0.1) (layer F.SilkS))
    (pad 1 thru_hole circle (at -8.89 11.176) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole circle (at -6.35 11.176) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 5 thru_hole circle (at 1.27 11.176) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(ADC2-Pad5)"))
    (pad 4 thru_hole circle (at -1.27 11.176) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 6 /CLK))
    (pad 3 thru_hole circle (at -3.81 11.176) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(ADC2-Pad3)"))
    (pad 6 thru_hole circle (at 3.81 11.176) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 8 /SDI))
    (pad 7 thru_hole circle (at 6.35 11.176) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 20 /CS_2))
    (pad 8 thru_hole circle (at 8.89 11.176) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(ADC2-Pad8)"))
    (pad 11 thru_hole circle (at -1.778 -10.414) (size 2.184 2.184) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(ADC2-Pad11)"))
    (pad 10 thru_hole circle (at 1.778 -10.414) (size 2.184 2.184) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(ADC2-Pad10)"))
    (pad 9 thru_hole circle (at 5.334 -10.414) (size 2.184 2.184) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(ADC2-Pad9)"))
    (pad 12 thru_hole circle (at -5.334 -10.414) (size 2.184 2.184) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(ADC2-Pad12)"))
  )
  (module Thermometry:MAX31865 (layer F.Cu) (tedit 6206DE05)
    (at 86.36 77.724)
    (fp_text reference ADC1 (at 0 -14.732) (layer F.SilkS))
    (fp_text value PT100 (at 0 14.986) (layer F.Fab))
    (fp_text user VIN (at -8.89 9.652) (layer F.SilkS))
    (fp_text user GND (at -6.35 12.7) (layer F.SilkS))
    (fp_text user 3V3 (at -3.81 9.652) (layer F.SilkS))
    (fp_text user CLK (at -1.27 12.7) (layer F.SilkS))
    (fp_text user SDO (at 1.27 9.652) (layer F.SilkS))
    (fp_text user SDI (at 3.81 12.7) (layer F.SilkS))
    (fp_text user CS (at 6.35 9.652) (layer F.SilkS))
    (fp_text user RDY (at 8.89 12.7) (layer F.SilkS))
    (fp_text user F- (at -5.334 -8.636) (layer F.SilkS))
    (fp_text user F+ (at 5.334 -12.192) (layer F.SilkS))
    (fp_text user RTD+ (at 1.778 -8.636 180) (layer F.SilkS))
    (fp_text user RTD- (at -1.524 -12.192 180) (layer F.SilkS))
    (fp_text user MAX31865 (at -0.1 -0.1) (layer F.SilkS))
    (pad 1 thru_hole circle (at -8.89 11.176) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole circle (at -6.35 11.176) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 5 thru_hole circle (at 1.27 11.176) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(ADC1-Pad5)"))
    (pad 4 thru_hole circle (at -1.27 11.176) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 6 /CLK))
    (pad 3 thru_hole circle (at -3.81 11.176) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(ADC1-Pad3)"))
    (pad 6 thru_hole circle (at 3.81 11.176) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 8 /SDI))
    (pad 7 thru_hole circle (at 6.35 11.176) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 9 /CS_1))
    (pad 8 thru_hole circle (at 8.89 11.176) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(ADC1-Pad8)"))
    (pad 11 thru_hole circle (at -1.778 -10.414) (size 2.184 2.184) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(ADC1-Pad11)"))
    (pad 10 thru_hole circle (at 1.778 -10.414) (size 2.184 2.184) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(ADC1-Pad10)"))
    (pad 9 thru_hole circle (at 5.334 -10.414) (size 2.184 2.184) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(ADC1-Pad9)"))
    (pad 12 thru_hole circle (at -5.334 -10.414) (size 2.184 2.184) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(ADC1-Pad12)"))
  )
  (module Thermometry:MAX31865 (layer F.Cu) (tedit 6206DE05)
    (at 32.766 77.724)
    (fp_text reference ADC3 (at 0 -14.732) (layer F.SilkS))
    (fp_text value PT100 (at 0 14.986) (layer F.Fab))
    (fp_text user VIN (at -8.89 9.652) (layer F.SilkS))
    (fp_text user GND (at -6.35 12.7) (layer F.SilkS))
    (fp_text user 3V3 (at -3.81 9.652) (layer F.SilkS))
    (fp_text user CLK (at -1.27 12.7) (layer F.SilkS))
    (fp_text user SDO (at 1.27 9.652) (layer F.SilkS))
    (fp_text user SDI (at 3.81 12.7) (layer F.SilkS))
    (fp_text user CS (at 6.35 9.652) (layer F.SilkS))
    (fp_text user RDY (at 8.89 12.7) (layer F.SilkS))
    (fp_text user F- (at -5.334 -8.636) (layer F.SilkS))
    (fp_text user F+ (at 5.334 -12.192) (layer F.SilkS))
    (fp_text user RTD+ (at 1.778 -8.636 180) (layer F.SilkS))
    (fp_text user RTD- (at -1.524 -12.192 180) (layer F.SilkS))
    (fp_text user MAX31865 (at -0.1 -0.1) (layer F.SilkS))
    (pad 1 thru_hole circle (at -8.89 11.176) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole circle (at -6.35 11.176) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 5 thru_hole circle (at 1.27 11.176) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(ADC3-Pad5)"))
    (pad 4 thru_hole circle (at -1.27 11.176) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 6 /CLK))
    (pad 3 thru_hole circle (at -3.81 11.176) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(ADC3-Pad3)"))
    (pad 6 thru_hole circle (at 3.81 11.176) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 8 /SDI))
    (pad 7 thru_hole circle (at 6.35 11.176) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 25 /CS_3))
    (pad 8 thru_hole circle (at 8.89 11.176) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(ADC3-Pad8)"))
    (pad 11 thru_hole circle (at -1.778 -10.414) (size 2.184 2.184) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(ADC3-Pad11)"))
    (pad 10 thru_hole circle (at 1.778 -10.414) (size 2.184 2.184) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(ADC3-Pad10)"))
    (pad 9 thru_hole circle (at 5.334 -10.414) (size 2.184 2.184) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(ADC3-Pad9)"))
    (pad 12 thru_hole circle (at -5.334 -10.414) (size 2.184 2.184) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(ADC3-Pad12)"))
  )
  (module Connector_RJ:RJ45_Cetus_J1B1211CCD_Horizontal (layer F.Cu) (tedit 5BBCB15F)
    (at 36.32 134.24 270)
    (descr "1 Port RJ45 Magjack Connector Through Hole 10/100 Base-T, Cetus, used and distributed by WIZnet (https://wizwiki.net/wiki/lib/exe/fetch.php?media=products:wiz550web:wiz550webds_kr:j1b1211ccd.pdf)")
    (tags "RJ45 Magjack")
    (fp_text reference Teensy_Ethernet1 (at 5 -5 90) (layer F.SilkS))
    (fp_text value RJ45_LED (at 4.445 18 90) (layer F.Fab))
    (fp_text user %R (at 4 16 90) (layer F.Fab))
    (pad 11 thru_hole circle (at 8.23 11.43 270) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 100 "Net-(Teensy_Ethernet1-Pad11)"))
    (pad 12 thru_hole circle (at 10.77 9.73 270) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 99 "Net-(Teensy_Ethernet1-Pad12)"))
    (pad 10 thru_hole circle (at 0.66 9.73 270) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 94 "Net-(MCU1-Pad61)"))
    (pad 9 thru_hole circle (at -1.88 11.43 270) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 "Net-(0.1uF1-Pad2)"))
    (pad 13 thru_hole circle (at 12.32 3.3 270) (size 2.5 2.5) (drill 1.6) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 8.89 -2.54 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(0.1uF1-Pad2)"))
    (pad 13 thru_hole circle (at -3.43 3.3 270) (size 2.5 2.5) (drill 1.6) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 7.62 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 98 "Net-(Teensy_Ethernet1-Pad7)"))
    (pad 6 thru_hole circle (at 6.35 -2.54 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 93 "Net-(MCU1-Pad65)"))
    (pad 5 thru_hole circle (at 5.08 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(0.1uF1-Pad1)"))
    (pad 4 thru_hole circle (at 3.81 -2.54 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 92 "Net-(MCU1-Pad60)"))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 96 "Net-(MCU1-Pad62)"))
    (pad 2 thru_hole circle (at 1.27 -2.54 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(0.1uF1-Pad1)"))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.167)
      (net 95 "Net-(MCU1-Pad63)"))
    (pad "" np_thru_hole circle (at -1.27 6.35 270) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 10.16 6.35 270) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_RJ.3dshapes/RJ45_Cetus_J1B1211CCD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 98.06 139.7)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 22 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 97 "Net-(R10-Pad2)"))
    (pad 1 smd roundrect (at -1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 65 /SDO))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 44.45 137.2 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference 0.1uF1 (at 1.25 -2.05 90) (layer F.SilkS))
    (fp_text value C1 (at 1.25 2.05 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(0.1uF1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(0.1uF1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 41.91 100.33 180)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference CP1 (at 1 -3.75) (layer F.SilkS))
    (fp_text value 47uF (at 1 3.75) (layer F.Fab))
    (fp_text user %R (at 1 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 "Net-(CP1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_BarrelJack:BarrelJack_Horizontal (layer F.Cu) (tedit 5A1DBF6A)
    (at 32.21 98.17)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference J2 (at -8.45 5.75) (layer F.SilkS))
    (fp_text value Barrel_Jack (at -6.2 -5.5) (layer F.Fab))
    (fp_text user %R (at -3 -2.95) (layer F.Fab))
    (pad 3 thru_hole roundrect (at -3 4.7) (size 3.5 3.5) (drill oval 3 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
    (pad 2 thru_hole roundrect (at -6 0) (size 3 3.5) (drill oval 1 3) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 1 thru_hole rect (at 0 0) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 61 "Net-(CP1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_BarrelJack.3dshapes/BarrelJack_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 50.8 118.38 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 22 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 8 /SDI))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 84 "Net-(MCU1-Pad13)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 55.61 111.76 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 22 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 77 "Net-(MCU1-Pad35)"))
    (pad 1 smd roundrect (at -1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 6 /CLK))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 114.3 84.82 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 22 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 38 "Net-(ADC4-Pad5)"))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 65 /SDO))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 84.09 110.49)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 22 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at -1.016 0.508) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 39 "Net-(ADC5-Pad5)"))
    (pad 1 smd roundrect (at -1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 65 /SDO))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 34.29 83.55 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 22 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 23 "Net-(ADC3-Pad5)"))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 65 /SDO))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 60.96 84.82 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 22 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 22 "Net-(ADC2-Pad5)"))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 65 /SDO))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 87.63 84.82 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 22 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 5 "Net-(ADC1-Pad5)"))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 65 /SDO))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 61.23 127)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 22 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 47 "Net-(ADC6-Pad5)"))
    (pad 1 smd roundrect (at -1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 65 /SDO))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 86.63 135.89)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 22 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 60 "Net-(ADC7-Pad5)"))
    (pad 1 smd roundrect (at -1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 65 /SDO))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 128.524 112.268 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R11 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 22 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 65 /SDO))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 104 "Net-(ILI9341TFT3-Pad9)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 130.81 110.236 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R12 (at 0 -1.524 90) (layer F.SilkS))
    (fp_text value 22 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 65 /SDO))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 105 "Net-(ILI9341TFT3-Pad13)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 124.0536 98.1456)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R13 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 0 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 103 "Net-(J1-Pad0)"))
    (pad 1 smd roundrect (at -1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 4 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Thermometry:MAX31856 (layer F.Cu) (tedit 61257442)
    (at 62.23 139.065 180)
    (fp_text reference ADC6 (at 0 -11.684) (layer F.SilkS))
    (fp_text value thermocouple1 (at 0 11.938) (layer F.Fab))
    (fp_text user MAX31856 (at 0 0) (layer F.SilkS))
    (fp_text user + (at -1.778 -8.89) (layer F.SilkS))
    (fp_text user - (at 1.778 -8.89) (layer F.SilkS))
    (fp_text user VIN (at -10.16 6.604) (layer F.SilkS))
    (fp_text user 3Vo (at -7.62 9.906) (layer F.SilkS))
    (fp_text user GND (at -5.08 6.604) (layer F.SilkS))
    (fp_text user SCK (at -2.54 9.906) (layer F.SilkS))
    (fp_text user SDO (at 0 6.604) (layer F.SilkS))
    (fp_text user SDI (at 2.54 9.906) (layer F.SilkS))
    (fp_text user CS (at 5.08 6.604) (layer F.SilkS))
    (fp_text user FLT (at 7.62 9.906) (layer F.SilkS))
    (fp_text user DRDY (at 10.16 6.604) (layer F.SilkS))
    (pad 5 thru_hole circle (at 0 8.255 180) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(ADC6-Pad5)"))
    (pad 4 thru_hole circle (at -2.54 8.255 180) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 6 /CLK))
    (pad 3 thru_hole circle (at -5.08 8.255 180) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at -7.62 8.255 180) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(ADC6-Pad2)"))
    (pad 1 thru_hole circle (at -10.16 8.255 180) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 6 thru_hole circle (at 2.54 8.255 180) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 8 /SDI))
    (pad 7 thru_hole circle (at 5.08 8.255 180) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 49 /CS_6))
    (pad 8 thru_hole circle (at 7.62 8.255 180) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(ADC6-Pad8)"))
    (pad 9 thru_hole circle (at 10.16 8.255 180) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(ADC6-Pad9)"))
    (pad 10 thru_hole circle (at -1.778 -6.985 180) (size 2.184 2.184) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(ADC6-Pad10)"))
    (pad 11 thru_hole circle (at 1.778 -6.985 180) (size 2.184 2.184) (drill 1) (layers *.Cu *.Mask)
      (net 53 "Net-(ADC6-Pad11)"))
  )
  (module Thermometry:MAX31856 (layer F.Cu) (tedit 61257442)
    (at 87.63 139.065 180)
    (fp_text reference ADC7 (at 0 -11.684) (layer F.SilkS))
    (fp_text value thermocouple2 (at 0 11.938) (layer F.Fab))
    (fp_text user MAX31856 (at 0 0) (layer F.SilkS))
    (fp_text user + (at -1.778 -8.89) (layer F.SilkS))
    (fp_text user - (at 1.778 -8.89) (layer F.SilkS))
    (fp_text user VIN (at -10.16 6.604) (layer F.SilkS))
    (fp_text user 3Vo (at -7.62 9.906) (layer F.SilkS))
    (fp_text user GND (at -5.08 6.604) (layer F.SilkS))
    (fp_text user SCK (at -2.54 9.906) (layer F.SilkS))
    (fp_text user SDO (at 0 6.604) (layer F.SilkS))
    (fp_text user SDI (at 2.54 9.906) (layer F.SilkS))
    (fp_text user CS (at 5.08 6.604) (layer F.SilkS))
    (fp_text user FLT (at 7.62 9.906) (layer F.SilkS))
    (fp_text user DRDY (at 10.16 6.604) (layer F.SilkS))
    (pad 5 thru_hole circle (at 0 8.255 180) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(ADC7-Pad5)"))
    (pad 4 thru_hole circle (at -2.54 8.255 180) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 6 /CLK))
    (pad 3 thru_hole circle (at -5.08 8.255 180) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at -7.62 8.255 180) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(ADC7-Pad2)"))
    (pad 1 thru_hole circle (at -10.16 8.255 180) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 6 thru_hole circle (at 2.54 8.255 180) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 8 /SDI))
    (pad 7 thru_hole circle (at 5.08 8.255 180) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 58 /CS_7))
    (pad 8 thru_hole circle (at 7.62 8.255 180) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(ADC7-Pad8)"))
    (pad 9 thru_hole circle (at 10.16 8.255 180) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(ADC7-Pad9)"))
    (pad 10 thru_hole circle (at -1.778 -6.985 180) (size 2.184 2.184) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(ADC7-Pad10)"))
    (pad 11 thru_hole circle (at 1.778 -6.985 180) (size 2.184 2.184) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Net-(ADC7-Pad11)"))
  )
  (module Thermometry:BME280 (layer F.Cu) (tedit 61257448)
    (at 109.22 137.16 270)
    (fp_text reference U1 (at 0 -9.652 90) (layer F.SilkS))
    (fp_text value BME280 (at 0 9.906 90) (layer F.Fab))
    (fp_text user BME280 (at 0 0 90) (layer F.SilkS))
    (fp_text user CS (at 7.62 4.826 90) (layer F.SilkS))
    (fp_text user SDI (at 5.08 7.874 90) (layer F.SilkS))
    (fp_text user SDO (at 2.54 4.826 90) (layer F.SilkS))
    (fp_text user SCK (at 0 7.874 90) (layer F.SilkS))
    (fp_text user GND (at -2.54 4.826 90) (layer F.SilkS))
    (fp_text user 3Vo (at -5.08 7.874 90) (layer F.SilkS))
    (fp_text user VIN (at -7.62 4.826 90) (layer F.SilkS))
    (pad 7 thru_hole circle (at 7.62 6.35 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 102 /CS_8))
    (pad 6 thru_hole circle (at 5.08 6.35 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 8 /SDI))
    (pad 5 thru_hole circle (at 2.54 6.35 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 97 "Net-(R10-Pad2)"))
    (pad 1 thru_hole circle (at -7.62 6.35 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole circle (at -5.08 6.35 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 101 "Net-(U1-Pad2)"))
    (pad 3 thru_hole circle (at -2.54 6.35 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 4 thru_hole circle (at 0 6.35 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 6 /CLK))
  )
  (module Thermometry:ILI9341_1x14_connector (layer F.Cu) (tedit 611DBBDE)
    (at 134.874 123.19 90)
    (fp_text reference ILI9341TFT3 (at -10.16 -2.54 90) (layer F.SilkS))
    (fp_text value Conn_01x14 (at 0 6.35 90) (layer F.Fab))
    (fp_text user T_IRQ (at 16.51 2.794) (layer F.SilkS))
    (fp_text user T_DO (at 13.97 2.54) (layer F.SilkS))
    (fp_text user T_DIN (at 11.43 2.794) (layer F.SilkS))
    (fp_text user T_CS (at 8.89 2.54) (layer F.SilkS))
    (fp_text user T_CLK (at 6.35 3.048) (layer F.SilkS))
    (fp_text user SDO (at 3.81 2.286) (layer F.SilkS))
    (fp_text user LED (at 1.27 2.286) (layer F.SilkS))
    (fp_text user SCK (at -1.27 2.286) (layer F.SilkS))
    (fp_text user SDI (at -3.81 2.032) (layer F.SilkS))
    (fp_text user D/C (at -6.35 2.286) (layer F.SilkS))
    (fp_text user RESET (at -8.89 3.048) (layer F.SilkS))
    (fp_text user CS (at -11.43 1.778) (layer F.SilkS))
    (fp_text user GND (at -13.97 2.286) (layer F.SilkS))
    (fp_text user VCC (at -16.51 2.286) (layer F.SilkS))
    (pad 14 thru_hole circle (at 16.51 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 67 /T_IRQ))
    (pad 13 thru_hole circle (at 13.97 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 105 "Net-(ILI9341TFT3-Pad13)"))
    (pad 12 thru_hole circle (at 11.43 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 /SDI))
    (pad 11 thru_hole circle (at 8.89 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 66 /T_CS))
    (pad 10 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 /CLK))
    (pad 9 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 104 "Net-(ILI9341TFT3-Pad9)"))
    (pad 1 thru_hole circle (at -16.51 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole circle (at -13.97 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -11.43 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 64 /TFT_CS))
    (pad 4 thru_hole circle (at -8.89 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 5 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 63 /TFT_DC))
    (pad 8 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 6 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 /SDI))
    (pad 7 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 /CLK))
  )
  (module Thermometry:ILI9341_2x7_connector (layer F.Cu) (tedit 611DBDC4)
    (at 71.12 99.06)
    (fp_text reference ILI9341TFT1 (at -10.16 -1.27 90) (layer F.SilkS))
    (fp_text value Conn_01x14 (at 0 7.62) (layer F.Fab))
    (fp_text user T_IRQ (at -7.62 -4.064 270) (layer F.SilkS))
    (fp_text user T_DO (at -5.08 -3.81 270) (layer F.SilkS))
    (fp_text user T_DIN (at -2.54 -4.064 270) (layer F.SilkS))
    (fp_text user T_CS (at 0 -4.064 270) (layer F.SilkS))
    (fp_text user T_CLK (at 2.54 -4.318 90) (layer F.SilkS))
    (fp_text user SDO (at 5.08 -3.556 270) (layer F.SilkS))
    (fp_text user LED (at 7.62 -3.556 270) (layer F.SilkS))
    (fp_text user SCK (at 7.62 3.556 90) (layer F.SilkS))
    (fp_text user SDI (at 5.08 3.302 90) (layer F.SilkS))
    (fp_text user D/C (at 2.54 3.556 90) (layer F.SilkS))
    (fp_text user RESET (at 0 4.318 270) (layer F.SilkS))
    (fp_text user CS (at -2.54 3.048 90) (layer F.SilkS))
    (fp_text user GND (at -5.08 3.556 90) (layer F.SilkS))
    (fp_text user VCC (at -7.62 3.556 90) (layer F.SilkS))
    (pad 14 thru_hole circle (at -7.62 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 67 /T_IRQ))
    (pad 13 thru_hole circle (at -5.08 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 65 /SDO))
    (pad 12 thru_hole circle (at -2.54 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 /SDI))
    (pad 11 thru_hole circle (at 0 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 66 /T_CS))
    (pad 10 thru_hole circle (at 2.54 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 /CLK))
    (pad 9 thru_hole circle (at 5.08 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 65 /SDO))
    (pad 1 thru_hole circle (at -7.62 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole circle (at -5.08 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -2.54 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 64 /TFT_CS))
    (pad 4 thru_hole circle (at 0 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 5 thru_hole circle (at 2.54 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 63 /TFT_DC))
    (pad 8 thru_hole circle (at 7.62 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 6 thru_hole circle (at 5.08 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 /SDI))
    (pad 7 thru_hole circle (at 7.62 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 /CLK))
  )
  (module Thermometry:ILI9341_2x7_connector (layer B.Cu) (tedit 611DBDC4)
    (at 126.492 123.19 270)
    (fp_text reference ILI9341TFT2 (at -9.906 2.286 180) (layer B.SilkS))
    (fp_text value Conn_01x14 (at 0 -7.62 270) (layer B.Fab))
    (fp_text user T_IRQ (at -7.62 4.064 180) (layer B.SilkS))
    (fp_text user T_DO (at -5.08 3.81 180) (layer B.SilkS))
    (fp_text user T_DIN (at -2.54 4.064 180) (layer B.SilkS))
    (fp_text user T_CS (at 0 4.064 180) (layer B.SilkS))
    (fp_text user T_CLK (at 2.54 4.318) (layer B.SilkS))
    (fp_text user SDO (at 5.08 3.556 180) (layer B.SilkS))
    (fp_text user LED (at 7.62 3.556 180) (layer B.SilkS))
    (fp_text user SCK (at 7.62 -3.556) (layer B.SilkS))
    (fp_text user SDI (at 5.08 -3.302) (layer B.SilkS))
    (fp_text user D/C (at 2.54 -3.556) (layer B.SilkS))
    (fp_text user RESET (at 0 -4.318) (layer B.SilkS))
    (fp_text user CS (at -2.54 -3.048) (layer B.SilkS))
    (fp_text user GND (at -5.08 -3.556) (layer B.SilkS))
    (fp_text user VCC (at -7.62 -3.556) (layer B.SilkS))
    (pad 14 thru_hole circle (at -7.62 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 67 /T_IRQ))
    (pad 13 thru_hole circle (at -5.08 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 65 /SDO))
    (pad 12 thru_hole circle (at -2.54 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 /SDI))
    (pad 11 thru_hole circle (at 0 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 66 /T_CS))
    (pad 10 thru_hole circle (at 2.54 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 /CLK))
    (pad 9 thru_hole circle (at 5.08 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 65 /SDO))
    (pad 1 thru_hole circle (at -7.62 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole circle (at -5.08 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -2.54 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 64 /TFT_CS))
    (pad 4 thru_hole circle (at 0 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 5 thru_hole circle (at 2.54 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 63 /TFT_DC))
    (pad 8 thru_hole circle (at 7.62 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 6 thru_hole circle (at 5.08 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 /SDI))
    (pad 7 thru_hole circle (at 7.62 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 /CLK))
  )
  (module Thermometry:D15_Female_Horizontal (layer F.Cu) (tedit 6125740B)
    (at 132.08 82.9564 90)
    (descr "15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 4.9399999999999995mm, distance of mounting holes 33.3mm, distance of mounting holes to PCB edge 7.4799999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "15-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 4.9399999999999995mm mounting-holes-distance 33.3mm mounting-hole-offset 33.3mm")
    (fp_text reference J1 (at 0 -6.54 90) (layer F.SilkS))
    (fp_text value DB15_Female (at 0 9.6 90) (layer F.Fab))
    (fp_text user "DB15 Female" (at -14.1 7 90) (layer F.SilkS))
    (fp_text user FRONT (at 0 7 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 9.59 -2.84 90) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "Net-(ADC1-Pad12)"))
    (pad 2 thru_hole circle (at 6.85 -2.84 90) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 "Net-(ADC1-Pad9)"))
    (pad 3 thru_hole circle (at 4.11 -2.84 90) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 17 "Net-(ADC2-Pad10)"))
    (pad 4 thru_hole circle (at 1.37 -2.84 90) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 30 "Net-(ADC3-Pad12)"))
    (pad 5 thru_hole circle (at -1.37 -2.84 90) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 29 "Net-(ADC3-Pad9)"))
    (pad 6 thru_hole circle (at -4.11 -2.84 90) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 33 "Net-(ADC4-Pad10)"))
    (pad 7 thru_hole circle (at -6.85 -2.84 90) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 46 "Net-(ADC5-Pad12)"))
    (pad 8 thru_hole circle (at -9.59 -2.84 90) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 45 "Net-(ADC5-Pad9)"))
    (pad 9 thru_hole circle (at 8.22 0 90) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "Net-(ADC1-Pad10)"))
    (pad 10 thru_hole circle (at 5.48 0 90) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Net-(ADC2-Pad12)"))
    (pad 11 thru_hole circle (at 2.74 0 90) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 "Net-(ADC2-Pad9)"))
    (pad 12 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 28 "Net-(ADC3-Pad10)"))
    (pad 13 thru_hole circle (at -2.74 0 90) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 31 "Net-(ADC4-Pad12)"))
    (pad 14 thru_hole circle (at -5.48 0 90) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 32 "Net-(ADC4-Pad9)"))
    (pad 15 thru_hole circle (at -8.22 0 90) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 44 "Net-(ADC5-Pad10)"))
    (pad 0 thru_hole circle (at -16.66 -1.42 90) (size 3.3 3.3) (drill 3.1) (layers *.Cu *.Mask)
      (net 103 "Net-(J1-Pad0)"))
    (pad 0 thru_hole circle (at 16.66 -1.42 90) (size 3.3 3.3) (drill 3.1) (layers *.Cu *.Mask)
      (net 103 "Net-(J1-Pad0)"))
    (model ${KISYS3DMOD}/Connector_Dsub.3dshapes/DSUB-15_Female_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset7.48mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Thermometry:Teensy41 (layer F.Cu) (tedit 612139A8)
    (at 50.8 115.57)
    (fp_text reference MCU1 (at 0 -10.16) (layer F.SilkS))
    (fp_text value Teensy4.1 (at 0 10.16) (layer F.Fab))
    (fp_text user "Micro SD" (at 27.94 0 90) (layer F.SilkS))
    (fp_text user USB (at -26.67 0 270) (layer F.SilkS))
    (fp_text user Ethernet (at -12.065 -3.2766 90) (layer F.SilkS))
    (pad 48 thru_hole circle (at -29.21 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 62 /5V))
    (pad 47 thru_hole circle (at -26.67 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 46 thru_hole circle (at -24.13 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 45 thru_hole circle (at -21.59 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 68 "Net-(MCU1-Pad45)"))
    (pad 44 thru_hole circle (at -19.05 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 69 "Net-(MCU1-Pad44)"))
    (pad 43 thru_hole circle (at -16.51 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 70 "Net-(MCU1-Pad43)"))
    (pad 42 thru_hole circle (at -13.97 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 71 "Net-(MCU1-Pad42)"))
    (pad 41 thru_hole circle (at -11.43 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 72 "Net-(MCU1-Pad41)"))
    (pad 40 thru_hole circle (at -8.89 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 25 /CS_3))
    (pad 39 thru_hole circle (at -6.35 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 73 "Net-(MCU1-Pad39)"))
    (pad 38 thru_hole circle (at -3.81 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 74 "Net-(MCU1-Pad38)"))
    (pad 37 thru_hole circle (at -1.27 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 75 "Net-(MCU1-Pad37)"))
    (pad 36 thru_hole circle (at 1.27 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 76 "Net-(MCU1-Pad36)"))
    (pad 35 thru_hole circle (at 3.81 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 77 "Net-(MCU1-Pad35)"))
    (pad 1 thru_hole rect (at -29.21 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 78 "Net-(MCU1-Pad1)"))
    (pad 2 thru_hole circle (at -26.67 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 79 "Net-(MCU1-Pad2)"))
    (pad 3 thru_hole circle (at -24.13 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 80 "Net-(MCU1-Pad3)"))
    (pad 4 thru_hole circle (at -21.59 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 81 "Net-(MCU1-Pad4)"))
    (pad 5 thru_hole circle (at -19.05 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 82 "Net-(MCU1-Pad5)"))
    (pad 6 thru_hole circle (at -16.51 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 83 "Net-(MCU1-Pad6)"))
    (pad 7 thru_hole circle (at -13.97 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 106 "Net-(MCU1-Pad7)"))
    (pad 8 thru_hole circle (at -11.43 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 107 "Net-(MCU1-Pad8)"))
    (pad 9 thru_hole circle (at -8.89 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 108 "Net-(MCU1-Pad9)"))
    (pad 10 thru_hole circle (at -6.35 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 109 "Net-(MCU1-Pad10)"))
    (pad 11 thru_hole circle (at -3.81 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 110 "Net-(MCU1-Pad11)"))
    (pad 12 thru_hole circle (at -1.27 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 111 "Net-(MCU1-Pad12)"))
    (pad 13 thru_hole circle (at 1.27 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 84 "Net-(MCU1-Pad13)"))
    (pad 34 thru_hole circle (at 6.35 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 33 thru_hole circle (at 8.89 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 20 /CS_2))
    (pad 32 thru_hole circle (at 11.43 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 64 /TFT_CS))
    (pad 31 thru_hole circle (at 13.97 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 67 /T_IRQ))
    (pad 30 thru_hole circle (at 16.51 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 112 "Net-(MCU1-Pad30)"))
    (pad 29 thru_hole circle (at 19.05 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 66 /T_CS))
    (pad 28 thru_hole circle (at 21.59 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 63 /TFT_DC))
    (pad 27 thru_hole circle (at 24.13 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 /CS_1))
    (pad 26 thru_hole circle (at 26.67 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 36 /CS_4))
    (pad 25 thru_hole circle (at 29.21 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 41 /CS_5))
    (pad 24 thru_hole circle (at 29.21 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 85 "Net-(MCU1-Pad24)"))
    (pad 23 thru_hole circle (at 26.67 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 86 "Net-(MCU1-Pad23)"))
    (pad 22 thru_hole circle (at 24.13 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 87 "Net-(MCU1-Pad22)"))
    (pad 21 thru_hole circle (at 21.59 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 58 /CS_7))
    (pad 14 thru_hole circle (at 3.81 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 65 /SDO))
    (pad 15 thru_hole circle (at 6.35 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 88 "Net-(MCU1-Pad15)"))
    (pad 16 thru_hole circle (at 8.89 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 49 /CS_6))
    (pad 20 thru_hole circle (at 19.05 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 89 "Net-(MCU1-Pad20)"))
    (pad 19 thru_hole circle (at 16.51 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 102 /CS_8))
    (pad 18 thru_hole circle (at 13.97 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 90 "Net-(MCU1-Pad18)"))
    (pad 17 thru_hole circle (at 11.43 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 91 "Net-(MCU1-Pad17)"))
    (pad 60 thru_hole rect (at -16.24 -5.1816) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 92 "Net-(MCU1-Pad60)"))
    (pad 65 thru_hole circle (at -14.24 -5.1816) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 93 "Net-(MCU1-Pad65)"))
    (pad 61 thru_hole circle (at -16.24 -3.1816) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 94 "Net-(MCU1-Pad61)"))
    (pad 64 thru_hole circle (at -14.24 -3.1816) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(0.1uF1-Pad2)"))
    (pad 63 thru_hole circle (at -14.24 -1.1816) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 95 "Net-(MCU1-Pad63)"))
    (pad 62 thru_hole circle (at -16.24 -1.1816) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 "Net-(MCU1-Pad62)"))
    (model ${KICAD_USER_DIR}/teensy.pretty/Teensy_4.1_Assembly.STEP
      (offset (xyz 0 0 0.762))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 140.97 152.4) (end 140.97 60.96) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 17.78 152.4) (end 17.78 60.96) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 17.78 152.4) (end 140.97 152.4) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 17.78 60.96) (end 140.97 60.96) (layer Edge.Cuts) (width 0.0254))
  (gr_text "PC-246-112-05-C01\nEXOThermometry\nEric Cheng / Brian Mong\n" (at 29.972 127.127) (layer F.SilkS))
)
