(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 0)
    (zones 0)
    (modules 10)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.6)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (user_trace_width 2)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.381)
    (via_drill 0.254)
    (via_min_size 0.381)
    (via_min_drill 0.254)
    (user_via 0.4 0.254)
    (user_via 0.6 0.4)
    (user_via 0.8 0.6)
    (user_via 1 0.8)
    (user_via 1.3 1)
    (user_via 1.5 1.2)
    (user_via 1.7 1.4)
    (user_via 1.9 1.6)
    (uvia_size 0.381)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.381)
    (uvia_min_drill 0.254)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (solder_mask_min_width 0.1)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "OSH_Park_2_layer_plots"))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.381)
    (via_drill 0.254)
    (uvia_dia 0.381)
    (uvia_drill 0.254)
  )
  (module SquantorConnectors:Header-0254-1X10-H010 (layer F.Cu) (tedit 5C55B66B)
    (at 132.08 82.55 270)
    (descr "PIN HEADER")
    (tags "PIN HEADER")
    (attr virtual)
    (fp_text reference J1 (at 13.335 1.905 270) (layer F.SilkS) hide)
    (fp_text value PINS_1X10 (at 0 2.1 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at -11.43 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -8.89 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -6.35 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -3.81 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -1.27 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 1.27 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 3.81 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 6.35 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 8.89 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at 11.43 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
  )
  (module SquantorProto:proto-TH-0127-06X06-P010-H006 (layer F.Cu) (tedit 5C55B515)
    (at 144.78 73.66)
    (fp_text reference J2 (at 0 -5.08) (layer F.SilkS) hide)
    (fp_text value Proto (at 0 5.08) (layer F.Fab) hide)
    (pad NC thru_hole rect (at -3.175 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
  )
  (module SquantorProto:proto-TH-0127-06X06-P010-H006 (layer F.Cu) (tedit 5C55B515)
    (at 137.16 73.66)
    (fp_text reference J3 (at 0 -5.08) (layer F.SilkS) hide)
    (fp_text value Proto (at 0 5.08) (layer F.Fab) hide)
    (pad NC thru_hole rect (at -3.175 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
  )
  (module SquantorProto:proto-TH-0127-06X06-P010-H006 (layer F.Cu) (tedit 5C55B515)
    (at 137.16 81.28)
    (fp_text reference J4 (at 0 -5.08) (layer F.SilkS) hide)
    (fp_text value Proto (at 0 5.08) (layer F.Fab) hide)
    (pad NC thru_hole rect (at -3.175 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
  )
  (module SquantorProto:proto-TH-0127-02X06-P010-H006 (layer F.Cu) (tedit 5C55B551)
    (at 137.16 93.98)
    (fp_text reference J5 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value Proto (at 0 2.54) (layer F.Fab) hide)
    (pad NC thru_hole rect (at 0.635 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
  )
  (module SquantorProto:proto-TH-0127-06X06-P010-H006 (layer F.Cu) (tedit 5C55B515)
    (at 144.78 88.9)
    (fp_text reference J6 (at 0 -5.08) (layer F.SilkS) hide)
    (fp_text value Proto (at 0 5.08) (layer F.Fab) hide)
    (pad NC thru_hole rect (at 1.905 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
  )
  (module SquantorProto:proto-TH-0127-06X06-P010-H006 (layer F.Cu) (tedit 5C55B515)
    (at 144.78 81.28)
    (fp_text reference J7 (at 0 -5.08) (layer F.SilkS) hide)
    (fp_text value Proto (at 0 5.08) (layer F.Fab) hide)
    (pad NC thru_hole rect (at 1.905 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
  )
  (module SquantorProto:proto-TH-0127-06X06-P010-H006 (layer F.Cu) (tedit 5C55B515)
    (at 137.16 88.9)
    (fp_text reference J8 (at 0 -5.08) (layer F.SilkS) hide)
    (fp_text value Proto (at 0 5.08) (layer F.Fab) hide)
    (pad NC thru_hole rect (at 1.905 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
  )
  (module SquantorProto:proto-TH-0127-02X06-P010-H006 (layer F.Cu) (tedit 5C55B551)
    (at 144.78 93.98)
    (fp_text reference J9 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value Proto (at 0 2.54) (layer F.Fab) hide)
    (pad NC thru_hole rect (at 1.905 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 3.175 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -3.175 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
  )
  (module SquantorConnectors:Header-0254-1X10-H010 (layer F.Cu) (tedit 5C55B661)
    (at 149.86 82.55 90)
    (descr "PIN HEADER")
    (tags "PIN HEADER")
    (attr virtual)
    (fp_text reference J10 (at -13.97 1.905 90) (layer F.SilkS) hide)
    (fp_text value PINS_1X10 (at 0 2.1 90) (layer F.Fab) hide)
    (pad 10 thru_hole circle (at 11.43 0 270) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 8.89 0 270) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 6.35 0 270) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 3.81 0 270) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 1.27 0 270) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -1.27 0 270) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -3.81 0 270) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -6.35 0 270) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -8.89 0 270) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at -11.43 0 270) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
  )
  (gr_line (start 130.175 95.885) (end 130.175 69.215) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 151.765 95.885) (end 130.175 95.885) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 151.765 69.215) (end 151.765 95.885) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 130.175 69.215) (end 151.765 69.215) (layer Edge.Cuts) (width 0.2))
)
