(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
		(47 "User.5" user)
		(49 "User.6" user)
		(51 "User.7" user)
		(53 "User.8" user)
		(55 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(D1-K)")
	(net 2 "+3.3VA")
	(net 3 "+5V")
	(net 4 "Net-(C3-Pad1)")
	(net 5 "Net-(C3-Pad2)")
	(net 6 "/CS_7")
	(net 7 "Net-(D1-A)")
	(net 8 "Net-(D2-A)")
	(net 9 "Net-(J1-Pin_1)")
	(net 10 "Net-(J2-Pin_1)")
	(net 11 "unconnected-(J2-Pin_2-Pad2)")
	(net 12 "unconnected-(J3-Pin_4-Pad4)")
	(net 13 "unconnected-(J3-Pin_5-Pad5)")
	(net 14 "unconnected-(J4-Pin_1-Pad1)")
	(net 15 "Net-(J5-Pin_2)")
	(net 16 "I2C_SCL")
	(net 17 "I2C_SDA")
	(net 18 "Net-(JP1-A)")
	(net 19 "unconnected-(MCU1-VUSB-Pad49)")
	(net 20 "unconnected-(MCU1-GND-Pad59)")
	(net 21 "unconnected-(MCU1-GND-Pad58)")
	(net 22 "unconnected-(MCU1-D+-Pad57)")
	(net 23 "unconnected-(MCU1-D--Pad56)")
	(net 24 "unconnected-(MCU1-5V-Pad55)")
	(net 25 "+3.3V")
	(net 26 "unconnected-(MCU1-23_A9_CRX1_MCLK1-Pad45)")
	(net 27 "unconnected-(MCU1-22_A8_CTX1-Pad44)")
	(net 28 "unconnected-(MCU1-21_A7_RX5_BCLK1-Pad43)")
	(net 29 "unconnected-(MCU1-20_A6_TX5_LRCLK1-Pad42)")
	(net 30 "unconnected-(MCU1-19_A5_SCL-Pad41)")
	(net 31 "/CS_3")
	(net 32 "Net-(MCU1-13_SCK_LED)")
	(net 33 "unconnected-(MCU1-GND-Pad1)")
	(net 34 "unconnected-(MCU1-0_RX1_CRX2_CS1-Pad2)")
	(net 35 "unconnected-(MCU1-1_TX1_CTX2_MISO1-Pad3)")
	(net 36 "unconnected-(MCU1-2_OUT2-Pad4)")
	(net 37 "unconnected-(MCU1-3_LRCLK2-Pad5)")
	(net 38 "unconnected-(MCU1-4_BCLK2-Pad6)")
	(net 39 "unconnected-(MCU1-5_IN2-Pad7)")
	(net 40 "unconnected-(MCU1-6_OUT1D-Pad8)")
	(net 41 "unconnected-(MCU1-9_OUT1C-Pad11)")
	(net 42 "unconnected-(MCU1-10_CS_MQSR-Pad12)")
	(net 43 "Net-(MCU1-11_MOSI_CTX1)")
	(net 44 "unconnected-(MCU1-GND-Pad34)")
	(net 45 "/CS_2")
	(net 46 "Net-(U13A-Cext)")
	(net 47 "unconnected-(MCU1-36_CS-Pad28)")
	(net 48 "unconnected-(MCU1-37_CS-Pad29)")
	(net 49 "unconnected-(MCU1-38_CS1_IN1-Pad30)")
	(net 50 "unconnected-(MCU1-39_MISO1_OUT1A-Pad31)")
	(net 51 "/CS_1")
	(net 52 "/CS_4")
	(net 53 "/CS_5")
	(net 54 "unconnected-(MCU1-32_OUT1B-Pad24)")
	(net 55 "unconnected-(MCU1-31_CTX3-Pad23)")
	(net 56 "unconnected-(MCU1-15_A1_RX3_SPDIF_IN-Pad37)")
	(net 57 "unconnected-(MCU1-40_A16-Pad32)")
	(net 58 "/SDO")
	(net 59 "/CS_8")
	(net 60 "unconnected-(U8-FLT-Pad8)")
	(net 61 "/CS_6")
	(net 62 "Net-(MCU1-R+)")
	(net 63 "Net-(MCU1-R-)")
	(net 64 "Net-(MCU1-LED)")
	(net 65 "Net-(MCU1-T+)")
	(net 66 "Net-(MCU1-T-)")
	(net 67 "unconnected-(MCU1-VBAT-Pad50)")
	(net 68 "unconnected-(MCU1-3V3-Pad51)")
	(net 69 "unconnected-(MCU1-GND-Pad52)")
	(net 70 "unconnected-(MCU1-PROGRAM-Pad53)")
	(net 71 "unconnected-(MCU1-ON_OFF-Pad54)")
	(net 72 "unconnected-(MCU1-D+-Pad67)")
	(net 73 "unconnected-(MCU1-D--Pad66)")
	(net 74 "/SDI")
	(net 75 "/CLK")
	(net 76 "unconnected-(Teensy_Ethernet1-Pad7)")
	(net 77 "unconnected-(Teensy_Ethernet1-Pad11)")
	(net 78 "unconnected-(Teensy_Ethernet1-Pad12)")
	(net 79 "unconnected-(U2-NC-Pad4)")
	(net 80 "unconnected-(U3-3vo-Pad2)")
	(net 81 "unconnected-(U3-FLT-Pad8)")
	(net 82 "unconnected-(U3-DRDY-Pad9)")
	(net 83 "unconnected-(U3---Pad10)")
	(net 84 "unconnected-(U3-+-Pad11)")
	(net 85 "unconnected-(U4-3vo-Pad2)")
	(net 86 "unconnected-(U4-FLT-Pad8)")
	(net 87 "unconnected-(U4-DRDY-Pad9)")
	(net 88 "unconnected-(U4---Pad10)")
	(net 89 "unconnected-(U4-+-Pad11)")
	(net 90 "unconnected-(U5-FLT-Pad8)")
	(net 91 "unconnected-(U5-DRDY-Pad9)")
	(net 92 "unconnected-(U5---Pad10)")
	(net 93 "unconnected-(U5-+-Pad11)")
	(net 94 "unconnected-(U6-3vo-Pad2)")
	(net 95 "unconnected-(U6-FLT-Pad8)")
	(net 96 "unconnected-(U6-DRDY-Pad9)")
	(net 97 "unconnected-(U6---Pad10)")
	(net 98 "unconnected-(U6-+-Pad11)")
	(net 99 "unconnected-(U7-3vo-Pad2)")
	(net 100 "unconnected-(U7-FLT-Pad8)")
	(net 101 "unconnected-(U7-DRDY-Pad9)")
	(net 102 "unconnected-(U7---Pad10)")
	(net 103 "unconnected-(U7-+-Pad11)")
	(net 104 "unconnected-(J4-Pin_2-Pad2)")
	(net 105 "GND")
	(net 106 "Net-(U13A-RCext)")
	(net 107 "/CS_9")
	(net 108 "unconnected-(U5-3vo-Pad2)")
	(net 109 "Net-(U13A-Q)")
	(net 110 "/SSR Control")
	(net 111 "unconnected-(U8-3vo-Pad2)")
	(net 112 "unconnected-(U8---Pad10)")
	(net 113 "unconnected-(U8-+-Pad11)")
	(net 114 "unconnected-(U8-DRDY-Pad9)")
	(net 115 "unconnected-(U9-+-Pad11)")
	(net 116 "unconnected-(U9-DRDY-Pad9)")
	(net 117 "unconnected-(U9---Pad10)")
	(net 118 "unconnected-(U9-FLT-Pad8)")
	(net 119 "unconnected-(U9-3vo-Pad2)")
	(net 120 "unconnected-(U10-DRDY-Pad9)")
	(net 121 "unconnected-(U10---Pad10)")
	(net 122 "unconnected-(U10-+-Pad11)")
	(net 123 "unconnected-(U10-3vo-Pad2)")
	(net 124 "unconnected-(U10-FLT-Pad8)")
	(net 125 "unconnected-(U11-+-Pad11)")
	(net 126 "unconnected-(U11-3vo-Pad2)")
	(net 127 "unconnected-(U11---Pad10)")
	(net 128 "unconnected-(U11-DRDY-Pad9)")
	(net 129 "unconnected-(U11-FLT-Pad8)")
	(footprint "Connector_Phoenix_MC:PhoenixContact_MCV_1,5_5-G-3.5_1x05_P3.50mm_Vertical"
		(layer "F.Cu")
		(at 235 102 -90)
		(descr "Generic Phoenix Contact connector footprint for: MCV_1,5/5-G-3.5; number of pins: 05; pin pitch: 3.50mm; Vertical || order number: 1843635 8A 160V")
		(tags "phoenix_contact connector MCV_01x05_G_3.5mm")
		(property "Reference" "J3"
			(at 7 -5.45 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x05_Socket"
			(at 7 4.2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7 -3.55 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.138889)
			(net 105 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 3.5 0 270)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 7 0 270)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 105 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 10.5 0 270)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "unconnected-(J3-Pin_4-Pad4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 14 0 270)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "unconnected-(J3-Pin_5-Pad5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Phoenix_MC.3dshapes/PhoenixContact_MCV_1,5_5-G-3.5_1x05_P3.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 106.68 83.82 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "22R"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source URL" "https://www.mouser.com/ProductDetail/ROHM-Semiconductor/SDR10EZPJ220?qs=sGAEpiMZZMvdGkrng054t2cqbZCzJY7NDw0Xs38rGaFeqcyL79Zqrg%3D%3D"
			(at 190.5 -22.86 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 75 "/CLK")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 32 "Net-(MCU1-13_SCK_LED)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "adafruitMAX31856:MAX31856"
		(layer "F.Cu")
		(at 227.88 61.485)
		(property "Reference" "U7"
			(at 0 -11.684 0)
			(layer "F.SilkS")
		)
		(property "Value" "thermo_max31856"
			(at 0 11.938 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr through_hole)
		(fp_text user "FLT"
			(at 7.62 9.906 0)
			(layer "F.SilkS")
		)
		(fp_text user "SDI"
			(at 2.54 9.906 0)
			(layer "F.SilkS")
		)
		(fp_text user "-"
			(at 1.778 -8.89 0)
			(layer "F.SilkS")
		)
		(fp_text user "SDO"
			(at 0 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "SCK"
			(at -2.54 9.906 0)
			(layer "F.SilkS")
		)
		(fp_text user "DRDY"
			(at 9.894447 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "CS"
			(at 5.08 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "+"
			(at -1.778 -8.89 0)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at -5.08 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "VIN"
			(at -10.16 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "3Vo"
			(at -7.62 9.906 0)
			(layer "F.SilkS")
		)
		(fp_text user "MAX31856"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole circle
			(at -10.16 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "VIN")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at -7.62 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 99 "unconnected-(U7-3vo-Pad2)")
			(pinfunction "3vo")
			(pintype "output")
		)
		(pad "3" thru_hole circle
			(at -5.08 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 105 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at -2.54 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 75 "/CLK")
			(pinfunction "SCK")
			(pintype "input")
		)
		(pad "5" thru_hole circle
			(at 0 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "/SDO")
			(pinfunction "SDO")
			(pintype "output")
		)
		(pad "6" thru_hole circle
			(at 2.54 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "/SDI")
			(pinfunction "SDI")
			(pintype "input")
		)
		(pad "7" thru_hole circle
			(at 5.08 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "/CS_5")
			(pinfunction "CS")
			(pintype "input")
		)
		(pad "8" thru_hole circle
			(at 7.62 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "unconnected-(U7-FLT-Pad8)")
			(pinfunction "FLT")
			(pintype "output")
		)
		(pad "9" thru_hole circle
			(at 10.16 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "unconnected-(U7-DRDY-Pad9)")
			(pinfunction "DRDY")
			(pintype "output")
		)
		(pad "10" thru_hole circle
			(at -1.778 -6.985)
			(size 2.184 2.184)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 102 "unconnected-(U7---Pad10)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "11" thru_hole circle
			(at 1.778 -6.985)
			(size 2.184 2.184)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 103 "unconnected-(U7-+-Pad11)")
			(pinfunction "+")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_DIN965"
		(layer "F.Cu")
		(at 44 123.5)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 DIN965")
		(property "Reference" "H8"
			(at 0 -3.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 3.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 123.19 83.82 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C5"
			(at 0 -1.68 90)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at -0.2325 -0.352 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source URL" "https://www.mouser.com/ProductDetail/KYOCERA-AVX/08055C105K4T4A?qs=byeeYqUIh0Oh891bMlItEA%3D%3D"
			(at 39.37 207.01 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.2325 -2.032 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "+3.3VA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 105 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 57.15 84.82 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "1.5k"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source URL" "https://www.mouser.com/ProductDetail/71-CRCW0805-1.5K-E3"
			(at -27.67 141.97 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.625 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 8 "Net-(D2-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Teensy41:Teensy41"
		(layer "F.Cu")
		(at 90.678 81.28 -90)
		(property "Reference" "MCU1"
			(at 0 -10.16 90)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 10.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source URL" "https://www.mouser.com/ProductDetail/SparkFun/DEV-16771?qs=vmHwEFxEFR%2FenEKd%2FmWpTA%3D%3D"
			(at 9.398 171.958 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr through_hole)
		(fp_text user "Micro SD"
			(at 24.13 0 90)
			(layer "F.SilkS")
		)
		(fp_text user "MIMXRT1062"
			(at -1.27 0 0)
			(layer "F.SilkS")
		)
		(fp_text user "USB Host"
			(at -18.4658 2.4892 90)
			(layer "F.SilkS")
		)
		(fp_text user "DVJ6A"
			(at -2.54 -0.18 0)
			(layer "F.SilkS")
		)
		(fp_text user "Ethernet"
			(at -12.065 -3.2766 0)
			(layer "F.SilkS")
		)
		(fp_text user "USB"
			(at -26.67 0 0)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole rect
			(at -29.21 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "unconnected-(MCU1-GND-Pad1)")
			(pinfunction "GND")
			(pintype "power_in+no_connect")
		)
		(pad "2" thru_hole circle
			(at -26.67 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "unconnected-(MCU1-0_RX1_CRX2_CS1-Pad2)")
			(pinfunction "0_RX1_CRX2_CS1")
			(pintype "bidirectional+no_connect")
		)
		(pad "3" thru_hole circle
			(at -24.13 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "unconnected-(MCU1-1_TX1_CTX2_MISO1-Pad3)")
			(pinfunction "1_TX1_CTX2_MISO1")
			(pintype "bidirectional+no_connect")
		)
		(pad "4" thru_hole circle
			(at -21.59 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "unconnected-(MCU1-2_OUT2-Pad4)")
			(pinfunction "2_OUT2")
			(pintype "bidirectional+no_connect")
		)
		(pad "5" thru_hole circle
			(at -19.05 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "unconnected-(MCU1-3_LRCLK2-Pad5)")
			(pinfunction "3_LRCLK2")
			(pintype "bidirectional+no_connect")
		)
		(pad "6" thru_hole circle
			(at -16.51 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "unconnected-(MCU1-4_BCLK2-Pad6)")
			(pinfunction "4_BCLK2")
			(pintype "bidirectional+no_connect")
		)
		(pad "7" thru_hole circle
			(at -13.97 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "unconnected-(MCU1-5_IN2-Pad7)")
			(pinfunction "5_IN2")
			(pintype "bidirectional+no_connect")
		)
		(pad "8" thru_hole circle
			(at -11.43 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "unconnected-(MCU1-6_OUT1D-Pad8)")
			(pinfunction "6_OUT1D")
			(pintype "bidirectional+no_connect")
		)
		(pad "9" thru_hole circle
			(at -8.89 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 104 "unconnected-(J4-Pin_2-Pad2)")
			(pinfunction "7_RX2_OUT1A")
			(pintype "bidirectional")
		)
		(pad "10" thru_hole circle
			(at -6.35 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "unconnected-(J4-Pin_1-Pad1)")
			(pinfunction "8_TX2_IN1")
			(pintype "bidirectional")
		)
		(pad "11" thru_hole circle
			(at -3.81 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "unconnected-(MCU1-9_OUT1C-Pad11)")
			(pinfunction "9_OUT1C")
			(pintype "bidirectional+no_connect")
		)
		(pad "12" thru_hole circle
			(at -1.27 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "unconnected-(MCU1-10_CS_MQSR-Pad12)")
			(pinfunction "10_CS_MQSR")
			(pintype "bidirectional+no_connect")
		)
		(pad "13" thru_hole circle
			(at 1.27 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(MCU1-11_MOSI_CTX1)")
			(pinfunction "11_MOSI_CTX1")
			(pintype "bidirectional")
		)
		(pad "14" thru_hole circle
			(at 3.81 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "/SDO")
			(pinfunction "12_MISO_MQSL")
			(pintype "bidirectional")
		)
		(pad "15" thru_hole circle
			(at 6.35 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(J5-Pin_2)")
			(pinfunction "3V3")
			(pintype "power_in")
		)
		(pad "16" thru_hole circle
			(at 8.89 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "I2C_SCL")
			(pinfunction "24_A10_TX6_SCL2")
			(pintype "bidirectional")
		)
		(pad "17" thru_hole circle
			(at 11.43 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "I2C_SDA")
			(pinfunction "25_A11_RX6_SDA2")
			(pintype "bidirectional")
		)
		(pad "18" thru_hole circle
			(at 13.97 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "/CS_6")
			(pinfunction "26_A12_MOSI1")
			(pintype "bidirectional")
		)
		(pad "19" thru_hole circle
			(at 16.51 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/CS_7")
			(pinfunction "27_A13_SCK1")
			(pintype "bidirectional")
		)
		(pad "20" thru_hole circle
			(at 19.05 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "/CS_8")
			(pinfunction "28_RX7")
			(pintype "bidirectional")
		)
		(pad "21" thru_hole circle
			(at 21.59 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 107 "/CS_9")
			(pinfunction "29_TX7")
			(pintype "bidirectional")
		)
		(pad "22" thru_hole circle
			(at 24.13 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 110 "/SSR Control")
			(pinfunction "30_CRX3")
			(pintype "bidirectional")
		)
		(pad "23" thru_hole circle
			(at 26.67 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "unconnected-(MCU1-31_CTX3-Pad23)")
			(pinfunction "31_CTX3")
			(pintype "bidirectional")
		)
		(pad "24" thru_hole circle
			(at 29.21 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "unconnected-(MCU1-32_OUT1B-Pad24)")
			(pinfunction "32_OUT1B")
			(pintype "bidirectional+no_connect")
		)
		(pad "25" thru_hole circle
			(at 29.21 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "/CS_5")
			(pinfunction "33_MCLK2")
			(pintype "bidirectional")
		)
		(pad "26" thru_hole circle
			(at 26.67 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "/CS_4")
			(pinfunction "34_RX8")
			(pintype "bidirectional")
		)
		(pad "27" thru_hole circle
			(at 24.13 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/CS_3")
			(pinfunction "35_TX8")
			(pintype "bidirectional")
		)
		(pad "28" thru_hole circle
			(at 21.59 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "unconnected-(MCU1-36_CS-Pad28)")
			(pinfunction "36_CS")
			(pintype "bidirectional")
		)
		(pad "29" thru_hole circle
			(at 19.05 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "unconnected-(MCU1-37_CS-Pad29)")
			(pinfunction "37_CS")
			(pintype "bidirectional")
		)
		(pad "30" thru_hole circle
			(at 16.51 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "unconnected-(MCU1-38_CS1_IN1-Pad30)")
			(pinfunction "38_CS1_IN1")
			(pintype "bidirectional")
		)
		(pad "31" thru_hole circle
			(at 13.97 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "unconnected-(MCU1-39_MISO1_OUT1A-Pad31)")
			(pinfunction "39_MISO1_OUT1A")
			(pintype "bidirectional")
		)
		(pad "32" thru_hole circle
			(at 11.43 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "unconnected-(MCU1-40_A16-Pad32)")
			(pinfunction "40_A16")
			(pintype "bidirectional")
		)
		(pad "33" thru_hole circle
			(at 8.89 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "/CS_2")
			(pinfunction "41_A17")
			(pintype "bidirectional")
		)
		(pad "34" thru_hole circle
			(at 6.35 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "unconnected-(MCU1-GND-Pad34)")
			(pinfunction "GND")
			(pintype "power_in+no_connect")
		)
		(pad "35" thru_hole circle
			(at 3.81 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(MCU1-13_SCK_LED)")
			(pinfunction "13_SCK_LED")
			(pintype "bidirectional")
		)
		(pad "36" thru_hole circle
			(at 1.27 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "unconnected-(J2-Pin_2-Pad2)")
			(pinfunction "14_A0_TX3_SPDIF_OUT")
			(pintype "bidirectional")
		)
		(pad "37" thru_hole circle
			(at -1.27 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "unconnected-(MCU1-15_A1_RX3_SPDIF_IN-Pad37)")
			(pinfunction "15_A1_RX3_SPDIF_IN")
			(pintype "bidirectional+no_connect")
		)
		(pad "38" thru_hole circle
			(at -3.81 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "unconnected-(J3-Pin_5-Pad5)")
			(pinfunction "16_A2_RX4_SCL1")
			(pintype "bidirectional")
		)
		(pad "39" thru_hole circle
			(at -6.35 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "unconnected-(J3-Pin_4-Pad4)")
			(pinfunction "17_A3_TX4_SDA1")
			(pintype "bidirectional")
		)
		(pad "40" thru_hole circle
			(at -8.89 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "/CS_1")
			(pinfunction "18_A4_SDA")
			(pintype "bidirectional")
		)
		(pad "41" thru_hole circle
			(at -11.43 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "unconnected-(MCU1-19_A5_SCL-Pad41)")
			(pinfunction "19_A5_SCL")
			(pintype "bidirectional+no_connect")
		)
		(pad "42" thru_hole circle
			(at -13.97 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "unconnected-(MCU1-20_A6_TX5_LRCLK1-Pad42)")
			(pinfunction "20_A6_TX5_LRCLK1")
			(pintype "bidirectional+no_connect")
		)
		(pad "43" thru_hole circle
			(at -16.51 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "unconnected-(MCU1-21_A7_RX5_BCLK1-Pad43)")
			(pinfunction "21_A7_RX5_BCLK1")
			(pintype "bidirectional+no_connect")
		)
		(pad "44" thru_hole circle
			(at -19.05 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "unconnected-(MCU1-22_A8_CTX1-Pad44)")
			(pinfunction "22_A8_CTX1")
			(pintype "bidirectional+no_connect")
		)
		(pad "45" thru_hole circle
			(at -21.59 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "unconnected-(MCU1-23_A9_CRX1_MCLK1-Pad45)")
			(pinfunction "23_A9_CRX1_MCLK1")
			(pintype "bidirectional+no_connect")
		)
		(pad "46" thru_hole circle
			(at -24.13 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "+3.3V")
			(pinfunction "3V3")
			(pintype "output")
		)
		(pad "47" thru_hole circle
			(at -26.67 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 105 "GND")
			(pinfunction "GND")
			(pintype "output")
		)
		(pad "48" thru_hole circle
			(at -29.21 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(pad "49" thru_hole circle
			(at -26.67 -5.08 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "unconnected-(MCU1-VUSB-Pad49)")
			(pinfunction "VUSB")
			(pintype "power_out+no_connect")
		)
		(pad "50" thru_hole circle
			(at 16.51 5.08 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "unconnected-(MCU1-VBAT-Pad50)")
			(pinfunction "VBAT")
			(pintype "power_in+no_connect")
		)
		(pad "51" thru_hole circle
			(at 16.51 2.54 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "unconnected-(MCU1-3V3-Pad51)")
			(pinfunction "3V3")
			(pintype "power_in+no_connect")
		)
		(pad "52" thru_hole circle
			(at 16.51 0 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "unconnected-(MCU1-GND-Pad52)")
			(pinfunction "GND")
			(pintype "input+no_connect")
		)
		(pad "53" thru_hole circle
			(at 16.51 -2.54 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "unconnected-(MCU1-PROGRAM-Pad53)")
			(pinfunction "PROGRAM")
			(pintype "input+no_connect")
		)
		(pad "54" thru_hole circle
			(at 16.51 -5.08 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "unconnected-(MCU1-ON_OFF-Pad54)")
			(pinfunction "ON_OFF")
			(pintype "input+no_connect")
		)
		(pad "55" thru_hole rect
			(at -22.9108 4.5692 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "unconnected-(MCU1-5V-Pad55)")
			(pinfunction "5V")
			(pintype "power_out+no_connect")
		)
		(pad "56" thru_hole circle
			(at -20.3708 4.5692 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "unconnected-(MCU1-D--Pad56)")
			(pinfunction "D-")
			(pintype "bidirectional+no_connect")
		)
		(pad "57" thru_hole circle
			(at -17.8308 4.5692 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "unconnected-(MCU1-D+-Pad57)")
			(pinfunction "D+")
			(pintype "bidirectional+no_connect")
		)
		(pad "58" thru_hole circle
			(at -15.2908 4.5692 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "unconnected-(MCU1-GND-Pad58)")
			(pinfunction "GND")
			(pintype "power_in+no_connect")
		)
		(pad "59" thru_hole circle
			(at -12.7508 4.5692 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "unconnected-(MCU1-GND-Pad59)")
			(pinfunction "GND")
			(pintype "power_in+no_connect")
		)
		(pad "60" thru_hole rect
			(at -16.24 -5.1816 270)
			(size 1.3 1.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "Net-(MCU1-R+)")
			(pinfunction "R+")
			(pintype "bidirectional")
		)
		(pad "61" thru_hole circle
			(at -16.24 -3.1816 270)
			(size 1.3 1.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "Net-(MCU1-LED)")
			(pinfunction "LED")
			(pintype "bidirectional")
		)
		(pad "62" thru_hole circle
			(at -16.24 -1.1816 270)
			(size 1.3 1.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "Net-(MCU1-T-)")
			(pinfunction "T-")
			(pintype "bidirectional")
		)
		(pad "63" thru_hole circle
			(at -14.24 -1.1816 270)
			(size 1.3 1.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "Net-(MCU1-T+)")
			(pinfunction "T+")
			(pintype "bidirectional")
		)
		(pad "64" thru_hole circle
			(at -14.24 -3.1816 270)
			(size 1.3 1.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(C3-Pad2)")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "65" thru_hole circle
			(at -14.24 -5.1816 270)
			(size 1.3 1.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "Net-(MCU1-R-)")
			(pinfunction "R-")
			(pintype "bidirectional")
		)
		(pad "66" thru_hole circle
			(at -28.48 -1.27 270)
			(size 1.3 1.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 73 "unconnected-(MCU1-D--Pad66)")
			(pinfunction "D-")
			(pintype "bidirectional+no_connect")
		)
		(pad "67" thru_hole circle
			(at -28.48 1.27 270)
			(size 1.3 1.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "unconnected-(MCU1-D+-Pad67)")
			(pinfunction "D+")
			(pintype "bidirectional+no_connect")
		)
		(embedded_fonts no)
		(model "${KICAD_USER_DIR}/teensy.pretty/Teensy_4.1_Assembly.STEP"
			(offset
				(xyz 0 0 0.762)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5"
		(layer "F.Cu")
		(at 118.11 83.82)
		(descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U2"
			(at 0 -2.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "NCP163ASN330T1G"
			(at 0 2.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/ncp163-d.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source URL" "https://www.mouser.com/ProductDetail/onsemi/NCP163ASN330T1G?qs=vLWxofP3U2ykJIQb1%252BPKcA%3D%3D"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 105 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 79 "unconnected-(U2-NC-Pad4)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "5" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.3VA")
			(pinfunction "VOUT")
			(pintype "power_out")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.00mm"
		(layer "F.Cu")
		(at 64.04 77.47)
		(descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
		(property "Reference" "C1"
			(at 2.46 -3.238269 0)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 1 3.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source URL" "https://www.mouser.com/ProductDetail/Panasonic/EEU-FC1H100L?qs=y21It3NrCcwTwLLc39Q8Gg%3D%3D"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 105 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "adafruitMAX31856:MAX31856"
		(layer "F.Cu")
		(at 136.800342 108 180)
		(property "Reference" "U11"
			(at 0 -11.684 0)
			(layer "F.SilkS")
		)
		(property "Value" "thermo_max31856"
			(at 0 11.938 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr through_hole)
		(fp_text user "DRDY"
			(at 10.16 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "3Vo"
			(at -7.62 9.906 0)
			(layer "F.SilkS")
		)
		(fp_text user "CS"
			(at 5.08 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at -5.08 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "SDO"
			(at 0 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "-"
			(at 1.778 -8.89 0)
			(layer "F.SilkS")
		)
		(fp_text user "MAX31856"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(fp_text user "FLT"
			(at 7.62 9.906 0)
			(layer "F.SilkS")
		)
		(fp_text user "SCK"
			(at -2.54 9.906 0)
			(layer "F.SilkS")
		)
		(fp_text user "+"
			(at -1.778 -8.89 0)
			(layer "F.SilkS")
		)
		(fp_text user "SDI"
			(at 2.54 9.906 0)
			(layer "F.SilkS")
		)
		(fp_text user "VIN"
			(at -10.16 6.604 0)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole circle
			(at -10.16 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "VIN")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at -7.62 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 126 "unconnected-(U11-3vo-Pad2)")
			(pinfunction "3vo")
			(pintype "output")
		)
		(pad "3" thru_hole circle
			(at -5.08 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 105 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at -2.54 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 75 "/CLK")
			(pinfunction "SCK")
			(pintype "input")
		)
		(pad "5" thru_hole circle
			(at 0 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "/SDO")
			(pinfunction "SDO")
			(pintype "output")
		)
		(pad "6" thru_hole circle
			(at 2.54 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "/SDI")
			(pinfunction "SDI")
			(pintype "input")
		)
		(pad "7" thru_hole circle
			(at 5.08 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 107 "/CS_9")
			(pinfunction "CS")
			(pintype "input")
		)
		(pad "8" thru_hole circle
			(at 7.62 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 129 "unconnected-(U11-FLT-Pad8)")
			(pinfunction "FLT")
			(pintype "output")
		)
		(pad "9" thru_hole circle
			(at 10.16 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 128 "unconnected-(U11-DRDY-Pad9)")
			(pinfunction "DRDY")
			(pintype "output")
		)
		(pad "10" thru_hole circle
			(at -1.778 -6.985 180)
			(size 2.184 2.184)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "unconnected-(U11---Pad10)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "11" thru_hole circle
			(at 1.778 -6.985 180)
			(size 2.184 2.184)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 125 "unconnected-(U11-+-Pad11)")
			(pinfunction "+")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_DIN965"
		(layer "F.Cu")
		(at 248 46.5)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 DIN965")
		(property "Reference" "H5"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 3.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "adafruitMAX31856:MAX31856"
		(layer "F.Cu")
		(at 163.5 108 180)
		(property "Reference" "U10"
			(at 0 -11.684 0)
			(layer "F.SilkS")
		)
		(property "Value" "thermo_max31856"
			(at 0 11.938 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr through_hole)
		(fp_text user "VIN"
			(at -10.16 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "MAX31856"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(fp_text user "SCK"
			(at -2.54 9.906 0)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at -5.08 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "+"
			(at -1.778 -8.89 0)
			(layer "F.SilkS")
		)
		(fp_text user "CS"
			(at 5.08 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "-"
			(at 1.778 -8.89 0)
			(layer "F.SilkS")
		)
		(fp_text user "SDI"
			(at 2.54 9.906 0)
			(layer "F.SilkS")
		)
		(fp_text user "3Vo"
			(at -7.62 9.906 0)
			(layer "F.SilkS")
		)
		(fp_text user "DRDY"
			(at 10.16 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "FLT"
			(at 7.62 9.906 0)
			(layer "F.SilkS")
		)
		(fp_text user "SDO"
			(at 0 6.604 0)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole circle
			(at -10.16 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "VIN")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at -7.62 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 123 "unconnected-(U10-3vo-Pad2)")
			(pinfunction "3vo")
			(pintype "output")
		)
		(pad "3" thru_hole circle
			(at -5.08 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 105 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at -2.54 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 75 "/CLK")
			(pinfunction "SCK")
			(pintype "input")
		)
		(pad "5" thru_hole circle
			(at 0 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "/SDO")
			(pinfunction "SDO")
			(pintype "output")
		)
		(pad "6" thru_hole circle
			(at 2.54 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "/SDI")
			(pinfunction "SDI")
			(pintype "input")
		)
		(pad "7" thru_hole circle
			(at 5.08 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "/CS_8")
			(pinfunction "CS")
			(pintype "input")
		)
		(pad "8" thru_hole circle
			(at 7.62 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 124 "unconnected-(U10-FLT-Pad8)")
			(pinfunction "FLT")
			(pintype "output")
		)
		(pad "9" thru_hole circle
			(at 10.16 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 120 "unconnected-(U10-DRDY-Pad9)")
			(pinfunction "DRDY")
			(pintype "output")
		)
		(pad "10" thru_hole circle
			(at -1.778 -6.985 180)
			(size 2.184 2.184)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 121 "unconnected-(U10---Pad10)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "11" thru_hole circle
			(at 1.778 -6.985 180)
			(size 2.184 2.184)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 122 "unconnected-(U10-+-Pad11)")
			(pinfunction "+")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "MeanWell-DC-DC:N78051C"
		(layer "F.Cu")
		(at 67.31 84.935)
		(descr "N7805-1C-2")
		(tags "Power Supply")
		(property "Reference" "U1"
			(at 2.54 3.965 0)
			(layer "F.SilkS")
		)
		(property "Value" "N7805"
			(at 2.54 3.965 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source URL" "https://www.mouser.com/ProductDetail/MEAN-WELL/N7805-1C?qs=7D1LtPJG0i2aXH7i3d%252BGOw%3D%3D"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO?252* TO?263* TO?220*")
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 3.965 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(D1-K)")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 105 "GND")
			(pinfunction "GND/-Vout")
			(pintype "power_out")
		)
		(pad "3" thru_hole circle
			(at 5.08 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(JP1-A)")
			(pinfunction "+Vout/GND")
			(pintype "power_out")
		)
		(embedded_fonts no)
		(model "Y:\\KiCAD\\LED-driver\\mouser\\SamacSys_Parts.3dshapes\\N7805-1C.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 72.39 80.01 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "JP1"
			(at 0 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "PS"
			(at 0 4.87 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jumper* TestPoint*2Pads* TestPoint*Bridge*")
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(JP1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "B")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MC:PhoenixContact_MCV_1,5_5-G-3.5_1x05_P3.50mm_Vertical"
		(layer "F.Cu")
		(at 234.5 79.5 -90)
		(descr "Generic Phoenix Contact connector footprint for: MCV_1,5/5-G-3.5; number of pins: 05; pin pitch: 3.50mm; Vertical || order number: 1843635 8A 160V")
		(tags "phoenix_contact connector MCV_01x05_G_3.5mm")
		(property "Reference" "J2"
			(at 7 -5.45 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x05_Socket"
			(at 7 4.2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7 -3.55 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.138889)
			(net 10 "Net-(J2-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 3.5 0 270)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "unconnected-(J2-Pin_2-Pad2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 7 0 270)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 105 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 10.5 0 270)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 14 0 270)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 105 "GND")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Phoenix_MC.3dshapes/PhoenixContact_MCV_1,5_5-G-3.5_1x05_P3.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "adafruitMAX31856:MAX31856"
		(layer "F.Cu")
		(at 216.778 108.015 180)
		(property "Reference" "U8"
			(at 0 -11.684 0)
			(layer "F.SilkS")
		)
		(property "Value" "thermo_max31856"
			(at 0 11.938 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr through_hole)
		(fp_text user "-"
			(at 1.778 -8.89 0)
			(layer "F.SilkS")
		)
		(fp_text user "DRDY"
			(at 10.16 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "3Vo"
			(at -7.62 9.906 0)
			(layer "F.SilkS")
		)
		(fp_text user "SDI"
			(at 2.54 9.906 0)
			(layer "F.SilkS")
		)
		(fp_text user "VIN"
			(at -10.16 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "FLT"
			(at 7.62 9.906 0)
			(layer "F.SilkS")
		)
		(fp_text user "MAX31856"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(fp_text user "+"
			(at -1.778 -8.89 0)
			(layer "F.SilkS")
		)
		(fp_text user "SCK"
			(at -2.54 9.906 0)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at -5.08 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "CS"
			(at 5.08 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "SDO"
			(at 0 6.604 0)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole circle
			(at -10.16 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "VIN")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at -7.62 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 111 "unconnected-(U8-3vo-Pad2)")
			(pinfunction "3vo")
			(pintype "output")
		)
		(pad "3" thru_hole circle
			(at -5.08 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 105 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at -2.54 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 75 "/CLK")
			(pinfunction "SCK")
			(pintype "input")
		)
		(pad "5" thru_hole circle
			(at 0 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "/SDO")
			(pinfunction "SDO")
			(pintype "output")
		)
		(pad "6" thru_hole circle
			(at 2.54 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "/SDI")
			(pinfunction "SDI")
			(pintype "input")
		)
		(pad "7" thru_hole circle
			(at 5.08 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "/CS_6")
			(pinfunction "CS")
			(pintype "input")
		)
		(pad "8" thru_hole circle
			(at 7.62 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "unconnected-(U8-FLT-Pad8)")
			(pinfunction "FLT")
			(pintype "output")
		)
		(pad "9" thru_hole circle
			(at 10.16 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 114 "unconnected-(U8-DRDY-Pad9)")
			(pinfunction "DRDY")
			(pintype "output")
		)
		(pad "10" thru_hole circle
			(at -1.778 -6.985 180)
			(size 2.184 2.184)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 112 "unconnected-(U8---Pad10)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "11" thru_hole circle
			(at 1.778 -6.985 180)
			(size 2.184 2.184)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 113 "unconnected-(U8-+-Pad11)")
			(pinfunction "+")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.00mm"
		(layer "F.Cu")
		(at 72.39 73.66)
		(descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
		(property "Reference" "C2"
			(at 1 -3.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "22u"
			(at 1 3.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source URL" "https://www.mouser.com/ProductDetail/Panasonic/ECE-A1AKS220B?qs=rMMd5vBiahr9Q6YeOXDNwQ%3D%3D"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 105 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "adafruitMAX31856:MAX31856"
		(layer "F.Cu")
		(at 145.796 61.595)
		(property "Reference" "U4"
			(at 0 -11.684 0)
			(layer "F.SilkS")
		)
		(property "Value" "thermo_max31856"
			(at 0 11.938 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr through_hole)
		(fp_text user "GND"
			(at -5.08 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "SDI"
			(at 2.54 9.906 0)
			(layer "F.SilkS")
		)
		(fp_text user "+"
			(at -1.778 -8.89 0)
			(layer "F.SilkS")
		)
		(fp_text user "FLT"
			(at 7.62 9.906 0)
			(layer "F.SilkS")
		)
		(fp_text user "SCK"
			(at -2.54 9.906 0)
			(layer "F.SilkS")
		)
		(fp_text user "CS"
			(at 5.08 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "VIN"
			(at -10.16 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "-"
			(at 1.778 -8.89 0)
			(layer "F.SilkS")
		)
		(fp_text user "DRDY"
			(at 9.704 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "MAX31856"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(fp_text user "3Vo"
			(at -7.62 9.906 0)
			(layer "F.SilkS")
		)
		(fp_text user "SDO"
			(at 0 6.604 0)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole circle
			(at -10.16 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "VIN")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at -7.62 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 85 "unconnected-(U4-3vo-Pad2)")
			(pinfunction "3vo")
			(pintype "output")
		)
		(pad "3" thru_hole circle
			(at -5.08 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 105 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at -2.54 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 75 "/CLK")
			(pinfunction "SCK")
			(pintype "input")
		)
		(pad "5" thru_hole circle
			(at 0 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "/SDO")
			(pinfunction "SDO")
			(pintype "output")
		)
		(pad "6" thru_hole circle
			(at 2.54 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "/SDI")
			(pinfunction "SDI")
			(pintype "input")
		)
		(pad "7" thru_hole circle
			(at 5.08 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "/CS_2")
			(pinfunction "CS")
			(pintype "input")
		)
		(pad "8" thru_hole circle
			(at 7.62 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 86 "unconnected-(U4-FLT-Pad8)")
			(pinfunction "FLT")
			(pintype "output")
		)
		(pad "9" thru_hole circle
			(at 10.16 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 87 "unconnected-(U4-DRDY-Pad9)")
			(pinfunction "DRDY")
			(pintype "output")
		)
		(pad "10" thru_hole circle
			(at -1.778 -6.985)
			(size 2.184 2.184)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 88 "unconnected-(U4---Pad10)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "11" thru_hole circle
			(at 1.778 -6.985)
			(size 2.184 2.184)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 89 "unconnected-(U4-+-Pad11)")
			(pinfunction "+")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "adafruitMAX31856:MAX31856"
		(layer "F.Cu")
		(at 201.222 61.485)
		(property "Reference" "U6"
			(at 0 -11.684 0)
			(layer "F.SilkS")
		)
		(property "Value" "thermo_max31856"
			(at 0 11.938 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr through_hole)
		(fp_text user "-"
			(at 1.778 -8.89 0)
			(layer "F.SilkS")
		)
		(fp_text user "DRDY"
			(at 9.874948 6.583522 0)
			(layer "F.SilkS")
		)
		(fp_text user "+"
			(at -1.778 -8.89 0)
			(layer "F.SilkS")
		)
		(fp_text user "SCK"
			(at -2.54 9.906 0)
			(layer "F.SilkS")
		)
		(fp_text user "CS"
			(at 5.08 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "SDI"
			(at 2.54 9.906 0)
			(layer "F.SilkS")
		)
		(fp_text user "SDO"
			(at 0 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "MAX31856"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at -5.08 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "FLT"
			(at 7.62 9.906 0)
			(layer "F.SilkS")
		)
		(fp_text user "VIN"
			(at -10.16 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "3Vo"
			(at -7.62 9.906 0)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole circle
			(at -10.16 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "VIN")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at -7.62 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 94 "unconnected-(U6-3vo-Pad2)")
			(pinfunction "3vo")
			(pintype "output")
		)
		(pad "3" thru_hole circle
			(at -5.08 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 105 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at -2.54 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 75 "/CLK")
			(pinfunction "SCK")
			(pintype "input")
		)
		(pad "5" thru_hole circle
			(at 0 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "/SDO")
			(pinfunction "SDO")
			(pintype "output")
		)
		(pad "6" thru_hole circle
			(at 2.54 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "/SDI")
			(pinfunction "SDI")
			(pintype "input")
		)
		(pad "7" thru_hole circle
			(at 5.08 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "/CS_4")
			(pinfunction "CS")
			(pintype "input")
		)
		(pad "8" thru_hole circle
			(at 7.62 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 95 "unconnected-(U6-FLT-Pad8)")
			(pinfunction "FLT")
			(pintype "output")
		)
		(pad "9" thru_hole circle
			(at 10.16 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 96 "unconnected-(U6-DRDY-Pad9)")
			(pinfunction "DRDY")
			(pintype "output")
		)
		(pad "10" thru_hole circle
			(at -1.778 -6.985)
			(size 2.184 2.184)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 97 "unconnected-(U6---Pad10)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "11" thru_hole circle
			(at 1.778 -6.985)
			(size 2.184 2.184)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 98 "unconnected-(U6-+-Pad11)")
			(pinfunction "+")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "adafruitMAX31856:MAX31856"
		(layer "F.Cu")
		(at 173.736 61.485)
		(property "Reference" "U5"
			(at 0 -11.684 0)
			(layer "F.SilkS")
		)
		(property "Value" "thermo_max31856"
			(at 0 11.938 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr through_hole)
		(fp_text user "3Vo"
			(at -7.62 9.906 0)
			(layer "F.SilkS")
		)
		(fp_text user "VIN"
			(at -10.16 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "SCK"
			(at -2.54 9.906 0)
			(layer "F.SilkS")
		)
		(fp_text user "SDO"
			(at 0 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "-"
			(at 1.778 -8.89 0)
			(layer "F.SilkS")
		)
		(fp_text user "FLT"
			(at 7.62 9.906 0)
			(layer "F.SilkS")
		)
		(fp_text user "MAX31856"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(fp_text user "DRDY"
			(at 9.911932 6.58158 0)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at -5.08 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "SDI"
			(at 2.54 9.906 0)
			(layer "F.SilkS")
		)
		(fp_text user "CS"
			(at 5.08 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "+"
			(at -1.778 -8.89 0)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole circle
			(at -10.16 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "VIN")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at -7.62 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 108 "unconnected-(U5-3vo-Pad2)")
			(pinfunction "3vo")
			(pintype "output")
		)
		(pad "3" thru_hole circle
			(at -5.08 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 105 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at -2.54 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 75 "/CLK")
			(pinfunction "SCK")
			(pintype "input")
		)
		(pad "5" thru_hole circle
			(at 0 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "/SDO")
			(pinfunction "SDO")
			(pintype "output")
		)
		(pad "6" thru_hole circle
			(at 2.54 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "/SDI")
			(pinfunction "SDI")
			(pintype "input")
		)
		(pad "7" thru_hole circle
			(at 5.08 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/CS_3")
			(pinfunction "CS")
			(pintype "input")
		)
		(pad "8" thru_hole circle
			(at 7.62 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 90 "unconnected-(U5-FLT-Pad8)")
			(pinfunction "FLT")
			(pintype "output")
		)
		(pad "9" thru_hole circle
			(at 10.16 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "unconnected-(U5-DRDY-Pad9)")
			(pinfunction "DRDY")
			(pintype "output")
		)
		(pad "10" thru_hole circle
			(at -1.778 -6.985)
			(size 2.184 2.184)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 92 "unconnected-(U5---Pad10)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "11" thru_hole circle
			(at 1.778 -6.985)
			(size 2.184 2.184)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 93 "unconnected-(U5-+-Pad11)")
			(pinfunction "+")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_DIN965"
		(layer "F.Cu")
		(at 248 123.5)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 DIN965")
		(property "Reference" "H6"
			(at 0 -3.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 3.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 151.5 80.764 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C7"
			(at 0 -1.68 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 105 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_RJ:RJ45_Cetus_J1B1211CCD_Horizontal"
		(layer "F.Cu")
		(at 64.77 101.6)
		(descr "1 Port RJ45 Magjack Connector Through Hole 10/100 Base-T, Cetus, used and distributed by WIZnet (https://wizwiki.net/wiki/lib/exe/fetch.php?media=products:wiz550web:wiz550webds_kr:j1b1211ccd.pdf)")
		(tags "RJ45 Magjack")
		(property "Reference" "Teensy_Ethernet1"
			(at 5 -5.6 0)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 4.445 18 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source URL" "https://www.mouser.com/ProductDetail/WIZnet/J1B1211CCD?qs=6pHq9bjOlanFLUlTDcmBeQ%3D%3Dhttps://www.mouser.com/ProductDetail/WIZnet/J1B1211CCD?qs=6pHq9bjOlanFLUlTDcmBeQ%3D%3D"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "8P8C* RJ45*")
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 4 16 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -1.27 6.35)
			(size 3.25 3.25)
			(drill 3.25)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 10.16 6.35)
			(size 3.25 3.25)
			(drill 3.25)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.5 1.5)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.167)
			(net 65 "Net-(MCU1-T+)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.27 -2.54)
			(size 1.5 1.5)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(C3-Pad1)")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 2.54 0)
			(size 1.5 1.5)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "Net-(MCU1-T-)")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 3.81 -2.54)
			(size 1.5 1.5)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "Net-(MCU1-R+)")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 5.08 0)
			(size 1.5 1.5)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(C3-Pad1)")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 6.35 -2.54)
			(size 1.5 1.5)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "Net-(MCU1-R-)")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 7.62 0)
			(size 1.5 1.5)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "unconnected-(Teensy_Ethernet1-Pad7)")
			(pintype "passive+no_connect")
		)
		(pad "8" thru_hole circle
			(at 8.89 -2.54)
			(size 1.5 1.5)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(C3-Pad2)")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at -1.88 11.43)
			(size 1.5 1.5)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(C3-Pad2)")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 0.66 9.73)
			(size 1.5 1.5)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "Net-(MCU1-LED)")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 8.23 11.43)
			(size 1.5 1.5)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "unconnected-(Teensy_Ethernet1-Pad11)")
			(pintype "passive+no_connect")
		)
		(pad "12" thru_hole circle
			(at 10.77 9.73)
			(size 1.5 1.5)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 78 "unconnected-(Teensy_Ethernet1-Pad12)")
			(pintype "passive+no_connect")
		)
		(pad "13" thru_hole circle
			(at -3.43 3.3)
			(size 2.5 2.5)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "13" thru_hole circle
			(at 12.32 3.3)
			(size 2.5 2.5)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_RJ.3dshapes/RJ45_Cetus_J1B1211CCD.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 88.138 82.28 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "22R"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source URL" "https://www.mouser.com/ProductDetail/ROHM-Semiconductor/SDR10EZPJ220?qs=sGAEpiMZZMvdGkrng054t2cqbZCzJY7NDw0Xs38rGaFeqcyL79Zqrg%3D%3D"
			(at 170.418 -5.858 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 43 "Net-(MCU1-11_MOSI_CTX1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 74 "/SDI")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SSOP-8_2.95x2.8mm_P0.65mm"
		(layer "F.Cu")
		(at 138.5 86.765)
		(descr "SSOP-8 2.9 x2.8mm Pitch 0.65mm")
		(tags "SSOP-8 2.95x2.8mm Pitch 0.65mm")
		(property "Reference" "U13"
			(at 0 -2.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "74LVC1G123"
			(at 0 2.6 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74lvc1g123.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Single Retriggerable Monostable Multivibrator, Low-Voltage CMOS"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SSOP*2.95x2.8mm*P0.65* VSSOP*2.3x2mm*P0.5mm*")
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 -0.975 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 105 "GND")
			(pinfunction "~{A}")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -1.7 -0.325 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 55 "unconnected-(MCU1-31_CTX3-Pad23)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -1.7 0.325 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "+5V")
			(pinfunction "~{CLR}")
			(pintype "input")
		)
		(pad "4" smd rect
			(at -1.7 0.975 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 105 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" smd rect
			(at 1.7 0.975 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 109 "Net-(U13A-Q)")
			(pinfunction "Q")
			(pintype "output")
		)
		(pad "6" smd rect
			(at 1.7 0.325 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "Net-(U13A-Cext)")
			(pinfunction "Cext")
			(pintype "input")
		)
		(pad "7" smd rect
			(at 1.7 -0.325 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 106 "Net-(U13A-RCext)")
			(pinfunction "RCext")
			(pintype "input")
		)
		(pad "8" smd rect
			(at 1.7 -0.975 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SSOP-8_2.95x2.8mm_P0.65mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5_HandSoldering"
		(layer "F.Cu")
		(at 150.15 86.95)
		(descr "5-pin SOT23 package")
		(tags "SOT-23-5 hand-soldering")
		(property "Reference" "U12"
			(at 0 -2.9 0)
			(layer "F.SilkS")
		)
		(property "Value" "74LVC1G08"
			(at 0 2.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc1g08.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Single AND Gate, Low-Voltage CMOS"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*")
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.35 -0.95)
			(size 1.56 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 109 "Net-(U13A-Q)")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.35 0)
			(size 1.56 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 110 "/SSR Control")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -1.35 0.95)
			(size 1.56 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 105 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at 1.35 0.95)
			(size 1.56 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "Net-(J2-Pin_1)")
			(pintype "output")
		)
		(pad "5" smd roundrect
			(at 1.35 -0.95)
			(size 1.56 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScrewTerminals:TB00750802BE"
		(layer "F.Cu")
		(at 67.31 55.88)
		(descr "TB007-508-02BE-2")
		(tags "Connector")
		(property "Reference" "J1"
			(at 2.54 0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x02"
			(at 2.54 0.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source URL" "https://www.mouser.com/ProductDetail/CUI-Devices/TB007-508-02BE?qs=vLWxofP3U2y6PFKAfCqKUQ%3D%3D"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0.05 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.4 2.4)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(J1-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0)
			(size 2.4 2.4)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 105 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "Y:\\KiCAD\\LED-driver\\mouser\\SamacSys_Parts.3dshapes\\TB007-508-02BE.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 144 80.764 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R4"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "470k"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 106 "Net-(U13A-RCext)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 57.3825 91.44)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C3"
			(at 0 -1.68 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source URL" "https://www.mouser.com/ProductDetail/KYOCERA-AVX/0805DD104KAT2A?qs=qVfB0%2FDaMDa6X8LeFyoDIw%3D%3D"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 4 "Net-(C3-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "Net-(C3-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 111.76 83.82 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C4"
			(at -0.2325 -3.712 90)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source URL" "https://www.mouser.com/ProductDetail/KYOCERA-AVX/08055C105K4T4A?qs=byeeYqUIh0Oh891bMlItEA%3D%3D"
			(at 27.94 195.58 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.2325 -2.032 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 105 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 58.42 72.39 180)
		(descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x04 2.54mm single row")
		(property "Reference" "J5"
			(at 0 -2.77 0)
			(layer "F.SilkS")
		)
		(property "Value" "OLED Display I2C"
			(at 0 10.39 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source URL" "https://www.mouser.com/ProductDetail/Harwin/M20-7820442?qs=vF78I%252BjhbY9ZgDLCXkGx4w%3D%3D"
			(at 116.84 144.78 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 3.81 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 105 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(J5-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "I2C_SCL")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "I2C_SDA")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SMD-Fuse:smd_fuse"
		(layer "F.Cu")
		(at 69.85 66.04)
		(property "Reference" "F1"
			(at 0 -3.556 180)
			(layer "F.SilkS")
		)
		(property "Value" "1A"
			(at 33.149775 40.816 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source URL" "https://www.mouser.com/ProductDetail/Littelfuse/0154001.DRT?qs=gu7KAQ731UQPKHSDuMkClg%3D%3D"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*Fuse*")
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -3.5 0)
			(size 4.24 3.81)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(D1-A)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 3.5 0)
			(size 4.24 3.81)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "Net-(J1-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_DIN965"
		(layer "F.Cu")
		(at 44.5 47)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 DIN965")
		(property "Reference" "H7"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 3.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "adafruitMAX31856:MAX31856"
		(layer "F.Cu")
		(at 190 108.015 180)
		(property "Reference" "U9"
			(at 0 -11.684 0)
			(layer "F.SilkS")
		)
		(property "Value" "thermo_max31856"
			(at 0 11.938 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr through_hole)
		(fp_text user "SCK"
			(at -2.54 9.906 0)
			(layer "F.SilkS")
		)
		(fp_text user "SDO"
			(at 0 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "3Vo"
			(at -7.62 9.906 0)
			(layer "F.SilkS")
		)
		(fp_text user "SDI"
			(at 2.54 9.906 0)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at -5.08 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "MAX31856"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(fp_text user "VIN"
			(at -10.16 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "DRDY"
			(at 10.16 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "-"
			(at 1.778 -8.89 0)
			(layer "F.SilkS")
		)
		(fp_text user "CS"
			(at 5.08 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "+"
			(at -1.778 -8.89 0)
			(layer "F.SilkS")
		)
		(fp_text user "FLT"
			(at 7.62 9.906 0)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole circle
			(at -10.16 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "VIN")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at -7.62 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "unconnected-(U9-3vo-Pad2)")
			(pinfunction "3vo")
			(pintype "output")
		)
		(pad "3" thru_hole circle
			(at -5.08 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 105 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at -2.54 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 75 "/CLK")
			(pinfunction "SCK")
			(pintype "input")
		)
		(pad "5" thru_hole circle
			(at 0 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "/SDO")
			(pinfunction "SDO")
			(pintype "output")
		)
		(pad "6" thru_hole circle
			(at 2.54 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "/SDI")
			(pinfunction "SDI")
			(pintype "input")
		)
		(pad "7" thru_hole circle
			(at 5.08 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/CS_7")
			(pinfunction "CS")
			(pintype "input")
		)
		(pad "8" thru_hole circle
			(at 7.62 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 118 "unconnected-(U9-FLT-Pad8)")
			(pinfunction "FLT")
			(pintype "output")
		)
		(pad "9" thru_hole circle
			(at 10.16 8.255 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 116 "unconnected-(U9-DRDY-Pad9)")
			(pinfunction "DRDY")
			(pintype "output")
		)
		(pad "10" thru_hole circle
			(at -1.778 -6.985 180)
			(size 2.184 2.184)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 117 "unconnected-(U9---Pad10)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "11" thru_hole circle
			(at 1.778 -6.985 180)
			(size 2.184 2.184)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 115 "unconnected-(U9-+-Pad11)")
			(pinfunction "+")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 144 86 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C6"
			(at 0 -1.68 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7u"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 106 "Net-(U13A-RCext)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 46 "Net-(U13A-Cext)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 57.15 78.74 90)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D2"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED 5VOK"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source URL" "https://www.mouser.com/ProductDetail/604-APTD2012LQBCD"
			(at 135.89 21.59 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -2.785 2.032 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.025 0 90)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 105 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.025 0 90)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 8 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MC:PhoenixContact_MCV_1,5_5-G-3.5_1x05_P3.50mm_Vertical"
		(layer "F.Cu")
		(at 52.578 115.57 90)
		(descr "Generic Phoenix Contact connector footprint for: MCV_1,5/5-G-3.5; number of pins: 05; pin pitch: 3.50mm; Vertical || order number: 1843635 8A 160V")
		(tags "phoenix_contact connector MCV_01x05_G_3.5mm")
		(property "Reference" "J4"
			(at 7 -5.45 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x05_Socket"
			(at 7 4.2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7 -3.55 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.138889)
			(net 14 "unconnected-(J4-Pin_1-Pad1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 3.5 0 90)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 104 "unconnected-(J4-Pin_2-Pad2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 7 0 90)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 105 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 10.5 0 90)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 14 0 90)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 105 "GND")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Phoenix_MC.3dshapes/PhoenixContact_MCV_1,5_5-G-3.5_1x05_P3.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 65.15 72.39)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D1"
			(at 0 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 0 2.1 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source URL" "https://www.mouser.com/ProductDetail/ROHM-Semiconductor/RBR2L40ADDTE25?qs=4v%252BiZTmLVHGLyDHjy5J8KA%3D%3D"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "adafruitMAX31856:MAX31856"
		(layer "F.Cu")
		(at 117.856 61.595)
		(property "Reference" "U3"
			(at 0 -11.684 0)
			(layer "F.SilkS")
		)
		(property "Value" "thermo_max31856"
			(at 0 11.938 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "TeensyHumTC_baily.kicad_sch")
		(attr through_hole)
		(fp_text user "SCK"
			(at -2.54 9.906 0)
			(layer "F.SilkS")
		)
		(fp_text user "3Vo"
			(at -7.62 9.906 0)
			(layer "F.SilkS")
		)
		(fp_text user "+"
			(at -1.778 -8.89 0)
			(layer "F.SilkS")
		)
		(fp_text user "SDI"
			(at 2.54 9.906 0)
			(layer "F.SilkS")
		)
		(fp_text user "SDO"
			(at 0 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "FLT"
			(at 7.62 9.906 0)
			(layer "F.SilkS")
		)
		(fp_text user "DRDY"
			(at 9.644 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "CS"
			(at 5.08 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at -5.08 6.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "MAX31856"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(fp_text user "-"
			(at 1.778 -8.89 0)
			(layer "F.SilkS")
		)
		(fp_text user "VIN"
			(at -10.16 6.604 0)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole circle
			(at -10.16 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "VIN")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at -7.62 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 80 "unconnected-(U3-3vo-Pad2)")
			(pinfunction "3vo")
			(pintype "output")
		)
		(pad "3" thru_hole circle
			(at -5.08 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 105 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at -2.54 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 75 "/CLK")
			(pinfunction "SCK")
			(pintype "input")
		)
		(pad "5" thru_hole circle
			(at 0 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "/SDO")
			(pinfunction "SDO")
			(pintype "output")
		)
		(pad "6" thru_hole circle
			(at 2.54 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "/SDI")
			(pinfunction "SDI")
			(pintype "input")
		)
		(pad "7" thru_hole circle
			(at 5.08 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "/CS_1")
			(pinfunction "CS")
			(pintype "input")
		)
		(pad "8" thru_hole circle
			(at 7.62 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 81 "unconnected-(U3-FLT-Pad8)")
			(pinfunction "FLT")
			(pintype "output")
		)
		(pad "9" thru_hole circle
			(at 10.16 8.255)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "unconnected-(U3-DRDY-Pad9)")
			(pinfunction "DRDY")
			(pintype "output")
		)
		(pad "10" thru_hole circle
			(at -1.778 -6.985)
			(size 2.184 2.184)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "unconnected-(U3---Pad10)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "11" thru_hole circle
			(at 1.778 -6.985)
			(size 2.184 2.184)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 84 "unconnected-(U3-+-Pad11)")
			(pinfunction "+")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(gr_rect
		(start 40.64 43.18)
		(end 251.31 127)
		(fill no)
		(layer "Edge.Cuts")
	)
	(zone
		(net 105)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 49.57 48.26) (xy 48 121) (xy 243 120.65) (xy 243 48.26)
			)
		)
	)
	(embedded_fonts no)
)
