(kicad_pcb (version 20171130) (host pcbnew 5.1.5+dfsg1-2build2)
  (general
    (thickness 1.6)
    (drawings 13)
    (tracks 15)
    (zones 0)
    (modules 5)
    (nets 6)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0)
    (zone_45_only yes)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 4)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 N$1)
  (net 2 N$2)
  (net 3 N$3)
  (net 4 N$4)
  (net 5 GND)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net N$1)
    (add_net N$2)
    (add_net N$3)
    (add_net N$4)
  )
  (module Connector_Wire:SolderWirePad_custom (layer Top) (tedit 642D019C)
    (at 150.011 108.9566)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (fp_text reference REF** (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_custom (at 0 6.35) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.3048 0.4318) (size 1.5 4) (layers Top F.Paste F.Mask)
      (net 1 N$1))
  )
  (module Connector_Wire:SolderWirePad_custom (layer Top) (tedit 642D0180)
    (at 142.7306 108.9566)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (fp_text reference REF** (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_custom (at 0 6.35) (layer F.Fab) hide)
    (pad 4 smd rect (at -0.3048 0.4318) (size 1.5 4) (layers Top F.Paste F.Mask)
      (net 4 N$4))
  )
  (module Connector_Wire:SolderWirePad_custom (layer Top) (tedit 642D0189)
    (at 145.1492 108.9566)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (fp_text reference REF** (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_custom (at 0 6.35) (layer F.Fab) hide)
    (pad 3 smd rect (at -0.3048 0.4318) (size 1.5 4) (layers Top F.Paste F.Mask)
      (net 3 N$3))
  )
  (module Connector_Wire:SolderWirePad_custom (layer Top) (tedit 642D0193)
    (at 147.5682 108.9566)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (fp_text reference REF** (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_custom (at 0 6.35) (layer F.Fab) hide)
    (pad 2 smd rect (at -0.3048 0.4318) (size 1.5 4) (layers Top F.Paste F.Mask)
      (net 2 N$2))
  )
  (module 3-way:3WAY-NAV-SWITCH (layer Top) (tedit 0)
    (at 148.4756 102.8396)
    (fp_text reference S1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (fp_text user "Nomad RGBDRV Nav Adapter" (at -8.4708 -5.3036 unlocked) (layer F.SilkS))
    (fp_text user C (at 6.8962 -3.297) (layer F.Fab))
    (fp_text user 2 (at 3.235 3.3222) (layer F.Fab))
    (fp_text user T (at 0.735 3.3222) (layer F.Fab))
    (fp_text user 1 (at -1.765 3.3222) (layer F.Fab))
    (pad "" np_thru_hole circle (at -2.5 -2.9) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad "" np_thru_hole circle (at 2.5 -2.9) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad NULL smd rect (at -5.4 -3.85) (size 1.6 1.5) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad P$C smd rect (at 5.4 -3.85) (size 1.6 1.5) (layers Top F.Paste F.Mask)
      (net 4 N$4) (solder_mask_margin 0.1016))
    (pad P$2 smd rect (at 2.5 0.9) (size 1.9 1.8) (layers Top F.Paste F.Mask)
      (net 1 N$1) (solder_mask_margin 0.1016))
    (pad P$T smd rect (at 0 0.9) (size 1.9 1.8) (layers Top F.Paste F.Mask)
      (net 2 N$2) (solder_mask_margin 0.1016))
    (pad P$1 smd rect (at -2.5 0.9) (size 1.9 1.8) (layers Top F.Paste F.Mask)
      (net 3 N$3) (solder_mask_margin 0.1016))
  )
  (gr_text "Sega Nomad RGBDRV Screen Control Adapter\n2023-04-04 SMK" (at 148.5392 105.5878 180) (layer F.SilkS))
  (gr_text "Sparkfun COM-08184 \nAdapter for Sega Nomad \nRGBDRV Screen Control" (at 146.0246 109.9058 180) (layer B.SilkS))
  (gr_line (start 151.0161 108.2776) (end 155.9011 108.2776) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 151.0161 111.2776) (end 151.0161 108.2776) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 141.1011 111.2776) (end 151.0161 111.2776) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 155.9011 108.2776) (end 155.9011 98.2776) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 155.9011 98.2776) (end 141.1011 98.2776) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 141.1011 98.2776) (end 141.1011 111.2776) (layer Edge.Cuts) (width 0.05))
  (gr_text 2 (at 149.3774 106.2482 270) (layer F.SilkS))
  (gr_text T (at 146.8628 106.3498 270) (layer F.SilkS))
  (gr_text 1 (at 144.5006 106.2736 270) (layer F.SilkS))
  (gr_text C (at 141.9606 106.2482 270) (layer F.SilkS))
  (zone (net 5) (net_name GND) (layer Bottom) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 159.7406 108.5342) (xy 159.6898 108.4834) (xy 159.6898 108.5088) (xy 137.1346 108.5088) (xy 137.1346 95.7326)
        (xy 159.7406 95.7326)
      )
    )
  )
)
