(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 14)
    (tracks 97)
    (zones 0)
    (modules 5)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.6096)
    (user_trace_width 0.3048)
    (user_trace_width 0.6096)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad3)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad1)")
  (net 4 "Net-(J2-Pad5)")
  (net 5 "Net-(J2-Pad6)")
  (net 6 "Net-(J2-Pad7)")
  (net 7 VDD)
  (net 8 GND)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net VDD)
  )
  (module Custom_KICAD:W-PDFN-8 (layer F.Cu) (tedit 5E35CB85)
    (at 152.4508 100.33)
    (fp_text reference U1 (at -2.3368 -4.318) (layer F.SilkS))
    (fp_text value MT25QL512ABB (at 0 -6.625) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -4 -1.905) (size 1 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 3 "Net-(J1-Pad1)"))
    (pad 2 smd roundrect (at -4 -0.635) (size 1 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 smd roundrect (at -4 0.635) (size 1 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 1 "Net-(J1-Pad3)"))
    (pad 4 smd roundrect (at -4 1.905) (size 1 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 8 GND))
    (pad 5 smd roundrect (at 4 1.905) (size 1 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 4 "Net-(J2-Pad5)"))
    (pad 6 smd roundrect (at 4 0.635) (size 1 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 5 "Net-(J2-Pad6)"))
    (pad 7 smd roundrect (at 4 -0.635) (size 1 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 6 "Net-(J2-Pad7)"))
    (pad 8 smd roundrect (at 4 -1.905) (size 1 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 7 VDD))
    (pad EP smd rect (at 0 0) (size 3.4 4.3) (layers F.Cu F.Mask)
      (net 8 GND))
    (pad "" smd rect (at 0.65 1.1) (size 1 1.8) (layers F.Paste))
    (pad 9 smd rect (at -0.65 -1.1) (size 1 1.8) (layers F.Paste))
    (pad 10 smd rect (at 0.65 -1.1) (size 1 1.8) (layers F.Paste))
    (pad 11 smd rect (at -0.65 1.1) (size 1 1.8) (layers F.Paste))
    (pad EP thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 8 GND))
  )
  (module Connector_PinSocket_1.27mm:PinSocket_2x04_P1.27mm_Vertical_SMD (layer B.Cu) (tedit 5E3503FD)
    (at 152.4 96.774 180)
    (descr "surface-mounted straight socket strip, 2x04, 1.27mm pitch, double cols (from Kicad 4.0.7!), script generated")
    (tags "Surface mounted socket strip SMD 2x04 1.27mm double row")
    (attr smd)
    (fp_text reference J2 (at 0 4.04 180) (layer B.SilkS) hide)
    (fp_text value BOTTOM (at 0 -4.04 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer B.Fab) hide)
    (pad 1 smd rect (at 1.8 1.905 180) (size 2.1 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J1-Pad1)"))
    (pad 8 smd rect (at -1.8 1.905 180) (size 2.1 0.75) (layers B.Cu B.Paste B.Mask)
      (net 7 VDD))
    (pad 2 smd rect (at 1.8 0.635 180) (size 2.1 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 7 smd rect (at -1.8 0.635 180) (size 2.1 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(J2-Pad7)"))
    (pad 3 smd rect (at 1.8 -0.635 180) (size 2.1 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(J1-Pad3)"))
    (pad 6 smd rect (at -1.8 -0.635 180) (size 2.1 0.75) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J2-Pad6)"))
    (pad 4 smd rect (at 1.8 -1.905 180) (size 2.1 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 5 smd rect (at -1.8 -1.905 180) (size 2.1 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J2-Pad5)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_1.27mm.3dshapes/PinSocket_2x04_P1.27mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 156.5425 95.25)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 -1.65) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 VDD))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.27mm:PinHeader_1x04_P1.27mm_Vertical (layer F.Cu) (tedit 59FED6E3)
    (at 144.78 96.52)
    (descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x04 1.27mm single row")
    (fp_text reference J1 (at 0 -1.695) (layer F.SilkS) hide)
    (fp_text value LEFT (at 0 5.505) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.905 90) (layer F.Fab) hide)
    (pad 4 thru_hole oval (at 0 3.81) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 3 thru_hole oval (at 0 2.54) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 1.27) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x04_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.27mm:PinHeader_1x04_P1.27mm_Vertical (layer F.Cu) (tedit 59FED6E3)
    (at 160.02 96.52)
    (descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x04 1.27mm single row")
    (fp_text reference J3 (at 0 -1.695) (layer F.SilkS) hide)
    (fp_text value RIGHT (at 0 5.505) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.905 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 7 VDD))
    (pad 2 thru_hole oval (at 0 1.27) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad7)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad6)"))
    (pad 4 thru_hole oval (at 0 3.81) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad5)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x04_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "svcguy\n01/20\nREV A" (at 147.574 97.282) (layer B.SilkS))
  (gr_text MT25QLBreakout (at 154.94 102.362) (layer B.SilkS))
  (gr_text DQ0 (at 158.75 100.33) (layer F.SilkS))
  (gr_text C (at 158.75 99.06) (layer F.SilkS))
  (gr_text DQ3 (at 158.75 97.79) (layer F.SilkS))
  (gr_text VDD (at 158.75 96.52) (layer F.SilkS))
  (gr_text GND (at 146.05 100.33) (layer F.SilkS))
  (gr_text DQ2 (at 146.05 99.06) (layer F.SilkS))
  (gr_text DQ1 (at 146.05 98.044) (layer F.SilkS))
  (gr_text ~S (at 146.05 96.774) (layer F.SilkS))
  (gr_line (start 162.56 104.14) (end 162.56 93.98) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 142.24 104.14) (end 162.56 104.14) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 142.24 93.98) (end 142.24 104.14) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 162.56 93.98) (end 142.24 93.98) (layer Edge.Cuts) (width 0.05))
  (zone (net 8) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.24 93.98) (xy 142.24 104.14) (xy 162.56 104.14) (xy 162.56 93.98)
      )
    )
  )
  (zone (net 8) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.24 93.98) (xy 142.24 104.14) (xy 162.56 104.14) (xy 162.56 93.98)
      )
    )
  )
)
