(kicad_pcb (version 20171130) (host pcbnew "(5.0.1-3-g963ef8bb5)")
  (general
    (thickness 1.6)
    (drawings 7)
    (tracks 92)
    (zones 0)
    (modules 21)
    (nets 13)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 1)
    (user_trace_width 2)
    (user_trace_width 2.5)
    (user_trace_width 5)
    (trace_clearance 0.2)
    (zone_clearance 0.25)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.5 4.5)
    (pad_drill 1.5)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(Q1-Pad1)")
  (net 2 "Net-(Q2-Pad1)")
  (net 3 "Net-(Q3-Pad1)")
  (net 4 "Net-(Q4-Pad1)")
  (net 5 "Net-(R1-Pad1)")
  (net 6 "Net-(R2-Pad1)")
  (net 7 "Net-(R3-Pad1)")
  (net 8 "Net-(Q1-Pad2)")
  (net 9 "Net-(R4-Pad2)")
  (net 10 "Net-(R5-Pad2)")
  (net 11 "Net-(Q1-Pad3)")
  (net 12 "Net-(Q3-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q3-Pad1)")
    (add_net "Net-(Q3-Pad3)")
    (add_net "Net-(Q4-Pad1)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad2)")
  )
  (net_class wide ""
    (clearance 0.2)
    (trace_width 2.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module nor:simple-transistor (layer F.Cu) (tedit 5CC7DBB9)
    (at 124.217 83.5025)
    (descr "TO-264, Vertical, RM 5.45mm")
    (tags "TO-264 Vertical RM 5.45mm")
    (fp_text reference Q1 (at 5.45 -3.02) (layer F.SilkS) hide)
    (fp_text value Q_NPN_BEC (at 5.45 6.47) (layer F.Fab) hide)
    (pad 3 thru_hole oval (at 10.9 0) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 11 "Net-(Q1-Pad3)"))
    (pad 2 thru_hole oval (at 5.45 0) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 8 "Net-(Q1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-264_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module nor:simple-transistor (layer F.Cu) (tedit 5CC7DBB9)
    (at 124.725 103.505)
    (descr "TO-264, Vertical, RM 5.45mm")
    (tags "TO-264 Vertical RM 5.45mm")
    (fp_text reference Q2 (at 5.45 -3.02) (layer F.SilkS) hide)
    (fp_text value Q_NPN_BEC (at 5.45 6.47) (layer F.Fab) hide)
    (pad 3 thru_hole oval (at 10.9 0) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 11 "Net-(Q1-Pad3)"))
    (pad 2 thru_hole oval (at 5.45 0) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 8 "Net-(Q1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 "Net-(Q2-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-264_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module nor:simple-transistor (layer F.Cu) (tedit 5CC7DBB9)
    (at 147.32 125.465 90)
    (descr "TO-264, Vertical, RM 5.45mm")
    (tags "TO-264 Vertical RM 5.45mm")
    (fp_text reference Q3 (at 5.45 -3.02 90) (layer F.SilkS) hide)
    (fp_text value Q_NPN_BEC (at 5.45 6.47 90) (layer F.Fab) hide)
    (pad 3 thru_hole oval (at 10.9 0 90) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 12 "Net-(Q3-Pad3)"))
    (pad 2 thru_hole oval (at 5.45 0 90) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 8 "Net-(Q1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 3 "Net-(Q3-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-264_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module nor:simple-transistor (layer F.Cu) (tedit 5CC7DBB9)
    (at 156.21 104.14 270)
    (descr "TO-264, Vertical, RM 5.45mm")
    (tags "TO-264 Vertical RM 5.45mm")
    (fp_text reference Q4 (at 5.45 -3.02 270) (layer F.SilkS) hide)
    (fp_text value Q_NPN_BEC (at 5.45 6.47 270) (layer F.Fab) hide)
    (pad 3 thru_hole oval (at 10.9 0 270) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 12 "Net-(Q3-Pad3)"))
    (pad 2 thru_hole oval (at 5.45 0 270) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 8 "Net-(Q1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 4 "Net-(Q4-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-264_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 0)
    (at 104.521 65.405)
    (fp_text reference TP1 (at 0 -2.54) (layer Eco1.User))
    (fp_text value TestPoint (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (net 5 "Net-(R1-Pad1)"))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 0)
    (at 105.664 95.504)
    (fp_text reference TP2 (at 0 -2.54) (layer Eco1.User))
    (fp_text value TestPoint (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (net 6 "Net-(R2-Pad1)"))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 0)
    (at 104.902 122.047)
    (fp_text reference TP3 (at 0 -2.54) (layer Eco1.User))
    (fp_text value TestPoint (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (net 7 "Net-(R3-Pad1)"))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 0)
    (at 140.2715 145.7325)
    (fp_text reference TP4 (at 0 -2.54) (layer Eco1.User))
    (fp_text value TestPoint (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (net 8 "Net-(Q1-Pad2)"))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 0)
    (at 157.226 63.881)
    (fp_text reference TP5 (at 0 -2.54) (layer Eco1.User))
    (fp_text value TestPoint (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (net 9 "Net-(R4-Pad2)"))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 0)
    (at 184.7215 144.78)
    (fp_text reference TP6 (at 0 -2.54) (layer Eco1.User))
    (fp_text value TestPoint (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (net 10 "Net-(R5-Pad2)"))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 0)
    (at 184.7215 89.7255)
    (fp_text reference TP7 (at 0 -2.54) (layer Eco1.User))
    (fp_text value TestPoint (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (net 12 "Net-(Q3-Pad3)"))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 0)
    (at 184.4675 65.4685)
    (fp_text reference TP8 (at 0 -2.54) (layer Eco1.User))
    (fp_text value TestPoint (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (net 11 "Net-(Q1-Pad3)"))
  )
  (module nor:die (layer F.Cu) (tedit 0)
    (at 145.4785 103.4415)
    (fp_text reference G*** (at 0 0) (layer Eco1.User) hide)
    (fp_text value LOGO (at 0.75 0) (layer Eco1.User) hide)
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 103.632 79.9465)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 -2.31) (layer Eco1.User))
    (fp_text value SPARKFUN-RESISTORS_4.7KOHM-0603-1_10W-1% (at 5.08 2.31) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(Q1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 103.8225 108.712)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.08 -2.31) (layer Eco1.User))
    (fp_text value SPARKFUN-RESISTORS_4.7KOHM-0603-1_10W-1% (at 5.08 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(R2-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(Q2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 121.158 133.35)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 5.08 -2.31) (layer Eco1.User))
    (fp_text value SPARKFUN-RESISTORS_4.7KOHM-0603-1_10W-1% (at 5.08 2.31) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(Q3-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 162.6235 78.2955 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 5.08 -2.31 180) (layer Eco1.User))
    (fp_text value SPARKFUN-RESISTORS_4.7KOHM-0603-1_10W-1% (at 5.08 2.31 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(Q1-Pad3)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 175.641 122.682)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 5.08 -2.31) (layer Eco1.User))
    (fp_text value SPARKFUN-RESISTORS_4.7KOHM-0603-1_10W-1% (at 5.08 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(Q4-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 168.5925 96.5835 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 5.08 -2.31 270) (layer Eco1.User))
    (fp_text value SPARKFUN-RESISTORS_4.7KOHM-0603-1_10W-1% (at 5.08 2.31 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(Q3-Pad3)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module nor:silkscreen500 (layer F.Cu) (tedit 0)
    (at 145.288 103.378)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module nor:soldermask500 (layer F.Cu) (tedit 0)
    (at 145.288 103.378)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (gr_text V+ (at 199.898 33.782) (layer F.Mask))
  (gr_text W6 (at 163.195 145.415) (layer F.Cu))
  (gr_text 9914 (at 164.465 139.7) (layer F.Cu))
  (gr_line (start 95.25 155.575) (end 95.25 53.975) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 195.58 155.575) (end 95.25 155.575) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 195.58 53.975) (end 195.58 155.575) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 95.25 53.975) (end 195.58 53.975) (layer Edge.Cuts) (width 0.15))
  (zone (net 8) (net_name "Net-(Q1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 152.4 108.585) (xy 156.845 108.585) (xy 156.845 110.49) (xy 154.178 110.49) (xy 154.178 119.38)
        (xy 151.892 119.38) (xy 151.892 110.49) (xy 150.114 110.49) (xy 150.114 104.648) (xy 152.4 104.648)
      )
    )
  )
  (zone (net 4) (net_name "Net-(Q4-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.75 103.505) (xy 154.305 103.505) (xy 154.305 106.68) (xy 158.75 106.68)
      )
    )
  )
  (zone (net 11) (net_name "Net-(Q1-Pad3)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 177.546 72.644) (xy 177.546 74.676) (xy 181.864 71.12)
      )
    )
  )
  (zone (net 3) (net_name "Net-(Q3-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 131.318 134.62) (xy 130.048 134.62) (xy 130.048 131.064) (xy 138.684 131.064) (xy 138.684 123.19)
        (xy 149.606 123.19) (xy 149.606 126.492) (xy 140.716 126.492) (xy 139.7 133.858)
      )
    )
  )
  (zone (net 4) (net_name "Net-(Q4-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 179.07 123.952) (xy 179.07 124.968) (xy 173.482 124.968) (xy 173.482 123.952)
      )
    )
  )
  (zone (net 10) (net_name "Net-(R5-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 183.388 120.65) (xy 192.024 120.65) (xy 192.024 124.968) (xy 183.388 124.968)
      )
    )
  )
  (zone (net 11) (net_name "Net-(Q1-Pad3)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 164.465 82.423) (xy 156.337 82.4865) (xy 158.369 79.502) (xy 160.8455 76.8985) (xy 164.465 77.0255)
      )
    )
  )
  (zone (net 4) (net_name "Net-(Q4-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 173.736 120.142) (xy 179.1335 120.2055) (xy 179.07 124.2695) (xy 173.482 124.3965)
      )
    )
  )
  (zone (net 8) (net_name "Net-(Q1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.6185 114.6175) (xy 132.715 114.6175) (xy 132.715 124.1425) (xy 122.682 124.1425)
      )
    )
  )
  (zone (net 2) (net_name "Net-(Q2-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.0615 110.1725) (xy 111.0615 106.2355) (xy 114.4905 106.1085) (xy 118.8085 101.7905) (xy 126.8095 101.727)
        (xy 126.6825 104.902) (xy 120.142 104.9655) (xy 115.3795 110.109)
      )
    )
  )
  (zone (net 1) (net_name "Net-(Q1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.9345 77.5335) (xy 126.492 77.5335) (xy 126.4285 85.05825) (xy 122.301 85.12175) (xy 122.301 82.55)
        (xy 110.9345 82.6135)
      )
    )
  )
  (zone (net 9) (net_name "Net-(R4-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 164.084 57.8485) (xy 150.5585 57.8485) (xy 150.5585 80.899) (xy 153.9875 80.899) (xy 153.9875 76.708)
        (xy 156.9085 72.39) (xy 164.6555 72.39) (xy 166.5605 74.295) (xy 167.4495 75.1205) (xy 167.4495 98.2345)
        (xy 169.799 98.2345) (xy 169.799 80.2005) (xy 171.196 77.47) (xy 171.196 74.422) (xy 164.1475 68.326)
        (xy 164.1475 57.9755)
      )
    )
  )
  (zone (net 6) (net_name "Net-(R2-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0))
    (min_thickness 0.03)
    (fill yes (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0))
    (polygon
      (pts
        (xy 98.679 87.122) (xy 112.4585 87.122) (xy 112.4585 100.457) (xy 109.7915 100.457) (xy 106.6165 103.632)
        (xy 106.6165 111.1885) (xy 102.235 111.1885) (xy 102.235 104.0765) (xy 98.7425 100.584)
      )
    )
  )
  (zone (net 11) (net_name "Net-(Q1-Pad3)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 191.9605 72.7075) (xy 191.9605 58.674) (xy 177.6095 58.674) (xy 177.6095 72.5805)
      )
    )
  )
  (zone (net 12) (net_name "Net-(Q3-Pad3)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 178.054 82.931) (xy 191.008 82.931) (xy 191.008 95.6945) (xy 191.008 96.5835) (xy 181.8005 96.5835)
        (xy 178.562 99.822) (xy 178.562 110.49) (xy 168.656 110.49) (xy 163.83 105.664) (xy 175.768 105.664)
        (xy 175.768 99.568) (xy 177.9905 97.282)
      )
    )
  )
  (zone (net 10) (net_name "Net-(R5-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 177.546 137.414) (xy 177.6095 151.892) (xy 192.024 151.892) (xy 192.024 121.412) (xy 183.515 121.412)
        (xy 183.515 124.2695) (xy 188.4045 124.2695) (xy 188.4045 134.747) (xy 186.69 137.414)
      )
    )
  )
  (zone (net 5) (net_name "Net-(R1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 98.7425 58.42) (xy 112.7125 58.42) (xy 112.7125 72.644) (xy 109.5375 72.644) (xy 106.68 75.565)
        (xy 106.7435 82.677) (xy 102.235 82.55) (xy 102.235 76.2) (xy 98.7425 72.1995)
      )
    )
  )
  (zone (net 7) (net_name "Net-(R3-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 98.3615 128.5875) (xy 98.3615 114.681) (xy 112.649 114.681) (xy 112.649 127.762) (xy 115.824 130.937)
        (xy 123.6345 130.937) (xy 123.6345 136.2075) (xy 116.205 136.2075) (xy 108.966 128.9685)
      )
    )
  )
  (zone (net 8) (net_name "Net-(Q1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.096 138.43) (xy 148.082 138.43) (xy 148.082 151.8285) (xy 139.0015 151.8285) (xy 134.112 151.8285)
        (xy 126.746 151.892) (xy 126.746 148.336) (xy 130.81 148.336) (xy 133.096 146.2405)
      )
    )
  )
  (zone (net 11) (net_name "Net-(Q1-Pad3)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.924 85.344) (xy 152.908 86.36) (xy 135.89 86.36) (xy 136.144 83.312) (xy 154.94 83.312)
      )
    )
  )
)
