(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 4.69)
  )
  (paper "A4")
  (title_block
    (rev "A")
  )
  (layers
    (0 "F.Cu" signal)
    (1 "In1.Cu" power "PWR")
    (2 "In2.Cu" power "GND")
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In1.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 2" (type "prepreg") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In2.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 3" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "/signal_in")
  (net 3 "Net-(D1-Pad2)")
  (net 4 "+5V")
  (net 5 "/row0_out")
  (net 6 "Net-(D2-Pad2)")
  (net 7 "/row1_out")
  (net 8 "Net-(D3-Pad2)")
  (net 9 "/row2_out")
  (net 10 "Net-(D4-Pad2)")
  (net 11 "/row3_out")
  (net 12 "Net-(D10-Pad4)")
  (net 13 "Net-(D11-Pad4)")
  (net 14 "Net-(D12-Pad4)")
  (net 15 "Net-(D13-Pad4)")
  (net 16 "Net-(D14-Pad4)")
  (net 17 "Net-(D10-Pad2)")
  (net 18 "Net-(D11-Pad2)")
  (net 19 "Net-(D12-Pad2)")
  (net 20 "Net-(D13-Pad2)")
  (net 21 "Net-(D14-Pad2)")
  (net 22 "Net-(D15-Pad2)")
  (net 23 "Net-(D16-Pad2)")
  (net 24 "Net-(D17-Pad2)")
  (net 25 "Net-(D18-Pad2)")
  (net 26 "Net-(D19-Pad2)")
  (net 27 "Net-(D20-Pad2)")
  (net 28 "/signal_out")
  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (tedit 5AA4B285)
    (at 115 115)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "LCSC" "C2761795")
    (property "Sheetfile" "led-matrix-5x5.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D5" (at 0 -0.074) (layer "F.SilkS"))
    (fp_text value "WS2812B" (at 0 0) (layer "F.Fab"))
    (fp_text user "1" (at -4.15 -1.6) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect locked (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(D10-Pad4)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd rect locked (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect locked (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/row3_out") (pinfunction "DIN") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (tedit 5AA4B285)
    (at 145 85)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "LCSC" "C2761795")
    (property "Sheetfile" "led-matrix-5x5.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D17" (at 0 -0.064) (layer "F.SilkS"))
    (fp_text value "WS2812B" (at 0 0) (layer "F.Fab"))
    (fp_text user "1" (at -4.15 -1.6) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect locked (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(D17-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd rect locked (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect locked (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "Net-(D12-Pad2)") (pinfunction "DIN") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "matrix:MatrixConn" (layer "F.Cu")
    (tedit 625241E0)
    (at 111.8 95 -90)
    (property "Sheetfile" "led-matrix-5x5.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J1" (at 0 0 -90 unlocked) (layer "B.SilkS") hide)
    (fp_text value "IN" (at 0 -3 unlocked) (layer "B.SilkS"))
    (fp_text user "-" (at 2.3 -1.6 -90 unlocked) (layer "B.SilkS"))
    (fp_text user "+" (at 0 -1.6 -90 unlocked) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd rect (at -2.3 0 270) (size 2 2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "/signal_in") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at 0 0 270) (size 2 2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "+5V") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect (at 2.3 0 270) (size 2 2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "Pin_3") (pintype "passive"))
  )
  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (tedit 5AA4B285)
    (at 155 85)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "LCSC" "C2761795")
    (property "Sheetfile" "led-matrix-5x5.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D22" (at 0 0.114) (layer "F.SilkS"))
    (fp_text value "WS2812B" (at 0 0) (layer "F.Fab"))
    (fp_text user "1" (at -4.15 -1.6) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect locked (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/row1_out") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd rect locked (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect locked (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(D17-Pad2)") (pinfunction "DIN") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (tedit 5AA4B285)
    (at 135 85)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "LCSC" "C2761795")
    (property "Sheetfile" "led-matrix-5x5.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D12" (at 0 0.114) (layer "F.SilkS"))
    (fp_text value "WS2812B" (at 0 0) (layer "F.Fab"))
    (fp_text user "1" (at -4.15 -1.6) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect locked (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "Net-(D12-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd rect locked (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect locked (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(D12-Pad4)") (pinfunction "DIN") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (tedit 5AA4B285)
    (at 155 104.75)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "LCSC" "C2761795")
    (property "Sheetfile" "led-matrix-5x5.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D24" (at 0 -0.074) (layer "F.SilkS"))
    (fp_text value "WS2812B" (at 0 0) (layer "F.Fab"))
    (fp_text user "1" (at -4.15 -1.6) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect locked (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/row3_out") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd rect locked (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect locked (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "Net-(D19-Pad2)") (pinfunction "DIN") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (tedit 5AA4B285)
    (at 115 85)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "LCSC" "C2761795")
    (property "Sheetfile" "led-matrix-5x5.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D2" (at 0 0) (layer "F.SilkS"))
    (fp_text value "WS2812B" (at 0 0) (layer "F.Fab"))
    (fp_text user "1" (at -4.15 -1.6) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect locked (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(D2-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd rect locked (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect locked (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/row0_out") (pinfunction "DIN") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (tedit 5AA4B285)
    (at 125 75)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "LCSC" "C2761795")
    (property "Sheetfile" "led-matrix-5x5.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D6" (at 0 -0.046) (layer "F.SilkS"))
    (fp_text value "WS2812B" (at 0 0) (layer "F.Fab"))
    (fp_text user "1" (at -4.15 -1.6) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect locked (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(D11-Pad4)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd rect locked (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect locked (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(D1-Pad2)") (pinfunction "DIN") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (tedit 5AA4B285)
    (at 125 85)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "LCSC" "C2761795")
    (property "Sheetfile" "led-matrix-5x5.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D7" (at 0 -0.14) (layer "F.SilkS"))
    (fp_text value "WS2812B" (at 0 0) (layer "F.Fab"))
    (fp_text user "1" (at -4.15 -1.6) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect locked (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(D12-Pad4)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd rect locked (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect locked (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(D2-Pad2)") (pinfunction "DIN") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (tedit 5AA4B285)
    (at 135 95)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "LCSC" "C2761795")
    (property "Sheetfile" "led-matrix-5x5.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D13" (at 0 0.02) (layer "F.SilkS"))
    (fp_text value "WS2812B" (at 0 0) (layer "F.Fab"))
    (fp_text user "1" (at -4.15 -1.6) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect locked (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(D13-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd rect locked (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect locked (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Net-(D13-Pad4)") (pinfunction "DIN") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (tedit 5AA4B285)
    (at 155 95)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "LCSC" "C2761795")
    (property "Sheetfile" "led-matrix-5x5.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D23" (at 0 0.02) (layer "F.SilkS"))
    (fp_text value "WS2812B" (at 0 0) (layer "F.Fab"))
    (fp_text user "1" (at -4.15 -1.6) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect locked (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "/row2_out") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd rect locked (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect locked (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "Net-(D18-Pad2)") (pinfunction "DIN") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (tedit 5AA4B285)
    (at 125 104.75)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "LCSC" "C2761795")
    (property "Sheetfile" "led-matrix-5x5.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D9" (at 0 -0.074) (layer "F.SilkS"))
    (fp_text value "WS2812B" (at 0 0) (layer "F.Fab"))
    (fp_text user "1" (at -4.15 -1.6) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect locked (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(D14-Pad4)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd rect locked (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect locked (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(D4-Pad2)") (pinfunction "DIN") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (tedit 5AA4B285)
    (at 135 75)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "LCSC" "C2761795")
    (property "Sheetfile" "led-matrix-5x5.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D11" (at 0 -0.046) (layer "F.SilkS"))
    (fp_text value "WS2812B" (at 0 0) (layer "F.Fab"))
    (fp_text user "1" (at -4.15 -1.6) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect locked (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "Net-(D11-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd rect locked (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect locked (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(D11-Pad4)") (pinfunction "DIN") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (tedit 5AA4B285)
    (at 135 115)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "LCSC" "C2761795")
    (property "Sheetfile" "led-matrix-5x5.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D15" (at 0 0.086) (layer "F.SilkS"))
    (fp_text value "WS2812B" (at 0 0) (layer "F.Fab"))
    (fp_text user "1" (at -4.15 -1.6) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect locked (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "Net-(D15-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd rect locked (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect locked (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "Net-(D10-Pad2)") (pinfunction "DIN") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (tedit 5AA4B285)
    (at 145 115)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "LCSC" "C2761795")
    (property "Sheetfile" "led-matrix-5x5.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D20" (at 0 0.086) (layer "F.SilkS"))
    (fp_text value "WS2812B" (at 0 0) (layer "F.Fab"))
    (fp_text user "1" (at -4.15 -1.6) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect locked (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "Net-(D20-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd rect locked (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect locked (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "Net-(D15-Pad2)") (pinfunction "DIN") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (tedit 5AA4B285)
    (at 125 95)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "LCSC" "C2761795")
    (property "Sheetfile" "led-matrix-5x5.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D8" (at 0.062 -0.234) (layer "F.SilkS"))
    (fp_text value "WS2812B" (at 0 0) (layer "F.Fab"))
    (fp_text user "1" (at -4.15 -1.6) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect locked (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Net-(D13-Pad4)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd rect locked (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect locked (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(D3-Pad2)") (pinfunction "DIN") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (tedit 5AA4B285)
    (at 145 75)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "LCSC" "C2761795")
    (property "Sheetfile" "led-matrix-5x5.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D16" (at 0 0.03) (layer "F.SilkS"))
    (fp_text value "WS2812B" (at 0 0) (layer "F.Fab"))
    (fp_text user "1" (at -4.15 -1.6) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect locked (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "Net-(D16-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd rect locked (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect locked (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "Net-(D11-Pad2)") (pinfunction "DIN") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (tedit 5AA4B285)
    (at 115 75)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "LCSC" "C2761795")
    (property "Sheetfile" "led-matrix-5x5.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at 0 -0.07) (layer "F.SilkS"))
    (fp_text value "WS2812B" (at 0 0) (layer "F.Fab"))
    (fp_text user "1" (at -4.15 -1.6) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect locked (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(D1-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd rect locked (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect locked (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/signal_in") (pinfunction "DIN") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (tedit 5AA4B285)
    (at 115 95)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "LCSC" "C2761795")
    (property "Sheetfile" "led-matrix-5x5.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D3" (at 0 -0.14) (layer "F.SilkS"))
    (fp_text value "WS2812B" (at 0 0) (layer "F.Fab"))
    (fp_text user "1" (at -4.15 -1.6) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect locked (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(D3-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd rect locked (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect locked (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/row1_out") (pinfunction "DIN") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (tedit 5AA4B285)
    (at 155 115)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "LCSC" "C2761795")
    (property "Sheetfile" "led-matrix-5x5.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D25" (at 0 0.086) (layer "F.SilkS"))
    (fp_text value "WS2812B" (at 0 0) (layer "F.Fab"))
    (fp_text user "1" (at -4.15 -1.6) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect locked (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "/signal_out") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd rect locked (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect locked (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "Net-(D20-Pad2)") (pinfunction "DIN") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (tedit 5AA4B285)
    (at 145 104.75)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "LCSC" "C2761795")
    (property "Sheetfile" "led-matrix-5x5.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D19" (at 0 0) (layer "F.SilkS"))
    (fp_text value "WS2812B" (at 0 0) (layer "F.Fab"))
    (fp_text user "1" (at -4.15 -1.6) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect locked (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "Net-(D19-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd rect locked (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect locked (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "Net-(D14-Pad2)") (pinfunction "DIN") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "matrix:MatrixConn" (layer "F.Cu")
    (tedit 625241E0)
    (at 158.2 95.1 -90)
    (property "Sheetfile" "led-matrix-5x5.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J2" (at 0 0 -90 unlocked) (layer "B.SilkS") hide)
    (fp_text value "OUT" (at 0.1 4 unlocked) (layer "B.SilkS"))
    (fp_text user "+" (at 0 1.6 -90 unlocked) (layer "B.SilkS"))
    (fp_text user "-" (at 2.3 1.6 -90 unlocked) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -2.3 0 270) (size 2 2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 28 "/signal_out") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at 0 0 270) (size 2 2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "+5V") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect (at 2.3 0 270) (size 2 2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "Pin_3") (pintype "passive"))
  )
  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (tedit 5AA4B285)
    (at 125 115)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "LCSC" "C2761795")
    (property "Sheetfile" "led-matrix-5x5.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D10" (at 0 -0.168) (layer "F.SilkS"))
    (fp_text value "WS2812B" (at 0 0) (layer "F.Fab"))
    (fp_text user "1" (at -4.15 -1.6) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect locked (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "Net-(D10-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd rect locked (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect locked (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(D10-Pad4)") (pinfunction "DIN") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (tedit 5AA4B285)
    (at 155 75)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "LCSC" "C2761795")
    (property "Sheetfile" "led-matrix-5x5.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D21" (at 0 -0.046) (layer "F.SilkS"))
    (fp_text value "WS2812B" (at 0 0) (layer "F.Fab"))
    (fp_text user "1" (at -4.15 -1.6) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect locked (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/row0_out") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd rect locked (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect locked (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "Net-(D16-Pad2)") (pinfunction "DIN") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (tedit 5AA4B285)
    (at 115 104.75)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "LCSC" "C2761795")
    (property "Sheetfile" "led-matrix-5x5.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D4" (at 0 0.02) (layer "F.SilkS"))
    (fp_text value "WS2812B" (at 0 0) (layer "F.Fab"))
    (fp_text user "1" (at -4.15 -1.6) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect locked (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(D4-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd rect locked (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect locked (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "/row2_out") (pinfunction "DIN") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (tedit 5AA4B285)
    (at 135 104.75)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "LCSC" "C2761795")
    (property "Sheetfile" "led-matrix-5x5.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D14" (at 0 -0.074) (layer "F.SilkS"))
    (fp_text value "WS2812B" (at 0 0) (layer "F.Fab"))
    (fp_text user "1" (at -4.15 -1.6) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect locked (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "Net-(D14-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd rect locked (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect locked (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(D14-Pad4)") (pinfunction "DIN") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (tedit 5AA4B285)
    (at 145 95)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "LCSC" "C2761795")
    (property "Sheetfile" "led-matrix-5x5.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D18" (at 0 0.02) (layer "F.SilkS"))
    (fp_text value "WS2812B" (at 0 0.02) (layer "F.Fab"))
    (fp_text user "1" (at -4.15 -1.6) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect locked (at -2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "Net-(D18-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd rect locked (at 2.45 1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect locked (at 2.45 -1.6) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(D13-Pad2)") (pinfunction "DIN") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 160 119.4) (mid 159.824264 119.824264) (end 159.4 120) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 110.6 120) (mid 110.175736 119.824264) (end 110 119.4) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 110.6 120) (end 159.4 120) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 110 70.6) (end 110 119.4) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 159.4 70) (mid 159.824264 70.175736) (end 160 70.6) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 160 119.4) (end 160 70.6) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 110 70.6) (mid 110.175736 70.175736) (end 110.6 70) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 159.4 70) (end 110.6 70) (layer "Edge.Cuts") (width 0.1))
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 159.8 119.8)
        (xy 110.2 119.8)
        (xy 110.2 70.2)
        (xy 159.8 70.2)
      )
    )
  )
  (zone (net 4) (net_name "+5V") (layer "In1.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 159.8 119.8)
        (xy 110.2 119.8)
        (xy 110.2 70.2)
        (xy 159.8 70.2)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "In2.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 159.8 119.8)
        (xy 110.2 119.8)
        (xy 110.2 70.2)
        (xy 159.8 70.2)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (mode hatch) (thermal_gap 0.508) (thermal_bridge_width 0.508)
      (hatch_thickness 1.016) (hatch_gap 1.524) (hatch_orientation 0)
      (hatch_border_algorithm hatch_thickness) (hatch_min_hole_area 0.3))
    (polygon
      (pts
        (xy 159.8 119.8)
        (xy 110.2 119.8)
        (xy 110.2 70.2)
        (xy 159.8 70.2)
      )
    )
  )
)
