<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0.0508" y1="66.7446875" x2="5.0480875" y2="60.3504" width="0.1524" layer="20" curve="80"/>
<wire x1="5.0480875" y1="60.3504" x2="5.08" y2="60.3504" width="0" layer="20"/>
<wire x1="5.08" y1="60.3504" x2="5.08" y2="12.5222" width="0.1524" layer="20"/>
<wire x1="5.08" y1="12.5222" x2="0" y2="6.4008" width="0.1524" layer="20" curve="80"/>
<wire x1="0" y1="6.4008" x2="0" y2="6.285734375" width="0.1524" layer="20"/>
<wire x1="0" y1="6.285734375" x2="6.285734375" y2="0" width="0.1524" layer="20" curve="90"/>
<wire x1="6.285734375" y1="0" x2="6.35" y2="0" width="0" layer="20"/>
<wire x1="6.35" y1="0" x2="12.7" y2="5.08" width="0.1524" layer="20" curve="75"/>
<wire x1="12.7" y1="5.08" x2="17.78" y2="5.08" width="0.1524" layer="20"/>
<wire x1="17.78" y1="5.08" x2="17.78" y2="67.818" width="0.1524" layer="20"/>
<wire x1="17.78" y1="67.818" x2="12.7" y2="67.818" width="0.1524" layer="20"/>
<wire x1="12.7" y1="67.818" x2="12.6238" y2="67.789103125" width="0" layer="20"/>
<wire x1="12.6238" y1="67.789103125" x2="6.4481125" y2="72.888" width="0.1524" layer="20" curve="80"/>
<wire x1="6.4481125" y1="72.888" x2="0.0508" y2="66.7446875" width="0.1524" layer="20" curve="90"/>
<hole x="6.35" y="6.35" drill="7.874"/>
<hole x="6.35" y="66.675" drill="7.874"/>
<text>GND</text>
<text>12V</text>
<text>Jumper A 
Side Only</text>
<text>A</text>
<text>A</text>
<text>C</text>
<text>C</text>
<text>RV-Project.Com  LED Halo Light Board A
V1.2     2/9/2019</text>
<wire x1="14.7574" y1="25.49993125" x2="14.7574" y2="23.12406875" width="0.1524" layer="20"/>
<wire x1="14.7574" y1="23.12406875" x2="13.50273125" y2="21.8694" width="0.1524" layer="20" curve="-90"/>
<wire x1="13.50273125" y1="21.8694" x2="13.3185875" y2="21.8694" width="0.1524" layer="20"/>
<wire x1="13.3185875" y1="21.8694" x2="11.9888" y2="23.1991875" width="0.1524" layer="20" curve="-90"/>
<wire x1="11.9888" y1="23.1991875" x2="11.9888" y2="25.624396875" width="0.1524" layer="20"/>
<wire x1="11.9888" y1="25.624396875" x2="13.288403125" y2="26.924" width="0.1524" layer="20" curve="-90"/>
<wire x1="13.288403125" y1="26.924" x2="13.33333125" y2="26.924" width="0.1524" layer="20"/>
<wire x1="13.33333125" y1="26.924" x2="14.7574" y2="25.49993125" width="0.1524" layer="20" curve="-90"/>
<hole x="13.4112" y="36.5506" drill="6.4008"/>
<text>Cut Out</text>
<text>A</text>
<text>B</text>
<text>Side A</text>
<text>Side B</text>
<wire x1="14.7574" y1="50.017709375" x2="14.7574" y2="47.27776875" width="0.1524" layer="20"/>
<wire x1="14.7574" y1="47.27776875" x2="13.63143125" y2="46.1518" width="0.1524" layer="20" curve="-90"/>
<wire x1="13.63143125" y1="46.1518" x2="13.24346875" y2="46.1518" width="0.1524" layer="20"/>
<wire x1="13.24346875" y1="46.1518" x2="11.9888" y2="47.40646875" width="0.1524" layer="20" curve="-90"/>
<wire x1="11.9888" y1="47.40646875" x2="11.9888" y2="49.931" width="0.1524" layer="20"/>
<wire x1="11.9888" y1="49.931" x2="13.2896" y2="51.2318" width="0.1524" layer="20" curve="-90"/>
<wire x1="13.2896" y1="51.2318" x2="13.543309375" y2="51.2318" width="0.1524" layer="20"/>
<wire x1="13.543309375" y1="51.2318" x2="14.7574" y2="50.017709375" width="0.1524" layer="20" curve="-90"/>
<text>Cut Out</text>
<text>Watch LED Orientation</text>
<text>Watch LED Orientation</text>
</plain>
<libraries>
<library name="a-lib">
<description>&lt;b&gt;Al's Components.&lt;/b&gt;
&lt;p&gt;Including:
&lt;ul&gt;
&lt;li&gt;GPS Receivers
&lt;li&gt;ASK Transmitters and Receivers
&lt;li&gt;Specialtiy Switches
&lt;/ul&gt;</description>
<packages>
<package name="SURFACEPAD25X1">
</package>
<package name="PAD-1.5X4.5">
</package>
<package name="LED-1206">
</package>
<package name="1206-RES">
</package>
<package name="1X01_HEADER">
</package>
<package name="SMD-JUMPER_2A">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="a-lib" package="PAD-1.5X4.5" value=""/>
<element name="JP2" library="a-lib" package="PAD-1.5X4.5" value=""/>
<element name="JP3" library="a-lib" package="PAD-1.5X4.5" value=""/>
<element name="JP4" library="a-lib" package="PAD-1.5X4.5" value=""/>
<element name="LED1" library="a-lib" package="LED-1206" value="">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="a-lib" package="LED-1206" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="a-lib" package="SURFACEPAD25X1" value=""/>
<element name="JP7" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="JP10" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="a-lib" package="SMD-JUMPER_2A" value="M2JUMPER2(OFFSET)"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="R2" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="1"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="JP5" pad="P$1"/>
<contactref element="JP3" pad="P$1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="JP2" pad="P$1"/>
<contactref element="LED2" pad="C"/>
</signal>
<signal name="N$9">
<contactref element="JP1" pad="P$1"/>
<contactref element="R1" pad="2"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="GND">
<contactref element="JP4" pad="P$1"/>
<contactref element="LED1" pad="C"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$4">
</signal>
</signals>
</board>
</drawing>
</eagle>
