(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 10)
    (no_connects 0)
    (area 151.079999 110.439999 189.280001 135.940001)
    (thickness 1.6)
    (drawings 8)
    (tracks 45)
    (zones 0)
    (modules 7)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010b0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(6-12V1-Pad1)")
  (net 2 "Net-(6-12V1-Pad2)")
  (net 3 "Net-(D1-Pad1)")
  (net 4 "Net-(EndStopCB1-Pad1)")
  (net 5 "Net-(EndStopCB1-Pad2)")
  (net 6 "Net-(EndStopCB1-Pad3)")
  (net 7 "Net-(Opto1-Pad2)")
  (net 8 "Net-(R1-Pad2)")
  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(6-12V1-Pad1)")
    (add_net "Net-(6-12V1-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(EndStopCB1-Pad1)")
    (add_net "Net-(EndStopCB1-Pad2)")
    (add_net "Net-(EndStopCB1-Pad3)")
    (add_net "Net-(Opto1-Pad2)")
    (add_net "Net-(R1-Pad2)")
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MKDS1.5-2pol (layer F.Cu) (tedit 59ECEE2C)
    (at 160.02 128.27 270)
    (descr "2-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference "6-12V +" (at 2.54 6.35 270) (layer F.SilkS))
    (fp_text value AK500/2 (at 2.5 -6.6 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(6-12V1-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 "Net-(6-12V1-Pad2)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MKDS1.5-2pol.wrl
      (at (xyz 0.0984 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 59ECCB1B)
    (at 171.45 123.19 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D1 (at 5.08 0 270) (layer F.SilkS))
    (fp_text value "LED klein" (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(6-12V1-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-4_W7.62mm (layer F.Cu) (tedit 59ECF265)
    (at 171.45 127 270)
    (descr "4-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference OP1 (at 3.81 5.08 270) (layer F.SilkS))
    (fp_text value PC817 (at 3.81 4.87 270) (layer F.Fab))
    (fp_text user %R (at 3.81 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (pad 3 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(EndStopCB1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(Opto1-Pad2)"))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(EndStopCB1-Pad1)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-4_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 59ECCB13)
    (at 171.45 119.38 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 3.81 -2.31 90) (layer F.SilkS))
    (fp_text value 680Ω (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(Opto1-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_S03B-XH-A_03x2.50mm_Angled (layer F.Cu) (tedit 59ECE2FA)
    (at 179.07 132.08 90)
    (descr "JST XH series connector, S03B-XH-A, side entry type, through hole")
    (tags "connector jst xh tht side horizontal angled 2.50mm")
    (fp_text reference "End Stop OUT" (at 2.5 -3.5 90) (layer F.SilkS))
    (fp_text value "JST XH 3" (at 2.5 10.3 90) (layer F.Fab))
    (fp_text user %R (at 2.5 2.25 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(EndStopCB1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(EndStopCB1-Pad2)"))
    (pad 3 thru_hole circle (at 5 0 90) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(EndStopCB1-Pad3)"))
    (model Connectors_JST.3dshapes/JST_XH_S03B-XH-A_03x2.50mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_S02B-XH-A_02x2.50mm_Angled (layer F.Cu) (tedit 59ECE2ED)
    (at 179.07 116.84 90)
    (descr "JST XH series connector, S02B-XH-A, side entry type, through hole")
    (tags "connector jst xh tht side horizontal angled 2.50mm")
    (fp_text reference "End Stop IN" (at 1.25 -3.5 90) (layer F.SilkS))
    (fp_text value "JST XH 2" (at 1.25 10.3 90) (layer F.Fab))
    (fp_text user %R (at 1.25 2.25 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(EndStopCB1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(EndStopCB1-Pad3)"))
    (model Connectors_JST.3dshapes/JST_XH_S02B-XH-A_02x2.50mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MKDS1.5-3pol (layer F.Cu) (tedit 59ECE4E2)
    (at 160.02 113.03 270)
    (descr "3-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference Sensor (at 1.27 -6.35 270) (layer F.SilkS))
    (fp_text value AK500/3 (at 5 -6.6 270) (layer F.Fab))
    (pad 3 thru_hole circle (at 10 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 "Net-(6-12V1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(6-12V1-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 8 "Net-(R1-Pad2)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MKDS1.5-3pol.wrl
      (at (xyz 0.1968 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "optokoppler board" (at 154.94 123.19 90) (layer B.SilkS))
  (gr_text "BK\nblack" (at 153.67 118.11 90) (layer F.SilkS))
  (gr_text "BN\nbrown" (at 153.67 113.03 90) (layer F.SilkS))
  (gr_text "BU \nblue" (at 153.67 123.19 90) (layer F.SilkS))
  (gr_line (start 151.13 135.89) (end 151.13 110.49) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 189.23 135.89) (end 151.13 135.89) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 189.23 110.49) (end 189.23 135.89) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 151.13 110.49) (end 189.23 110.49) (angle 90) (layer Edge.Cuts) (width 0.1))
)
