<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="2" y1="0" x2="53" y2="0" width="0" layer="20"/>
<wire x1="53" y1="0" x2="55" y2="2" width="0" layer="20" curve="90"/>
<wire x1="55" y1="2" x2="55" y2="68" width="0" layer="20"/>
<wire x1="55" y1="68" x2="53" y2="70" width="0" layer="20" curve="90"/>
<wire x1="53" y1="70" x2="2" y2="70" width="0" layer="20"/>
<wire x1="2" y1="70" x2="0" y2="68" width="0" layer="20" curve="90"/>
<wire x1="0" y1="68" x2="0" y2="2" width="0" layer="20"/>
<wire x1="0" y1="2" x2="2" y2="0" width="0" layer="20" curve="90"/>
<text>JAW 2022-12</text>
<text>www.A791.com</text>
<text>espresso/HX/a</text>
</plain>
<libraries>
<library name="jaw-conn">
<packages>
<package name="TERM5MM-6">
</package>
<package name="HEADER-6X1-PTH">
</package>
</packages>
</library>
<library name="jaw-ic">
<packages>
<package name="DIP-05">
</package>
</packages>
</library>
<library name="jaw">
<packages>
<package name="AXIAL-0.3">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="TO220V">
<description>&lt;b&gt;TO 220 Vertical&lt;/b&gt; Package works with various parts including N-Channel MOSFET SparkFun SKU: COM-10213</description>
</package>
<package name="CUIPSK3D">
<description>power supply</description>
</package>
<package name="AXIAL-0.5">
<description>1/2W Resistor, 0.5" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="jaw-conn" package="TERM5MM-6" value="HEADER-6X1-5MM"/>
<element name="J2" library="jaw-conn" package="HEADER-6X1-PTH" value="HEADER-6X1-PTH">
<attribute name="NAME"/>
</element>
<element name="U1" library="jaw-ic" package="DIP-05" value="MOC3063-DIP">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U2" library="jaw-ic" package="DIP-05" value="MOC3063-DIP">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U3" library="jaw-ic" package="DIP-05" value="MOC3063-DIP">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U4" library="jaw-ic" package="DIP-05" value="MOC3063-DIP">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R1" library="jaw" package="AXIAL-0.3" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="jaw" package="AXIAL-0.3" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="jaw" package="AXIAL-0.3" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="jaw" package="TO220V" value="TRIAC-TO220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="jaw" package="TO220V" value="TRIAC-TO220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="jaw" package="TO220V" value="TRIAC-TO220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PWR1" library="jaw" package="CUIPSK3D" value="ACDC-PWR-PSK3D">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="jaw" package="AXIAL-0.3" value="360">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="jaw" package="AXIAL-0.3" value="360">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="jaw" package="AXIAL-0.3" value="360">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="jaw" package="AXIAL-0.5" value="12R/3W">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MOV1" library="jaw" package="AXIAL-0.3" value="mov">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F1" library="jaw" package="AXIAL-0.3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="ACL">
<contactref element="J1" pad="P$1"/>
<contactref element="R4" pad="P$2"/>
<contactref element="Q1" pad="2"/>
<contactref element="R5" pad="P$2"/>
<contactref element="Q2" pad="2"/>
<contactref element="R6" pad="P$2"/>
<contactref element="Q3" pad="2"/>
<contactref element="U1" pad="6"/>
<contactref element="F1" pad="P$2"/>
</signal>
<signal name="ACN">
<contactref element="PWR1" pad="ACN"/>
<contactref element="J1" pad="P$3"/>
<contactref element="MOV1" pad="P$1"/>
</signal>
<signal name="HEATER">
<contactref element="J1" pad="P$2"/>
<contactref element="R3" pad="P$2"/>
<contactref element="Q3" pad="1"/>
</signal>
<signal name="SOLEN">
<contactref element="J1" pad="P$4"/>
<contactref element="R2" pad="P$2"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="PUMP">
<contactref element="J1" pad="P$5"/>
<contactref element="R1" pad="P$2"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="LAMP">
<contactref element="J1" pad="P$6"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="N$1">
<contactref element="U4" pad="4"/>
<contactref element="R6" pad="P$1"/>
</signal>
<signal name="N$3">
<contactref element="U3" pad="4"/>
<contactref element="R5" pad="P$1"/>
</signal>
<signal name="N$5">
<contactref element="Q2" pad="3"/>
<contactref element="U3" pad="6"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="N$6">
<contactref element="U4" pad="6"/>
<contactref element="Q3" pad="3"/>
<contactref element="R3" pad="P$1"/>
</signal>
<signal name="N$9">
<contactref element="U2" pad="4"/>
<contactref element="R4" pad="P$1"/>
</signal>
<signal name="N$11">
<contactref element="U2" pad="6"/>
<contactref element="Q1" pad="3"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="IOLAMP">
<contactref element="J2" pad="P$1"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="IOPUMP">
<contactref element="J2" pad="P$2"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="IOSOLEN">
<contactref element="J2" pad="P$3"/>
<contactref element="U3" pad="1"/>
</signal>
<signal name="IOHEATER">
<contactref element="J2" pad="P$4"/>
<contactref element="U4" pad="1"/>
</signal>
<signal name="VP">
<contactref element="J2" pad="P$5"/>
<contactref element="PWR1" pad="VP"/>
</signal>
<signal name="VM">
<contactref element="J2" pad="P$6"/>
<contactref element="PWR1" pad="VM"/>
<contactref element="U1" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="U3" pad="2"/>
<contactref element="U4" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="PWR1" pad="ACL"/>
<contactref element="R7" pad="P$2"/>
</signal>
<signal name="N$4">
<contactref element="R7" pad="P$1"/>
<contactref element="MOV1" pad="P$2"/>
<contactref element="F1" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
