<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="50" y2="0" width="0" layer="20"/>
<wire x1="50" y1="0" x2="50" y2="50" width="0" layer="20"/>
<wire x1="50" y1="50" x2="0" y2="50" width="0" layer="20"/>
<wire x1="0" y1="50" x2="0" y2="0" width="0" layer="20"/>
<hole x="2.5" y="2.5" drill="3"/>
<hole x="47.5" y="2.5" drill="3"/>
<hole x="25" y="12.5" drill="3"/>
<hole x="12.5" y="25" drill="3"/>
<hole x="25" y="37.5" drill="3"/>
<hole x="37.5" y="25" drill="3"/>
<hole x="2.5" y="47.5" drill="3"/>
<hole x="47.5" y="47.5" drill="3"/>
<text>LED-DIN</text>
<text>+5V</text>
<text>GND</text>
<text>SW1</text>
<text>SW2</text>
<text>SW3</text>
<text>SW4</text>
<text>SW2</text>
<text>SW1</text>
<text>SW3</text>
<text>SW4</text>
<text>SWITCH
GNDS</text>
<text>Michael
Bennett</text>
<text>FOR USE WITH SPARKFUN.COM's
2x2 TRANSLUCENT BUTTON PAD
AND ADDRESSIBLE LEDs WITH
WS2812 CONTROL ICs</text>
<text>SW1</text>
<text>SW3</text>
<text>SW4</text>
<text>SW2</text>
<text>LED-DOUT</text>
<text>FOR USE WITH SPARKFUN.COM's
2x2 TRANSLUCENT BUTTON PAD
AND ADDRESSIBLE LEDs WITH
WS2812 CONTROL ICs</text>
<text>1N4148
DIODES</text>
<text>1N4148
DIODES</text>
</plain>
<libraries>
<library name="Bennett">
<packages>
<package name="2X2_BUTTON_RGB_ADDR">
</package>
<package name="1N4181">
</package>
<package name="J4X1">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="Bennett" package="2X2_BUTTON_RGB_ADDR" value="2X2_BUTTON_RGB_ADDR">
<attribute name="C1" value="C1"/>
</element>
<element name="C2" library="Bennett" package="2X2_BUTTON_RGB_ADDR" value="2X2_BUTTON_RGB_ADDR">
<attribute name="C1" value="C1"/>
</element>
<element name="C3" library="Bennett" package="2X2_BUTTON_RGB_ADDR" value="2X2_BUTTON_RGB_ADDR">
<attribute name="C1" value="C1"/>
</element>
<element name="C4" library="Bennett" package="2X2_BUTTON_RGB_ADDR" value="2X2_BUTTON_RGB_ADDR">
<attribute name="C1" value="C1"/>
</element>
<element name="U$1" library="Bennett" package="1N4181" value="1N4148"/>
<element name="U$2" library="Bennett" package="1N4181" value="1N4148"/>
<element name="U$3" library="Bennett" package="1N4181" value="1N4148"/>
<element name="U$4" library="Bennett" package="1N4181" value="1N4148"/>
<element name="U$5" library="Bennett" package="J4X1" value="JUMPER4X1"/>
<element name="U$6" library="Bennett" package="J4X1" value="JUMPER4X1"/>
</elements>
<signals>
<signal name="SIG2">
<contactref element="C2" pad="DIN"/>
<contactref element="C1" pad="DOUT"/>
</signal>
<signal name="SIG3">
<contactref element="C3" pad="DIN"/>
<contactref element="C2" pad="DOUT"/>
</signal>
<signal name="SIG4">
<contactref element="C4" pad="DIN"/>
<contactref element="C3" pad="DOUT"/>
</signal>
<signal name="N$4">
<contactref element="C4" pad="VDD"/>
<contactref element="C3" pad="VDD"/>
<contactref element="C2" pad="VDD"/>
<contactref element="C1" pad="VDD"/>
<contactref element="U$5" pad="P$2"/>
</signal>
<signal name="N$1">
<contactref element="C4" pad="GND"/>
<contactref element="C3" pad="GND"/>
<contactref element="C2" pad="GND"/>
<contactref element="C1" pad="GND"/>
<contactref element="U$5" pad="P$3"/>
</signal>
<signal name="N$3">
<contactref element="C4" pad="SWGND1"/>
<contactref element="U$1" pad="P$1"/>
</signal>
<signal name="N$5">
<contactref element="C2" pad="SWGND1"/>
<contactref element="U$3" pad="P$1"/>
</signal>
<signal name="N$7">
<contactref element="C1" pad="DIN"/>
<contactref element="U$5" pad="P$1"/>
</signal>
<signal name="N$9">
<contactref element="U$4" pad="P$2"/>
<contactref element="U$6" pad="P$1"/>
</signal>
<signal name="N$10">
<contactref element="U$3" pad="P$2"/>
<contactref element="U$6" pad="P$2"/>
</signal>
<signal name="N$11">
<contactref element="U$2" pad="P$2"/>
<contactref element="U$6" pad="P$3"/>
</signal>
<signal name="N$12">
<contactref element="U$1" pad="P$2"/>
<contactref element="U$6" pad="P$4"/>
</signal>
<signal name="N$6">
<contactref element="C1" pad="SWGND2"/>
<contactref element="U$4" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="C3" pad="SWGND2"/>
<contactref element="U$2" pad="P$1"/>
</signal>
<signal name="N$8">
<contactref element="U$5" pad="P$4"/>
<contactref element="C4" pad="DOUT"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
