(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "Avalache Transmitter")
    (date "2024-05-17")
    (rev "1.0")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Print/")
    )
  )
  (net 0 "")
  (net 1 "Net-(Q1-C)")
  (net 2 "+3V0")
  (net 3 "Net-(D1-K)")
  (net 4 "Net-(D1-A)")
  (net 5 "Net-(50%1-K)")
  (net 6 "Net-(50%1-A)")
  (net 7 "Net-(75%1-K)")
  (net 8 "Net-(75%1-A)")
  (net 9 "Net-(100%1-K)")
  (net 10 "Net-(100%1-A)")
  (net 11 "Net-(AE1-Pad2)")
  (net 12 "Net-(U2-8)")
  (net 13 "Net-(U2-12)")
  (net 14 "+6V")
  (net 15 "Net-(J1-Pin_1)")
  (net 16 "unconnected-(J1-Pin_2-Pad2)")
  (net 17 "unconnected-(J1-Pin_3-Pad3)")
  (net 18 "Net-(J1-Pin_4)")
  (net 19 "GND")
  (net 20 "Net-(Q1-B)")
  (net 21 "Net-(J1-Pin_5)")
  (net 22 "Net-(R7-Pad1)")
  (net 23 "Net-(R7-Pad2)")
  (net 24 "unconnected-(U2-bus-Pad3)")
  (net 25 "unconnected-(U2-TX-Pad10)")
  (net 26 "unconnected-(U2-RX-Pad11)")
  (net 27 "unconnected-(U2-RST-Pad12)")
  (net 28 "unconnected-(U2-9-Pad13)")
  (net 29 "unconnected-(U2-10-Pad14)")
  (net 30 "unconnected-(U2-11-Pad15)")
  (net 31 "unconnected-(U2-Ar-Pad18)")
  (net 32 "unconnected-(U2-A0-Pad19)")
  (net 33 "unconnected-(U2-A2-Pad21)")
  (net 34 "unconnected-(U2-A3-Pad22)")
  (net 35 "Net-(TRANSMITTING1-A)")
  (net 36 "Net-(TRANSMITTING1-K)")
  (net 37 "Net-(U2-A1)")
  (net 38 "unconnected-(SW2-C-Pad3)")
  (net 39 "/on{slash}off")
  (footprint "MountingHole:MountingHole_2.1mm" (layer "F.Cu")
    (at 122.38 149.618)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.1mm" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.05) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers "F&B.Cu" "*.Mask"))
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (at 126.134 101.137 90)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "avalanche_transmitter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "TRANSMITTING" (at 6.787 4.766 180) (layer "F.SilkS"))
    (fp_text value "GREEN_LED" (at 1.27 3.96 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 36 "Net-(TRANSMITTING1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(TRANSMITTING1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ta:pro_mini" (layer "F.Cu")
    (at 151.28 55.92 90)
    (property "Sheetfile" "avalanche_transmitter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 0 -21.59 90 unlocked) (layer "F.SilkS"))
    (fp_text value "~" (at 1.27 -5.35 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -1.27 -3.85 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 7.62 -13.97 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 39 "/on{slash}off") (pinfunction "bat") (pintype "input"))
    (pad "2" thru_hole circle (at 7.62 -11.43 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 19 "GND") (pinfunction "ground") (pintype "input"))
    (pad "3" thru_hole circle (at 7.62 -8.89 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 24 "unconnected-(U2-bus-Pad3)") (pinfunction "bus") (pintype "input"))
    (pad "4" thru_hole circle (at 7.62 -6.35 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "+3V0") (pinfunction "3V") (pintype "input"))
    (pad "5" thru_hole circle (at 7.62 -3.81 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(U2-8)") (pinfunction "8") (pintype "input"))
    (pad "6" thru_hole circle (at 7.62 -1.27 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D1-K)") (pinfunction "6") (pintype "input"))
    (pad "7" thru_hole circle (at 7.62 1.27 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(50%1-K)") (pinfunction "5") (pintype "input"))
    (pad "8" thru_hole circle (at 7.62 3.81 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(75%1-K)") (pinfunction "4") (pintype "input"))
    (pad "9" thru_hole circle (at 7.62 6.35 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(100%1-K)") (pinfunction "3") (pintype "input"))
    (pad "10" thru_hole circle (at 7.62 8.89 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 25 "unconnected-(U2-TX-Pad10)") (pinfunction "TX") (pintype "input"))
    (pad "11" thru_hole circle (at 7.62 11.43 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 26 "unconnected-(U2-RX-Pad11)") (pinfunction "RX") (pintype "input"))
    (pad "12" thru_hole circle (at 7.62 13.97 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 27 "unconnected-(U2-RST-Pad12)") (pinfunction "RST") (pintype "input"))
    (pad "13" thru_hole circle (at -7.62 -13.97 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 28 "unconnected-(U2-9-Pad13)") (pinfunction "9") (pintype "input"))
    (pad "14" thru_hole circle (at -7.62 -11.43 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 29 "unconnected-(U2-10-Pad14)") (pinfunction "10") (pintype "input"))
    (pad "15" thru_hole circle (at -7.62 -8.89 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 30 "unconnected-(U2-11-Pad15)") (pinfunction "11") (pintype "input"))
    (pad "16" thru_hole circle (at -7.62 -6.35 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(U2-12)") (pinfunction "12") (pintype "input"))
    (pad "17" thru_hole circle (at -7.62 -3.81 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 36 "Net-(TRANSMITTING1-K)") (pinfunction "13") (pintype "input"))
    (pad "18" thru_hole circle (at -7.62 -1.27 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 31 "unconnected-(U2-Ar-Pad18)") (pinfunction "Ar") (pintype "input"))
    (pad "19" thru_hole circle (at -7.62 1.27 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 32 "unconnected-(U2-A0-Pad19)") (pinfunction "A0") (pintype "input"))
    (pad "20" thru_hole circle (at -7.62 3.81 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 37 "Net-(U2-A1)") (pinfunction "A1") (pintype "input"))
    (pad "21" thru_hole circle (at -7.62 6.35 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 33 "unconnected-(U2-A2-Pad21)") (pinfunction "A2") (pintype "input"))
    (pad "22" thru_hole circle (at -7.62 8.89 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 34 "unconnected-(U2-A3-Pad22)") (pinfunction "A3") (pintype "input"))
    (pad "23" thru_hole circle (at -7.62 11.43 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(J1-Pin_5)") (pinfunction "A4") (pintype "input"))
    (pad "24" thru_hole circle (at -7.62 13.97 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(J1-Pin_4)") (pinfunction "A5") (pintype "input"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 152.169 135.549 -90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "avalanche_transmitter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr through_hole)
    (fp_text reference "R9" (at 3.81 -1.92 90) (layer "F.SilkS"))
    (fp_text value "R_Small" (at 3.81 1.92 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 37 "Net-(U2-A1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 39 "/on{slash}off") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 132.738 145.328)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "avalanche_transmitter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr through_hole)
    (fp_text reference "R4" (at 3.81 -1.92) (layer "F.SilkS"))
    (fp_text value "R_Small" (at 3.81 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(100%1-A)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 19 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 146.835 75.732 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "avalanche_transmitter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr through_hole)
    (fp_text reference "R8" (at 4.132 -1.785 90) (layer "F.SilkS"))
    (fp_text value "R_Small" (at 3.81 1.92 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(AE1-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "+3V0") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 146.454 143.169 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "avalanche_transmitter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr through_hole)
    (fp_text reference "R10" (at 3.81 -1.92 90) (layer "F.SilkS"))
    (fp_text value "R_Small" (at 3.81 1.92 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 19 "GND") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 37 "Net-(U2-A1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 132.46 77.918)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "avalanche_transmitter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr through_hole)
    (fp_text reference "R7" (at 1.62 -1.8) (layer "F.SilkS"))
    (fp_text value "R_Small" (at 3.81 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 22 "Net-(R7-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(R7-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-14_W7.62mm" (layer "F.Cu")
    (at 167.668 71.17 -90)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "avalanche_transmitter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "quad 2-input NAND gate")
    (property "ki_keywords" "HCMOS nand 2-input")
    (attr through_hole)
    (fp_text reference "U1" (at 3.81 -2.33 90) (layer "F.SilkS") hide)
    (fp_text value "74HC00" (at 2.43 12.218 -180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 7.62 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(J1-Pin_1)") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(U2-12)") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(R7-Pad2)") (pintype "output"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask"))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask"))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask"))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "8" thru_hole oval (at 7.62 15.24 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask"))
    (pad "9" thru_hole oval (at 7.62 12.7 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask"))
    (pad "10" thru_hole oval (at 7.62 10.16 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask"))
    (pad "11" thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask"))
    (pad "12" thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask"))
    (pad "13" thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask"))
    (pad "14" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "+3V0") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (at 135.532 68.152 -90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (property "Sheetfile" "avalanche_transmitter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C1" (at 2.5 2.282 90) (layer "F.SilkS"))
    (fp_text value "C" (at 2.5 2.5 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(AE1-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(Q1-C)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (at 126.134 114.467 90)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "avalanche_transmitter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "100%" (at 5.817 1.116 180) (layer "F.SilkS"))
    (fp_text value "RED_LED_25" (at 1.27 3.96 180) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x07_P2.54mm_Vertical" (layer "F.Cu")
    (at 150.772 107.355 90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (property "Sheetfile" "avalanche_transmitter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x07, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.33 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x07_Pin" (at 0 17.57 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 7.62) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(J1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "unconnected-(J1-Pin_2-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "unconnected-(J1-Pin_3-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(J1-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(J1-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 19 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "+3V0") (pinfunction "Pin_7") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x07_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 132.78 114.467)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "avalanche_transmitter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr through_hole)
    (fp_text reference "R1" (at 3.81 -1.92) (layer "F.SilkS"))
    (fp_text value "R_Small" (at 3.81 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D1-A)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 19 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (at 128.801 68.152 -90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (property "Sheetfile" "avalanche_transmitter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Variable capacitor")
    (property "ki_keywords" "trimmer capacitor")
    (attr through_hole)
    (fp_text reference "CV1" (at 2.798 2.201 90) (layer "F.SilkS"))
    (fp_text value "C_Variable" (at 2.748 -2.299 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(AE1-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(Q1-C)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 159.789 140.995 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "avalanche_transmitter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Switch, single pole double throw")
    (property "ki_keywords" "switch single-pole double-throw spdt ON-ON")
    (attr through_hole)
    (fp_text reference "On/Off" (at -0.161 7.795) (layer "F.SilkS"))
    (fp_text value "SW_SPDT" (at -1.811 -2.855) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 39 "/on{slash}off") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "+6V") (pinfunction "B") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 38 "unconnected-(SW2-C-Pad3)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_THT:Potentiometer_Bourns_3296W_Vertical" (layer "F.Cu")
    (at 130.325 82.971 90)
    (descr "Potentiometer, vertical, Bourns 3296W, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296W")
    (property "Sheetfile" "avalanche_transmitter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Potentiometer")
    (property "ki_keywords" "resistor variable")
    (attr through_hole)
    (fp_text reference "RV1" (at -2.54 -3.66 90) (layer "F.SilkS"))
    (fp_text value "R_Potentiometer" (at -2.54 3.67 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -3.175 0.005 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.44 1.44) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 22 "Net-(R7-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 0 90) (size 1.44 1.44) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(Q1-B)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -5.08 0 90) (size 1.44 1.44) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 19 "GND") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296W_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 132.78 101.168)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "avalanche_transmitter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr through_hole)
    (fp_text reference "R5" (at 3.81 -1.92) (layer "F.SilkS"))
    (fp_text value "R_Small" (at 3.81 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(TRANSMITTING1-A)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 19 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.1mm" (layer "F.Cu")
    (at 172.28 44.568)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.1mm" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers "*.Cu" "*.Mask"))
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (at 126.134 124.627 90)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "avalanche_transmitter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "75%" (at 5.827 0.766 180) (layer "F.SilkS"))
    (fp_text value "RED_LED" (at -2.423 1.166 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(50%1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(50%1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 132.738 124.627)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "avalanche_transmitter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr through_hole)
    (fp_text reference "R2" (at 3.81 -1.92) (layer "F.SilkS"))
    (fp_text value "R_Small" (at 3.81 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(50%1-A)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 19 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (at 144.93 84.495 90)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "avalanche_transmitter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, TO-92")
    (property "ki_keywords" "NPN Transistor")
    (attr through_hole)
    (fp_text reference "Q1" (at 4.845 -0.08 180) (layer "F.SilkS"))
    (fp_text value "2N3904" (at 1.27 2.79 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 19 "GND") (pinfunction "E") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.27 0 90) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(Q1-B)") (pinfunction "B") (pintype "passive"))
    (pad "3" thru_hole oval (at 2.54 0 90) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(Q1-C)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 170.78 144.068)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (attr through_hole)
    (fp_text reference "GND" (at -0.18 -2.718) (layer "F.SilkS"))
    (fp_text value "PinHeader_1x01_P2.54mm_Vertical" (at 0 2.33) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 19 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (at 126.134 134.914 90)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "avalanche_transmitter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "50%" (at 5.414 0.616 180) (layer "F.SilkS"))
    (fp_text value "RED_LED_75" (at 1.27 3.96 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(75%1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(75%1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 162.38 114.218 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "avalanche_transmitter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr through_hole)
    (fp_text reference "R6" (at 3.81 1.75) (layer "F.SilkS"))
    (fp_text value "R_Small" (at 3.81 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(U2-8)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 19 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.1mm" (layer "F.Cu")
    (at 122.78 44.568)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.1mm" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.05) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers "F&B.Cu" "*.Mask"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 141.2 71.922 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "avalanche_transmitter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Loop antenna")
    (property "ki_keywords" "loop antenna")
    (attr through_hole)
    (fp_text reference "AE1" (at 2.555 1.872 90) (layer "F.SilkS"))
    (fp_text value "ANT_IN" (at 0 4.87) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(Q1-C)") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(AE1-Pad2)") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (at 126.134 145.328 90)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "avalanche_transmitter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "25%" (at 5.278 0.616 180) (layer "F.SilkS"))
    (fp_text value "RED_LED_100" (at 1.27 3.96 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(100%1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(100%1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.1mm" (layer "F.Cu")
    (at 172.58 149.618)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.1mm" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers "F&B.Cu" "*.Mask"))
  )
  (footprint "Button_Switch_THT:SW_PUSH-12mm" (layer "F.Cu")
    (at 148.44 121.168)
    (descr "SW PUSH 12mm https://www.e-switch.com/system/asset/product_line/data_sheet/143/TL1100.pdf")
    (tags "tact sw push 12mm")
    (attr through_hole)
    (fp_text reference "REF**" (at 6.08 -4.66) (layer "F.SilkS") hide)
    (fp_text value "SW_PUSH-12mm" (at 6.62 9.93) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 6.35 2.54) (layer "F.Fab") hide)
    (pad "1" thru_hole oval (at 0 0) (size 3.048 1.85) (drill 1.3) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole oval (at 12.5 0) (size 3.048 1.85) (drill 1.3) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(U2-8)"))
    (pad "2" thru_hole oval (at 0 5) (size 3.048 1.85) (drill 1.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole oval (at 12.5 5) (size 3.048 1.85) (drill 1.3) (layers "*.Cu" "*.Mask")
      (net 2 "+3V0"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH-12mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 132.78 134.914)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "avalanche_transmitter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr through_hole)
    (fp_text reference "R3" (at 3.81 -1.92) (layer "F.SilkS"))
    (fp_text value "R_Small" (at 3.81 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(75%1-A)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 19 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 170.78 138.318)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (attr through_hole)
    (fp_text reference "Battery In (6V)" (at -1.88 -3.168 180) (layer "F.SilkS") hide)
    (fp_text value "PinHeader_1x01_P2.54mm_Vertical" (at 0 2.33) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "+6V"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 120.03 42.218) (end 175.03 152.218)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "Mini Pro" (at 132.3 58.15 90) (layer "F.SilkS"))
  (gr_text "Avalanche Transmitter\n457 kHz" (at 157.38 150.618) (layer "F.SilkS"))
  (gr_text "RED_LED" (at 126.65 137.6) (layer "F.SilkS"))
  (gr_text "BATTERY" (at 127.98 106.668) (layer "F.SilkS"))
  (gr_text "74HC00" (at 154.05 82.7) (layer "F.SilkS"))
  (gr_text "GREEN_LED" (at 129 103.6) (layer "F.SilkS"))
  (gr_text "Power\n6V" (at 170.9 134.85) (layer "F.SilkS"))
  (gr_text "Si5351" (at 153.15 88.05) (layer "F.SilkS"))
  (gr_text "RED_LED" (at 127.7 148.05) (layer "F.SilkS"))
  (gr_text "Battery Check" (at 151.5 116.25) (layer "F.SilkS"))
  (gr_text "RED_LED" (at 127.8 116.85) (layer "F.SilkS"))
  (zone (net 19) (net_name "GND") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 120.08 42.168)
        (xy 175.03 42.218)
        (xy 175.08 152.218)
        (xy 120.03 152.218)
        (xy 120.08 42.618)
      )
    )
  )
  (zone (net 19) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 120.03 42.168)
        (xy 175.03 42.218)
        (xy 175.08 152.218)
        (xy 120.03 152.168)
      )
    )
  )
)
