(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "USLetter")
  (title_block
    (title "AiXun T3A Soldering Station dormancy input protection module")
    (rev "1.0")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0508)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "/_{VCC}")
  (net 2 "/_{GND}")
  (net 3 "/_{INPUT}")
  (net 4 "Net-(D1-Pad1)")
  (net 5 "/_{MCU}")
  (net 6 "Net-(C3-Pad1)")
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 132.08 96.52)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Sheetfile" "AiXun T3A input protection_20220805.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D2" (at 3.81 -2.12) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 3.81 1.905) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -1.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.11 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "/_{INPUT}") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "/_{GND}") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 125.73 107.95 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "AiXun T3A input protection_20220805.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R1" (at 5.08 -2.54 90) (layer "F.SilkS"))
    (fp_text value "10 kOhm" (at 7.62 2.54 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "/_{VCC}") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_6.4mm_M6_Pad_TopBottom" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 154.305 99.06)
    (descr "Mounting Hole 6.4mm, M6")
    (tags "mounting hole 6.4mm m6")
    (property "Sheetfile" "AiXun T3A input protection_20220805.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J3" (at -7.62 -2.54) (layer "F.SilkS"))
    (fp_text value "GND" (at -9.525 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" connect circle (at 0 0) (size 12.8 12.8) (layers "F.Cu" "F.Mask")
      (net 2 "/_{GND}") (pinfunction "Pin_1") (pintype "passive"))
    (pad "1" connect circle (at 0 0) (size 12.8 12.8) (layers "B.Cu" "B.Mask")
      (net 2 "/_{GND}") (pinfunction "Pin_1") (pintype "passive"))
    (pad "1" thru_hole circle (at 0 0) (size 6.8 6.8) (drill 6.4) (layers *.Cu *.Mask)
      (net 2 "/_{GND}") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Connector_Wire:SolderWire-1.5sqmm_1x01_D1.7mm_OD3.9mm" (layer "F.Cu")
    (tedit 5EB70B45)
    (at 120.015 93.345)
    (descr "Soldered wire connection, for a single 1.5 mm² wire, reinforced insulation, conductor diameter 1.7mm, outer diameter 3.9mm, size source Multi-Contact FLEXI-xV 1.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 1.5sqmm")
    (property "Sheetfile" "AiXun T3A input protection_20220805.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J1" (at -1.905 3.175) (layer "F.SilkS"))
    (fp_text value "+24V" (at 4.445 -1.905 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 3.9 3.9) (drill 2.1) (layers *.Cu *.Mask) (roundrect_rratio 0.064103)
      (net 1 "/_{VCC}") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-1.5sqmm_1x01_D1.7mm_OD3.9mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 132.08 118.11)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Sheetfile" "AiXun T3A input protection_20220805.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D1" (at 3.81 -1.905) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 12.065 0) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -1.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.11 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "/_{INPUT}") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LOGO" (layer "F.Cu")
    (tedit 0)
    (at 146.685 105.41)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "Connector_Wire:SolderWire-1.5sqmm_1x01_D1.7mm_OD3.9mm" (layer "F.Cu")
    (tedit 5EB70B45)
    (at 120.015 111.76)
    (descr "Soldered wire connection, for a single 1.5 mm² wire, reinforced insulation, conductor diameter 1.7mm, outer diameter 3.9mm, size source Multi-Contact FLEXI-xV 1.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 1.5sqmm")
    (property "Sheetfile" "AiXun T3A input protection_20220805.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J4" (at -1.905 -3.175) (layer "F.SilkS"))
    (fp_text value "MCU" (at 0 3.81 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 3.9 3.9) (drill 2.1) (layers *.Cu *.Mask) (roundrect_rratio 0.064103)
      (net 5 "/_{MCU}") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-1.5sqmm_1x01_D1.7mm_OD3.9mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 124.46 94.615)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "AiXun T3A input protection_20220805.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C1" (at 2.5 0) (layer "F.SilkS"))
    (fp_text value "0.1 uF" (at 2.5 1.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "/_{VCC}") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "/_{GND}") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 124.46 98.425)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "AiXun T3A input protection_20220805.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C2" (at 2.5 0) (layer "F.SilkS"))
    (fp_text value "1 uF" (at 2.5 1.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "/_{VCC}") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "/_{GND}") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_6.4mm_M6_Pad_TopBottom" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 154.305 113.03)
    (descr "Mounting Hole 6.4mm, M6")
    (tags "mounting hole 6.4mm m6")
    (property "Sheetfile" "AiXun T3A input protection_20220805.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J2" (at -7.62 2.54) (layer "F.SilkS"))
    (fp_text value "Input" (at -9.525 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 6.8 6.8) (drill 6.4) (layers *.Cu *.Mask)
      (net 3 "/_{INPUT}") (pinfunction "Pin_1") (pintype "passive"))
    (pad "1" connect circle (at 0 0) (size 12.8 12.8) (layers "F.Cu" "F.Mask")
      (net 3 "/_{INPUT}") (pinfunction "Pin_1") (pintype "passive"))
    (pad "1" connect circle (at 0 0) (size 12.8 12.8) (layers "B.Cu" "B.Mask")
      (net 3 "/_{INPUT}") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 120.65 107.95 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "AiXun T3A input protection_20220805.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R2" (at 5.08 -2.37 90) (layer "F.SilkS"))
    (fp_text value "330 Ohm" (at 5.08 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "/_{MCU}") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C3-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 124.46 102.235)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "AiXun T3A input protection_20220805.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C3" (at 2.5 0) (layer "F.SilkS"))
    (fp_text value "1 uF" (at 2.5 1.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C3-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "/_{GND}") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-4_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 131.445 113.03 90)
    (descr "4-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "AiXun T3A input protection_20220805.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at 3.81 -2.33 90) (layer "F.SilkS"))
    (fp_text value "KENTO JC817" (at 3.81 4.445 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "/_{INPUT}") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "/_{GND}") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "/_{MCU}") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-4_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-201AE_P15.24mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 139.7 99.695 -90)
    (descr "Diode, DO-201AE series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=9*5.3mm^2, , http://www.farnell.com/datasheets/529758.pdf")
    (tags "Diode DO-201AE series Axial Horizontal pin pitch 15.24mm  length 9mm diameter 5.3mm")
    (property "Sheetfile" "AiXun T3A input protection_20220805.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D3" (at 10.16 -3.81 90) (layer "F.SilkS"))
    (fp_text value "1.5KE30CA" (at 8.89 1.905 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.3 90) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -2.3 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 8.295 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 "/_{GND}") (pinfunction "A1") (pintype "passive"))
    (pad "2" thru_hole oval (at 15.24 0 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 "/_{INPUT}") (pinfunction "A2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-201AE_P15.24mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LOGO" (layer "B.Cu")
    (tedit 0)
    (at 132.08 104.775 180)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (gr_line (start 161.29 120.015) (end 161.29 90.17) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 161.29 90.17) (end 116.84 90.17) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 116.84 90.17) (end 116.84 120.015) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 116.84 120.015) (end 161.29 120.015) (layer "Edge.Cuts") (width 0.1))
  (gr_text "T3A PROTECTOR v1.1           08.2022" (at 145.415 91.44) (layer "F.SilkS"))
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 161.29 90.17) (xy 161.29 120.015))
    (height -5.08)
    (gr_text "29.8450 mm" (at 164.57 105.0925 90) (layer "Dwgs.User"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.2) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 116.84 120.015) (xy 161.29 120.015))
    (height 5.715)
    (gr_text "44.4500 mm" (at 139.065 123.93) (layer "Dwgs.User"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.2) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
)
