(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.101)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers")
    )
  )
  (net 0 "")
  (net 1 "GNDREF")
  (net 2 "VCC")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C3-Pad2)")
  (net 5 "Net-(C3-Pad1)")
  (net 6 "Net-(J3-Pad2)")
  (net 7 "Net-(J3-Pad1)")
  (net 8 "Net-(ATTINY85-Pad7)")
  (net 9 "Net-(ATTINY85-Pad3)")
  (net 10 "Net-(ATTINY85-Pad6)")
  (net 11 "Net-(ATTINY85-Pad2)")
  (net 12 "Net-(ATTINY85-Pad5)")
  (net 13 "Net-(ATTINY85-Pad1)")
  (net 14 "Net-(SD/PB3-Pad2)")
  (net 15 "unconnected-(U1-Pad2)")
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 161 141.7)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "attinyspeaker8302.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.33) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x02" (at 0 4.87) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole roundrect locked (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 "GNDREF") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 620E8184)
    (at 161.25 149.5552 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "attinyspeaker8302.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -2.33 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x02" (at 0 4.87 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0)
      (chamfer_ratio 0.2) (chamfer top_left top_right bottom_left bottom_right)
      (net 7 "Net-(J3-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "attinyspeaker:Potentiometer_Piher_PT-6-V_Vertical_and_ct6ep" (layer "F.Cu")
    (tedit 6182CC87)
    (at 160.8328 138.7056)
    (descr "Potentiometer, vertical, Piher PT-6-V, http://www.piher-nacesa.com/pdf/11-PT6v03.pdf")
    (tags "Potentiometer vertical Piher PT-6-V")
    (property "Sheetfile" "attinyspeaker8302.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "VOL" (at 1.6672 -2.5) (layer "F.SilkS"))
    (fp_text value "10K" (at 2.5 2.06) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.55 -2.5 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 2.54 0) (size 1.62 1.62) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.62 1.62) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 -2.5) (size 1.62 1.62) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad1)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 2.54 -5) (size 1.62 1.62) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "GNDREF") (pinfunction "3") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 0 -5) (size 1.62 1.62) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "GNDREF") (pinfunction "3") (pintype "passive"))
    (model "${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Piher_PT-6-V_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-8_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 171.704 145.5166 90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "attinyspeaker8302.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "ATTINY85" (at 3.8166 3.896 180) (layer "F.SilkS"))
    (fp_text value "ATtiny85-20PU" (at 3.81 9.95 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0)
      (chamfer_ratio 0.2) (chamfer top_right bottom_left)
      (net 13 "Net-(ATTINY85-Pad1)") (pinfunction "~{RESET}/PB5") (pintype "bidirectional"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(ATTINY85-Pad2)") (pinfunction "XTAL1/PB3") (pintype "bidirectional"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(ATTINY85-Pad3)") (pinfunction "XTAL2/PB4") (pintype "bidirectional"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GNDREF") (pinfunction "GND") (pintype "power_in"))
    (pad "5" thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(ATTINY85-Pad5)") (pinfunction "AREF/PB0") (pintype "bidirectional"))
    (pad "6" thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(ATTINY85-Pad6)") (pinfunction "PB1") (pintype "bidirectional"))
    (pad "7" thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(ATTINY85-Pad7)") (pinfunction "PB2") (pintype "bidirectional"))
    (pad "8" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 166.86 150)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "attinyspeaker8302.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R 150" (at 2.54 0.2) (layer "F.SilkS"))
    (fp_text value "150" (at 2.74 -1.2) (layer "F.Fab"))
    (fp_text user "Rfilter" (at 2.54 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -0.05 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.15 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(ATTINY85-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.4mm_W2.1mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 174.8 147.85 -90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.4*2.1mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.4mm width 2.1mm Capacitor")
    (property "Sheetfile" "attinyspeaker8302.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference ".1uF" (at 1.45 -1.4 -270 unlocked) (layer "F.SilkS"))
    (fp_text value ".1" (at 1.25 2.3 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GNDREF") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.4mm_W2.1mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.4mm_W2.1mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 168.75 137.5 -90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.4*2.1mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.4mm width 2.1mm Capacitor")
    (property "Sheetfile" "attinyspeaker8302.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference ".1uF" (at 1.0468 1.27 90) (layer "F.SilkS"))
    (fp_text value ".1" (at 1.25 2.3 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.4mm_W2.1mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 182.88 149.3)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (property "Sheetfile" "attinyspeaker8302.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 182.88 134.62)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (property "Sheetfile" "attinyspeaker8302.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_THT:C_Disc_D3.4mm_W2.1mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 163.7 141.3)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.4*2.1mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.4mm width 2.1mm Capacitor")
    (property "Sheetfile" "attinyspeaker8302.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference ".1uF" (at 1.3 -1.4) (layer "F.SilkS"))
    (fp_text value "1" (at 1.38 0.264) (layer "F.Fab"))
    (fp_text user "1uF" (at 1.25 -0.9) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "VCC") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GNDREF") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.4mm_W2.1mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:Diodes_SO-8EP" (layer "F.Cu")
    (tedit 5B8826E6)
    (at 166.5 145.2 180)
    (descr "8-Lead Plastic SO, Exposed Die Pad (see https://www.diodes.com/assets/Package-Files/SO-8EP.pdf)")
    (tags "SO exposed pad")
    (property "Sheetfile" "attinyspeaker8302.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "8302" (at -1.15 0 90) (layer "F.SilkS"))
    (fp_text value "PAM8302AAD" (at 0 3.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.4975 -1.905 180) (size 1.505 0.802) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(SD/PB3-Pad2)") (pinfunction "~{SD}") (pintype "input"))
    (pad "2" smd rect (at -2.4975 -0.635 180) (size 1.505 0.802) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "unconnected-(U1-Pad2)") (pinfunction "NC") (pintype "no_connect"))
    (pad "3" smd rect (at -2.4975 0.635 180) (size 1.505 0.802) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(C3-Pad2)") (pinfunction "IN+") (pintype "input"))
    (pad "4" smd rect (at -2.4975 1.905 180) (size 1.505 0.802) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GNDREF") (pinfunction "IN-") (pintype "input"))
    (pad "5" smd rect (at 2.4975 1.905 180) (size 1.505 0.802) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(J3-Pad1)") (pinfunction "OUT+") (pintype "output"))
    (pad "6" smd rect (at 2.4975 0.635 180) (size 1.505 0.802) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "VDD") (pintype "power_in"))
    (pad "7" smd rect (at 2.4975 -0.635 180) (size 1.505 0.802) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GNDREF") (pinfunction "GND") (pintype "power_in"))
    (pad "8" smd rect (at 2.4975 -1.905 180) (size 1.505 0.802) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(J3-Pad2)") (pinfunction "OUT-") (pintype "output"))
    (pad "9" smd rect (at 0.05 0 180) (size 1.2 3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "unconnected-(U1-Pad2)") (solder_paste_margin_ratio -0.2))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/Diodes_SO-8EP.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "attinyspeaker:PinHeader_2x03_P2.54mm_edgecard" (layer "F.Cu")
    (tedit 620D53D8)
    (at 185.5216 141.9352)
    (descr "surface-mounted straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x03 2.54mm double row")
    (property "Sheetfile" "attinyspeaker8302.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J5" (at 0 -4.87) (layer "F.SilkS") hide)
    (fp_text value "Conn_02x03_Odd_Even" (at 0 4.87) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.525 -2.54) (size 3.15 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(ATTINY85-Pad6)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at -2.54 -2.54) (size 3.15 1.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd roundrect (at -2.525 0) (size 3.15 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(ATTINY85-Pad7)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd roundrect (at -2.54 0) (size 3.15 1.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(ATTINY85-Pad5)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd roundrect (at -2.525 2.54) (size 3.15 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(ATTINY85-Pad1)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd roundrect (at -2.54 2.54) (size 3.15 1.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GNDREF") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical_SMD.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 621D0847)
    (at 169.1 134.25 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (property "Sheetfile" "attinyspeaker8302.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.33 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x05" (at 0 12.49 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.08) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 "GNDREF") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole rect (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(ATTINY85-Pad7)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(ATTINY85-Pad6)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(ATTINY85-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 621D0870)
    (at 178.4096 149.5552 90)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "attinyspeaker8302.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 0 -2.33 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x01" (at 0 2.33 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(ATTINY85-Pad2)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "attinyspeaker:cutablejumper" (layer "B.Cu")
    (tedit 61835CF4)
    (at 171.6 147.2 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "attinyspeaker8302.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SD/PB3" (at 0.3 -1 unlocked) (layer "B.SilkS"))
    (fp_text value "Jumper_NC_Small" (at 0 -1.16) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.5675 0 180) (size 0.735 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(ATTINY85-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5675 0 180) (size 0.735 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(SD/PB3-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "attinyspeaker:makerlogo" (layer "B.Cu")
    (tedit 0)
    (at 174.9 142.6 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 90 unlocked) (layer "B.SilkS") hide)
    (fp_text value "makerlogo" (at 0 -1 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab"))
  )
  (gr_line (start 159.004 151.4) (end 159.004 132.588) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 184.7088 132.588) (end 184.7088 151.4) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 184.7088 151.4) (end 159.004 151.4) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 159.004 132.588) (end 184.7088 132.588) (layer "Edge.Cuts") (width 0.05))
  (gr_text "GND" (at 182.372 143.2) (layer "B.SilkS"))
  (gr_text "ICSP" (at 180.1368 141.5796 90) (layer "B.SilkS"))
  (gr_text "+" (at 160.1 148.3) (layer "B.SilkS"))
  (gr_text "GND" (at 160.8 146.3) (layer "B.SilkS"))
  (gr_text "SPKR" (at 162.5 147.7) (layer "B.SilkS"))
  (gr_text "PB1" (at 176.75 132.95 180) (layer "B.SilkS"))
  (gr_text "-" (at 164.6 148.4 180) (layer "B.SilkS"))
  (gr_text "MOSI" (at 182.5752 140.7) (layer "B.SilkS"))
  (gr_text "PB2" (at 174.25 132.95 180) (layer "B.SilkS"))
  (gr_text "GND" (at 168.95 132.95 180) (layer "B.SilkS"))
  (gr_text "VCC" (at 182.2704 138.1) (layer "B.SilkS"))
  (gr_text "VCC" (at 171.7 132.95 180) (layer "B.SilkS"))
  (gr_text "VCC" (at 161 140.2) (layer "B.SilkS"))
  (gr_text "PB0" (at 179.1 132.95 180) (layer "B.SilkS"))
  (gr_text "attiny85+\npam8302\naudio\nclass" (at 166.6 145) (layer "B.SilkS"))
  (gr_text "RST" (at 182.1688 143.2) (layer "F.SilkS"))
  (gr_text "PB1" (at 176.45 136.05 -180) (layer "F.SilkS"))
  (gr_text "PB3" (at 179 148.1) (layer "F.SilkS"))
  (gr_text "-" (at 164.4 148.4 180) (layer "F.SilkS"))
  (gr_text "PB2" (at 174.0408 136.05 -180) (layer "F.SilkS"))
  (gr_text "+" (at 160.3 148.1) (layer "F.SilkS"))
  (gr_text "SCK" (at 182.372 140.7) (layer "F.SilkS"))
  (gr_text "PB0" (at 179 135.95 -180) (layer "F.SilkS"))
  (gr_text "VCC" (at 171.6 136.05 180) (layer "F.SilkS"))
  (gr_text "GND" (at 169 136.05 180) (layer "F.SilkS"))
  (gr_text "+\n" (at 162 140.3) (layer "F.SilkS"))
  (gr_text "-" (at 160.8 146.2 90) (layer "F.SilkS"))
  (gr_text "MISO" (at 182.4736 138.1) (layer "F.SilkS"))
  (zone (net 1) (net_name "GNDREF") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 184.531 152.019)
        (xy 159.512 152.019)
        (xy 159.4485 132.7785)
        (xy 184.5056 132.8928)
      )
    )
  )
  (zone (net 1) (net_name "GNDREF") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 184.404 152.146)
        (xy 159.385 152.019)
        (xy 159.4485 132.7785)
        (xy 184.4548 132.842)
      )
    )
  )
)
