(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 268)
    (zones 0)
    (modules 38)
    (nets 33)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu power)
    (2 In2.Cu power)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.508)
    (user_trace_width 0.2)
    (user_trace_width 0.5)
    (user_trace_width 0.508)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /5V)
  (net 3 /BPSU_BIAS1)
  (net 4 /3.3V)
  (net 5 /12V)
  (net 6 /BPSU_VEN)
  (net 7 /BPSU_VDAC)
  (net 8 /SI_MOSI_P)
  (net 9 /CDH_MOSI_P)
  (net 10 /CDH_MISO_P)
  (net 11 /CDH_CSn_P)
  (net 12 /SI_CSn_P)
  (net 13 /CDH_PPS_P)
  (net 14 /SI_MOSI_N)
  (net 15 /CDH_MOSI_N)
  (net 16 /CDH_MISO_N)
  (net 17 /CDH_CSn_N)
  (net 18 /SI_CSn_N)
  (net 19 /CDH_PPS_N)
  (net 20 /CDH_SCLK_N)
  (net 21 /CDH_SCLK_P)
  (net 22 /SI_SCLK_N)
  (net 23 /SI_SCLK_P)
  (net 24 /JTAG_TRST)
  (net 25 /JTAG_TDO)
  (net 26 /JTAG_TMS)
  (net 27 /JTAG_VPUMP)
  (net 28 /JTAG_TCK)
  (net 29 /JTAG_VJTAG)
  (net 30 /JTAG_TDI)
  (net 31 GNDA)
  (net 32 "Net-(JTAG2-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /12V)
    (add_net /3.3V)
    (add_net /5V)
    (add_net /BPSU_BIAS1)
    (add_net /BPSU_VDAC)
    (add_net /BPSU_VEN)
    (add_net /CDH_CSn_N)
    (add_net /CDH_CSn_P)
    (add_net /CDH_MISO_N)
    (add_net /CDH_MISO_P)
    (add_net /CDH_MOSI_N)
    (add_net /CDH_MOSI_P)
    (add_net /CDH_PPS_N)
    (add_net /CDH_PPS_P)
    (add_net /CDH_SCLK_N)
    (add_net /CDH_SCLK_P)
    (add_net /JTAG_TCK)
    (add_net /JTAG_TDI)
    (add_net /JTAG_TDO)
    (add_net /JTAG_TMS)
    (add_net /JTAG_TRST)
    (add_net /JTAG_VJTAG)
    (add_net /JTAG_VPUMP)
    (add_net /SI_CSn_N)
    (add_net /SI_CSn_P)
    (add_net /SI_MOSI_N)
    (add_net /SI_MOSI_P)
    (add_net /SI_SCLK_N)
    (add_net /SI_SCLK_P)
    (add_net GND)
    (add_net GNDA)
    (add_net "Net-(JTAG2-Pad4)")
  )
  (module MSAG_Misc:Pin_Header_Straight_2x05_Pitch2.54mm (layer F.Cu) (tedit 5CA344C4)
    (at 142.1384 143.7132 270)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference JTAG2 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_02x05_Odd_Even (at 1.27 12.49 90) (layer F.Fab))
    (fp_text user %R (at 1.27 5.08) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /JTAG_TCK))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /JTAG_TDO))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(JTAG2-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /JTAG_TMS))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /JTAG_VJTAG))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /JTAG_VPUMP))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /JTAG_TRST))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /JTAG_TDI))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model C:/Users/gsuarezm/Documents/kicad/MSAG_KiCad/MSAG_KiCad3d/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_2x05_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:NANO_9_FLYLEADS_MALE (layer F.Cu) (tedit 5E970DB1)
    (at 157.5054 144.8054)
    (fp_text reference JTAG1 (at -7.62 -3.81 180) (layer F.SilkS))
    (fp_text value MDM_09_MALE (at 0 -3.81) (layer F.Fab))
    (fp_text user 9 (at 3.81 0) (layer F.SilkS))
    (fp_text user 8 (at 1.27 0) (layer F.SilkS))
    (fp_text user 7 (at -1.27 0) (layer F.SilkS))
    (fp_text user 6 (at -3.81 0) (layer F.SilkS))
    (fp_text user 5 (at 5.08 -2.54) (layer F.SilkS))
    (fp_text user 4 (at 2.54 -2.54) (layer F.SilkS))
    (fp_text user 3 (at 0 -2.54) (layer F.SilkS))
    (fp_text user 2 (at -2.54 -2.54) (layer F.SilkS))
    (fp_text user 1 (at -5.08 -2.54) (layer F.SilkS))
    (pad 9 thru_hole circle (at 3.81 1.27 180) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole circle (at 1.27 1.27 180) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 24 /JTAG_TRST))
    (pad 4 thru_hole circle (at 2.54 -1.27 180) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 25 /JTAG_TDO))
    (pad 3 thru_hole circle (at 0 -1.27 180) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 26 /JTAG_TMS))
    (pad 2 thru_hole circle (at -2.54 -1.27 180) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 27 /JTAG_VPUMP))
    (pad 5 thru_hole circle (at 5.08 -1.27 180) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 28 /JTAG_TCK))
    (pad 6 thru_hole circle (at -3.81 1.27 180) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole circle (at 8.89 0 180) (size 3.656 3.656) (drill 2.64) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole circle (at -8.89 0 180) (size 3.656 3.656) (drill 2.64) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole circle (at -1.27 1.27 180) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 29 /JTAG_VJTAG))
    (pad 1 thru_hole rect (at -5.08 -1.27 180) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 30 /JTAG_TDI))
  )
  (module MSAG_Misc:msag_logo2_0.4in (layer F.Cu) (tedit 0)
    (at 128.27 135.89)
    (fp_text reference G*** (at 0 -7.961245) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module MSAG_Misc:BurstCube_bwA_0p4in (layer F.Cu) (tedit 0)
    (at 128.27 119.38)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module MSAG_Misc:nasa_logo_0.4inA (layer F.Cu) (tedit 0)
    (at 128.27 102.235)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module MSAG_Misc:Pin_Header_Straight_2x04_Pitch2.54mm (layer F.Cu) (tedit 5C52EE1A)
    (at 161.3916 127.3086)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (fp_text reference JTX1 (at 1.27 -2.33) (layer F.SilkS))
    (fp_text value Conn_02x04_Odd_Even (at 1.27 9.95) (layer F.Fab))
    (fp_text user %R (at 1.27 3.81 90) (layer F.Fab))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /SI_SCLK_N))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /SI_SCLK_P))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /SI_CSn_N))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /SI_CSn_P))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /CDH_MISO_N))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /CDH_MISO_P))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /SI_MOSI_N))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /SI_MOSI_P))
    (model ${MSAG3D}/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_2x04_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:NANO_9_FLYLEADS_MALE (layer F.Cu) (tedit 5E970DB1)
    (at 151.13 86.36)
    (fp_text reference JBPSU1 (at -5.08 3.81) (layer F.SilkS))
    (fp_text value MDM_09_MALE (at 0 -5.08) (layer F.Fab))
    (fp_text user 9 (at 3.81 0) (layer F.SilkS))
    (fp_text user 8 (at 1.27 0) (layer F.SilkS))
    (fp_text user 7 (at -1.27 0) (layer F.SilkS))
    (fp_text user 6 (at -3.81 0) (layer F.SilkS))
    (fp_text user 5 (at 5.08 -2.54) (layer F.SilkS))
    (fp_text user 4 (at 2.54 -2.54) (layer F.SilkS))
    (fp_text user 3 (at 0 -2.54) (layer F.SilkS))
    (fp_text user 2 (at -2.54 -2.54) (layer F.SilkS))
    (fp_text user 1 (at -5.08 -2.54) (layer F.SilkS))
    (pad 9 thru_hole circle (at 3.81 1.27 180) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 5 /12V))
    (pad 8 thru_hole circle (at 1.27 1.27 180) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 5 /12V))
    (pad 4 thru_hole circle (at 2.54 -1.27 180) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 31 GNDA))
    (pad 3 thru_hole circle (at 0 -1.27 180) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 3 /BPSU_BIAS1))
    (pad 2 thru_hole circle (at -2.54 -1.27 180) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 3 /BPSU_BIAS1))
    (pad 5 thru_hole circle (at 5.08 -1.27 180) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 6 /BPSU_VEN))
    (pad 6 thru_hole circle (at -3.81 1.27 180) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 7 /BPSU_VDAC))
    (pad 11 thru_hole circle (at 8.89 0 180) (size 3.656 3.656) (drill 2.64) (layers *.Cu *.Mask)
      (net 31 GNDA))
    (pad 10 thru_hole circle (at -8.89 0 180) (size 3.656 3.656) (drill 2.64) (layers *.Cu *.Mask)
      (net 31 GNDA))
    (pad 7 thru_hole circle (at -1.27 1.27 180) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 31 GNDA))
    (pad 1 thru_hole rect (at -5.08 -1.27 180) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 31 GNDA))
  )
  (module MSAG_Misc:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5C52ECC1)
    (at 132.715 80.645)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /BPSU_VEN))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5C52ECC1)
    (at 132.715 88.265)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /BPSU_VDAC))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:SMA_TH (layer F.Cu) (tedit 5C81344B)
    (at 143.51 109.22)
    (descr "25-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 47.1mm")
    (fp_text reference J12V1 (at 0 -4.572) (layer F.SilkS))
    (fp_text value SMA (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 -1.55) (layer F.Fab))
    (pad 5 thru_hole circle (at 2.54 2.54) (size 2.2098 2.2098) (drill 1.4986) (layers *.Cu *.Mask)
      (net 31 GNDA))
    (pad 4 thru_hole circle (at -2.54 2.54) (size 2.2098 2.2098) (drill 1.4986) (layers *.Cu *.Mask)
      (net 31 GNDA))
    (pad 3 thru_hole circle (at -2.54 -2.54) (size 2.2098 2.2098) (drill 1.4986) (layers *.Cu *.Mask)
      (net 31 GNDA))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.2098 2.2098) (drill 1.4986) (layers *.Cu *.Mask)
      (net 31 GNDA))
    (pad 1 thru_hole circle (at 0 0) (size 2.1082 2.1082) (drill 1.397) (layers *.Cu *.Mask)
      (net 5 /12V))
    (model ${MSAG}/MSAG_KiCad3d/SMA_VERTICAL_TH.stp
      (offset (xyz 0 0 9.4742))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5C52ECC1)
    (at 152.4 107.95)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J12VH1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /12V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 GNDA))
    (model ${MSAG3D}/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:SMA_TH (layer F.Cu) (tedit 5C81344B)
    (at 143.51 134.62)
    (descr "25-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 47.1mm")
    (fp_text reference J3V1 (at 0 -4.572) (layer F.SilkS))
    (fp_text value SMA (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 -1.55) (layer F.Fab))
    (pad 5 thru_hole circle (at 2.54 2.54) (size 2.2098 2.2098) (drill 1.4986) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at -2.54 2.54) (size 2.2098 2.2098) (drill 1.4986) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at -2.54 -2.54) (size 2.2098 2.2098) (drill 1.4986) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.2098 2.2098) (drill 1.4986) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.1082 2.1082) (drill 1.397) (layers *.Cu *.Mask)
      (net 4 /3.3V))
    (model ${MSAG}/MSAG_KiCad3d/SMA_VERTICAL_TH.stp
      (offset (xyz 0 0 9.4742))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5C52ECC1)
    (at 152.4 133.35)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J3VH1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /3.3V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:SMA_TH (layer F.Cu) (tedit 5C81344B)
    (at 143.51 121.92)
    (descr "25-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 47.1mm")
    (fp_text reference J5V1 (at 0 -4.572) (layer F.SilkS))
    (fp_text value SMA (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 -1.55) (layer F.Fab))
    (pad 5 thru_hole circle (at 2.54 2.54) (size 2.2098 2.2098) (drill 1.4986) (layers *.Cu *.Mask)
      (net 31 GNDA))
    (pad 4 thru_hole circle (at -2.54 2.54) (size 2.2098 2.2098) (drill 1.4986) (layers *.Cu *.Mask)
      (net 31 GNDA))
    (pad 3 thru_hole circle (at -2.54 -2.54) (size 2.2098 2.2098) (drill 1.4986) (layers *.Cu *.Mask)
      (net 31 GNDA))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.2098 2.2098) (drill 1.4986) (layers *.Cu *.Mask)
      (net 31 GNDA))
    (pad 1 thru_hole circle (at 0 0) (size 2.1082 2.1082) (drill 1.397) (layers *.Cu *.Mask)
      (net 2 /5V))
    (model ${MSAG}/MSAG_KiCad3d/SMA_VERTICAL_TH.stp
      (offset (xyz 0 0 9.4742))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5C52ECC1)
    (at 152.4 120.65)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J5VH1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 GNDA))
    (model ${MSAG3D}/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:BNC_TE-5-1634503-1 (layer F.Cu) (tedit 5C5B374F)
    (at 153.67 96.52)
    (descr "25-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 47.1mm")
    (fp_text reference JBIAS1 (at 6.985 4.445) (layer F.SilkS))
    (fp_text value BNC (at 0 0.85) (layer F.Fab))
    (fp_text user %R (at 0 -1.55) (layer F.Fab))
    (pad 5 thru_hole circle (at 3.23 3.23) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 31 GNDA))
    (pad 4 thru_hole circle (at -3.23 3.23) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 31 GNDA))
    (pad 3 thru_hole circle (at -3.23 -3.23) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 31 GNDA))
    (pad 2 thru_hole circle (at 3.23 -3.23) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 31 GNDA))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 /BPSU_BIAS1))
    (model ${MSAG}/MSAG_KiCad3d/TE-5-1634503-1.stp
      (offset (xyz 0 0 13.33499979972839))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5C52ECC1)
    (at 163.83 95.25)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JBIAS1H1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /BPSU_BIAS1))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 GNDA))
    (model ${MSAG3D}/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5C52ECEF)
    (at 158.8516 127.3086)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference JG1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5C52ECEF)
    (at 158.75 111.76)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference JG2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:Pin_Header_Straight_2x04_Pitch2.54mm (layer F.Cu) (tedit 5C52EE1A)
    (at 161.29 111.76)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (fp_text reference JRX1 (at 1.27 -2.33) (layer F.SilkS))
    (fp_text value Conn_02x04_Odd_Even (at 1.27 9.95) (layer F.Fab))
    (fp_text user %R (at 1.27 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /CDH_MOSI_P))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /CDH_MOSI_N))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /CDH_SCLK_P))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /CDH_SCLK_N))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /CDH_CSn_P))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /CDH_CSn_N))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /CDH_PPS_P))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /CDH_PPS_N))
    (model ${MSAG3D}/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_2x04_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:C_0805 (layer F.Cu) (tedit 5BB7E3B0)
    (at 136.3345 117.7925)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 10u_100V (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 /5V))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 31 GNDA))
    (model ${MSAG3D}/Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:C_0805 (layer F.Cu) (tedit 5BB7E3B0)
    (at 143.51 93.98)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 10u_100V (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 /BPSU_BIAS1))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 31 GNDA))
    (model ${MSAG3D}/Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:C_0805 (layer F.Cu) (tedit 5BB7E3B0)
    (at 136.3345 121.6025)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 1u_100V (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 31 GNDA))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 /5V))
    (model ${MSAG3D}/Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:C_0805 (layer F.Cu) (tedit 5BB7E3B0)
    (at 143.51 97.79)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 1u_100V (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 31 GNDA))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 /BPSU_BIAS1))
    (model ${MSAG3D}/Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:C_0603 (layer F.Cu) (tedit 5BB7E356)
    (at 136.3345 125.4125)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 0.1u_100V (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 /5V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 31 GNDA))
    (model ${MSAG3D}/Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:C_0603 (layer F.Cu) (tedit 5BB7E356)
    (at 143.51 101.6)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 0.1u_100V (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 31 GNDA))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 /BPSU_BIAS1))
    (model ${MSAG3D}/Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:C_0805 (layer F.Cu) (tedit 5BB7E3B0)
    (at 136.3345 130.4925)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 10u_100V (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /3.3V))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:C_0805 (layer F.Cu) (tedit 5BB7E3B0)
    (at 136.3345 105.0925)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 10u_100V (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 /12V))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 31 GNDA))
    (model ${MSAG3D}/Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:C_0805 (layer F.Cu) (tedit 5BB7E3B0)
    (at 136.3345 134.3025)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 1u_100V (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /3.3V))
    (model ${MSAG3D}/Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:C_0805 (layer F.Cu) (tedit 5BB7E3B0)
    (at 136.3345 108.9025)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 1u_100V (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 31 GNDA))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 /12V))
    (model ${MSAG3D}/Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:C_0603 (layer F.Cu) (tedit 5BB7E356)
    (at 136.3345 138.1125)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 0.1u_100V (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 /3.3V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:C_0603 (layer F.Cu) (tedit 5BB7E356)
    (at 136.3345 112.7125)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 0.1u_100V (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 31 GNDA))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 /12V))
    (model ${MSAG3D}/Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:MountingHole_2.261mm_M2_ISO14580_Pad (layer F.Cu) (tedit 5C62D16A)
    (at 125.73 76.835)
    (descr "Mounting Hole 2.2mm, M2, ISO14580")
    (tags "mounting hole 2.2mm m2 iso14580")
    (attr virtual)
    (fp_text reference MH1 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 0.65) (layer F.Fab))
    (fp_text user %R (at -0.05 -0.65) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.261) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MSAG_Misc:MountingHole_2.261mm_M2_ISO14580_Pad (layer F.Cu) (tedit 5C62D16A)
    (at 172.72 76.835)
    (descr "Mounting Hole 2.2mm, M2, ISO14580")
    (tags "mounting hole 2.2mm m2 iso14580")
    (attr virtual)
    (fp_text reference MH2 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 0.65) (layer F.Fab))
    (fp_text user %R (at -0.05 -0.65) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.261) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MSAG_Misc:MountingHole_2.261mm_M2_ISO14580_Pad (layer F.Cu) (tedit 5C62D16A)
    (at 172.72 144.78)
    (descr "Mounting Hole 2.2mm, M2, ISO14580")
    (tags "mounting hole 2.2mm m2 iso14580")
    (attr virtual)
    (fp_text reference MH3 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 0.65) (layer F.Fab))
    (fp_text user %R (at -0.05 -0.65) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.261) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MSAG_Misc:MountingHole_2.261mm_M2_ISO14580_Pad (layer F.Cu) (tedit 5C62D16A)
    (at 125.73 144.78)
    (descr "Mounting Hole 2.2mm, M2, ISO14580")
    (tags "mounting hole 2.2mm m2 iso14580")
    (attr virtual)
    (fp_text reference MH4 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 0.65) (layer F.Fab))
    (fp_text user %R (at -0.05 -0.65) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.261) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MSAG_Misc:NANO_31_FLYLEADS_MALE (layer F.Cu) (tedit 5E99BB6E)
    (at 172.72 115.57 270)
    (fp_text reference JCDH1 (at 16.51 3.81 270) (layer F.SilkS))
    (fp_text value NANO_31_MALE (at -0.1778 -3.8608 90) (layer F.Fab))
    (fp_text user 1 (at -19.05 -2.54 90) (layer F.SilkS))
    (fp_text user 2 (at -16.51 -2.54 90) (layer F.SilkS))
    (fp_text user 3 (at -13.97 -2.54 90) (layer F.SilkS))
    (fp_text user 4 (at -11.43 -2.54 90) (layer F.SilkS))
    (fp_text user 5 (at -8.89 -2.54 90) (layer F.SilkS))
    (fp_text user 6 (at -6.35 -2.54 90) (layer F.SilkS))
    (fp_text user 7 (at -3.81 -2.54 90) (layer F.SilkS))
    (fp_text user 8 (at -1.27 -2.54 90) (layer F.SilkS))
    (fp_text user 9 (at 1.27 -2.54 90) (layer F.SilkS))
    (fp_text user 10 (at 3.81 -2.54 90) (layer F.SilkS))
    (fp_text user 11 (at 6.35 -2.54 90) (layer F.SilkS))
    (fp_text user 12 (at 8.89 -2.54 90) (layer F.SilkS))
    (fp_text user 13 (at 11.43 -2.54 90) (layer F.SilkS))
    (fp_text user 14 (at 13.97 -2.54 90) (layer F.SilkS))
    (fp_text user 15 (at 16.51 -2.54 90) (layer F.SilkS))
    (fp_text user 17 (at -17.78 0 90) (layer F.SilkS))
    (fp_text user 18 (at -15.24 0 90) (layer F.SilkS))
    (fp_text user 16 (at 19.05 -2.54 90) (layer F.SilkS))
    (fp_text user 19 (at -12.7 0 90) (layer F.SilkS))
    (fp_text user 22 (at -5.08 0 90) (layer F.SilkS))
    (fp_text user 23 (at -2.54 0 90) (layer F.SilkS))
    (fp_text user 25 (at 2.54 0 90) (layer F.SilkS))
    (fp_text user 20 (at -10.16 0 90) (layer F.SilkS))
    (fp_text user 21 (at -7.62 0 90) (layer F.SilkS))
    (fp_text user 24 (at 0 0 90) (layer F.SilkS))
    (fp_text user 26 (at 5.08 0 90) (layer F.SilkS))
    (fp_text user 27 (at 7.62 0 90) (layer F.SilkS))
    (fp_text user 28 (at 10.16 0 90) (layer F.SilkS))
    (fp_text user 29 (at 12.7 0 90) (layer F.SilkS))
    (fp_text user 30 (at 15.24 0 90) (layer F.SilkS))
    (fp_text user 31 (at 17.78 0 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -19.05 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 31 GNDA))
    (pad 7 thru_hole circle (at -3.81 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 4 /3.3V))
    (pad 32 thru_hole circle (at -22.86 0 90) (size 3.656 3.656) (drill 2.64) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 33 thru_hole circle (at 22.86 0 90) (size 3.656 3.656) (drill 2.64) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at -6.35 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 31 GNDA))
    (pad 5 thru_hole circle (at -8.89 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 31 GNDA))
    (pad 2 thru_hole circle (at -16.51 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 2 /5V))
    (pad 3 thru_hole circle (at -13.97 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 2 /5V))
    (pad 4 thru_hole circle (at -11.43 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 2 /5V))
    (pad 8 thru_hole circle (at -1.27 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole circle (at 1.27 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 17 /CDH_CSn_N))
    (pad 10 thru_hole circle (at 3.81 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 11 /CDH_CSn_P))
    (pad 11 thru_hole circle (at 6.35 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 15 /CDH_MOSI_N))
    (pad 12 thru_hole circle (at 8.89 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 9 /CDH_MOSI_P))
    (pad 13 thru_hole circle (at 11.43 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 18 /SI_CSn_N))
    (pad 19 thru_hole circle (at -12.7 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 5 /12V))
    (pad 17 thru_hole circle (at -17.78 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 31 GNDA))
    (pad 14 thru_hole circle (at 13.97 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 12 /SI_CSn_P))
    (pad 15 thru_hole circle (at 16.51 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 14 /SI_MOSI_N))
    (pad 18 thru_hole circle (at -15.24 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 5 /12V))
    (pad 16 thru_hole circle (at 19.05 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 8 /SI_MOSI_P))
    (pad 20 thru_hole circle (at -10.16 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 31 GNDA))
    (pad 22 thru_hole circle (at -5.08 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 4 /3.3V))
    (pad 21 thru_hole circle (at -7.62 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 31 GNDA))
    (pad 23 thru_hole circle (at -2.54 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 24 thru_hole circle (at 0 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 19 /CDH_PPS_N))
    (pad 25 thru_hole circle (at 2.54 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 13 /CDH_PPS_P))
    (pad 26 thru_hole circle (at 5.08 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 20 /CDH_SCLK_N))
    (pad 27 thru_hole circle (at 7.62 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 21 /CDH_SCLK_P))
    (pad 28 thru_hole circle (at 10.16 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 22 /SI_SCLK_N))
    (pad 29 thru_hole circle (at 12.7 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 23 /SI_SCLK_P))
    (pad 30 thru_hole circle (at 15.24 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 16 /CDH_MISO_N))
    (pad 31 thru_hole circle (at 17.78 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 10 /CDH_MISO_P))
  )
  (module MSAG_Misc:NANO_9_FLYLEADS_MALE (layer F.Cu) (tedit 5E970DB1)
    (at 151.13 78.74)
    (fp_text reference JBPSU2 (at -5.08 -3.81 180) (layer F.SilkS))
    (fp_text value MDM_09_MALE (at 0 -3.81) (layer F.Fab))
    (fp_text user 1 (at -5.08 -2.54) (layer F.SilkS))
    (fp_text user 2 (at -2.54 -2.54) (layer F.SilkS))
    (fp_text user 3 (at 0 -2.54) (layer F.SilkS))
    (fp_text user 4 (at 2.54 -2.54) (layer F.SilkS))
    (fp_text user 5 (at 5.08 -2.54) (layer F.SilkS))
    (fp_text user 6 (at -3.81 0) (layer F.SilkS))
    (fp_text user 7 (at -1.27 0) (layer F.SilkS))
    (fp_text user 8 (at 1.27 0) (layer F.SilkS))
    (fp_text user 9 (at 3.81 0) (layer F.SilkS))
    (pad 1 thru_hole rect (at -5.08 -1.27 180) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 31 GNDA))
    (pad 7 thru_hole circle (at -1.27 1.27 180) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 31 GNDA))
    (pad 10 thru_hole circle (at -8.89 0 180) (size 3.656 3.656) (drill 2.64) (layers *.Cu *.Mask)
      (net 31 GNDA))
    (pad 11 thru_hole circle (at 8.89 0 180) (size 3.656 3.656) (drill 2.64) (layers *.Cu *.Mask)
      (net 31 GNDA))
    (pad 6 thru_hole circle (at -3.81 1.27 180) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 7 /BPSU_VDAC))
    (pad 5 thru_hole circle (at 5.08 -1.27 180) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 6 /BPSU_VEN))
    (pad 2 thru_hole circle (at -2.54 -1.27 180) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 3 /BPSU_BIAS1))
    (pad 3 thru_hole circle (at 0 -1.27 180) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 3 /BPSU_BIAS1))
    (pad 4 thru_hole circle (at 2.54 -1.27 180) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 31 GNDA))
    (pad 8 thru_hole circle (at 1.27 1.27 180) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 5 /12V))
    (pad 9 thru_hole circle (at 3.81 1.27 180) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 5 /12V))
  )
  (gr_line (start 121.92 73.66) (end 121.92 82.55) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 176.53 82.55) (end 176.53 73.66) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 121.92 73.66) (end 176.53 73.66) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 121.92 148.59) (end 176.53 148.59) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 121.92 82.55) (end 121.92 148.59) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 176.53 148.59) (end 176.53 82.55) (layer Edge.Cuts) (width 0.12))
  (gr_text "GND\n" (at 128.905 92.075) (layer F.SilkS))
  (gr_text BPSU_VDAC (at 126.365 89.535) (layer F.SilkS))
  (gr_text "GND\n" (at 128.905 84.455) (layer F.SilkS))
  (gr_text BPSU_VEN (at 126.365 81.915) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 176.53 148.59) (xy 121.92 148.59) (xy 121.92 73.66) (xy 176.53 73.66)
      )
    )
  )
  (zone (net 4) (net_name /3.3V) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 176.5808 139.5476) (xy 121.9708 139.5476) (xy 121.8946 128.27) (xy 166.3446 128.27) (xy 166.37 109.22)
        (xy 176.53 109.22)
      )
    )
  )
  (zone (net 2) (net_name /5V) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 176.53 107.95) (xy 165.1 107.95) (xy 165.0746 126.9746) (xy 121.8946 126.9746) (xy 121.92 116.84)
        (xy 156.21 116.84) (xy 156.21 104.14) (xy 172.72 104.14) (xy 172.72 97.79) (xy 176.53 97.79)
      )
    )
  )
  (zone (net 3) (net_name /BPSU_BIAS1) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.0919 86.36) (xy 149.8473 86.36) (xy 149.86 91.44) (xy 165.1 91.44) (xy 165.1 99.1362)
        (xy 146.05 99.1362) (xy 146.05 102.87) (xy 121.92 102.87) (xy 121.92 73.66) (xy 151.1046 73.66)
      )
    )
  )
  (zone (net 5) (net_name /12V) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 176.53 96.52) (xy 171.45 96.52) (xy 171.45 102.87) (xy 154.94 102.87) (xy 154.94 115.57)
        (xy 121.92 115.57) (xy 121.92 104.14) (xy 147.32 104.14) (xy 147.32 100.2538) (xy 166.37 100.2538)
        (xy 166.37 90.17) (xy 151.384 90.1573) (xy 151.384 86.7791) (xy 152.4 86.7918) (xy 152.4 73.66)
        (xy 176.53 73.66)
      )
    )
  )
  (zone (net 31) (net_name GNDA) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 176.53 109.855) (xy 155.575 109.855) (xy 155.575 139.065) (xy 121.92 139.065) (xy 121.92 73.66)
        (xy 176.53 73.66)
      )
    )
  )
)
