(kicad_pcb (version 20171130) (host pcbnew "(5.1.6-87-g1447494bc)")
  (general
    (thickness 1.6)
    (drawings 104)
    (tracks 99)
    (zones 0)
    (modules 12)
    (nets 33)
  )
  (page USLetter)
  (title_block
    (title "Vectrex Stereo AY")
    (date 2021-07-21)
    (rev v1.0)
    (company "Brett Walach")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.254)
    (user_trace_width 0.4)
    (user_trace_width 0.6096)
    (trace_clearance 0.254)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.762)
    (via_drill 0.508)
    (via_min_size 0.6096)
    (via_min_drill 0.3302)
    (user_via 0.6096 0.3302)
    (user_via 1 0.6)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.1)
    (aux_axis_origin 0 0)
    (grid_origin 119.07 42.13)
    (visible_elements FFFFEF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "../gerbers"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 LEFT)
  (net 4 "Net-(C1-Pad1)")
  (net 5 RIGHT)
  (net 6 "Net-(C3-Pad1)")
  (net 7 CHAN_C)
  (net 8 CHAN_A)
  (net 9 CHAN_B)
  (net 10 DA0)
  (net 11 IOA0)
  (net 12 DA1)
  (net 13 IOA1)
  (net 14 DA2)
  (net 15 IOA2)
  (net 16 DA3)
  (net 17 IOA3)
  (net 18 DA4)
  (net 19 IOA4)
  (net 20 DA5)
  (net 21 IOA5)
  (net 22 DA6)
  (net 23 IOA6)
  (net 24 DA7)
  (net 25 IOA7)
  (net 26 BC1)
  (net 27 BC2)
  (net 28 BDIR)
  (net 29 A8)
  (net 30 _RESET)
  (net 31 TEST_1)
  (net 32 CLOCK)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.762)
    (via_drill 0.508)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net +5V)
    (add_net A8)
    (add_net BC1)
    (add_net BC2)
    (add_net BDIR)
    (add_net CHAN_A)
    (add_net CHAN_B)
    (add_net CHAN_C)
    (add_net CLOCK)
    (add_net DA0)
    (add_net DA1)
    (add_net DA2)
    (add_net DA3)
    (add_net DA4)
    (add_net DA5)
    (add_net DA6)
    (add_net DA7)
    (add_net GND)
    (add_net IOA0)
    (add_net IOA1)
    (add_net IOA2)
    (add_net IOA3)
    (add_net IOA4)
    (add_net IOA5)
    (add_net IOA6)
    (add_net IOA7)
    (add_net LEFT)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net RIGHT)
    (add_net TEST_1)
    (add_net _RESET)
  )
  (net_class Large ""
    (clearance 0.254)
    (trace_width 0.61)
    (via_dia 1)
    (via_drill 0.6)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
  )
  (module vectrex-stereo-ay:DIP-28_W15.24mm-socket (layer F.Cu) (tedit 5A02E8C5)
    (at 121.61 42.13)
    (descr "28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
    (fp_text reference U2 (at 7.62 -2.33) (layer F.SilkS) hide)
    (fp_text value "AY-3-8912 SOCKET" (at 7.62 35.35) (layer F.Fab))
    (fp_text user %R (at 7.62 16.51) (layer F.Fab))
    (pad 28 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 DA0))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 IOA0))
    (pad 27 thru_hole oval (at 15.24 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 DA1))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 IOA1))
    (pad 26 thru_hole oval (at 15.24 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 DA2))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 IOA2))
    (pad 25 thru_hole oval (at 15.24 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 DA3))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 IOA3))
    (pad 24 thru_hole oval (at 15.24 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 DA4))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 IOA4))
    (pad 23 thru_hole oval (at 15.24 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 DA5))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 IOA5))
    (pad 22 thru_hole oval (at 15.24 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 DA6))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 IOA6))
    (pad 21 thru_hole oval (at 15.24 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 DA7))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 IOA7))
    (pad 20 thru_hole oval (at 15.24 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 BC1))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 19 thru_hole oval (at 15.24 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 BC2))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 CHAN_A))
    (pad 18 thru_hole oval (at 15.24 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 BDIR))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 CHAN_B))
    (pad 17 thru_hole oval (at 15.24 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 A8))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 16 thru_hole oval (at 15.24 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 _RESET))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 TEST_1))
    (pad 15 thru_hole oval (at 15.24 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 CLOCK))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 CHAN_C))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-28_W15.24mm.wrlbak
      (offset (xyz 0 0 4))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-28_W15.24mm_Socket.wrlbak
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module vectrex-stereo-ay:DIP-28_W15.24mm-pins (layer F.Cu) (tedit 5FEB614B)
    (at 119.07 42.13)
    (descr "28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
    (fp_text reference U1 (at 7.62 -2.33) (layer F.SilkS) hide)
    (fp_text value "AY-3-8912 PINS" (at 7.62 35.35) (layer F.Fab))
    (fp_text user %R (at 7.62 16.51) (layer F.Fab))
    (pad 28 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 DA0))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 IOA0))
    (pad 27 thru_hole oval (at 15.24 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 DA1))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 IOA1))
    (pad 26 thru_hole oval (at 15.24 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 DA2))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 IOA2))
    (pad 25 thru_hole oval (at 15.24 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 DA3))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 IOA3))
    (pad 24 thru_hole oval (at 15.24 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 DA4))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 IOA4))
    (pad 23 thru_hole oval (at 15.24 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 DA5))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 IOA5))
    (pad 22 thru_hole oval (at 15.24 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 DA6))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 IOA6))
    (pad 21 thru_hole oval (at 15.24 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 DA7))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 IOA7))
    (pad 20 thru_hole oval (at 15.24 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 BC1))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 19 thru_hole oval (at 15.24 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 BC2))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 CHAN_A))
    (pad 18 thru_hole oval (at 15.24 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 BDIR))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 CHAN_B))
    (pad 17 thru_hole oval (at 15.24 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 A8))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 16 thru_hole oval (at 15.24 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 _RESET))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 TEST_1))
    (pad 15 thru_hole oval (at 15.24 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 CLOCK))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 CHAN_C))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-28_W15.24mm_Socket.wrlbak
      (offset (xyz 0 0 -4.1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 129.865 54.204 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at -0.026 2.105 180) (layer F.SilkS))
    (fp_text value "10k 1%" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2173904347826087)
      (net 9 CHAN_B))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2173904347826087)
      (net 6 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 129.865 46.965 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0.035 2.105 180) (layer F.SilkS))
    (fp_text value "15k 1%" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2173904347826087)
      (net 7 CHAN_C))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2173904347826087)
      (net 6 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 126.055 46.965 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0.035 -2.085 180) (layer F.SilkS))
    (fp_text value "15k 1%" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2173904347826087)
      (net 7 CHAN_C))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2173904347826087)
      (net 4 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 126.055 54.204 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at -0.026 -2.085 180) (layer F.SilkS))
    (fp_text value "10k 1%" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2173904347826087)
      (net 8 CHAN_A))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2173904347826087)
      (net 4 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 125.42 75.15 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J2 (at -0.762 -2.032 180) (layer F.SilkS) hide)
    (fp_text value "Audio Out" (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 RIGHT))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 LEFT))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 127.96 42.13)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value "Speech Mini Grabber" (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 CHAN_C))
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 129.865 64.745 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference C4 (at -0.015 -2.105 180) (layer F.SilkS))
    (fp_text value 2.2nF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2173904347826087)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2173904347826087)
      (net 5 RIGHT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 129.865 59.393 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference C3 (at 0.037 -2.105 180) (layer F.SilkS))
    (fp_text value 0.22uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2173904347826087)
      (net 5 RIGHT))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2173904347826087)
      (net 6 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 126.055 64.745 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference C2 (at -0.015 2.085 180) (layer F.SilkS))
    (fp_text value 2.2nF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2173904347826087)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2173904347826087)
      (net 3 LEFT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 126.055 59.393 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0.037 2.085 180) (layer F.SilkS))
    (fp_text value 0.22uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2173904347826087)
      (net 3 LEFT))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2173904347826087)
      (net 4 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text github.com/technobly/vectrex-stereo-ay (at 130.32 57.805 90) (layer B.SilkS))
  (gr_text JLCJLCJLCJLC (at 124.92 56.93 90) (layer B.SilkS))
  (gr_text BOOM (at 132.07 65.83) (layer F.SilkS))
  (gr_arc (start 137.358 41.622) (end 138.374 41.622) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 137.358 75.658) (end 137.358 76.674) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 118.562 75.658) (end 117.546 75.658) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 118.562 41.622) (end 118.562 40.606) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_text "L G R" (at 127.96 72.864) (layer F.SilkS))
  (gr_text "To\nR329" (at 131.07 42.13) (layer F.SilkS))
  (gr_text v1.0 (at 127.96 71.086) (layer F.SilkS))
  (gr_line (start 118.562 76.674) (end 137.358 76.674) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138.374 75.658) (end 138.374 41.622) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 117.546 41.622) (end 117.546 75.658) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "Vectrex\nStereo AY" (at 127.96 68.8) (layer F.SilkS))
  (gr_text "COMPONENT KEEPOUT\nBOT SIDE OF BOARD" (at 172.25 75.76) (layer F.Fab))
  (gr_text "Optional 47.1mm\nboard height" (at 108.8 96.4) (layer F.Fab))
  (dimension 47.1 (width 0.15) (layer F.Fab)
    (gr_text "47.100 mm" (at 114.6 113.25 90) (layer F.Fab))
    (feature1 (pts (xy 117.7 89.7) (xy 115.313579 89.7)))
    (feature2 (pts (xy 117.7 136.8) (xy 115.313579 136.8)))
    (crossbar (pts (xy 115.9 136.8) (xy 115.9 89.7)))
    (arrow1a (pts (xy 115.9 89.7) (xy 116.486421 90.826504)))
    (arrow1b (pts (xy 115.9 89.7) (xy 115.313579 90.826504)))
    (arrow2a (pts (xy 115.9 136.8) (xy 116.486421 135.673496)))
    (arrow2b (pts (xy 115.9 136.8) (xy 115.313579 135.673496)))
  )
  (dimension 48 (width 0.15) (layer F.Fab)
    (gr_text "48.000 mm" (at 141.7 65.600001) (layer F.Fab))
    (feature1 (pts (xy 117.7 70.7) (xy 117.7 66.31358)))
    (feature2 (pts (xy 165.7 70.7) (xy 165.7 66.31358)))
    (crossbar (pts (xy 165.7 66.900001) (xy 117.7 66.900001)))
    (arrow1a (pts (xy 117.7 66.900001) (xy 118.826504 66.31358)))
    (arrow1b (pts (xy 117.7 66.900001) (xy 118.826504 67.486422)))
    (arrow2a (pts (xy 165.7 66.900001) (xy 164.573496 66.31358)))
    (arrow2b (pts (xy 165.7 66.900001) (xy 164.573496 67.486422)))
  )
  (gr_text "COMPONENT KEEPOUT\nTOP SIDE OF BOARD" (at 141.85 75.8) (layer F.Fab))
  (gr_text "4.2mm hole\n" (at 141.9 91.825) (layer F.Fab))
  (gr_text "3.7mm hole\n" (at 123.375 113.35) (layer F.Fab))
  (gr_text "3.7mm hole\n" (at 160.8 113.5) (layer F.Fab))
  (gr_text "5.2mm hole" (at 142.125 113.45) (layer F.Fab))
  (gr_text "EDGE CHAMFERED\n45 DEGREES" (at 182.075 143.275) (layer F.Fab))
  (dimension 24 (width 0.15) (layer F.Fab)
    (gr_text "24.000 mm" (at 153.7 142.999999) (layer F.Fab))
    (feature1 (pts (xy 165.7 137.6) (xy 165.7 142.28642)))
    (feature2 (pts (xy 141.7 137.6) (xy 141.7 142.28642)))
    (crossbar (pts (xy 141.7 141.699999) (xy 165.7 141.699999)))
    (arrow1a (pts (xy 165.7 141.699999) (xy 164.573496 142.28642)))
    (arrow1b (pts (xy 165.7 141.699999) (xy 164.573496 141.113578)))
    (arrow2a (pts (xy 141.7 141.699999) (xy 142.826504 142.28642)))
    (arrow2b (pts (xy 141.7 141.699999) (xy 142.826504 141.113578)))
  )
  (dimension 24 (width 0.15) (layer F.Fab)
    (gr_text "24.000 mm" (at 129.7 143) (layer F.Fab))
    (feature1 (pts (xy 117.7 137.6) (xy 117.7 142.286421)))
    (feature2 (pts (xy 141.7 137.6) (xy 141.7 142.286421)))
    (crossbar (pts (xy 141.7 141.7) (xy 117.7 141.7)))
    (arrow1a (pts (xy 117.7 141.7) (xy 118.826504 141.113579)))
    (arrow1b (pts (xy 117.7 141.7) (xy 118.826504 142.286421)))
    (arrow2a (pts (xy 141.7 141.7) (xy 140.573496 141.113579)))
    (arrow2b (pts (xy 141.7 141.7) (xy 140.573496 142.286421)))
  )
  (dimension 19.2 (width 0.15) (layer F.Fab)
    (gr_text "19.200 mm" (at 176.5 127.2 270) (layer F.Fab))
    (feature1 (pts (xy 161.7 136.8) (xy 175.786421 136.8)))
    (feature2 (pts (xy 161.7 117.6) (xy 175.786421 117.6)))
    (crossbar (pts (xy 175.2 117.6) (xy 175.2 136.8)))
    (arrow1a (pts (xy 175.2 136.8) (xy 174.613579 135.673496)))
    (arrow1b (pts (xy 175.2 136.8) (xy 175.786421 135.673496)))
    (arrow2a (pts (xy 175.2 117.6) (xy 174.613579 118.726504)))
    (arrow2b (pts (xy 175.2 117.6) (xy 175.786421 118.726504)))
  )
  (dimension 18 (width 0.15) (layer F.Fab)
    (gr_text "18.000 mm" (at 173.5 126.6 270) (layer F.Fab))
    (feature1 (pts (xy 161.7 135.6) (xy 172.786421 135.6)))
    (feature2 (pts (xy 161.7 117.6) (xy 172.786421 117.6)))
    (crossbar (pts (xy 172.2 117.6) (xy 172.2 135.6)))
    (arrow1a (pts (xy 172.2 135.6) (xy 171.613579 134.473496)))
    (arrow1b (pts (xy 172.2 135.6) (xy 172.786421 134.473496)))
    (arrow2a (pts (xy 172.2 117.6) (xy 171.613579 118.726504)))
    (arrow2b (pts (xy 172.2 117.6) (xy 172.786421 118.726504)))
  )
  (dimension 13.6 (width 0.15) (layer F.Fab)
    (gr_text "13.600 mm" (at 170.5 124.4 270) (layer F.Fab))
    (feature1 (pts (xy 141.7 131.2) (xy 169.786421 131.2)))
    (feature2 (pts (xy 141.7 117.6) (xy 169.786421 117.6)))
    (crossbar (pts (xy 169.2 117.6) (xy 169.2 131.2)))
    (arrow1a (pts (xy 169.2 131.2) (xy 168.613579 130.073496)))
    (arrow1b (pts (xy 169.2 131.2) (xy 169.786421 130.073496)))
    (arrow2a (pts (xy 169.2 117.6) (xy 168.613579 118.726504)))
    (arrow2b (pts (xy 169.2 117.6) (xy 169.786421 118.726504)))
  )
  (dimension 66.1 (width 0.15) (layer F.Fab)
    (gr_text "66.100 mm" (at 111.3 103.75 270) (layer F.Fab))
    (feature1 (pts (xy 117 136.8) (xy 112.413579 136.8)))
    (feature2 (pts (xy 117 70.7) (xy 112.413579 70.7)))
    (crossbar (pts (xy 113 70.7) (xy 113 136.8)))
    (arrow1a (pts (xy 113 136.8) (xy 112.413579 135.673496)))
    (arrow1b (pts (xy 113 136.8) (xy 113.586421 135.673496)))
    (arrow2a (pts (xy 113 70.7) (xy 112.413579 71.826504)))
    (arrow2b (pts (xy 113 70.7) (xy 113.586421 71.826504)))
  )
  (dimension 12 (width 0.15) (layer F.Fab)
    (gr_text "12.000 mm" (at 147.7 84.700001) (layer F.Fab))
    (feature1 (pts (xy 141.7 87.6) (xy 141.7 85.41358)))
    (feature2 (pts (xy 153.7 87.6) (xy 153.7 85.41358)))
    (crossbar (pts (xy 153.7 86.000001) (xy 141.7 86.000001)))
    (arrow1a (pts (xy 141.7 86.000001) (xy 142.826504 85.41358)))
    (arrow1b (pts (xy 141.7 86.000001) (xy 142.826504 86.586422)))
    (arrow2a (pts (xy 153.7 86.000001) (xy 152.573496 85.41358)))
    (arrow2b (pts (xy 153.7 86.000001) (xy 152.573496 86.586422)))
  )
  (dimension 24 (width 0.15) (layer F.Fab)
    (gr_text "24.000 mm" (at 141.7 82.2) (layer F.Fab))
    (feature1 (pts (xy 153.7 87.6) (xy 153.7 82.913579)))
    (feature2 (pts (xy 129.7 87.6) (xy 129.7 82.913579)))
    (crossbar (pts (xy 129.7 83.5) (xy 153.7 83.5)))
    (arrow1a (pts (xy 153.7 83.5) (xy 152.573496 84.086421)))
    (arrow1b (pts (xy 153.7 83.5) (xy 152.573496 82.913579)))
    (arrow2a (pts (xy 129.7 83.5) (xy 130.826504 84.086421)))
    (arrow2b (pts (xy 129.7 83.5) (xy 130.826504 82.913579)))
  )
  (dimension 30 (width 0.15) (layer F.Fab)
    (gr_text "30.000 mm" (at 170.5 102.6 90) (layer F.Fab))
    (feature1 (pts (xy 161.7 87.6) (xy 169.786421 87.6)))
    (feature2 (pts (xy 161.7 117.6) (xy 169.786421 117.6)))
    (crossbar (pts (xy 169.2 117.6) (xy 169.2 87.6)))
    (arrow1a (pts (xy 169.2 87.6) (xy 169.786421 88.726504)))
    (arrow1b (pts (xy 169.2 87.6) (xy 168.613579 88.726504)))
    (arrow2a (pts (xy 169.2 117.6) (xy 169.786421 116.473496)))
    (arrow2b (pts (xy 169.2 117.6) (xy 168.613579 116.473496)))
  )
  (dimension 20 (width 0.15) (layer F.Fab)
    (gr_text "20.000 mm" (at 151.7 140.5) (layer F.Fab))
    (feature1 (pts (xy 161.7 117.6) (xy 161.7 139.786421)))
    (feature2 (pts (xy 141.7 117.6) (xy 141.7 139.786421)))
    (crossbar (pts (xy 141.7 139.2) (xy 161.7 139.2)))
    (arrow1a (pts (xy 161.7 139.2) (xy 160.573496 139.786421)))
    (arrow1b (pts (xy 161.7 139.2) (xy 160.573496 138.613579)))
    (arrow2a (pts (xy 141.7 139.2) (xy 142.826504 139.786421)))
    (arrow2b (pts (xy 141.7 139.2) (xy 142.826504 138.613579)))
  )
  (dimension 20 (width 0.15) (layer F.Fab)
    (gr_text "20.000 mm" (at 131.7 140.5) (layer F.Fab))
    (feature1 (pts (xy 141.7 117.6) (xy 141.7 139.786421)))
    (feature2 (pts (xy 121.7 117.6) (xy 121.7 139.786421)))
    (crossbar (pts (xy 121.7 139.2) (xy 141.7 139.2)))
    (arrow1a (pts (xy 141.7 139.2) (xy 140.573496 139.786421)))
    (arrow1b (pts (xy 141.7 139.2) (xy 140.573496 138.613579)))
    (arrow2a (pts (xy 121.7 139.2) (xy 122.826504 139.786421)))
    (arrow2b (pts (xy 121.7 139.2) (xy 122.826504 138.613579)))
  )
  (gr_line (start 137.358 40.606) (end 118.562 40.606) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.255))
    (polygon
      (pts
        (xy 138.374 76.674) (xy 117.546 76.674) (xy 117.546 40.606) (xy 138.374 40.606)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.255))
    (polygon
      (pts
        (xy 138.374 76.674) (xy 117.546 76.674) (xy 117.546 40.606) (xy 138.374 40.606)
      )
    )
  )
)
