(kicad_pcb (version 4) (host pcbnew 4.0.4+e1-6308~48~ubuntu16.04.1-stable)
  (general
    (links 14)
    (no_connects 0)
    (area 121.639267 86.8976 169.460734 109.550001)
    (thickness 1.6)
    (drawings 12)
    (tracks 57)
    (zones 0)
    (modules 6)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.3 2.3)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory pdf/))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(P2-Pad3)")
  (net 5 "Net-(P2-Pad4)")
  (net 6 "Net-(P2-Pad5)")
  (net 7 "Net-(P2-Pad1)")
  (net 8 "Net-(P2-Pad8)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(P2-Pad4)")
    (add_net "Net-(P2-Pad5)")
    (add_net "Net-(P2-Pad8)")
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L11_P2.5 (layer F.Cu) (tedit 57D2C4BC)
    (at 137.275 91.625 180)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 11mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C1 (at 1.25 -3.8 180) (layer F.SilkS))
    (fp_text value 10uF (at 1.25 3.8 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 180) (size 1.3 2.3) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 2 thru_hole oval (at 2.5 0 180) (size 1.3 2.3) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L11_P2.5 (layer F.Cu) (tedit 57961D50)
    (at 132.25 104.725 270)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 11mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C2 (at 1.25 -3.8 270) (layer F.SilkS))
    (fp_text value 100uF (at 1.25 3.8 270) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 270) (size 1.3 2.3) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.3 2.3) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x04 (layer F.Cu) (tedit 57D2C478)
    (at 151.95 98.53 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 -5.1 180) (layer F.SilkS))
    (fp_text value CONN_02X04 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 180) (size 1.8 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P2-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.8 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad1)"))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.8 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(P2-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.8 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P2-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.8 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P2-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.8 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad1)"))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.8 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.8 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P2-Pad8)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz 0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 57D2C49E)
    (at 161.98 106.74 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 2.4 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.4 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(P2-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 0)
    (at 140.5 98.5 90)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U1 (at 0 -0.762 90) (layer F.SilkS))
    (fp_text value LM1117-3.3 (at 0 0.762 90) (layer F.Fab))
    (pad 4 smd rect (at 0 -3.302 90) (size 3.6576 2.032) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0 3.302 90) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 3 smd rect (at 2.286 3.302 90) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 1 smd rect (at -2.286 3.302 90) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 0)
    (at 126.625 101.425 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 0 -5.1 180) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P2-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P2-Pad8)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text KTK (at 160.1 91.8) (layer B.Cu))
  (gr_line (start 123.825 88.125) (end 124.025 88.125) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text " ESP\nFRONT" (at 158.375 97.45) (layer F.Cu))
  (gr_text Tx (at 130.15 92.925) (layer F.Cu))
  (gr_text Rx (at 130.2 96.175) (layer F.Cu))
  (gr_line (start 123.825 109.475) (end 123.825 88.125) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.425 109.475) (end 123.825 109.475) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.425 88.125) (end 167.425 109.475) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.95 88.125) (end 167.425 88.125) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text + (at 129.725 99.85) (layer F.Cu))
  (gr_text - (at 129.625 102.375) (layer F.Cu))
  (gr_text ESP8266 (at 150.85 106.83) (layer F.Cu))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.425 88.125) (xy 167.425 109.5) (xy 123.825 109.475) (xy 123.825 88.1)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.825 88.1) (xy 123.825 109.475) (xy 167.425 109.475) (xy 167.45 88.1) (xy 123.85 88.1)
      )
    )
  )
)
