(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 41)
    (no_connects 0)
    (area 19.907999 18.202 115.739001 75.400001)
    (thickness 1.6)
    (drawings 7)
    (tracks 233)
    (zones 0)
    (modules 18)
    (nets 36)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.064 4.064)
    (pad_drill 3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory K:/YOU_TUBE/DC_Voltage_Calibrator_Part4/DC_Cal_TFT_Nano_Part4_Gerber_Files/))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(J2-Pad1)")
  (net 4 "Net-(J2-Pad2)")
  (net 5 "Net-(J3-Pad1)")
  (net 6 "Net-(J3-Pad2)")
  (net 7 "Net-(J3-Pad3)")
  (net 8 "Net-(J4-Pad1)")
  (net 9 "Net-(J4-Pad2)")
  (net 10 "Net-(J4-Pad3)")
  (net 11 "Net-(J4-Pad4)")
  (net 12 "Net-(J4-Pad5)")
  (net 13 "Net-(J4-Pad6)")
  (net 14 "Net-(J4-Pad7)")
  (net 15 "Net-(J4-Pad8)")
  (net 16 +5V)
  (net 17 "Net-(R1-Pad2)")
  (net 18 "Net-(R2-Pad1)")
  (net 19 "Net-(R2-Pad2)")
  (net 20 "Net-(R3-Pad1)")
  (net 21 "Net-(R3-Pad2)")
  (net 22 "Net-(R4-Pad1)")
  (net 23 "Net-(R4-Pad2)")
  (net 24 "Net-(R5-Pad2)")
  (net 25 "Net-(R6-Pad2)")
  (net 26 "Net-(R7-Pad1)")
  (net 27 "Net-(R7-Pad2)")
  (net 28 "Net-(R8-Pad1)")
  (net 29 "Net-(R8-Pad2)")
  (net 30 "Net-(R9-Pad1)")
  (net 31 "Net-(R9-Pad2)")
  (net 32 "Net-(R10-Pad1)")
  (net 33 "Net-(R10-Pad2)")
  (net 34 "Net-(U1-Pad13)")
  (net 35 "Net-(U1-Pad9)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 1)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J4-Pad4)")
    (add_net "Net-(J4-Pad5)")
    (add_net "Net-(J4-Pad6)")
    (add_net "Net-(J4-Pad7)")
    (add_net "Net-(J4-Pad8)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(R9-Pad1)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad9)")
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5A469D05)
    (at 72.4535 26.289 180)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference J1 (at -2.413 0.127 180) (layer F.SilkS))
    (fp_text value "+3V3 output (option)" (at 0 3 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x14_Pitch2.54mm (layer F.Cu) (tedit 5A3557EB)
    (at 103.251 61.595 180)
    (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x14 2.54mm single row")
    (fp_text reference U1 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value TFT_240x320_SPI_ILI9341 (at 3.175 16.637 270) (layer F.Fab))
    (fp_text user %R (at 0 16.51 270) (layer F.Fab))
    (pad 14 thru_hole oval (at 0 0 180) (size 2 1.7) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(R8-Pad2)"))
    (pad 13 thru_hole oval (at 0 2.54 180) (size 2 1.7) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(U1-Pad13)"))
    (pad 12 thru_hole oval (at 0 5.08 180) (size 2 1.7) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(R9-Pad2)"))
    (pad 11 thru_hole oval (at 0 7.62 180) (size 2 1.7) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(R4-Pad2)"))
    (pad 10 thru_hole oval (at 0 10.16 180) (size 2 1.7) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(R10-Pad2)"))
    (pad 9 thru_hole oval (at 0 12.7 180) (size 2 1.7) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(U1-Pad9)"))
    (pad 8 thru_hole oval (at 0 15.24 180) (size 2 1.7) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(R1-Pad2)"))
    (pad 7 thru_hole oval (at 0 17.78 180) (size 2 1.7) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(R5-Pad2)"))
    (pad 6 thru_hole oval (at 0 20.32 180) (size 2 1.7) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(R6-Pad2)"))
    (pad 5 thru_hole oval (at 0 22.86 180) (size 2 1.7) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(R7-Pad2)"))
    (pad 4 thru_hole oval (at 0 25.4 180) (size 2 1.7) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(R3-Pad2)"))
    (pad 3 thru_hole oval (at 0 27.94 180) (size 2 1.7) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(R2-Pad2)"))
    (pad 2 thru_hole oval (at 0 30.48 180) (size 2 1.7) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 33.02 180) (size 2 1.7) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 +5V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x14_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight (layer F.Cu) (tedit 5A440FDE)
    (at 34.925 65.151 180)
    (descr "JST XH series connector, B02B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference J2 (at 1.27 -4.0005 180) (layer F.SilkS))
    (fp_text value "Upgrade Option" (at 0.381 -4.064 180) (layer F.Fab))
    (fp_text user %R (at 1.25 2.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.75 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 2.5 0 180) (size 1.75 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad2)"))
    (model Connectors_JST.3dshapes/JST_XH_B02B-XH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B03B-XH-A_03x2.50mm_Straight (layer F.Cu) (tedit 5A2EB9BB)
    (at 38.608 33.401)
    (descr "JST XH series connector, B03B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference J3 (at 2.5 -3.5) (layer F.SilkS))
    (fp_text value "Upgrade Option" (at 2.5 4.5) (layer F.Fab))
    (fp_text user %R (at 2.5 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.75 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at 2.5 0) (size 1.75 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad2)"))
    (pad 3 thru_hole oval (at 5 0) (size 1.75 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad3)"))
    (model Connectors_JST.3dshapes/JST_XH_B03B-XH-A_03x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B10B-XH-A_10x2.50mm_Straight (layer F.Cu) (tedit 5A355722)
    (at 38.735 26.289)
    (descr "JST XH series connector, B10B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference J4 (at 11.25 -3.5) (layer F.SilkS))
    (fp_text value "Input from Main PCB" (at 5.7785 -3.937) (layer F.Fab))
    (fp_text user %R (at 11.25 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.75 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J4-Pad1)"))
    (pad 2 thru_hole oval (at 2.5 0) (size 1.75 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(J4-Pad2)"))
    (pad 3 thru_hole oval (at 5 0) (size 1.75 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(J4-Pad3)"))
    (pad 4 thru_hole oval (at 7.5 0) (size 1.75 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(J4-Pad4)"))
    (pad 5 thru_hole oval (at 10 0) (size 1.75 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(J4-Pad5)"))
    (pad 6 thru_hole oval (at 12.5 0) (size 1.75 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(J4-Pad6)"))
    (pad 7 thru_hole oval (at 15 0) (size 1.75 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(J4-Pad7)"))
    (pad 8 thru_hole oval (at 17.5 0) (size 1.75 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(J4-Pad8)"))
    (pad 9 thru_hole oval (at 20 0) (size 1.75 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at 22.5 0) (size 1.75 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 +5V))
    (model Connectors_JST.3dshapes/JST_XH_B10B-XH-A_10x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A355740)
    (at 107.315 28.3845 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 -2.31 270) (layer F.SilkS))
    (fp_text value 56 (at 4.6355 0.0635 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 +5V))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A469D10)
    (at 83.7565 25.8445)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at -2.3495 0.127) (layer F.SilkS))
    (fp_text value 10K (at 4.8895 0.127) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(R2-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A469D17)
    (at 83.7565 29.2735)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at -2.286 -0.254) (layer F.SilkS))
    (fp_text value 10K (at 4.8895 0.0635) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(R3-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A3557AA)
    (at 83.7565 50.7365)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at -2.667 0) (layer F.SilkS))
    (fp_text value 10K (at 5.08 0.127) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(R4-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A35579A)
    (at 83.7565 40.8305)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at -2.413 -0.0635) (layer F.SilkS))
    (fp_text value 10K (at 4.8895 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(J4-Pad7)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A44100D)
    (at 83.7565 37.5285)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at -2.4765 -0.127) (layer F.SilkS))
    (fp_text value 10K (at 4.953 -0.127) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(J4-Pad8)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A35578F)
    (at 83.7565 32.639)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at -2.286 -0.1905) (layer F.SilkS))
    (fp_text value 10K (at 4.8895 -0.127) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(R7-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A440FF6)
    (at 83.7565 60.7695)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R8 (at -2.4765 0.0635) (layer F.SilkS))
    (fp_text value 10K (at 6.096 -0.127) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(R8-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(R8-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A3557B3)
    (at 83.7565 54.0385)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R9 (at -2.6035 -0.254) (layer F.SilkS))
    (fp_text value 10K (at 5.1435 0.127) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(R9-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(R9-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A3557A4)
    (at 83.7565 47.4345)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R10 (at -2.9845 0) (layer F.SilkS))
    (fp_text value 10K (at 5.08 0.0635) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(R10-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Arduino_Socket:DIP-30_0_ELL (layer F.Cu) (tedit 0)
    (at 46.228 48.895)
    (fp_text reference U2 (at -20.18 0 90) (layer F.SilkS))
    (fp_text value arduino_nano (at 0 0) (layer F.Fab))
    (pad 30 thru_hole oval (at -17.78 -7.62) (size 1.4 2.5) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -17.78 7.62) (size 1.4 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad2)"))
    (pad 29 thru_hole oval (at -15.24 -7.62) (size 1.4 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at -15.24 7.62) (size 1.4 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad1)"))
    (pad 28 thru_hole oval (at -12.7 -7.62) (size 1.4 2.5) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -12.7 7.62) (size 1.4 2.5) (drill 0.8) (layers *.Cu *.Mask))
    (pad 27 thru_hole oval (at -10.16 -7.62) (size 1.4 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 +5V))
    (pad 4 thru_hole oval (at -10.16 7.62) (size 1.4 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 26 thru_hole oval (at -7.62 -7.62) (size 1.4 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J3-Pad1)"))
    (pad 5 thru_hole oval (at -7.62 7.62) (size 1.4 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(J4-Pad6)"))
    (pad 25 thru_hole oval (at -5.08 -7.62) (size 1.4 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad2)"))
    (pad 6 thru_hole oval (at -5.08 7.62) (size 1.4 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(R10-Pad1)"))
    (pad 24 thru_hole oval (at -2.54 -7.62) (size 1.4 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad3)"))
    (pad 7 thru_hole oval (at -2.54 7.62) (size 1.4 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(R4-Pad1)"))
    (pad 23 thru_hole oval (at 0 -7.62) (size 1.4 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(J4-Pad5)"))
    (pad 8 thru_hole oval (at 0 7.62) (size 1.4 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(R9-Pad1)"))
    (pad 22 thru_hole oval (at 2.54 -7.62) (size 1.4 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(J4-Pad4)"))
    (pad 9 thru_hole oval (at 2.54 7.62) (size 1.4 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(U1-Pad13)"))
    (pad 21 thru_hole oval (at 5.08 -7.62) (size 1.4 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(J4-Pad3)"))
    (pad 10 thru_hole oval (at 5.08 7.62) (size 1.4 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(R8-Pad1)"))
    (pad 20 thru_hole oval (at 7.62 -7.62) (size 1.4 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(J4-Pad2)"))
    (pad 11 thru_hole oval (at 7.62 7.62) (size 1.4 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(R3-Pad1)"))
    (pad 19 thru_hole oval (at 10.16 -7.62) (size 1.4 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J4-Pad1)"))
    (pad 12 thru_hole oval (at 10.16 7.62) (size 1.4 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(R7-Pad1)"))
    (pad 18 thru_hole oval (at 12.7 -7.62) (size 1.4 2.5) (drill 0.8) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 12.7 7.62) (size 1.4 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(R2-Pad1)"))
    (pad 17 thru_hole oval (at 15.24 -7.62) (size 1.4 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 14 thru_hole oval (at 15.24 7.62) (size 1.4 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(J4-Pad8)"))
    (pad 16 thru_hole oval (at 17.78 -7.62) (size 1.4 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(J4-Pad7)"))
    (pad 15 thru_hole oval (at 17.78 7.62) (size 1.4 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(U1-Pad9)"))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5A469D8B)
    (at 23.114 22.225)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference "" (at 0 -3.048) (layer F.SilkS))
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5A469D95)
    (at 22.733 67.818)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference "" (at 0 -3.048) (layer F.SilkS))
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3) (layers *.Cu *.Mask))
  )
  (gr_text "Ver 3.0" (at 76.6445 55.88) (layer B.Cu))
  (gr_text SCULLCOM (at 87.63 20.955) (layer B.Cu))
  (gr_text +3V3 (at 73.025 23.749) (layer B.Cu))
  (gr_line (start 20.2946 75.325) (end 20.2946 19.2184) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 115.664 75.325) (end 20.2946 75.325) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 115.664 19.2692) (end 115.664 75.325) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 20.2692 19.2692) (end 115.664 19.2692) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 35.687 58.2295) (xy 35.6235 58.2295) (xy 35.684332 58.223097)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 35.3695 57.4675) (xy 35.3695 53.467) (xy 31.369 53.467) (xy 39.751 44.7675) (xy 55.5625 44.7675)
        (xy 50.546 49.8475) (xy 40.132 49.8475) (xy 36.83 53.1495) (xy 36.83 58.1025) (xy 35.684332 58.223097)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 34.163 24.8285) (xy 34.163 37.5285) (xy 25.527 37.5285) (xy 25.5905 51.054) (xy 23.749 52.8955)
        (xy 23.749 64.135) (xy 33.655 74.041) (xy 92.1385 73.9775) (xy 96.774 69.342) (xy 108.458 69.342)
        (xy 114.427 63.373) (xy 114.554 30.734) (xy 108.585 24.7015) (xy 102.235 24.7015) (xy 98.933 26.8605)
        (xy 98.933 19.6215) (xy 115.316 19.6215) (xy 115.3795 75.057) (xy 20.447 75.057) (xy 20.5105 19.4945)
        (xy 40.4495 19.4945)
      )
    )
  )
)
