<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="35" y2="0" width="0" layer="20"/>
<wire x1="35" y1="0" x2="35" y2="35" width="0" layer="20"/>
<wire x1="35" y1="35" x2="0" y2="35" width="0" layer="20"/>
<wire x1="0" y1="35" x2="0" y2="0" width="0" layer="20"/>
<text>LO</text>
<text>MI</text>
<text>HI</text>
<text>HI</text>
<text>MI</text>
<text>LO</text>
<text>PAS</text>
<text>DRV</text>
<text>PAS</text>
<text>LO</text>
<text>MI</text>
<text>HI</text>
<text>LO</text>
<text>MI</text>
<text>HI</text>
<text>HEAT OUT</text>
<text>LED OUT</text>
<text>XTAL</text>
<text>PAS</text>
<text>DRV</text>
<text>+</text>
<text>-</text>
<text>H</text>
<text>ApHSC Rev. 4b</text>
<text>https://goo.gl/t2CsID</text>
<hole x="2.5" y="2.5" drill="1.5"/>
<hole x="2.5" y="32.5" drill="1.5"/>
<hole x="27.5" y="16.5" drill="1.5"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
<package name="1X06">
</package>
<package name="1X03">
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-lstb">
<description>&lt;b&gt;Pin Headers&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
MA = male&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MA03-2">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
</packages>
</library>
<library name="resistor">
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="murata-filter">
<packages>
<package name="CSTCE_V">
</package>
</packages>
</library>
<library name="Logo">
<packages>
<package name="OSHW_10X500_NOTEXT">
</package>
</packages>
</library>
<library name="Atmel_By_element14_Batch_1-00">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 27/07/2012 14:02:49</description>
<packages>
<package name="QFP80P900X900X120-32N">
</package>
</packages>
</library>
<library name="Roylib Drivers">
<description>Libraries For Drivers</description>
<packages>
<package name="SOIC16N">
<description>16-Lead Small Outline Integrated Circuit Narrow [SOIC]</description>
</package>
<package name="SOIC20W">
<description>SO 20 Pin Land Pattern (1.27mm Pin Pitch)</description>
</package>
</packages>
</library>
<library name="Roylib Regulator">
<description>&lt;b&gt;Libraries For Voltage Regulators&lt;/b&gt;</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BTN-IN" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="rcl" package="C0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="rcl" package="C0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H-OUT" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="VALUE"/>
</element>
<element name="ISP" library="con-lstb" package="MA03-2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED-OUT" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="VALUE"/>
</element>
<element name="ON" library="led" package="CHIP-LED0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PWR/H" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="resistor" package="R0603" value="15K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="resistor" package="R0603" value="15K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="resistor" package="R0603" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="resistor" package="R0603" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="resistor" package="R0603" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="resistor" package="R0603" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="XTAL" library="murata-filter" package="CSTCE_V" value="CSTCE_V"/>
<element name="U$1" library="Logo" package="OSHW_10X500_NOTEXT" value=""/>
<element name="U1" library="Atmel_By_element14_Batch_1-00" package="QFP80P900X900X120-32N" value="ATMEGA328P-AU">
<attribute name="OC_FARNELL" value="1715486"/>
<attribute name="OC_NEWARK" value="14R4631"/>
<attribute name="PACKAGE" value="TQFP-32"/>
<attribute name="MPN" value="ATMEGA328P-AU"/>
<attribute name="SUPPLIER" value="Atmel"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="Roylib Drivers" package="SOIC16N" value="TPL7407L">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="Roylib Drivers" package="SOIC20W" value="A2982">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="Roylib Regulator" package="SOT223" value="UA78M05">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="rcl" package="C0603" value="0.33uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="rcl" package="C0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L" library="led" package="CHIP-LED0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="resistor" package="R0603" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="PWR/H" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="XTAL" pad="P$2"/>
<contactref element="ON" pad="C"/>
<contactref element="ISP" pad="6"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="21"/>
<contactref element="U3" pad="8"/>
<contactref element="U4" pad="7"/>
<contactref element="U4" pad="12"/>
<contactref element="C2" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="L" pad="C"/>
</signal>
<signal name="D2">
<contactref element="U1" pad="32"/>
<contactref element="R4" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="D3">
<contactref element="U1" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="D-BTN">
<contactref element="BTN-IN" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="VIN">
<contactref element="PWR/H" pad="1"/>
<contactref element="U3" pad="9"/>
<contactref element="U4" pad="9"/>
<contactref element="U2" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="D4">
<contactref element="U1" pad="2"/>
<contactref element="U3" pad="7"/>
<contactref element="U4" pad="1"/>
</signal>
<signal name="D5">
<contactref element="U1" pad="9"/>
<contactref element="U3" pad="6"/>
<contactref element="U4" pad="2"/>
</signal>
<signal name="D10">
<contactref element="U1" pad="14"/>
<contactref element="U4" pad="8"/>
</signal>
<signal name="D7">
<contactref element="U1" pad="11"/>
<contactref element="U3" pad="3"/>
<contactref element="U4" pad="4"/>
</signal>
<signal name="D8">
<contactref element="U1" pad="12"/>
<contactref element="U3" pad="2"/>
<contactref element="U4" pad="5"/>
</signal>
<signal name="D9">
<contactref element="U1" pad="13"/>
<contactref element="U3" pad="1"/>
<contactref element="U4" pad="6"/>
</signal>
<signal name="DH-HIGH">
<contactref element="H-OUT" pad="1"/>
<contactref element="U4" pad="20"/>
</signal>
<signal name="DH-MID">
<contactref element="H-OUT" pad="2"/>
<contactref element="U4" pad="19"/>
</signal>
<signal name="DH-LOW">
<contactref element="H-OUT" pad="3"/>
<contactref element="U4" pad="18"/>
</signal>
<signal name="PH-HIGH">
<contactref element="H-OUT" pad="4"/>
<contactref element="U4" pad="17"/>
</signal>
<signal name="PH-MID">
<contactref element="H-OUT" pad="5"/>
<contactref element="U4" pad="16"/>
</signal>
<signal name="PH-LOW">
<contactref element="H-OUT" pad="6"/>
<contactref element="U4" pad="15"/>
</signal>
<signal name="DL-HIGH">
<contactref element="LED-OUT" pad="1"/>
<contactref element="U3" pad="10"/>
</signal>
<signal name="DL-MID">
<contactref element="LED-OUT" pad="2"/>
<contactref element="U3" pad="11"/>
</signal>
<signal name="DL-LOW">
<contactref element="LED-OUT" pad="3"/>
<contactref element="U3" pad="12"/>
</signal>
<signal name="PL-HIGH">
<contactref element="LED-OUT" pad="4"/>
<contactref element="U3" pad="14"/>
</signal>
<signal name="PL-MID">
<contactref element="LED-OUT" pad="5"/>
<contactref element="U3" pad="15"/>
</signal>
<signal name="PL-LOW">
<contactref element="LED-OUT" pad="6"/>
<contactref element="U3" pad="16"/>
</signal>
<signal name="D6">
<contactref element="U1" pad="10"/>
<contactref element="U3" pad="5"/>
<contactref element="U4" pad="3"/>
</signal>
<signal name="H-ON">
<contactref element="PWR/H" pad="3"/>
<contactref element="U4" pad="13"/>
</signal>
<signal name="RESET">
<contactref element="R5" pad="2"/>
<contactref element="ISP" pad="5"/>
<contactref element="U1" pad="29"/>
</signal>
<signal name="VDD">
<contactref element="R5" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="ISP" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="18"/>
<contactref element="C2" pad="1"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="AREF">
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="20"/>
</signal>
<signal name="D11">
<contactref element="ISP" pad="4"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="D12">
<contactref element="ISP" pad="1"/>
<contactref element="U1" pad="16"/>
</signal>
<signal name="D13">
<contactref element="ISP" pad="3"/>
<contactref element="U1" pad="17"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="PB6">
<contactref element="U1" pad="7"/>
<contactref element="XTAL" pad="P$1"/>
</signal>
<signal name="PB7">
<contactref element="XTAL" pad="P$3"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="N$3">
<contactref element="ON" pad="A"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="P-BTN">
<contactref element="R1" pad="1"/>
<contactref element="BTN-IN" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="L" pad="A"/>
<contactref element="R6" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
