(kicad_pcb (version 20170922) (host pcbnew no-vcs-found-6006b54~60~ubuntu17.04.1)
  (general
    (thickness 1.6)
    (drawings 62)
    (tracks 83)
    (zones 0)
    (modules 17)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.1525)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1525)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4 4)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x01000_7fffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 3)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(D1-Pad1)")
  (net 3 BAT+)
  (net 4 BAT-)
  (net 5 B2OUT+)
  (net 6 "Net-(SW1-Pad3)")
  (net 7 "Net-(BT1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1525)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net B2OUT+)
    (add_net BAT+)
    (add_net BAT-)
    (add_net "Net-(BT1-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(SW1-Pad3)")
  )
  (module SH_Batteries:Battery_Retainer_SR44_Keystone_2996 (layer F.Cu) (tedit 59D01827)
    (at 227.87758 100.33128)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.1)
    (attr smd)
    (fp_text reference BT1 (at 0.10242 -6.68128 180) (layer F.SilkS))
    (fp_text value Battery_Cell (at 0 -5.81128) (layer F.SilkS))
    (pad 1 smd rect (at -7.3 0) (size 3.18 3.18) (layers F.Cu F.Paste F.Mask)
      (net 3 BAT+))
    (pad 1 smd rect (at 7.3 0) (size 3.18 3.18) (layers F.Cu F.Paste F.Mask)
      (net 3 BAT+))
    (pad 2 connect circle (at 0 0) (size 10.5 10.5) (layers F.Cu F.Mask)
      (net 7 "Net-(BT1-Pad2)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer B.Cu) (tedit 59650532)
    (at 235.96 104.83)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 2.33) (layer B.SilkS))
    (fp_text value Pin_Header_Straight_1x01_Pitch2.54mm (at 0 -2.33) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer B.Cu) (tedit 59650532)
    (at 219.7 104.84)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 2.33) (layer B.SilkS))
    (fp_text value Pin_Header_Straight_1x01_Pitch2.54mm (at 0 -2.33) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer B.Cu) (tedit 59650532)
    (at 219.7 86.58)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 2.33) (layer B.SilkS))
    (fp_text value Pin_Header_Straight_1x01_Pitch2.54mm (at 0 -2.33) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer B.Cu) (tedit 59650532)
    (at 235.95 87.17)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 2.33) (layer B.SilkS))
    (fp_text value Pin_Header_Straight_1x01_Pitch2.54mm (at 0 -2.33) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 0)
    (at 229.32 89.405)
    (descr "Pontet Goute de soudure")
    (attr virtual)
    (fp_text reference J5 (at 1.778 0 90) (layer F.SilkS))
    (fp_text value B1OUT (at -2.7438 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.635) (size 1.27 0.9652) (layers F.Cu F.Paste F.Mask)
      (net 3 BAT+))
    (pad 2 smd rect (at 0 0.635) (size 1.27 0.9652) (layers F.Cu F.Paste F.Mask)
      (net 4 BAT-))
  )
  (module LEDs:LED_0805_HandSoldering (layer F.Cu) (tedit 595FCA25)
    (at 205.556 96.781)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D1 (at 0.144 -1.441) (layer F.SilkS))
    (fp_text value LED (at 0 1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 B2OUT+))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 194.854594 91.040406 45)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -0.031246 -1.615739 45) (layer F.SilkS))
    (fp_text value R (at 0 2.1 45) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 45) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 BAT+))
    (pad 2 smd rect (at 1.35 0 45) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 B2OUT+))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:GS2 (layer B.Cu) (tedit 586134A1)
    (at 207.01 101.34 180)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J1 (at 1.78 0 90) (layer B.SilkS))
    (fp_text value B3IN2 (at 3.08 0.01 90) (layer B.Fab))
    (pad 2 smd rect (at 0 -0.64 180) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 4 BAT-))
    (pad 1 smd rect (at 0 0.64 180) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 5 B2OUT+))
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 586134A1)
    (at 212.95 89.1758 270)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J6 (at -1.78 0) (layer F.SilkS))
    (fp_text value B2OUT2 (at -1.8 0) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 5 B2OUT+))
    (pad 2 smd rect (at 0 0.64 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 4 BAT-))
  )
  (module Connectors:GS2 (layer B.Cu) (tedit 586134A1)
    (at 187.9988 106.279189 270)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J7 (at -1.78339 0.0188 180) (layer B.SilkS))
    (fp_text value B2IN2 (at -1.8 0 180) (layer B.Fab))
    (pad 1 smd rect (at 0 0.64 270) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 3 BAT+))
    (pad 2 smd rect (at 0 -0.64 270) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 4 BAT-))
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 586134A1)
    (at 226.3513 89.416901)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J8 (at -1.8113 -0.016901 90) (layer F.SilkS))
    (fp_text value B1OUT2 (at -1.8 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.64) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 4 BAT-))
    (pad 1 smd rect (at 0 -0.64) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 BAT+))
  )
  (module LEDs:LED_0805_HandSoldering (layer F.Cu) (tedit 595FCA25)
    (at 205.25 105.91 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D2 (at -0.15 1.49 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 BAT-))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:GS2 (layer B.Cu) (tedit 586134A1)
    (at 212.950001 89.1733 90)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J3 (at 1.78 0) (layer B.SilkS))
    (fp_text value B2OUT (at -1.8 0) (layer B.Fab))
    (pad 1 smd rect (at 0 0.64 90) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 5 B2OUT+))
    (pad 2 smd rect (at 0 -0.64 90) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 4 BAT-))
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 586134A1)
    (at 187.9988 106.279189 90)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J4 (at 1.78 0 180) (layer F.SilkS))
    (fp_text value B2IN (at -1.8 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.64 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 4 BAT-))
    (pad 1 smd rect (at 0 -0.64 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 BAT+))
  )
  (module Connectors:GS2 (layer B.Cu) (tedit 586134A1)
    (at 204 101.359786 180)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J9 (at -1.75 0 90) (layer B.SilkS))
    (fp_text value B3IN (at -3.11 0 90) (layer B.Fab))
    (pad 1 smd rect (at 0 0.64 180) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 5 B2OUT+))
    (pad 2 smd rect (at 0 -0.64 180) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 4 BAT-))
  )
  (module Buttons_Switches_SMD:JS202011SCQN (layer B.Cu) (tedit 59D026A2)
    (at 233.09 97.4 90)
    (fp_text reference SW1 (at 0 -5.461 90) (layer B.SilkS))
    (fp_text value SW_SPDT (at 0 5.5 90) (layer B.Fab))
    (fp_text user C&K (at 3.25 0 90) (layer B.SilkS))
    (pad 1 smd rect (at -2.5 -3 90) (size 1.2 3) (layers B.Cu B.Paste B.Mask)
      (net 4 BAT-))
    (pad 2 smd rect (at 0 -3 90) (size 1.2 3) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(BT1-Pad2)"))
    (pad 3 smd rect (at 2.5 -3 90) (size 1.2 3) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(SW1-Pad3)"))
    (pad 4 smd rect (at -2.5 3 90) (size 1.2 3) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at 0 3 90) (size 1.2 3) (layers B.Cu B.Paste B.Mask))
    (pad 6 smd rect (at 2.5 3 90) (size 1.2 3) (layers B.Cu B.Paste B.Mask))
  )
  (gr_text LAMP (at 227.59 93.07) (layer B.SilkS))
  (gr_line (start 202.1761 106.9829) (end 204.02594 107.70891) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 200.6224 105.74388) (end 202.1761 106.9829) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 199.5029 104.10195) (end 200.6224 105.74388) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 198.9172 102.20301) (end 199.5029 104.10195) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 198.9172 100.21579) (end 198.9172 102.20301) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 199.5029 98.3169) (end 198.9172 100.21579) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 190.9265 102.55117) (end 192.2185 98.57468) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 190.4894 106.7094) (end 190.9265 102.55117) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 209.66599 95.9972) (end 207.94499 95.0036) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 211.01766 97.4539) (end 209.66599 95.9972) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 211.87988 99.24437) (end 211.01766 97.4539) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 212.17606 101.2094) (end 211.87988 99.24437) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 211.87988 103.17443) (end 212.17606 101.2094) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 210.4894 91.51) (end 215.29 91.51) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 210.4894 86.819) (end 210.4894 91.51) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 208.39884 86.819) (end 210.4894 86.819) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 204.30907 87.6883) (end 208.39884 86.819) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 200.48942 89.3889) (end 204.30907 87.6883) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 197.1068 91.8465) (end 200.48942 89.3889) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 187.8329 96.6221) (end 186.2308 101.55307) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 190.4253 92.132) (end 187.8329 96.6221) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 193.8946 88.279) (end 190.4253 92.132) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 198.0891 85.2315) (end 193.8946 88.279) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 202.8256 83.1226) (end 198.0891 85.2315) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 192.2185 98.57468) (end 194.3091 94.9537) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 194.3091 94.9537) (end 197.1068 91.8465) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 237.83 84.7094) (end 217.82999 84.7094) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 190.4894 108.70964) (end 190.4894 106.7094) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.6888 108.70964) (end 190.4894 108.70964) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.6888 106.7094) (end 185.6888 108.70964) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 186.2308 101.55307) (end 185.6888 106.7094) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 200.6224 96.6749) (end 199.5029 98.3169) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 202.1761 95.4359) (end 200.6224 96.6749) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 204.02594 94.7099) (end 202.1761 95.4359) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 206.0076 94.5614) (end 204.02594 94.7099) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 207.94499 95.0036) (end 206.0076 94.5614) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 211.01766 104.96486) (end 211.87988 103.17443) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 209.66599 106.4216) (end 211.01766 104.96486) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 207.94499 107.41521) (end 209.66599 106.4216) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 228.7571 91.90752) (end 226.9029 91.90752) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 228.7571 86.85292) (end 228.7571 91.90752) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 226.9029 86.85292) (end 228.7571 86.85292) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 226.9029 91.90752) (end 226.9029 86.85292) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 237.83 106.7094) (end 237.83 84.7094) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 217.82999 106.7094) (end 237.83 106.7094) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 217.82999 84.7094) (end 217.82999 106.7094) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 206.43649 103.7367) (end 204.58231 103.7367) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 206.43649 98.6821) (end 206.43649 103.7367) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 204.58231 98.6821) (end 206.43649 98.6821) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 204.58231 103.7367) (end 204.58231 98.6821) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 206.0076 107.85741) (end 207.94499 107.41521) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 204.02594 107.70891) (end 206.0076 107.85741) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 207.89704 82.0447) (end 202.8256 83.1226) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 210.4894 82.0447) (end 207.89704 82.0447) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 210.4894 81.9088) (end 210.4894 82.0447) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 215.29 81.9088) (end 210.4894 81.9088) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 215.29 91.51) (end 215.29 81.9088) (layer Edge.Cuts) (width 0.1))
  (dimension 21.88074 (width 0.3) (layer Margin)
    (gr_text "21.881 mm" (at 257.146975 108.540989 89.52865596) (layer Margin))
    (feature1 (pts (xy 242.53 97.48) (xy 258.58693 97.612095)))
    (feature2 (pts (xy 242.35 119.36) (xy 258.40693 119.492095)))
    (crossbar (pts (xy 255.707021 119.469884) (xy 255.887021 97.589884)))
    (arrow1a (pts (xy 255.887021 97.589884) (xy 256.464155 98.721174)))
    (arrow1b (pts (xy 255.887021 97.589884) (xy 255.291353 98.711526)))
    (arrow2a (pts (xy 255.707021 119.469884) (xy 256.302689 118.348242)))
    (arrow2b (pts (xy 255.707021 119.469884) (xy 255.129887 118.338594)))
  )
  (dimension 19.030095 (width 0.3) (layer Eco2.User)
    (gr_text "19.030 mm" (at 231.809548 128.46021 0.180648207) (layer Eco2.User))
    (feature1 (pts (xy 241.3004 120.771) (xy 241.328805 129.780204)))
    (feature2 (pts (xy 222.2704 120.831) (xy 222.298805 129.840204)))
    (crossbar (pts (xy 222.290292 127.140217) (xy 241.320292 127.080217)))
    (arrow1a (pts (xy 241.320292 127.080217) (xy 240.195643 127.670187)))
    (arrow1b (pts (xy 241.320292 127.080217) (xy 240.191945 126.497351)))
    (arrow2a (pts (xy 222.290292 127.140217) (xy 223.418639 127.723083)))
    (arrow2b (pts (xy 222.290292 127.140217) (xy 223.414941 126.550247)))
  )
  (dimension 24.3 (width 0.3) (layer Eco1.User)
    (gr_text "24.300 mm" (at 198.45 68.5442) (layer Eco1.User))
    (feature1 (pts (xy 210.6 82.8542) (xy 210.6 67.1942)))
    (feature2 (pts (xy 186.3 82.8542) (xy 186.3 67.1942)))
    (crossbar (pts (xy 186.3 69.8942) (xy 210.6 69.8942)))
    (arrow1a (pts (xy 210.6 69.8942) (xy 209.473496 70.480621)))
    (arrow1b (pts (xy 210.6 69.8942) (xy 209.473496 69.307779)))
    (arrow2a (pts (xy 186.3 69.8942) (xy 187.426504 70.480621)))
    (arrow2b (pts (xy 186.3 69.8942) (xy 187.426504 69.307779)))
  )
  (dimension 24.3 (width 0.3) (layer Eco1.User)
    (gr_text "24.300 mm" (at 171.99 95.0042 90) (layer Eco1.User))
    (feature1 (pts (xy 186.3 82.8542) (xy 170.64 82.8542)))
    (feature2 (pts (xy 186.3 107.1542) (xy 170.64 107.1542)))
    (crossbar (pts (xy 173.34 107.1542) (xy 173.34 82.8542)))
    (arrow1a (pts (xy 173.34 82.8542) (xy 173.926421 83.980704)))
    (arrow1b (pts (xy 173.34 82.8542) (xy 172.753579 83.980704)))
    (arrow2a (pts (xy 173.34 107.1542) (xy 173.926421 106.027696)))
    (arrow2b (pts (xy 173.34 107.1542) (xy 172.753579 106.027696)))
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 242.4902 79.9808) (xy 242.4902 130.0442) (xy 185.125 130.3792) (xy 185.125 80.1542) (xy 223.775 80.1542)
      )
    )
  )
)
