(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 29)
    (no_connects 0)
    (area 89.459999 76.759999 120.725001 104.850001)
    (thickness 1.6)
    (drawings 26)
    (tracks 88)
    (zones 0)
    (modules 7)
    (nets 17)
  )
  (page USLetter)
  (title_block
    (title "microSD Breakout Board")
    (date 2018-03-05)
    (rev A)
    (company LogicProbe.org)
    (comment 1 "Derek Konigsberg")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.635)
    (user_trace_width 1.27)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 1.27 0.7112)
    (user_via 2.54 1.3208)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J1-Pad3)")
  (net 5 "Net-(J1-Pad4)")
  (net 6 "Net-(J1-Pad5)")
  (net 7 "Net-(J1-Pad6)")
  (net 8 "Net-(J1-Pad7)")
  (net 9 "Net-(J1-Pad8)")
  (net 10 "Net-(J1-Pad9)")
  (net 11 "Net-(J2-Pad8)")
  (net 12 "Net-(J2-Pad1)")
  (net 13 "Net-(J2-Pad2)")
  (net 14 "Net-(J2-Pad3)")
  (net 15 "Net-(J2-Pad5)")
  (net 16 "Net-(J2-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net +3V3)
    (add_net GND)
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5A9E1228)
    (at 99.949 80.325 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 -1.85 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.85 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.955 0 270) (size 0.97 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.955 0 270) (size 0.97 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical (layer F.Cu) (tedit 5A9E124A)
    (at 92.075 79.375)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference J1 (at 2.921 -1.651) (layer F.SilkS))
    (fp_text value Header (at 0 25.19) (layer F.Fab))
    (fp_text user %R (at 0 11.43 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Card:microSD_HC_Hirose_DM3AT-SF-PEJM5 (layer F.Cu) (tedit 5A9E1FAE)
    (at 111.125 90.805 90)
    (descr "Micro SD, SMD, right-angle, push-pull (https://www.hirose.com/product/en/download_file/key_name/DM3AT-SF-PEJM5/category/Drawing%20(2D)/doc_file_id/44099/?file_category_id=6&item_id=06090031000&is_series=)")
    (tags "Micro SD")
    (attr smd)
    (fp_text reference J2 (at -8.001 -6.858 180) (layer F.SilkS))
    (fp_text value "microSD Socket" (at -0.075 9.575 90) (layer F.Fab))
    (fp_text user KEEPOUT (at -1.075 -1.925 90) (layer Cmts.User))
    (fp_text user %R (at -0.075 0.375 90) (layer F.Fab))
    (fp_text user KEEPOUT (at 4.2 7.65 90) (layer Cmts.User))
    (fp_text user KEEPOUT (at -6.85 -3.25 180) (layer Cmts.User))
    (fp_text user KEEPOUT (at -5.775 2.375 180) (layer Cmts.User))
    (pad 9 smd rect (at -5.875 -7.725 90) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad9)"))
    (pad 8 smd rect (at -4.925 -7.725 90) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J2-Pad8)"))
    (pad 1 smd rect (at 2.775 -7.725 90) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J2-Pad1)"))
    (pad 2 smd rect (at 1.675 -7.725 90) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J2-Pad2)"))
    (pad 3 smd rect (at 0.575 -7.725 90) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J2-Pad3)"))
    (pad 4 smd rect (at -0.525 -7.725 90) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 5 smd rect (at -1.625 -7.725 90) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J2-Pad5)"))
    (pad 6 smd rect (at -2.725 -7.725 90) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -3.825 -7.725 90) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J2-Pad7)"))
    (pad 11 smd rect (at 4.325 -7.725 90) (size 1 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at -6.825 -3.425 90) (size 1 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at -6.825 2.775 90) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at -6.825 6.925 90) (size 1 2.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 6.675 7.375 90) (size 1.3 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_Card.3dshapes/microSD_HC_Hirose_DM3AT-SF-PEJM5.wrl
      (at (xyz 0.1092519685 0.280511811 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5A9E121F)
    (at 98.933 98.806 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.85 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.85 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.955 0 270) (size 0.97 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 2 smd rect (at 0.955 0 270) (size 0.97 1.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad9)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib_fp:SLP4016P16_1.6x4mm_P0.5mm (layer F.Cu) (tedit 5A9E1F19)
    (at 99.06 90.805 180)
    (descr "SLP4016P16 16-pin package")
    (tags "UFDFN 0.5")
    (attr smd)
    (fp_text reference U1 (at 0 -3.556 180) (layer F.SilkS))
    (fp_text value EClamp2410P (at 0 3.2 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad "" smd rect (at 0 1.35 180) (size 0.35 0.35) (layers F.Paste))
    (pad "" smd rect (at 0 -1.35 180) (size 0.35 0.35) (layers F.Paste))
    (pad "" smd rect (at 0 0.9 180) (size 0.35 0.35) (layers F.Paste))
    (pad "" smd rect (at 0 0.45 180) (size 0.35 0.35) (layers F.Paste))
    (pad "" smd rect (at 0 -0.9 180) (size 0.35 0.35) (layers F.Paste))
    (pad "" smd rect (at 0 -0.45 180) (size 0.35 0.35) (layers F.Paste))
    (pad 1 smd rect (at -0.76 -1.75 180) (size 0.63 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J2-Pad8)"))
    (pad 2 smd rect (at -0.76 -1.25 180) (size 0.63 0.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J2-Pad7)"))
    (pad 3 smd rect (at -0.76 -0.75 180) (size 0.63 0.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J2-Pad5)"))
    (pad 4 smd rect (at -0.76 -0.25 180) (size 0.63 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 5 smd rect (at -0.76 0.25 180) (size 0.63 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 6 smd rect (at -0.76 0.75 180) (size 0.63 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J2-Pad3)"))
    (pad 7 smd rect (at -0.76 1.25 180) (size 0.63 0.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J2-Pad2)"))
    (pad 8 smd rect (at -0.76 1.75 180) (size 0.63 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J2-Pad1)"))
    (pad 9 smd rect (at 0.76 1.75 180) (size 0.63 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 10 smd rect (at 0.76 1.25 180) (size 0.63 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad4)"))
    (pad 11 smd rect (at 0.76 0.75 180) (size 0.63 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad5)"))
    (pad 12 smd rect (at 0.76 0.25 180) (size 0.63 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 13 smd rect (at 0.76 -0.25 180) (size 0.63 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 14 smd rect (at 0.76 -0.75 180) (size 0.63 0.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad6)"))
    (pad 15 smd rect (at 0.76 -1.25 180) (size 0.63 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad7)"))
    (pad 16 smd rect (at 0.76 -1.75 180) (size 0.63 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad8)"))
    (pad 17 smd rect (at 0 0 180) (size 0.45 3.3) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad "" smd rect (at 0 0 180) (size 0.35 0.35) (layers F.Paste))
  )
  (module lib_fp:LogicProbe (layer F.Cu) (tedit 0)
    (at 111.125 80.01)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module lib_fp:OSHW-logo_10mm (layer B.Cu) (tedit 5A9E1E68)
    (at 105.41 90.17 180)
    (fp_text reference G*** (at 0 -5.30352 180) (layer B.SilkS) hide)
    (fp_text value OSHW-logo_10mm (at 0 5.30352 180) (layer B.SilkS) hide)
  )
  (dimension 27.94 (width 0.3) (layer Cmts.User)
    (gr_text "1.1000 in" (at 85.772001 90.805 270) (layer Cmts.User))
    (feature1 (pts (xy 89.535 104.775) (xy 84.422001 104.775)))
    (feature2 (pts (xy 89.535 76.835) (xy 84.422001 76.835)))
    (crossbar (pts (xy 87.122001 76.835) (xy 87.122001 104.775)))
    (arrow1a (pts (xy 87.122001 104.775) (xy 86.53558 103.648496)))
    (arrow1b (pts (xy 87.122001 104.775) (xy 87.708422 103.648496)))
    (arrow2a (pts (xy 87.122001 76.835) (xy 86.53558 77.961504)))
    (arrow2b (pts (xy 87.122001 76.835) (xy 87.708422 77.961504)))
  )
  (dimension 31.115 (width 0.3) (layer Cmts.User)
    (gr_text "1.2250 in" (at 105.0925 73.199) (layer Cmts.User))
    (feature1 (pts (xy 120.65 76.835) (xy 120.65 71.849)))
    (feature2 (pts (xy 89.535 76.835) (xy 89.535 71.849)))
    (crossbar (pts (xy 89.535 74.549) (xy 120.65 74.549)))
    (arrow1a (pts (xy 120.65 74.549) (xy 119.523496 75.135421)))
    (arrow1b (pts (xy 120.65 74.549) (xy 119.523496 73.962579)))
    (arrow2a (pts (xy 89.535 74.549) (xy 90.661504 75.135421)))
    (arrow2b (pts (xy 89.535 74.549) (xy 90.661504 73.962579)))
  )
  (gr_text "Rev: A\n2018-03-05" (at 117.475 100.33) (layer B.SilkS))
  (gr_text "microSD Breakout Board" (at 109.22 102.235) (layer F.SilkS))
  (gr_arc (start 90.805 103.505) (end 90.805 104.775) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 119.38 103.505) (end 120.65 103.505) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 119.38 78.105) (end 119.38 76.835) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 90.805 78.105) (end 89.535 78.105) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.38 76.835) (end 90.805 76.835) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 120.65 103.505) (end 120.65 78.105) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 90.805 104.775) (end 119.38 104.775) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 89.535 78.105) (end 89.535 103.505) (layer Edge.Cuts) (width 0.15))
  (gr_text GND (at 93.98 102.235) (layer F.SilkS))
  (gr_text ~CD (at 93.98 99.695) (layer F.SilkS))
  (gr_text D1 (at 93.98 97.155) (layer F.SilkS))
  (gr_text D0 (at 93.98 94.615) (layer F.SilkS))
  (gr_text CLK (at 93.98 92.075) (layer F.SilkS))
  (gr_text CMD (at 93.98 89.535) (layer F.SilkS))
  (gr_text D3 (at 93.98 86.995) (layer F.SilkS))
  (gr_text D2 (at 93.98 84.455) (layer F.SilkS))
  (gr_text Vpu (at 93.98 81.915) (layer F.SilkS))
  (gr_text 3.3V (at 93.98 79.375) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.535 76.835) (xy 120.65 76.835) (xy 120.65 104.775) (xy 89.535 104.775)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.535 76.835) (xy 120.65 76.835) (xy 120.65 104.775) (xy 89.535 104.775)
      )
    )
  )
)
