<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="101.6" x2="40.64" y2="101.6" width="0" layer="20"/>
<wire x1="40.64" y1="101.6" x2="40.64" y2="0" width="0" layer="20"/>
<wire x1="40.64" y1="0" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="0" y2="101.6" width="0" layer="20"/>
<hole x="30.48" y="71.12" drill="3.175"/>
<hole x="31.75" y="7.62" drill="3.175"/>
<text>(solder on 
bottom)</text>
<text>J1</text>
<text>Subassembly:
  * 2x placements of J1 in BOM
    (two 2x3 male headers)</text>
</plain>
<libraries>
<library name="pi-frontpanel">
<packages>
<package name="3590P">
<description>Bourns 3590P precision POT</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3X04">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="P_GAIN" library="pi-frontpanel" package="3590P" value="BOURNS-3590P">
<attribute name="NAME"/>
<attribute name="PARTNO" value="3590P-1-103L-ND"/>
</element>
<element name="I_GAIN" library="pi-frontpanel" package="3590P" value="BOURNS-3590P">
<attribute name="NAME"/>
<attribute name="PARTNO" value="3590P-1-103L-ND"/>
</element>
<element name="OUTPUT_OFFSET" library="pi-frontpanel" package="3590P" value="BOURNS-3590P">
<attribute name="NAME"/>
<attribute name="PARTNO" value="3590P-1-103L-ND"/>
</element>
<element name="SWEEP_AMP" library="pi-frontpanel" package="3590P" value="BOURNS-3590P">
<attribute name="NAME"/>
<attribute name="PARTNO" value="3590P-1-103L-ND"/>
</element>
<element name="J1" library="pinhead" package="3X04" value="PINHD-3X4">
<attribute name="NAME"/>
<attribute name="PARTNO" value="952-2121-ND (2x)"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="P_GAIN" pad="1"/>
<contactref element="J1" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="I_GAIN" pad="1"/>
<contactref element="J1" pad="P$4"/>
</signal>
<signal name="N$3">
<contactref element="OUTPUT_OFFSET" pad="1"/>
<contactref element="J1" pad="P$7"/>
</signal>
<signal name="N$4">
<contactref element="J1" pad="P$10"/>
<contactref element="SWEEP_AMP" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="P_GAIN" pad="2"/>
<contactref element="J1" pad="P$2"/>
</signal>
<signal name="N$6">
<contactref element="I_GAIN" pad="2"/>
<contactref element="J1" pad="P$5"/>
</signal>
<signal name="N$7">
<contactref element="OUTPUT_OFFSET" pad="2"/>
<contactref element="J1" pad="P$8"/>
</signal>
<signal name="N$8">
<contactref element="J1" pad="P$11"/>
<contactref element="SWEEP_AMP" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="P_GAIN" pad="3"/>
<contactref element="J1" pad="P$3"/>
</signal>
<signal name="N$10">
<contactref element="I_GAIN" pad="3"/>
<contactref element="J1" pad="P$6"/>
</signal>
<signal name="N$11">
<contactref element="OUTPUT_OFFSET" pad="3"/>
<contactref element="J1" pad="P$9"/>
</signal>
<signal name="N$12">
<contactref element="J1" pad="P$12"/>
<contactref element="SWEEP_AMP" pad="3"/>
</signal>
<signal name="N$13">
</signal>
<signal name="N$14">
</signal>
</signals>
</board>
</drawing>
</eagle>
