(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 12)
    (tracks 58)
    (zones 0)
    (modules 3)
    (nets 17)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad8)")
  (net 2 "Net-(J1-Pad7)")
  (net 3 "Net-(J1-Pad6)")
  (net 4 "Net-(J1-Pad5)")
  (net 5 "Net-(J1-Pad4)")
  (net 6 "Net-(J1-Pad3)")
  (net 7 "Net-(J1-Pad2)")
  (net 8 "Net-(J1-Pad1)")
  (net 9 "Net-(J1-Pad9)")
  (net 10 "Net-(J1-Pad10)")
  (net 11 "Net-(J1-Pad11)")
  (net 12 "Net-(J1-Pad12)")
  (net 13 "Net-(J1-Pad13)")
  (net 14 "Net-(J1-Pad14)")
  (net 15 "Net-(J1-Pad15)")
  (net 16 "Net-(J1-Pad16)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
  )
  (module "Coil Library:coil_design_6mil_nonneg" (layer F.Cu) (tedit 5D83B7DF)
    (at 151.12746 92.70492)
    (fp_text reference J2 (at 0 0) (layer F.Cu) hide)
    (fp_text value Conn_01x08_Female (at 0.75 0) (layer F.Cu) hide)
    (pad 8 thru_hole circle (at -8.3058 5.1562) (size 0.762 0.762) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad8)"))
    (pad 7 thru_hole circle (at -8.3058 4.0132) (size 0.762 0.762) (drill 0.381) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad7)"))
    (pad 6 thru_hole circle (at -8.3058 2.8702) (size 0.762 0.762) (drill 0.381) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad 5 thru_hole circle (at -8.3312 1.7272) (size 0.762 0.762) (drill 0.381) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad5)"))
    (pad 4 thru_hole circle (at -8.3312 -1.7272) (size 0.762 0.762) (drill 0.381) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad4)"))
    (pad 3 thru_hole circle (at -8.3312 -2.8702) (size 0.762 0.762) (drill 0.381) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad3)"))
    (pad 2 thru_hole circle (at -8.3312 -4.0132) (size 0.762 0.762) (drill 0.381) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad2)"))
    (pad 1 thru_hole circle (at -8.3058 -5.1562) (size 0.762 0.762) (drill 0.381) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad1)"))
  )
  (module "Coil Library:coil_design_6mil_nonneg_2nd" (layer F.Cu) (tedit 5D83B9A5)
    (at 151.12746 92.70492)
    (fp_text reference J3 (at 0 0) (layer B.Cu) hide)
    (fp_text value Conn_01x08_Female (at 0.75 0) (layer B.Cu) hide)
    (pad 8 thru_hole circle (at -8.3312 9.7282) (size 0.762 0.762) (drill 0.381) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad16)"))
    (pad 7 thru_hole circle (at -8.3312 8.5852) (size 0.762 0.762) (drill 0.381) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad15)"))
    (pad 6 thru_hole circle (at -8.3058 7.4422) (size 0.762 0.762) (drill 0.381) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad14)"))
    (pad 5 thru_hole circle (at -8.3058 6.2992) (size 0.762 0.762) (drill 0.381) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad13)"))
    (pad 4 thru_hole circle (at -8.3312 -6.2992) (size 0.762 0.762) (drill 0.381) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad12)"))
    (pad 3 thru_hole circle (at -8.3312 -7.4422) (size 0.762 0.762) (drill 0.381) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad11)"))
    (pad 2 thru_hole circle (at -8.3312 -8.5852) (size 0.762 0.762) (drill 0.381) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad10)"))
    (pad 1 thru_hole circle (at -8.3058 -9.7282) (size 0.762 0.762) (drill 0.381) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad9)"))
  )
  (module "Coil Library:flex_port_16_3_5" (layer F.Cu) (tedit 5D83C92E)
    (at 127.75 85 270)
    (fp_text reference J1 (at -0.0508 5.5372 90) (layer F.SilkS))
    (fp_text value Conn_01x16_Male (at 0 -3.8862 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 270) (size 0.7 4) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 0.7 4) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad2)"))
    (pad 3 smd rect (at 2 0 270) (size 0.7 4) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad3)"))
    (pad 4 smd rect (at 3 0 270) (size 0.7 4) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad4)"))
    (pad 5 smd rect (at 4 0 270) (size 0.7 4) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad5)"))
    (pad 6 smd rect (at 5 0 270) (size 0.7 4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad 7 smd rect (at 6 0 270) (size 0.7 4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad7)"))
    (pad 8 smd rect (at 7 0 270) (size 0.7 4) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad8)"))
    (pad 9 smd rect (at 8 0 270) (size 0.7 4) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad9)"))
    (pad 10 smd rect (at 9 0 270) (size 0.7 4) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad10)"))
    (pad 11 smd rect (at 10 0 270) (size 0.7 4) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J1-Pad11)"))
    (pad 12 smd rect (at 11 0 270) (size 0.7 4) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-Pad12)"))
    (pad 13 smd rect (at 12 0 270) (size 0.7 4) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J1-Pad13)"))
    (pad 14 smd rect (at 13 0 270) (size 0.7 4) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J1-Pad14)"))
    (pad 15 smd rect (at 14 0 270) (size 0.7 4) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J1-Pad15)"))
    (pad 16 smd rect (at 15 0 270) (size 0.7 4) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J1-Pad16)"))
  )
  (gr_line (start 138.25 101) (end 138.43 100.965) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 136 101) (end 138.25 101) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 126 101) (end 136 101) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125.73 73.66) (end 176.53 73.66) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125.73 111.76) (end 125.73 73.66) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 176.53 111.76) (end 125.73 111.76) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 176.53 73.66) (end 176.53 111.76) (layer Edge.Cuts) (width 0.05))
)
