(kicad_pcb (version 20171130) (host pcbnew "(5.1.9)-1")
  (general
    (thickness 1.6)
    (drawings 6)
    (tracks 110)
    (zones 0)
    (modules 3)
    (nets 5)
  )
  (page A4)
  (title_block
    (title "Hive Scale w/GPS")
    (date 2018-09-14)
    (rev 1)
    (comment 1 "Dave Selfors")
  )
  (layers
    (0 F.Cu mixed)
    (31 B.Cu power)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.254)
    (user_trace_width 0.34036)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (user_trace_width 1.016)
    (user_trace_width 1.27)
    (user_trace_width 1.524)
    (user_trace_width 1.778)
    (user_trace_width 2.032)
    (trace_clearance 0.1524)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.254)
    (via_min_drill 0.254)
    (user_via 0.349758 0.254)
    (user_via 0.508 0.254)
    (user_via 1 0.6)
    (uvia_size 0.7)
    (uvia_drill 0.4)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (edge_width 0.254)
    (segment_width 0.254)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.299999 4.299999)
    (pad_drill 4.299999)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 51.054 120.015)
    (grid_origin 51.054 120.015)
    (visible_elements 7FFDFE7F)
    (pcbplotparams
      (layerselection 0x010fc_7ffffffe)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerbers/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J1-Pad1)")
  (net 3 "Net-(J2-Pad1)")
  (net 4 "Net-(J2-PadS1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.7)
    (uvia_drill 0.4)
    (diff_pair_width 0.2032)
    (diff_pair_gap 0.25)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-PadS1)")
  )
  (module SamacSys_Parts:MABACT0039 (layer F.Cu) (tedit 0)
    (at 78.178 102.87 180)
    (descr MABACT0039-1)
    (tags Transformer)
    (attr smd)
    (fp_text reference T1 (at 0.618 0) (layer F.SilkS))
    (fp_text value MABACT0039 (at 0.618 0) (layer F.SilkS) hide)
    (fp_text user %R (at 0.618 0) (layer F.Fab))
    (pad 5 smd rect (at -2.105 -1.5 270) (size 0.91 1.92) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 4 smd rect (at -2.105 1.5 270) (size 0.91 1.92) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 2.105 1.5 270) (size 0.91 1.92) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J2-PadS1)"))
    (pad 2 smd rect (at 2.105 0 270) (size 0.91 1.92) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 2.105 -1.5 270) (size 0.91 1.92) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J2-Pad1)"))
    (model "C:\\Users\\Den PC\\Documents\\KiCad\\Libraries\\SamacSys_Parts.3dshapes\\MABACT0039.stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Libraries:LINX_CONSMA013.062 (layer F.Cu) (tedit 601583CE)
    (at 67.31 104.267 270)
    (fp_text reference J2 (at -2.978 -6.9964 90) (layer F.SilkS))
    (fp_text value CONSMA013.062 (at 2.3052 -5.9564 90) (layer F.Fab))
    (fp_text user PCB~Edge (at 5 0.97 90) (layer F.Fab))
    (pad S4 smd rect (at 2.54 -2.54 270) (size 1.52 5.08) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J2-PadS1)"))
    (pad S3 smd rect (at -2.54 -2.54 270) (size 1.52 5.08) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J2-PadS1)"))
    (pad S2 smd rect (at 2.54 -2.54 270) (size 1.52 5.08) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J2-PadS1)"))
    (pad 1 smd rect (at 0 -2.54 270) (size 1.52 5.08) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J2-Pad1)"))
    (pad S1 smd rect (at -2.54 -2.54 270) (size 1.52 5.08) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J2-PadS1)"))
  )
  (module Libraries:LINX_CONSMA013.062 (layer F.Cu) (tedit 601583CE)
    (at 87.63 104.267 90)
    (fp_text reference J1 (at -2.978 -6.9964 90) (layer F.SilkS))
    (fp_text value CONSMA013.062 (at 2.3052 -5.9564 90) (layer F.Fab))
    (fp_text user PCB~Edge (at 5 0.97 90) (layer F.Fab))
    (pad S4 smd rect (at 2.54 -2.54 90) (size 1.52 5.08) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad S3 smd rect (at -2.54 -2.54 90) (size 1.52 5.08) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad S2 smd rect (at 2.54 -2.54 90) (size 1.52 5.08) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 -2.54 90) (size 1.52 5.08) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad S1 smd rect (at -2.54 -2.54 90) (size 1.52 5.08) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (gr_text Balanced (at 73.406 104.267) (layer B.SilkS))
  (gr_text Unbalanced (at 82.169 104.14) (layer B.SilkS))
  (gr_line (start 88.011 100.457) (end 88.011 108.077) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 66.929 100.457) (end 88.011 100.457) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 66.929 108.077) (end 66.929 100.457) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.011 108.077) (end 66.929 108.077) (layer Edge.Cuts) (width 0.1))
  (zone (net 4) (net_name "Net-(J2-PadS1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.232 108.077) (xy 67.056 108.077) (xy 66.929 100.457) (xy 78.232 100.457)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.011 108.077) (xy 78.486 108.077) (xy 78.486 100.203) (xy 88.011 100.203)
      )
    )
  )
  (zone (net 4) (net_name "Net-(J2-PadS1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.232 107.95) (xy 66.929 108.077) (xy 66.929 100.457) (xy 78.232 100.457)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.011 108.077) (xy 78.486 108.077) (xy 78.486 100.457) (xy 88.011 100.457)
      )
    )
  )
)
