(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 69)
    (no_connects 0)
    (area 129.60858 77.1779 159.07162 120.773802)
    (thickness 1.6002)
    (drawings 45)
    (tracks 876)
    (zones 0)
    (modules 25)
    (nets 38)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.254)
    (zone_clearance 0.1524)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.127)
    (edge_width 0.127)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x3ffff_80000001)
      (usegerberextensions true)
      (usegerberattributes true)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory CAM/))
  )
  (net 0 "")
  (net 1 GPIO0)
  (net 2 RST)
  (net 3 GND)
  (net 4 +3V3)
  (net 5 "Net-(C9-Pad2)")
  (net 6 "Net-(U5-Pad5)")
  (net 7 ADC)
  (net 8 GPIO16)
  (net 9 GPIO14)
  (net 10 GPIO12)
  (net 11 GPIO13)
  (net 12 GPIO15)
  (net 13 GPIO2)
  (net 14 GPIO4)
  (net 15 "Net-(U5-Pad20)")
  (net 16 "Net-(U5-Pad21)")
  (net 17 "Net-(U5-Pad22)")
  (net 18 "Net-(U5-Pad23)")
  (net 19 GPIO5)
  (net 20 RXD)
  (net 21 TXD)
  (net 22 "Net-(C5-Pad1)")
  (net 23 "Net-(C6-Pad1)")
  (net 24 "Net-(R2-Pad1)")
  (net 25 "Net-(R8-Pad1)")
  (net 26 "Net-(ANT1-Pad1)")
  (net 27 "Net-(C9-Pad1)")
  (net 28 A0)
  (net 29 "Net-(D2-PadA)")
  (net 30 GPIO9)
  (net 31 GPIO10)
  (net 32 "Net-(J1-Pad1)")
  (net 33 "Net-(J2-Pad1)")
  (net 34 "Net-(J2-Pad9)")
  (net 35 "Net-(J2-Pad10)")
  (net 36 "Net-(J2-Pad11)")
  (net 37 CH_PD)
  (net_class Default "Imperial - this is the standard class"
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net CH_PD)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad9)")
  )
  (net_class 0.2mm ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class 50ohm ""
    (clearance 0.15)
    (trace_width 0.8)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(R8-Pad1)")
  )
  (net_class Minimal ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class "small clearance" ""
    (clearance 0.2)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +3V3)
    (add_net A0)
    (add_net ADC)
    (add_net GND)
    (add_net GPIO0)
    (add_net GPIO10)
    (add_net GPIO12)
    (add_net GPIO13)
    (add_net GPIO14)
    (add_net GPIO15)
    (add_net GPIO16)
    (add_net GPIO2)
    (add_net GPIO4)
    (add_net GPIO5)
    (add_net GPIO9)
    (add_net "Net-(ANT1-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(D2-PadA)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(U5-Pad20)")
    (add_net "Net-(U5-Pad21)")
    (add_net "Net-(U5-Pad22)")
    (add_net "Net-(U5-Pad23)")
    (add_net "Net-(U5-Pad5)")
    (add_net RST)
    (add_net RXD)
    (add_net TXD)
  )
  (module SparkFun-LED:SparkFun-LED-LED-0603 placed (layer F.Cu) (tedit 59F297D8)
    (at 149.606 85.852)
    (descr "LED 0603 SMT")
    (tags "LED 0603 SMT")
    (attr smd)
    (fp_text reference D2 (at -0.127 -0.9398) (layer F.SilkS))
    (fp_text value LED-TX (at 0.127 1.143) (layer F.SilkS) hide)
    (pad A smd rect (at -0.8763 0 270) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D2-PadA)"))
    (pad C smd rect (at 0.8763 0 270) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 21 TXD))
  )
  (module SparkFun-Connectors:SparkFun-Connectors-1X11_NO_SILK_KIT locked (layer F.Cu) (tedit 5958039C)
    (at 154.94 111.76 90)
    (descr "PLATED THROUGH HOLE -11 PIN NO SILK  KIT")
    (tags "PLATED THROUGH HOLE -11 PIN NO SILK  KIT")
    (attr virtual)
    (fp_text reference J2 (at -3.302 1.778 90) (layer F.SilkS) hide)
    (fp_text value RIGHT (at 0.5588 1.7272 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 33 "Net-(J2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 3 GND))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 13 GPIO2))
    (pad 4 thru_hole circle (at 7.62 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 1 GPIO0))
    (pad 5 thru_hole circle (at 10.16 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 14 GPIO4))
    (pad 6 thru_hole circle (at 12.7 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 19 GPIO5))
    (pad 7 thru_hole circle (at 15.24 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 20 RXD))
    (pad 8 thru_hole circle (at 17.78 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 21 TXD))
    (pad 9 thru_hole circle (at 20.32 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 34 "Net-(J2-Pad9)"))
    (pad 10 thru_hole circle (at 22.86 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 35 "Net-(J2-Pad10)"))
    (pad 11 thru_hole circle (at 25.4 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 36 "Net-(J2-Pad11)"))
  )
  (module nixiemisc:nixiemisc-CRYSTAL2.0X1.6 placed (layer F.Cu) (tedit 59F2A0C7)
    (at 149.6615 96.385 90)
    (attr smd)
    (fp_text reference Y1 (at -0.516 -1.4732 90) (layer F.SilkS) hide)
    (fp_text value 26MHz (at -0.0508 1.5955 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.6985 0.54356 90) (size 0.889 0.7874) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.6985 0.54356 90) (size 0.889 0.7874) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at 0.6985 -0.54356 90) (size 0.889 0.7874) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C6-Pad1)"))
    (pad 4 smd rect (at -0.6985 -0.54356 90) (size 0.889 0.7874) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
  )
  (module ANT_2450AT18B100E (layer F.Cu) (tedit 59F151EC)
    (at 153.035 78.74)
    (attr smd)
    (fp_text reference ANT1 (at 0 2.159) (layer F.SilkS))
    (fp_text value 2450AT18B100E (at -0.265 2.055) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.3 0) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(ANT1-Pad1)"))
    (pad 2 smd rect (at 1.3 0) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
  )
  (module SparkFun-Connectors:SparkFun-Connectors-1X11_NO_SILK_KIT locked (layer F.Cu) (tedit 59F298B0)
    (at 132.08 86.36 270)
    (descr "PLATED THROUGH HOLE -11 PIN NO SILK  KIT")
    (tags "PLATED THROUGH HOLE -11 PIN NO SILK  KIT")
    (attr virtual)
    (fp_text reference J1 (at 0.254 -1.7018 270) (layer F.SilkS) hide)
    (fp_text value LEFT (at 0.5588 1.7272 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 32 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 30 GPIO9))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 31 GPIO10))
    (pad 4 thru_hole circle (at 7.62 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 2 RST))
    (pad 5 thru_hole circle (at 10.16 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 28 A0))
    (pad 6 thru_hole circle (at 12.7 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 8 GPIO16))
    (pad 7 thru_hole circle (at 15.24 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 9 GPIO14))
    (pad 8 thru_hole circle (at 17.78 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 10 GPIO12))
    (pad 9 thru_hole circle (at 20.32 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 11 GPIO13))
    (pad 10 thru_hole circle (at 22.86 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 12 GPIO15))
    (pad 11 thru_hole circle (at 25.4 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 4 +3V3))
  )
  (module Socket_Strips:Socket_Strip_Straight_2x04_Pitch2.54mm (layer B.Cu) (tedit 59F29874)
    (at 139.7 115.57 270)
    (descr "Through hole straight socket strip, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x04 2.54mm double row")
    (fp_text reference J3 (at -1.27 2.33 270) (layer B.SilkS) hide)
    (fp_text value "ESP01 Header" (at -1.27 -9.95 270) (layer B.Fab))
    (fp_text user %R (at -1.27 2.33 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 TXD))
    (pad 2 thru_hole oval (at -2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 CH_PD))
    (pad 4 thru_hole oval (at -2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 GPIO2))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 RST))
    (pad 6 thru_hole oval (at -2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GPIO0))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 8 thru_hole oval (at -2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 RXD))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x04_Pitch2.54mm.wrl
      (at (xyz -0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module nixiemisc:nixiemisc-QFN-32 (layer F.Cu) (tedit 59F29800)
    (at 144.0307 96.1263 180)
    (descr "QFN 32-PIN PACKAGE W/ THERMAL PAD")
    (tags "QFN 32-PIN PACKAGE W/ THERMAL PAD")
    (attr smd)
    (fp_text reference U5 (at -3.4798 0 270) (layer F.SilkS) hide)
    (fp_text value ESP8285QFN-32 (at 3.5052 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.74752 2.49936 270) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at -1.24968 2.49936 270) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C9-Pad2)"))
    (pad 3 smd rect (at -0.7493 2.49936 270) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 4 smd rect (at -0.24892 2.49936 270) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 5 smd rect (at 0.24892 2.49936 270) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U5-Pad5)"))
    (pad 6 smd rect (at 0.7493 2.49936 270) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 7 ADC))
    (pad 7 smd rect (at 1.24968 2.49936 270) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 37 CH_PD))
    (pad 8 smd rect (at 1.74752 2.49936 270) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 8 GPIO16))
    (pad 9 smd rect (at 2.49936 1.74752) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 9 GPIO14))
    (pad 10 smd rect (at 2.49936 1.24968) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 10 GPIO12))
    (pad 11 smd rect (at 2.49936 0.7493) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 12 smd rect (at 2.49936 0.24892) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 11 GPIO13))
    (pad 13 smd rect (at 2.49936 -0.24892) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 12 GPIO15))
    (pad 14 smd rect (at 2.49936 -0.7493) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 13 GPIO2))
    (pad 15 smd rect (at 2.49936 -1.24968) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 1 GPIO0))
    (pad 16 smd rect (at 2.49936 -1.74752) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 14 GPIO4))
    (pad 17 smd rect (at 1.74752 -2.49936 90) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 18 smd rect (at 1.24968 -2.49936 90) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 30 GPIO9))
    (pad 19 smd rect (at 0.7493 -2.49936 90) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 31 GPIO10))
    (pad 20 smd rect (at 0.24892 -2.49936 90) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U5-Pad20)"))
    (pad 21 smd rect (at -0.24892 -2.49936 90) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U5-Pad21)"))
    (pad 22 smd rect (at -0.7493 -2.49936 90) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U5-Pad22)"))
    (pad 23 smd rect (at -1.24968 -2.49936 90) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U5-Pad23)"))
    (pad 24 smd rect (at -1.74752 -2.49936 90) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 19 GPIO5))
    (pad 25 smd rect (at -2.49936 -1.74752 180) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 20 RXD))
    (pad 26 smd rect (at -2.49936 -1.24968 180) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 21 TXD))
    (pad 27 smd rect (at -2.49936 -0.7493 180) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C5-Pad1)"))
    (pad 28 smd rect (at -2.49936 -0.24892 180) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C6-Pad1)"))
    (pad 29 smd rect (at -2.49936 0.24892 180) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 30 smd rect (at -2.49936 0.7493 180) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 31 smd rect (at -2.49936 1.24968 180) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R2-Pad1)"))
    (pad 32 smd rect (at -2.49936 1.74752 180) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 2 RST))
    (pad EP smd rect (at 0 0 180) (size 3.1496 3.1496) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
  )
  (module SparkFun-Resistors:SparkFun-Resistors-0603 (layer F.Cu) (tedit 59F2980E)
    (at 137.922 105.41)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference R7 (at 0 -1.0668) (layer F.SilkS))
    (fp_text value 10k (at 0 1.0668) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.84836 0) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.84836 0) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 2 RST))
  )
  (module SparkFun-Resistors:SparkFun-Resistors-0603 (layer F.Cu) (tedit 59F156AF)
    (at 137.668 99.568 180)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference R14 (at 0 -1.0668 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.0668 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.84836 0 180) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 13 GPIO2))
    (pad 2 smd rect (at 0.84836 0 180) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
  )
  (module SparkFun-Capacitors:SparkFun-Capacitors-0603 (layer F.Cu) (tedit 59F156BD)
    (at 137.287 96.139)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference C7 (at 0 -0.889) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.0668) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.84836 0) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.84836 0) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
  )
  (module SparkFun-Resistors:SparkFun-Resistors-0603 (layer F.Cu) (tedit 59F2981B)
    (at 137.922 108.712)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference R9 (at 0 -1.0668) (layer F.SilkS))
    (fp_text value 10k (at 0 1.0668) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.84836 0) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 12 GPIO15))
    (pad 2 smd rect (at 0.84836 0) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
  )
  (module SparkFun-Capacitors:SparkFun-Capacitors-0603 (layer F.Cu) (tedit 59F156CA)
    (at 149.725 98.9 180)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference C5 (at 0 -1.0668 180) (layer F.SilkS))
    (fp_text value 12pF (at 0 1.0668 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.84836 0 180) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.84836 0 180) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
  )
  (module SparkFun-Capacitors:SparkFun-Capacitors-0603 (layer F.Cu) (tedit 59F156D4)
    (at 149.64836 94.1)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference C6 (at 0 -1.0668) (layer F.SilkS))
    (fp_text value 12pF (at 0 1.0668) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.84836 0) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.84836 0) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
  )
  (module SparkFun-Resistors:SparkFun-Resistors-0603 (layer F.Cu) (tedit 59F156DC)
    (at 149.606 92)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference R2 (at 0 -1.0668) (layer F.SilkS))
    (fp_text value 12K (at 0 1.0668) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.84836 0) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 0.84836 0) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
  )
  (module SparkFun-Resistors:SparkFun-Resistors-0603 (layer F.Cu) (tedit 59F297DE)
    (at 149.606 88.646)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference R15 (at 0 -1.0668) (layer F.SilkS))
    (fp_text value 470 (at 0 1.0668) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.84836 0) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.84836 0) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D2-PadA)"))
  )
  (module SparkFun-Resistors:SparkFun-Resistors-0603 (layer F.Cu) (tedit 59F29799)
    (at 137.16 90.424)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference R11 (at 0 1.016) (layer F.SilkS))
    (fp_text value 220K (at 0 1.0668) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.84836 0) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 28 A0))
    (pad 2 smd rect (at 0.84836 0) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 7 ADC))
  )
  (module SparkFun-Resistors:SparkFun-Resistors-0603 (layer F.Cu) (tedit 59F2979F)
    (at 137.16 88.646 180)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference R12 (at 0.127 1.016 180) (layer F.SilkS))
    (fp_text value 100K (at 0 1.0668 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.84836 0 180) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 7 ADC))
    (pad 2 smd rect (at 0.84836 0 180) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
  )
  (module adafruit:adafruit-U.FL locked (layer F.Cu) (tedit 59F298A2)
    (at 134.62 81.28)
    (attr smd)
    (fp_text reference X1 (at 1.27 -3.048) (layer F.SilkS) hide)
    (fp_text value ANTENNA_U.FL (at 1.1684 2.7686) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 -1.37414) (size 2.19964 1.04902) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0 1.37414) (size 2.19964 1.04902) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at 1.524 0) (size 0.79756 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R8-Pad1)"))
  )
  (module SparkFun-Capacitors:SparkFun-Capacitors-0603 (layer F.Cu) (tedit 59F297CC)
    (at 145.288 83.566 270)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference C9 (at 0 -1.0668 270) (layer F.SilkS))
    (fp_text value 5.6pF (at 0 1.0668 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.84836 0 270) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 0.84836 0 270) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C9-Pad2)"))
  )
  (module SparkFun-Resistors:SparkFun-Resistors-0603 (layer F.Cu) (tedit 200000)
    (at 146.05 79.756 315)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference R8 (at 0 -1.0668 315) (layer F.SilkS))
    (fp_text value DNP (at 0 1.0668 315) (layer F.SilkS))
    (pad 1 smd rect (at -0.84836 0 315) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R8-Pad1)"))
    (pad 2 smd rect (at 0.84836 0 315) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C9-Pad1)"))
  )
  (module SparkFun-Resistors:SparkFun-Resistors-0603 (layer F.Cu) (tedit 59F2988F)
    (at 147.32 79.756 225)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference R10 (at 0 -1.0668 225) (layer F.SilkS))
    (fp_text value 0 (at 0 1.0668 225) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.84836 0 225) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(ANT1-Pad1)"))
    (pad 2 smd rect (at 0.84836 0 225) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C9-Pad1)"))
  )
  (module SparkFun-Capacitors:SparkFun-Capacitors-0603 (layer F.Cu) (tedit 59F156B6)
    (at 137.287 94.234)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference C8 (at 0 -1.0668) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.0668) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.84836 0) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.84836 0) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
  )
  (module SparkFun-Capacitors:SparkFun-Capacitors-0603 (layer F.Cu) (tedit 59F1599F)
    (at 137.16 116.84 270)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference C10 (at 0 -1.0668 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.0668 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.84836 0 270) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 2 RST))
    (pad 2 smd rect (at 0.84836 0 270) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
  )
  (module "nixiemisc:nixiemisc-B3U-1100P(M)" (layer F.Cu) (tedit 59F2A0D4)
    (at 133.35 116.84 90)
    (attr smd)
    (fp_text reference K1 (at 0.635 -1.651 90) (layer F.SilkS) hide)
    (fp_text value RST (at -2.667 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.74752 0 90) (size 0.59944 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 1.74752 0 90) (size 0.59944 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 2 RST))
    (pad GND smd rect (at 0 1.64846 90) (size 0.79756 1.09982) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
  )
  (module logos:mermaid_l (layer B.Cu) (tedit 0)
    (at 152.019 114.554 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (gr_text RXD (at 147.32 110.49 90) (layer F.SilkS))
  (gr_text GPIO0 (at 144.78 109.728 90) (layer F.SilkS))
  (gr_text GPIO2 (at 142.24 109.855 90) (layer F.SilkS))
  (gr_text GND (at 139.7 110.49 90) (layer F.SilkS))
  (gr_text TXD (at 139.7 117.856 90) (layer F.SilkS))
  (gr_text CHEN (at 142.24 117.475 90) (layer F.SilkS))
  (gr_text 3V3 (at 147.32 117.856 90) (layer F.SilkS))
  (gr_text RST (at 144.78 117.856 90) (layer F.SilkS))
  (gr_text nixies.us (at 150.876 116.332) (layer B.Mask))
  (gr_text "ESP8285 v0.3" (at 143.637 117.856) (layer B.SilkS))
  (gr_text NC (at 133.223 86.36) (layer F.SilkS))
  (gr_text IO9 (at 133.223 88.9) (layer F.SilkS))
  (gr_text IO10 (at 133.223 91.44) (layer F.SilkS))
  (gr_text 3V3 (at 133.223 111.76) (layer F.SilkS))
  (gr_text IO15 (at 133.35 109.22) (layer F.SilkS))
  (gr_text IO13 (at 133.223 106.68) (layer F.SilkS))
  (gr_text IO12 (at 133.223 104.14) (layer F.SilkS))
  (gr_text IO14 (at 133.35 101.6) (layer F.SilkS))
  (gr_text IO16 (at 133.223 99.06) (layer F.SilkS))
  (gr_text A0 (at 133.223 96.52) (layer F.SilkS))
  (gr_text RST (at 133.223 93.98) (layer F.SilkS))
  (gr_text NC (at 153.924 111.76) (layer F.SilkS))
  (gr_text Gnd (at 153.924 109.22) (layer F.SilkS))
  (gr_text IO2 (at 153.924 106.68) (layer F.SilkS))
  (gr_text IO0 (at 153.924 104.14) (layer F.SilkS))
  (gr_text IO4 (at 153.924 101.6) (layer F.SilkS))
  (gr_text IO5 (at 153.924 99.06) (layer F.SilkS))
  (gr_text RX (at 153.924 96.52) (layer F.SilkS))
  (gr_text TX (at 153.924 93.98) (layer F.SilkS))
  (gr_text NC (at 153.924 91.44) (layer F.SilkS))
  (gr_text NC (at 153.924 88.9) (layer F.SilkS))
  (gr_text NC (at 153.924 86.36) (layer F.SilkS))
  (gr_line (start 130.81 120.65) (end 138.43 120.65) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 148.59 120.65) (end 156.21 120.65) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 148.59 119.38) (end 148.59 120.65) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 138.43 119.38) (end 148.59 119.38) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 138.43 120.65) (end 138.43 119.38) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 156.21 120.65) (end 156.21 77.47) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 130.81 77.47) (end 130.81 120.65) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 156.21 77.47) (end 130.81 77.47) (layer Edge.Cuts) (width 0.127))
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 156 84) (xy 149.7 84) (xy 149.7 77.7) (xy 131 77.7) (xy 131 120.4)
        (xy 138.1 120.4) (xy 138.1 119.1) (xy 148.9 119.1) (xy 148.9 120.3) (xy 156 120.3)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 156 84) (xy 149.7 84) (xy 149.7 77.7) (xy 131 77.7) (xy 131 120.4)
        (xy 138.1 120.4) (xy 138.1 119.1) (xy 148.9 119.1) (xy 148.9 120.3) (xy 156 120.3)
      )
    )
  )
)
