(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 13)
    (tracks 536)
    (zones 0)
    (modules 11)
    (nets 50)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.2 3.2)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF9F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 L1)
  (net 2 D-RIGHT)
  (net 3 D-LEFT)
  (net 4 VDD)
  (net 5 GND)
  (net 6 "Net-(J1-Pad5)")
  (net 7 "Net-(J1-Pad4)")
  (net 8 "Net-(J1-Pad3)")
  (net 9 "Net-(J1-Pad2)")
  (net 10 PIC-6)
  (net 11 START)
  (net 12 SELECT)
  (net 13 "Net-(J2-Pad1)")
  (net 14 CIRCLE)
  (net 15 CROSS)
  (net 16 TRIANGLE)
  (net 17 SQUARE)
  (net 18 R2)
  (net 19 R1)
  (net 20 L2)
  (net 21 RX)
  (net 22 DAT)
  (net 23 "Net-(J4-Pad7)")
  (net 24 "Net-(J4-Pad6)")
  (net 25 "Net-(J4-Pad5)")
  (net 26 R3)
  (net 27 CLK)
  (net 28 L3)
  (net 29 LY)
  (net 30 LX)
  (net 31 D-UP)
  (net 32 D-DOWN)
  (net 33 "Net-(J5-Pad5)")
  (net 34 "Net-(J5-Pad4)")
  (net 35 "Net-(J5-Pad3)")
  (net 36 ATN)
  (net 37 ACK)
  (net 38 RY)
  (net 39 CMD)
  (net 40 "Net-(U1-Pad37)")
  (net 41 "Net-(U1-Pad36)")
  (net 42 "Net-(U1-Pad35)")
  (net 43 "Net-(U1-Pad25)")
  (net 44 "Net-(U1-Pad24)")
  (net 45 "Net-(U1-Pad23)")
  (net 46 "Net-(U1-Pad5)")
  (net 47 "Net-(U1-Pad4)")
  (net 48 "Net-(U1-Pad3)")
  (net 49 "Net-(U1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net ACK)
    (add_net ATN)
    (add_net CIRCLE)
    (add_net CLK)
    (add_net CMD)
    (add_net CROSS)
    (add_net D-DOWN)
    (add_net D-LEFT)
    (add_net D-RIGHT)
    (add_net D-UP)
    (add_net DAT)
    (add_net GND)
    (add_net L1)
    (add_net L2)
    (add_net L3)
    (add_net LX)
    (add_net LY)
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J4-Pad5)")
    (add_net "Net-(J4-Pad6)")
    (add_net "Net-(J4-Pad7)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J5-Pad4)")
    (add_net "Net-(J5-Pad5)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad24)")
    (add_net "Net-(U1-Pad25)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad35)")
    (add_net "Net-(U1-Pad36)")
    (add_net "Net-(U1-Pad37)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net PIC-6)
    (add_net R1)
    (add_net R2)
    (add_net R3)
    (add_net RX)
    (add_net RY)
    (add_net SELECT)
    (add_net SQUARE)
    (add_net START)
    (add_net TRIANGLE)
    (add_net VDD)
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 168.80332 96.62922)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 144.24152 73.34504)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 163.83 96.52 270)
    (descr "Through hole angled pin header, 1x06, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x06 2.54mm single row")
    (fp_text reference J2 (at 4.385 -2.27 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x06_Female (at 4.385 14.97 90) (layer F.Fab) hide)
    (fp_text user %R (at 2.77 6.35) (layer F.Fab) hide)
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 PIC-6))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 VDD))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 START))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 SELECT))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbol:BB_small_Silkscrn_negative (layer F.Cu) (tedit 0)
    (at 146.38274 94.99346)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Symbol:Computerman_Frontslkscrn (layer F.Cu) (tedit 0)
    (at 168.02608 73.57618)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Connector_PinHeader_1.27mm:PinHeader_1x10_P1.27mm_Vertical (layer F.Cu) (tedit 59FED6E3)
    (at 151.13 91.44 90)
    (descr "Through hole straight pin header, 1x10, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x10 1.27mm single row")
    (fp_text reference J3 (at 0 -1.695 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x10_Female (at 0 13.125 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 5.715) (layer F.Fab) hide)
    (pad 10 thru_hole oval (at 0 11.43 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 14 CIRCLE))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 15 CROSS))
    (pad 8 thru_hole oval (at 0 8.89 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 16 TRIANGLE))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 17 SQUARE))
    (pad 6 thru_hole oval (at 0 6.35 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 10 PIC-6))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 11 START))
    (pad 4 thru_hole oval (at 0 3.81 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 12 SELECT))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 18 R2))
    (pad 2 thru_hole oval (at 0 1.27 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 19 R1))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 20 L2))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x10_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-40-1EP_5x5mm_P0.4mm_EP3.8x3.8mm_ThermalVias (layer F.Cu) (tedit 5CF6F3A4)
    (at 156.21 81.28)
    (descr "QFN, 40 Pin (http://www.issi.com/WW/pdf/31FL3736.pdf#page=28), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference U1 (at 0 -3.82) (layer F.SilkS))
    (fp_text value Pic16F18876 (at 0 3.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 40 smd roundrect (at -1.8 -2.4875) (size 0.2 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 RX))
    (pad 39 smd roundrect (at -1.4 -2.4875) (size 0.2 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 DAT))
    (pad 38 smd roundrect (at -1 -2.4875) (size 0.2 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 CMD))
    (pad 37 smd roundrect (at -0.6 -2.4875) (size 0.2 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(U1-Pad37)"))
    (pad 36 smd roundrect (at -0.2 -2.4875) (size 0.2 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 "Net-(U1-Pad36)"))
    (pad 35 smd roundrect (at 0.2 -2.4875) (size 0.2 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 "Net-(U1-Pad35)"))
    (pad 34 smd roundrect (at 0.6 -2.4875) (size 0.2 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 R3))
    (pad 33 smd roundrect (at 1 -2.4875) (size 0.2 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 CLK))
    (pad 32 smd roundrect (at 1.4 -2.4875) (size 0.2 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 L3))
    (pad 31 smd roundrect (at 1.8 -2.4875) (size 0.2 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 LY))
    (pad 30 smd roundrect (at 2.4875 -1.8) (size 0.775 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 LX))
    (pad 29 smd roundrect (at 2.4875 -1.4) (size 0.775 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 D-UP))
    (pad 28 smd roundrect (at 2.4875 -1) (size 0.775 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 D-DOWN))
    (pad 27 smd roundrect (at 2.4875 -0.6) (size 0.775 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (pad 26 smd roundrect (at 2.4875 -0.2) (size 0.775 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VDD))
    (pad 25 smd roundrect (at 2.4875 0.2) (size 0.775 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 "Net-(U1-Pad25)"))
    (pad 24 smd roundrect (at 2.4875 0.6) (size 0.775 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 "Net-(U1-Pad24)"))
    (pad 23 smd roundrect (at 2.4875 1) (size 0.775 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 "Net-(U1-Pad23)"))
    (pad 22 smd roundrect (at 2.4875 1.4) (size 0.775 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 ATN))
    (pad 21 smd roundrect (at 2.4875 1.8) (size 0.775 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 ACK))
    (pad 20 smd roundrect (at 1.8 2.4875) (size 0.2 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 CIRCLE))
    (pad 19 smd roundrect (at 1.4 2.4875) (size 0.2 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 CROSS))
    (pad 18 smd roundrect (at 1 2.4875) (size 0.2 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 TRIANGLE))
    (pad 17 smd roundrect (at 0.6 2.4875) (size 0.2 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 SQUARE))
    (pad 16 smd roundrect (at 0.2 2.4875) (size 0.2 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 PIC-6))
    (pad 15 smd roundrect (at -0.2 2.4875) (size 0.2 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 START))
    (pad 14 smd roundrect (at -0.6 2.4875) (size 0.2 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 SELECT))
    (pad 13 smd roundrect (at -1 2.4875) (size 0.2 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 R2))
    (pad 12 smd roundrect (at -1.4 2.4875) (size 0.2 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 R1))
    (pad 11 smd roundrect (at -1.8 2.4875) (size 0.2 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 L2))
    (pad 10 smd roundrect (at -2.4875 1.8) (size 0.775 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 L1))
    (pad 9 smd roundrect (at -2.4875 1.4) (size 0.775 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 D-RIGHT))
    (pad 8 smd roundrect (at -2.4875 1) (size 0.775 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 D-LEFT))
    (pad 7 smd roundrect (at -2.4875 0.6) (size 0.775 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VDD))
    (pad 6 smd roundrect (at -2.4875 0.2) (size 0.775 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (pad 5 smd roundrect (at -2.4875 -0.2) (size 0.775 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(U1-Pad5)"))
    (pad 4 smd roundrect (at -2.4875 -0.6) (size 0.775 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 "Net-(U1-Pad4)"))
    (pad 3 smd roundrect (at -2.4875 -1) (size 0.775 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 "Net-(U1-Pad3)"))
    (pad 2 smd roundrect (at -2.4875 -1.4) (size 0.775 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 "Net-(U1-Pad2)"))
    (pad 1 smd roundrect (at -2.4875 -1.8) (size 0.775 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 RY))
    (pad "" smd custom (at 1.1 1.1) (size 0.865191 0.865191) (layers F.Paste)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.374613 -0.278545) (xy -0.278545 -0.374613) (xy 0.278545 -0.374613) (xy 0.374613 -0.278545) (xy 0.374613 0.278545)
           (xy 0.278545 0.374613) (xy -0.278545 0.374613) (xy -0.374613 0.278545)) (width 0.231929))
      ))
    (pad "" smd custom (at 1.1 0) (size 0.865191 0.865191) (layers F.Paste)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.374613 -0.278545) (xy -0.278545 -0.374613) (xy 0.278545 -0.374613) (xy 0.374613 -0.278545) (xy 0.374613 0.278545)
           (xy 0.278545 0.374613) (xy -0.278545 0.374613) (xy -0.374613 0.278545)) (width 0.231929))
      ))
    (pad "" smd custom (at 1.1 -1.1) (size 0.865191 0.865191) (layers F.Paste)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.374613 -0.278545) (xy -0.278545 -0.374613) (xy 0.278545 -0.374613) (xy 0.374613 -0.278545) (xy 0.374613 0.278545)
           (xy 0.278545 0.374613) (xy -0.278545 0.374613) (xy -0.374613 0.278545)) (width 0.231929))
      ))
    (pad "" smd custom (at 0 1.1) (size 0.865191 0.865191) (layers F.Paste)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.374613 -0.278545) (xy -0.278545 -0.374613) (xy 0.278545 -0.374613) (xy 0.374613 -0.278545) (xy 0.374613 0.278545)
           (xy 0.278545 0.374613) (xy -0.278545 0.374613) (xy -0.374613 0.278545)) (width 0.231929))
      ))
    (pad "" smd custom (at 0 0) (size 0.865191 0.865191) (layers F.Paste)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.374613 -0.278545) (xy -0.278545 -0.374613) (xy 0.278545 -0.374613) (xy 0.374613 -0.278545) (xy 0.374613 0.278545)
           (xy 0.278545 0.374613) (xy -0.278545 0.374613) (xy -0.374613 0.278545)) (width 0.231929))
      ))
    (pad "" smd custom (at 0 -1.1) (size 0.865191 0.865191) (layers F.Paste)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.374613 -0.278545) (xy -0.278545 -0.374613) (xy 0.278545 -0.374613) (xy 0.374613 -0.278545) (xy 0.374613 0.278545)
           (xy 0.278545 0.374613) (xy -0.278545 0.374613) (xy -0.374613 0.278545)) (width 0.231929))
      ))
    (pad "" smd custom (at -1.1 1.1) (size 0.865191 0.865191) (layers F.Paste)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.374613 -0.278545) (xy -0.278545 -0.374613) (xy 0.278545 -0.374613) (xy 0.374613 -0.278545) (xy 0.374613 0.278545)
           (xy 0.278545 0.374613) (xy -0.278545 0.374613) (xy -0.374613 0.278545)) (width 0.231929))
      ))
    (pad "" smd custom (at -1.1 0) (size 0.865191 0.865191) (layers F.Paste)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.374613 -0.278545) (xy -0.278545 -0.374613) (xy 0.278545 -0.374613) (xy 0.374613 -0.278545) (xy 0.374613 0.278545)
           (xy 0.278545 0.374613) (xy -0.278545 0.374613) (xy -0.374613 0.278545)) (width 0.231929))
      ))
    (pad "" smd custom (at -1.1 -1.1) (size 0.865191 0.865191) (layers F.Paste)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.374613 -0.278545) (xy -0.278545 -0.374613) (xy 0.278545 -0.374613) (xy 0.374613 -0.278545) (xy 0.374613 0.278545)
           (xy 0.278545 0.374613) (xy -0.278545 0.374613) (xy -0.374613 0.278545)) (width 0.231929))
      ))
    (pad 41 smd roundrect (at 0 0) (size 3.8 3.8) (layers B.Cu) (roundrect_rratio 0.065789)
      (net 5 GND))
    (pad 41 thru_hole circle (at 1.65 1.65) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 5 GND))
    (pad 41 thru_hole circle (at 0.55 1.65) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 5 GND))
    (pad 41 thru_hole circle (at -0.55 1.65) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 5 GND))
    (pad 41 thru_hole circle (at -1.65 1.65) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 5 GND))
    (pad 41 thru_hole circle (at 1.65 0.55) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 5 GND))
    (pad 41 thru_hole circle (at 0.55 0.55) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 5 GND))
    (pad 41 thru_hole circle (at -0.55 0.55) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 5 GND))
    (pad 41 thru_hole circle (at -1.65 0.55) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 5 GND))
    (pad 41 thru_hole circle (at 1.65 -0.55) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 5 GND))
    (pad 41 thru_hole circle (at 0.55 -0.55) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 5 GND))
    (pad 41 thru_hole circle (at -0.55 -0.55) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 5 GND))
    (pad 41 thru_hole circle (at -1.65 -0.55) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 5 GND))
    (pad 41 thru_hole circle (at 1.65 -1.65) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 5 GND))
    (pad 41 thru_hole circle (at 0.55 -1.65) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 5 GND))
    (pad 41 thru_hole circle (at -0.55 -1.65) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 5 GND))
    (pad 41 thru_hole circle (at -1.65 -1.65) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 5 GND))
    (pad 41 smd roundrect (at 0 0) (size 3.8 3.8) (layers F.Cu F.Mask) (roundrect_rratio 0.065789)
      (net 5 GND))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-40-1EP_5x5mm_P0.4mm_EP3.8x3.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_FFC-FPC:Hirose_FH12-30S-0.5SH_1x30-1MP_P0.50mm_Horizontal (layer B.Cu) (tedit 5D24667B)
    (at 156.55798 86.90102 180)
    (descr "Hirose FH12, FFC/FPC connector, FH12-30S-0.5SH, 30 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator")
    (tags "connector Hirose FH12 horizontal")
    (attr smd)
    (fp_text reference J6 (at 0 3.7) (layer B.SilkS))
    (fp_text value Conn_01x30_Female (at 0 -5.6) (layer B.Fab))
    (fp_text user %R (at 0 -3.7) (layer B.Fab))
    (pad 30 smd rect (at 7.25 1.85 180) (size 0.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (pad 29 smd rect (at 6.75 1.85 180) (size 0.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (pad 28 smd rect (at 6.25 1.85 180) (size 0.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 4 VDD))
    (pad 27 smd rect (at 5.75 1.85 180) (size 0.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 4 VDD))
    (pad 26 smd rect (at 5.25 1.85 180) (size 0.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 4 VDD))
    (pad 25 smd rect (at 4.75 1.85 180) (size 0.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 28 L3))
    (pad 24 smd rect (at 4.25 1.85 180) (size 0.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 26 R3))
    (pad 23 smd rect (at 3.75 1.85 180) (size 0.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 29 LY))
    (pad 22 smd rect (at 3.25 1.85 180) (size 0.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 30 LX))
    (pad 21 smd rect (at 2.75 1.85 180) (size 0.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 38 RY))
    (pad 20 smd rect (at 2.25 1.85 180) (size 0.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 21 RX))
    (pad 19 smd rect (at 1.75 1.85 180) (size 0.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 20 L2))
    (pad 18 smd rect (at 1.25 1.85 180) (size 0.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 L1))
    (pad 17 smd rect (at 0.75 1.85 180) (size 0.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 18 R2))
    (pad 16 smd rect (at 0.25 1.85 180) (size 0.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 19 R1))
    (pad 15 smd rect (at -0.25 1.85 180) (size 0.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 D-RIGHT))
    (pad 14 smd rect (at -0.75 1.85 180) (size 0.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 D-LEFT))
    (pad 13 smd rect (at -1.25 1.85 180) (size 0.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 32 D-DOWN))
    (pad 12 smd rect (at -1.75 1.85 180) (size 0.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 31 D-UP))
    (pad 11 smd rect (at -2.25 1.85 180) (size 0.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 12 SELECT))
    (pad 10 smd rect (at -2.75 1.85 180) (size 0.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 11 START))
    (pad 9 smd rect (at -3.25 1.85 180) (size 0.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 17 SQUARE))
    (pad 8 smd rect (at -3.75 1.85 180) (size 0.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 16 TRIANGLE))
    (pad 7 smd rect (at -4.25 1.85 180) (size 0.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 14 CIRCLE))
    (pad 6 smd rect (at -4.75 1.85 180) (size 0.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 15 CROSS))
    (pad 5 smd rect (at -5.25 1.85 180) (size 0.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 37 ACK))
    (pad 4 smd rect (at -5.75 1.85 180) (size 0.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 36 ATN))
    (pad 3 smd rect (at -6.25 1.85 180) (size 0.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 27 CLK))
    (pad 2 smd rect (at -6.75 1.85 180) (size 0.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 39 CMD))
    (pad 1 smd rect (at -7.25 1.85 180) (size 0.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 22 DAT))
    (pad MP smd rect (at -9.15 -1.4 180) (size 1.8 2.2) (layers B.Cu B.Paste B.Mask))
    (pad MP smd rect (at 9.15 -1.4 180) (size 1.8 2.2) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/Connector_FFC-FPC.3dshapes/Hirose_FH12-30S-0.5SH_1x30-1MP_P0.50mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.27mm:PinHeader_1x10_P1.27mm_Vertical (layer F.Cu) (tedit 59FED6E3)
    (at 170.18 87.63 180)
    (descr "Through hole straight pin header, 1x10, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x10 1.27mm single row")
    (fp_text reference J5 (at 0 -1.695) (layer F.SilkS) hide)
    (fp_text value Conn_01x10_Female (at 0 13.125) (layer F.Fab) hide)
    (fp_text user %R (at 0 5.715 90) (layer F.Fab) hide)
    (pad 10 thru_hole oval (at 0 11.43 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 30 LX))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 31 D-UP))
    (pad 8 thru_hole oval (at 0 8.89 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 32 D-DOWN))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 6 thru_hole oval (at 0 6.35 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 4 VDD))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 33 "Net-(J5-Pad5)"))
    (pad 4 thru_hole oval (at 0 3.81 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 34 "Net-(J5-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 35 "Net-(J5-Pad3)"))
    (pad 2 thru_hole oval (at 0 1.27 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 36 ATN))
    (pad 1 thru_hole rect (at 0 0 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 37 ACK))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x10_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.27mm:PinHeader_1x10_P1.27mm_Vertical (layer F.Cu) (tedit 59FED6E3)
    (at 162.56 72.39 270)
    (descr "Through hole straight pin header, 1x10, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x10 1.27mm single row")
    (fp_text reference J4 (at 0 -1.695 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x10_Female (at 0 13.125 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 5.715) (layer F.Fab) hide)
    (pad 10 thru_hole oval (at 0 11.43 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 21 RX))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 22 DAT))
    (pad 8 thru_hole oval (at 0 8.89 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 39 CMD))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 23 "Net-(J4-Pad7)"))
    (pad 6 thru_hole oval (at 0 6.35 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 24 "Net-(J4-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 25 "Net-(J4-Pad5)"))
    (pad 4 thru_hole oval (at 0 3.81 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 26 R3))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 27 CLK))
    (pad 2 thru_hole oval (at 0 1.27 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 28 L3))
    (pad 1 thru_hole rect (at 0 0 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 29 LY))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x10_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.27mm:PinHeader_1x10_P1.27mm_Vertical (layer F.Cu) (tedit 59FED6E3)
    (at 143.51 76.2)
    (descr "Through hole straight pin header, 1x10, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x10 1.27mm single row")
    (fp_text reference J1 (at 0 -1.695) (layer F.SilkS) hide)
    (fp_text value Conn_01x10_Female (at 0 13.125) (layer F.Fab) hide)
    (fp_text user %R (at 0 5.715 90) (layer F.Fab) hide)
    (pad 10 thru_hole oval (at 0 11.43) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 L1))
    (pad 9 thru_hole oval (at 0 10.16) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 D-RIGHT))
    (pad 8 thru_hole oval (at 0 8.89) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 3 D-LEFT))
    (pad 7 thru_hole oval (at 0 7.62) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 4 VDD))
    (pad 6 thru_hole oval (at 0 6.35) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 5 thru_hole oval (at 0 5.08) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at 0 3.81) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 1.27) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 38 RY))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x10_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "30\n" (at 149.352 83.53806 270) (layer B.SilkS))
  (gr_text 1 (at 163.84778 83.75142 180) (layer B.SilkS))
  (gr_text "1\n\n2\n\n3\n\n4\n\n5\n\n6" (at 157.4165 94.89186 270) (layer F.SilkS))
  (gr_text "L2\nR1\nR2\nSELECT\nSTART\nPIC \"6\"\nSQUARE\nTRIANGLE\nCROSS\nCIRCLE" (at 156.98978 88.0237 90) (layer F.SilkS))
  (gr_text "RY\n--\n--\n--\n--\nGND\nVDD\n D-LEFT\n  D-RIGHT\nL1\n" (at 146.812 81.8896) (layer F.SilkS))
  (gr_text "RX\nDAT\nCMD\n--\n--\n--\nR3\nCLK\nL3\nLY" (at 156.96946 74.80808 90) (layer F.SilkS))
  (gr_text "LX\nD-UP\nD-DOWN\nGND\nVDD\n--\n--\n--\nATN\nACK" (at 166.45382 82.0801) (layer F.SilkS))
  (gr_line (start 142.24 71.12) (end 171.45 71.12) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 142.24 99.06) (end 142.24 71.12) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 143.51 99.06) (end 142.24 99.06) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 171.45 99.06) (end 168.91 99.06) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 171.45 71.12) (end 171.45 99.06) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 170.18 99.06) (end 143.51 99.06) (layer Edge.Cuts) (width 0.05))
  (zone (net 4) (net_name VDD) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.18076 71.4121) (xy 171.2341 98.88474) (xy 142.46098 98.8568) (xy 142.43304 71.35876)
      )
    )
  )
  (zone (net 5) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.26204 71.47052) (xy 171.23918 98.91014) (xy 142.40256 98.84156) (xy 142.41272 71.4248)
      )
    )
  )
)
