(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 75)
    (no_connects 8)
    (area 124.384999 73.584999 172.795001 99.135001)
    (thickness 1.6)
    (drawings 22)
    (tracks 108)
    (zones 0)
    (modules 10)
    (nets 35)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3048)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.4064)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.8 1.2)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /OUT1)
  (net 3 /OUT2)
  (net 4 /OUT3)
  (net 5 /OUT4)
  (net 6 /OUT5)
  (net 7 /OUT6)
  (net 8 /OUT7)
  (net 9 /OUT8)
  (net 10 /IN1)
  (net 11 /IN2)
  (net 12 /IN3)
  (net 13 /IN4)
  (net 14 /IN5)
  (net 15 /IN6)
  (net 16 /IN7)
  (net 17 /IN8)
  (net 18 /OUT9)
  (net 19 /OUT10)
  (net 20 /OUT11)
  (net 21 /OUT12)
  (net 22 /OUT13)
  (net 23 /OUT14)
  (net 24 /OUT15)
  (net 25 /OUT16)
  (net 26 /IN9)
  (net 27 /IN10)
  (net 28 /IN11)
  (net 29 /IN12)
  (net 30 /IN13)
  (net 31 /IN14)
  (net 32 /IN15)
  (net 33 /IN16)
  (net 34 /A0)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /A0)
    (add_net /IN1)
    (add_net /IN10)
    (add_net /IN11)
    (add_net /IN12)
    (add_net /IN13)
    (add_net /IN14)
    (add_net /IN15)
    (add_net /IN16)
    (add_net /IN2)
    (add_net /IN3)
    (add_net /IN4)
    (add_net /IN5)
    (add_net /IN6)
    (add_net /IN7)
    (add_net /IN8)
    (add_net /IN9)
    (add_net /OUT1)
    (add_net /OUT10)
    (add_net /OUT11)
    (add_net /OUT12)
    (add_net /OUT13)
    (add_net /OUT14)
    (add_net /OUT15)
    (add_net /OUT16)
    (add_net /OUT2)
    (add_net /OUT3)
    (add_net /OUT4)
    (add_net /OUT5)
    (add_net /OUT6)
    (add_net /OUT7)
    (add_net /OUT8)
    (add_net /OUT9)
  )
  (module footprints:Molex_PicoClasp_501331-1207_1x12_P1.0mm_Vertical (layer F.Cu) (tedit 5FB31BBB)
    (at 162.56 86.36 270)
    (descr "Molex Pico-Clasp header, 12 contacts, 1.00mm pitch, http://www.molex.com/pdm_docs/sd/5013310207_sd.pdf")
    (tags "connector molex pico clasp 501331-1207")
    (attr smd)
    (fp_text reference J2 (at -3.81 -6.985 360) (layer F.SilkS))
    (fp_text value PicoClasp_12 (at 0 8.6 270) (layer F.Fab))
    (fp_text user %R (at 0.675 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1.325 -5.5 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 /IN12))
    (pad 2 smd rect (at -1.325 -4.5 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /IN11))
    (pad 3 smd rect (at -1.325 -3.5 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /IN10))
    (pad 4 smd rect (at -1.325 -2.5 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 /IN9))
    (pad 5 smd rect (at -1.325 -1.5 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /IN8))
    (pad 6 smd rect (at -1.325 -0.5 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /IN7))
    (pad 7 smd rect (at -1.325 0.5 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /IN6))
    (pad 8 smd rect (at -1.325 1.5 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 /IN5))
    (pad 9 smd rect (at -1.325 2.5 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 /IN4))
    (pad 10 smd rect (at -1.325 3.5 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 /IN3))
    (pad 11 smd rect (at -1.325 4.5 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 /IN2))
    (pad 12 smd rect (at -1.325 5.5 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 /IN1))
    (pad 13 smd rect (at 1.2 -6.8 270) (size 1.8 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 1.2 6.8 270) (size 1.8 1.2) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_PicoClasp_501331-1207_1x12_P1.0mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x18_Pitch2.54mm (layer F.Cu) (tedit 5FB3FD60)
    (at 127 96.52 90)
    (descr "Through hole straight pin header, 1x18, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x18 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X18 (at 0 45.51 90) (layer F.Fab))
    (fp_text user %R (at 0 21.59 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /A0))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /A0))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /OUT1))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /OUT3))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /OUT5))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /OUT7))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /OUT9))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /OUT11))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /OUT13))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /OUT15))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /IN1))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /IN3))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /IN5))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /IN7))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /IN9))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /IN11))
    (pad 17 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /IN13))
    (pad 18 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /IN15))
  )
  (module Pin_Headers:Pin_Header_Straight_1x18_Pitch2.54mm (layer F.Cu) (tedit 5FB31035)
    (at 127 76.2 90)
    (descr "Through hole straight pin header, 1x18, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x18 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X18 (at 0 45.51 90) (layer F.Fab))
    (fp_text user %R (at 0 21.59 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /A0))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /A0))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /OUT2))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /OUT4))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /OUT6))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /OUT8))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /OUT10))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /OUT12))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /OUT14))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /OUT16))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /IN2))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /IN4))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /IN6))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /IN8))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /IN10))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /IN12))
    (pad 17 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /IN14))
    (pad 18 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /IN16))
  )
  (module footprints:Molex_PicoClasp_501331-1207_1x12_P1.0mm_Vertical (layer F.Cu) (tedit 5FB31BAE)
    (at 134.62 86.36 90)
    (descr "Molex Pico-Clasp header, 12 contacts, 1.00mm pitch, http://www.molex.com/pdm_docs/sd/5013310207_sd.pdf")
    (tags "connector molex pico clasp 501331-1207")
    (attr smd)
    (fp_text reference J1 (at -3.81 -6.985 180) (layer F.SilkS))
    (fp_text value PicoClasp_12 (at 0 8.6 90) (layer F.Fab))
    (fp_text user %R (at 0.675 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.325 -5.5 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 /OUT1))
    (pad 2 smd rect (at -1.325 -4.5 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /OUT2))
    (pad 3 smd rect (at -1.325 -3.5 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /OUT3))
    (pad 4 smd rect (at -1.325 -2.5 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /OUT4))
    (pad 5 smd rect (at -1.325 -1.5 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /OUT5))
    (pad 6 smd rect (at -1.325 -0.5 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /OUT6))
    (pad 7 smd rect (at -1.325 0.5 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /OUT7))
    (pad 8 smd rect (at -1.325 1.5 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /OUT8))
    (pad 9 smd rect (at -1.325 2.5 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 /OUT9))
    (pad 10 smd rect (at -1.325 3.5 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 /OUT10))
    (pad 11 smd rect (at -1.325 4.5 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 /OUT11))
    (pad 12 smd rect (at -1.325 5.5 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 /OUT12))
    (pad 13 smd rect (at 1.2 -6.8 90) (size 1.8 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 1.2 6.8 90) (size 1.8 1.2) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_PicoClasp_501331-1207_1x12_P1.0mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x18_Pitch2.54mm (layer F.Cu) (tedit 5FB3FD63)
    (at 127 93.98 90)
    (descr "Through hole straight pin header, 1x18, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x18 2.54mm single row")
    (fp_text reference J33 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X18 (at 0 45.51 90) (layer F.Fab))
    (fp_text user %R (at 0 21.59 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /A0))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /A0))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /OUT1))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /OUT3))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /OUT5))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /OUT7))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /OUT9))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /OUT11))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /OUT13))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /OUT15))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /IN1))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /IN3))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /IN5))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /IN7))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /IN9))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /IN11))
    (pad 17 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /IN13))
    (pad 18 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /IN15))
  )
  (module Pin_Headers:Pin_Header_Straight_1x18_Pitch2.54mm (layer F.Cu) (tedit 5FB3FD5C)
    (at 127 78.74 90)
    (descr "Through hole straight pin header, 1x18, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x18 2.54mm single row")
    (fp_text reference J44 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X18 (at 0 45.51 90) (layer F.Fab))
    (fp_text user %R (at 0 21.59 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /A0))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /A0))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /OUT2))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /OUT4))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /OUT6))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /OUT8))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /OUT10))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /OUT12))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /OUT14))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /OUT16))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /IN2))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /IN4))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /IN6))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /IN8))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /IN10))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /IN12))
    (pad 17 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /IN14))
    (pad 18 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /IN16))
  )
  (module footprints:R_0805_JMP_NC (layer B.Cu) (tedit 5FB548B6)
    (at 127 88.9 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference A0 (at -2.75 0 360) (layer B.SilkS))
    (fp_text value Jumper_NC_Small (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 34 /A0))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 34 /A0))
    (pad 1 smd rect (at 0 0 90) (size 2 0.25) (layers B.Cu B.Paste B.Mask)
      (net 34 /A0))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0805_JMP_NC (layer B.Cu) (tedit 5FB548B6)
    (at 129.54 88.9 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference A1 (at -2.75 0 360) (layer B.SilkS))
    (fp_text value Jumper_NC_Small (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 34 /A0))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 34 /A0))
    (pad 1 smd rect (at 0 0 90) (size 2 0.25) (layers B.Cu B.Paste B.Mask)
      (net 34 /A0))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0805_JMP_NC (layer B.Cu) (tedit 5FB548B6)
    (at 127 83.82 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference A2 (at -2.75 0 540) (layer B.SilkS))
    (fp_text value Jumper_NC_Small (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 34 /A0))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 34 /A0))
    (pad 1 smd rect (at 0 0 270) (size 2 0.25) (layers B.Cu B.Paste B.Mask)
      (net 34 /A0))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0805_JMP_NC (layer B.Cu) (tedit 5FB548B6)
    (at 129.54 83.82 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference A3 (at -2.75 0 540) (layer B.SilkS))
    (fp_text value Jumper_NC_Small (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 34 /A0))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 34 /A0))
    (pad 1 smd rect (at 0 0 270) (size 2 0.25) (layers B.Cu B.Paste B.Mask)
      (net 34 /A0))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "16 14 12 10  8  6  4  2" (at 161.29 81.28) (layer B.SilkS))
  (gr_text "16 14 12 10  8  6  4  2" (at 140.97 81.28) (layer B.SilkS))
  (gr_text "15 13 11 9  7  5  3  1" (at 161.29 91.44) (layer B.SilkS))
  (gr_text "15 13 11 9  7  5  3  1" (at 140.97 91.44) (layer B.SilkS))
  (gr_text "Rev 0.0\nNov 2020" (at 165.1 87.63) (layer B.SilkS))
  (gr_text "UCT - Pico-Clasp 12 Pos." (at 149.86 81.28) (layer F.SilkS))
  (dimension 25.4 (width 0.3) (layer Dwgs.User)
    (gr_text "1.0000 in" (at 121.92 86.36 270) (layer Dwgs.User))
    (feature1 (pts (xy 124.46 99.06) (xy 121.92 99.06)))
    (feature2 (pts (xy 124.46 73.66) (xy 121.92 73.66)))
    (crossbar (pts (xy 121.92 73.66) (xy 121.92 99.06)))
    (arrow1a (pts (xy 121.92 99.06) (xy 121.333579 97.933496)))
    (arrow1b (pts (xy 121.92 99.06) (xy 122.506421 97.933496)))
    (arrow2a (pts (xy 121.92 73.66) (xy 121.333579 74.786504)))
    (arrow2b (pts (xy 121.92 73.66) (xy 122.506421 74.786504)))
  )
  (dimension 48.26 (width 0.3) (layer Dwgs.User)
    (gr_text "1.9000 in" (at 148.59 67.23) (layer Dwgs.User))
    (feature1 (pts (xy 172.72 73.66) (xy 172.72 65.88)))
    (feature2 (pts (xy 124.46 73.66) (xy 124.46 65.88)))
    (crossbar (pts (xy 124.46 68.58) (xy 172.72 68.58)))
    (arrow1a (pts (xy 172.72 68.58) (xy 171.593496 69.166421)))
    (arrow1b (pts (xy 172.72 68.58) (xy 171.593496 67.993579)))
    (arrow2a (pts (xy 124.46 68.58) (xy 125.586504 69.166421)))
    (arrow2b (pts (xy 124.46 68.58) (xy 125.586504 67.993579)))
  )
  (gr_text "500-044337 Rev D" (at 149.86 91.44) (layer F.SilkS))
  (gr_line (start 124.46 96.52) (end 124.46 76.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170.18 99.06) (end 127 99.06) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 172.72 76.2) (end 172.72 96.52) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127 73.66) (end 170.18 73.66) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 127 76.2) (end 124.46 76.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 127 96.52) (end 127 99.06) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 170.18 96.52) (end 172.72 96.52) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 170.18 76.2) (end 170.18 73.66) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.45 90.17) (xy 167.005 90.17) (xy 167.005 85.725) (xy 171.45 85.725)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157.48 91.44) (xy 153.035 91.44) (xy 153.035 85.09) (xy 157.48 85.09)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 144.145 86.995) (xy 139.065 86.995) (xy 139.065 83.185) (xy 144.145 83.185)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.365 83.185) (xy 129.54 83.185) (xy 129.54 86.995) (xy 125.73 86.995) (xy 125.73 83.185)
      )
    )
  )
)
