(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "CERBERUS 2100(tm) Digital Discovery(tm) Adapter")
		(date "2024-04-12")
		(rev "1")
		(company "@baldengineer")
	)
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
				(color "White")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Purple")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(color "FR4 natural")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Purple")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
				(color "White")
			)
			(copper_finish "ENIG")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0.0508)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "dd la adapter gerbs v1/")
		)
	)
	(net 0 "")
	(net 1 "/XA3")
	(net 2 "GND")
	(net 3 "/XA8")
	(net 4 "/XA11")
	(net 5 "/XD6")
	(net 6 "/XBUSREQ")
	(net 7 "/XD3")
	(net 8 "/XA7")
	(net 9 "/XA0")
	(net 10 "/XD0")
	(net 11 "+5V")
	(net 12 "/XE")
	(net 13 "/XCLK")
	(net 14 "/XWR")
	(net 15 "/XA14")
	(net 16 "/XIRQ")
	(net 17 "/XA2")
	(net 18 "/XA6")
	(net 19 "/XD1")
	(net 20 "/XA15")
	(net 21 "/XD2")
	(net 22 "/XA13")
	(net 23 "/XD5")
	(net 24 "/XA5")
	(net 25 "/XSLC")
	(net 26 "/XA10")
	(net 27 "/XRD")
	(net 28 "/XA12")
	(net 29 "/XBUSACK")
	(net 30 "/XA4")
	(net 31 "/XA9")
	(net 32 "/XD4")
	(net 33 "/XA1")
	(net 34 "/XIN")
	(net 35 "/XD7")
	(net 36 "Net-(D1-A)")
	(footprint "Connector_PinSocket_2.54mm:PinSocket_2x16_P2.54mm_Vertical"
		(locked yes)
		(layer "F.Cu")
		(at 139.72 78.486)
		(descr "Through hole straight socket strip, 2x16, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 2x16 2.54mm double row")
		(property "Reference" "J4"
			(at -1.27 -2.77 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Addr_Data"
			(at -1.27 40.87 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinSocket_2.54mm:PinSocket_2x16_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "Digilent Discovery LA Adapter.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -1.27 19.05 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at -2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/XA0")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at -2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/XA1")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/XA2")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at -2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/XA3")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "/XA4")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at -2.54 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/XA5")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/XA6")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at -2.54 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/XA7")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at -2.54 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/XA8")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole oval
			(at -2.54 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/XA9")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole oval
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/XA10")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" thru_hole oval
			(at -2.54 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/XA11")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" thru_hole oval
			(at 0 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "/XA12")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" thru_hole oval
			(at -2.54 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/XA13")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" thru_hole oval
			(at 0 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/XA14")
			(pinfunction "Pin_19")
			(pintype "passive")
		)
		(pad "20" thru_hole oval
			(at -2.54 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/XA15")
			(pinfunction "Pin_20")
			(pintype "passive")
		)
		(pad "21" thru_hole oval
			(at 0 25.4)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_21")
			(pintype "passive")
		)
		(pad "22" thru_hole oval
			(at -2.54 25.4)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_22")
			(pintype "passive")
		)
		(pad "23" thru_hole oval
			(at 0 27.94)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/XD0")
			(pinfunction "Pin_23")
			(pintype "passive")
		)
		(pad "24" thru_hole oval
			(at -2.54 27.94)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/XD1")
			(pinfunction "Pin_24")
			(pintype "passive")
		)
		(pad "25" thru_hole oval
			(at 0 30.48)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/XD2")
			(pinfunction "Pin_25")
			(pintype "passive")
		)
		(pad "26" thru_hole oval
			(at -2.54 30.48)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/XD3")
			(pinfunction "Pin_26")
			(pintype "passive")
		)
		(pad "27" thru_hole oval
			(at 0 33.02)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/XD4")
			(pinfunction "Pin_27")
			(pintype "passive")
		)
		(pad "28" thru_hole oval
			(at -2.54 33.02)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/XD5")
			(pinfunction "Pin_28")
			(pintype "passive")
		)
		(pad "29" thru_hole oval
			(at 0 35.56)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/XD6")
			(pinfunction "Pin_29")
			(pintype "passive")
		)
		(pad "30" thru_hole oval
			(at -2.54 35.56)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "/XD7")
			(pinfunction "Pin_30")
			(pintype "passive")
		)
		(pad "31" thru_hole oval
			(at 0 38.1)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_31")
			(pintype "passive")
		)
		(pad "32" thru_hole oval
			(at -2.54 38.1)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_32")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x16_P2.54mm_Vertical.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x16_P2.54mm_Horizontal.step"
			(offset
				(xyz 0 -37.965 -1.905)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 180 0 0)
			)
		)
	)
	(footprint "My Libraries:Harwin-S1751-46-Test-Point"
		(layer "F.Cu")
		(at 164.846 120.015)
		(property "Reference" "TP1"
			(at 0.254 2.286 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint_Harwin"
			(at 0 -1.778 0)
			(layer "F.Fab")
		)
		(property "Footprint" "My Libraries:Harwin-S1751-46-Test-Point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Digilent Discovery LA Adapter.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0 0)
			(size 3.45 1.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(model "C:/Users/balde/Dropbox/KiCad/Downloaded Libraries/s1751-46.stp"
			(offset
				(xyz 0 0.825 2)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_1206_3216Metric_Pad1.42x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 153.797 120.269 180)
		(descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D1"
			(at 0 -1.82 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Pwr"
			(at 0 1.82 180)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_1206_3216Metric_Pad1.42x1.75mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "Digilent Discovery LA Adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4875 0 180)
			(size 1.425 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.175439)
			(net 2 "GND")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 1.4875 0 180)
			(size 1.425 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.175439)
			(net 36 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 137.155 120.65 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J6"
			(at 0 -2.33 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "XIN_LA"
			(at 0 4.87 270)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Digilent Discovery LA Adapter.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 360)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/XIN")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "My Libraries:Harwin-S1751-46-Test-Point"
		(layer "F.Cu")
		(at 162.56 61.595)
		(property "Reference" "TP2"
			(at 0.254 2.286 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint_Harwin"
			(at 0 -1.778 0)
			(layer "F.Fab")
		)
		(property "Footprint" "My Libraries:Harwin-S1751-46-Test-Point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Digilent Discovery LA Adapter.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0 0)
			(size 3.45 1.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(model "C:/Users/balde/Dropbox/KiCad/Downloaded Libraries/s1751-46.stp"
			(offset
				(xyz 0 0.825 2)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 137.155 59.944 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J7"
			(at 0 -2.33 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Power"
			(at 0 4.87 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Digilent Discovery LA Adapter.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "+5V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x20_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 162.56 66.039293)
		(descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x20 2.54mm double row")
		(property "Reference" "J2"
			(at 1.27 -2.33 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Card_Header"
			(at 1.27 50.59 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x20_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x20, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "Digilent Discovery LA Adapter.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 24.13 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/XCLK")
			(pinfunction "Pin_1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "+5V")
			(pinfunction "Pin_3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/XE")
			(pinfunction "Pin_4")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/XBUSREQ")
			(pinfunction "Pin_5")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/XSLC")
			(pinfunction "Pin_6")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/XBUSACK")
			(pinfunction "Pin_7")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" thru_hole oval
			(at 2.54 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/XIRQ")
			(pinfunction "Pin_8")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/XRD")
			(pinfunction "Pin_9")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" thru_hole oval
			(at 2.54 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/XWR")
			(pinfunction "Pin_10")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" thru_hole oval
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/XA0")
			(pinfunction "Pin_11")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" thru_hole oval
			(at 2.54 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/XA1")
			(pinfunction "Pin_12")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" thru_hole oval
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/XA2")
			(pinfunction "Pin_13")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" thru_hole oval
			(at 2.54 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/XA3")
			(pinfunction "Pin_14")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" thru_hole oval
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "/XA4")
			(pinfunction "Pin_15")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" thru_hole oval
			(at 2.54 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/XA5")
			(pinfunction "Pin_16")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" thru_hole oval
			(at 0 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/XA6")
			(pinfunction "Pin_17")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" thru_hole oval
			(at 2.54 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/XA7")
			(pinfunction "Pin_18")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" thru_hole oval
			(at 0 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/XA8")
			(pinfunction "Pin_19")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" thru_hole oval
			(at 2.54 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/XA9")
			(pinfunction "Pin_20")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "21" thru_hole oval
			(at 0 25.4)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/XA10")
			(pinfunction "Pin_21")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "22" thru_hole oval
			(at 2.54 25.4)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/XA11")
			(pinfunction "Pin_22")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "23" thru_hole oval
			(at 0 27.94)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "/XA12")
			(pinfunction "Pin_23")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "24" thru_hole oval
			(at 2.54 27.94)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/XA13")
			(pinfunction "Pin_24")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "25" thru_hole oval
			(at 0 30.48)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/XA14")
			(pinfunction "Pin_25")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "26" thru_hole oval
			(at 2.54 30.48)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/XA15")
			(pinfunction "Pin_26")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "27" thru_hole oval
			(at 0 33.02)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/XD0")
			(pinfunction "Pin_27")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "28" thru_hole oval
			(at 2.54 33.02)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/XD1")
			(pinfunction "Pin_28")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "29" thru_hole oval
			(at 0 35.56)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/XD2")
			(pinfunction "Pin_29")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "30" thru_hole oval
			(at 2.54 35.56)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/XD3")
			(pinfunction "Pin_30")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "31" thru_hole oval
			(at 0 38.1)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/XD4")
			(pinfunction "Pin_31")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "32" thru_hole oval
			(at 2.54 38.1)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/XD5")
			(pinfunction "Pin_32")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "33" thru_hole oval
			(at 0 40.64)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/XD6")
			(pinfunction "Pin_33")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "34" thru_hole oval
			(at 2.54 40.64)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "/XD7")
			(pinfunction "Pin_34")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "35" thru_hole oval
			(at 0 43.18)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "+5V")
			(pinfunction "Pin_35")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "36" thru_hole oval
			(at 2.54 43.18)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_36")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "37" thru_hole oval
			(at 0 45.72)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "+5V")
			(pinfunction "Pin_37")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "38" thru_hole oval
			(at 2.54 45.72)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_38")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "39" thru_hole oval
			(at 0 48.26)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/XIN")
			(pinfunction "Pin_39")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "40" thru_hole oval
			(at 2.54 48.26)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_40")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_2x05_P2.54mm_Vertical"
		(locked yes)
		(layer "F.Cu")
		(at 139.72 64.038)
		(descr "Through hole straight socket strip, 2x05, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 2x05 2.54mm double row")
		(property "Reference" "J5"
			(at -1.27 -2.77 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "CTRL2"
			(at -1.27 12.93 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinSocket_2.54mm:PinSocket_2x05_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "Digilent Discovery LA Adapter.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -1.27 5.08 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/XCLK")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at -2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/XE")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/XBUSREQ")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at -2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/XSLC")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/XBUSACK")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at -2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/XIRQ")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/XRD")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at -2.54 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/XWR")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at -2.54 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x05_P2.54mm_Vertical.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x05_P2.54mm_Horizontal.step"
			(hide yes)
			(offset
				(xyz 0 -10 -2)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 180 0 0)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.step"
			(offset
				(xyz -2.5 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 148.844 120.142)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0.127 1.651 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1k"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol with 0805 Package"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Digilent Discovery LA Adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 11 "+5V")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 36 "Net-(D1-A)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 148.59 59.944 90)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J3"
			(at 0 -2.33 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "XE_Header"
			(at 0 7.41 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Digilent Discovery LA Adapter.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "+5V")
			(pinfunction "Pin_1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/XE")
			(pinfunction "Pin_2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_2x20_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 149.86 66.04 180)
		(descr "Through hole straight socket strip, 2x20, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 2x20 2.54mm double row")
		(property "Reference" "J1"
			(at -1.27 2.77 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Cerberus_Expansion"
			(at -1.27 -51.03 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinSocket_2.54mm:PinSocket_2x20_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x20, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "Digilent Discovery LA Adapter.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -1.27 -24.13 -90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/XCLK")
			(pinfunction "Pin_1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at -2.54 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole oval
			(at 0 -2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "+5V")
			(pinfunction "Pin_3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" thru_hole oval
			(at -2.54 -2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/XE")
			(pinfunction "Pin_4")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" thru_hole oval
			(at 0 -5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/XBUSREQ")
			(pinfunction "Pin_5")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" thru_hole oval
			(at -2.54 -5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/XSLC")
			(pinfunction "Pin_6")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" thru_hole oval
			(at 0 -7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/XBUSACK")
			(pinfunction "Pin_7")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" thru_hole oval
			(at -2.54 -7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/XIRQ")
			(pinfunction "Pin_8")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole oval
			(at 0 -10.16 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/XRD")
			(pinfunction "Pin_9")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" thru_hole oval
			(at -2.54 -10.16 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/XWR")
			(pinfunction "Pin_10")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" thru_hole oval
			(at 0 -12.7 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/XA0")
			(pinfunction "Pin_11")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" thru_hole oval
			(at -2.54 -12.7 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/XA1")
			(pinfunction "Pin_12")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" thru_hole oval
			(at 0 -15.24 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/XA2")
			(pinfunction "Pin_13")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" thru_hole oval
			(at -2.54 -15.24 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/XA3")
			(pinfunction "Pin_14")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" thru_hole oval
			(at 0 -17.78 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "/XA4")
			(pinfunction "Pin_15")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" thru_hole oval
			(at -2.54 -17.78 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/XA5")
			(pinfunction "Pin_16")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" thru_hole oval
			(at 0 -20.32 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/XA6")
			(pinfunction "Pin_17")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" thru_hole oval
			(at -2.54 -20.32 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/XA7")
			(pinfunction "Pin_18")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" thru_hole oval
			(at 0 -22.86 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/XA8")
			(pinfunction "Pin_19")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" thru_hole oval
			(at -2.54 -22.86 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/XA9")
			(pinfunction "Pin_20")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "21" thru_hole oval
			(at 0 -25.4 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/XA10")
			(pinfunction "Pin_21")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "22" thru_hole oval
			(at -2.54 -25.4 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/XA11")
			(pinfunction "Pin_22")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "23" thru_hole oval
			(at 0 -27.94 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "/XA12")
			(pinfunction "Pin_23")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "24" thru_hole oval
			(at -2.54 -27.94 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/XA13")
			(pinfunction "Pin_24")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "25" thru_hole oval
			(at 0 -30.48 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/XA14")
			(pinfunction "Pin_25")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "26" thru_hole oval
			(at -2.54 -30.48 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/XA15")
			(pinfunction "Pin_26")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "27" thru_hole oval
			(at 0 -33.02 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/XD0")
			(pinfunction "Pin_27")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "28" thru_hole oval
			(at -2.54 -33.02 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/XD1")
			(pinfunction "Pin_28")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "29" thru_hole oval
			(at 0 -35.56 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/XD2")
			(pinfunction "Pin_29")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "30" thru_hole oval
			(at -2.54 -35.56 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/XD3")
			(pinfunction "Pin_30")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "31" thru_hole oval
			(at 0 -38.1 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/XD4")
			(pinfunction "Pin_31")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "32" thru_hole oval
			(at -2.54 -38.1 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/XD5")
			(pinfunction "Pin_32")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "33" thru_hole oval
			(at 0 -40.64 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/XD6")
			(pinfunction "Pin_33")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "34" thru_hole oval
			(at -2.54 -40.64 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "/XD7")
			(pinfunction "Pin_34")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "35" thru_hole oval
			(at 0 -43.18 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "+5V")
			(pinfunction "Pin_35")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "36" thru_hole oval
			(at -2.54 -43.18 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_36")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "37" thru_hole oval
			(at 0 -45.72 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "+5V")
			(pinfunction "Pin_37")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "38" thru_hole oval
			(at -2.54 -45.72 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_38")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "39" thru_hole oval
			(at 0 -48.26 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/XIN")
			(pinfunction "Pin_39")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "40" thru_hole oval
			(at -2.54 -48.26 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_40")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 5)
				(filter_ratio 0.9)
				(enabled no)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x20_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_arc
		(start 165.14 57.15)
		(mid 166.907767 57.882233)
		(end 167.64 59.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 135.382 120.69)
		(end 135.382 59.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 165.14 123.19)
		(end 137.882 123.19)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 137.882 123.19)
		(mid 136.114233 122.457767)
		(end 135.382 120.69)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.64 59.65)
		(end 167.64 120.69)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 167.64 120.69)
		(mid 166.907767 122.457767)
		(end 165.14 123.19)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 137.882 57.15)
		(end 165.14 57.15)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 135.382 59.65)
		(mid 136.114233 57.882233)
		(end 137.882 57.15)
		(layer "Edge.Cuts")
	)
	(gr_text "GND"
		(at 144.78 74.93 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "+5V"
		(at 146.812 60.452 -0)
		(layer "B.SilkS")
	)
	(gr_text "XE"
		(at 152.146 62.992 -0)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 144.907 79.121 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "GND"
		(at 157.861 112.395 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "GND"
		(at 157.861 114.935 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "GND"
		(at 144.78 104.521 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "GND"
		(at 144.907 117.348 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "GND"
		(at 157.861 109.855 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "cerberus 2100 DD LA adapter\nrev1, @baldengineer"
		(at 166.497 121.539 0)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 158.877 60.579 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "GND"
		(at 144.78 91.948 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "GND"
		(at 158.115 66.675 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "Power"
		(at 149.098 122.555 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 154.686 66.675 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "XA5|XA4"
		(at 141.478 86.614 0)
		(layer "F.SilkS")
	)
	(gr_text "A15|A14"
		(at 141.478 101.854 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 141.478 74.93 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "GND"
		(at 141.5415 91.948 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "A11|A10"
		(at 141.478 96.774 0)
		(layer "F.SilkS")
	)
	(gr_text "XD5|XD4"
		(at 141.478 112.268 0)
		(layer "F.SilkS")
	)
	(gr_text "IRQ|ACK"
		(at 141.859 69.596 0)
		(layer "F.SilkS")
	)
	(gr_text "XD3|XD2"
		(at 141.478 109.728 0)
		(layer "F.SilkS")
	)
	(gr_text "XA7|XA6"
		(at 141.478 89.154 0)
		(layer "F.SilkS")
	)
	(gr_text "+5V"
		(at 143.256 60.452 0)
		(layer "F.SilkS")
	)
	(gr_text "XE |CLK"
		(at 141.605 64.643 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 141.5415 104.521 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "XIN"
		(at 142.875 121.285 0)
		(layer "F.SilkS")
	)
	(gr_text "XD1|XD0"
		(at 141.478 106.934 0)
		(layer "F.SilkS")
	)
	(gr_text "SLC|REQ"
		(at 141.605 67.056 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 155.62973 60.579 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "XA3|XA2"
		(at 141.478 84.074 0)
		(layer "F.SilkS")
	)
	(gr_text "XE"
		(at 150.241 63.246 0)
		(layer "F.SilkS")
	)
	(gr_text "A13|A12"
		(at 141.478 99.314 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 154.432 109.855 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "XWR|XRD"
		(at 141.351 72.263 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 154.432 112.395 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "GND"
		(at 141.5415 117.348 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "XD7|XD6"
		(at 141.478 114.808 0)
		(layer "F.SilkS")
	)
	(gr_text "XA9|XA8"
		(at 141.478 94.488 0)
		(layer "F.SilkS")
	)
	(gr_text "XA1|XA0"
		(at 141.478 81.534 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 141.5415 79.121 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "GND"
		(at 154.432 114.935 0)
		(layer "F.SilkS" knockout)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.2032)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 4)
		)
		(polygon
			(pts
				(xy 166.497 66.929) (xy 166.497 59.055) (xy 152.4 59.182) (xy 152.4 63.881) (xy 163.83 63.881) (xy 163.83 67.056)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.2032)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 4)
		)
		(polygon
			(pts
				(xy 164.084 108.331) (xy 168.021 108.331) (xy 167.894 123.317) (xy 162.179 123.317) (xy 162.179 118.237)
				(xy 164.084 118.237)
			)
		)
	)
	(zone
		(net 11)
		(net_name "+5V")
		(layer "F.Cu")
		(name "+5V")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.2032)
		)
		(min_thickness 0.2032)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.2)
			(thermal_bridge_width 1)
		)
		(polygon
			(pts
				(xy 148.59 108.458) (xy 163.83 108.458) (xy 163.83 113.03) (xy 148.59 113.03)
			)
		)
	)
	(zone
		(net 11)
		(net_name "+5V")
		(layer "F.Cu")
		(name "+5V")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.2032)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 148.336 107.95) (xy 163.83 107.95) (xy 163.83 113.03) (xy 148.336 113.03)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(name "GND")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 133.35 57.15) (xy 168.91 57.15) (xy 168.91 123.698) (xy 133.35 123.698)
			)
		)
	)
	(zone
		(net 11)
		(net_name "+5V")
		(layer "B.Cu")
		(name "+5V")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.2032)
		)
		(min_thickness 0.2032)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.2)
			(thermal_bridge_width 1)
		)
		(polygon
			(pts
				(xy 147.955 67.056) (xy 163.703 67.183) (xy 163.83 70.104) (xy 148.082 69.977)
			)
		)
	)
)