(kicad_pcb (version 4) (host pcbnew 4.0.6-e0-6349~53~ubuntu16.04.1)
  (general
    (links 126)
    (no_connects 3)
    (area 126.924999 29.134999 162.635001 161.365001)
    (thickness 1.6)
    (drawings 4)
    (tracks 310)
    (zones 0)
    (modules 21)
    (nets 27)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.3048)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEEF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +12V)
  (net 2 GND)
  (net 3 +5V)
  (net 4 /PIC16F1829LIN/LBUS)
  (net 5 /D1)
  (net 6 /E1)
  (net 7 /D2)
  (net 8 /E2)
  (net 9 /D3)
  (net 10 /E3)
  (net 11 /D4)
  (net 12 /E4)
  (net 13 /D5)
  (net 14 /E5)
  (net 15 /D6)
  (net 16 /E6)
  (net 17 /D7)
  (net 18 /E7)
  (net 19 /D8)
  (net 20 /E8)
  (net 21 /PIC16F1829LIN//MCLR)
  (net 22 "Net-(U1-Pad12)")
  (net 23 /PIC16F1829LIN/ICSPCLK)
  (net 24 /PIC16F1829LIN/ICSPDAT)
  (net 25 "Net-(C1-Pad1)")
  (net 26 GNDPWR)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.3048)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /D8)
    (add_net /PIC16F1829LIN//MCLR)
    (add_net /PIC16F1829LIN/ICSPCLK)
    (add_net /PIC16F1829LIN/ICSPDAT)
    (add_net /PIC16F1829LIN/LBUS)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(U1-Pad12)")
  )
  (net_class Power ""
    (clearance 0.254)
    (trace_width 1.27)
    (via_dia 1.27)
    (via_drill 0.635)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net /E1)
    (add_net /E2)
    (add_net /E3)
    (add_net /E4)
    (add_net /E5)
    (add_net /E6)
    (add_net /E7)
    (add_net /E8)
    (add_net GNDPWR)
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 135.89 141.35 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D2 (at 3.43 0 270) (layer F.SilkS))
    (fp_text value 1N4148W-7-F (at 0 2.1 270) (layer F.Fab))
    (fp_text user %R (at 0 -2 270) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 +12V))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 58AA84FB)
    (at 139.065 140.875 270)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C1 (at 4.54 0 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.25 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 153.67 136.545 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 3.79 0 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fluffy-potato:SOD-323_HandSoldering (layer F.Cu) (tedit 57E36C55)
    (at 151.765 136.74 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D1 (at 2.96 0 270) (layer F.SilkS))
    (fp_text value RSB36V (at 0.1 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.055 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 /PIC16F1829LIN/LBUS))
    (pad 2 smd rect (at 1.055 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
    (model /home/cpriscal/Projets/lin_modules/13a_switch/sod323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module edge-connector-motherboard:TERM_SCREW_M3 (layer F.Cu) (tedit 595A133F)
    (at 133.35 154.94)
    (fp_text reference J1 (at -5.08 -12.7) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x01 (at 0 5) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.5 -3.5) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 1 thru_hole circle (at 2.5 -3.5) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 1 thru_hole circle (at 2.5 3.5) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 1 thru_hole circle (at -2.5 3.5) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 1 +12V))
  )
  (module edge-connector-motherboard:TERM_SCREW_M3 (layer F.Cu) (tedit 595A133F)
    (at 144.78 154.94)
    (fp_text reference J2 (at 0 0) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x01 (at 0 5) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.5 -3.5) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 4 /PIC16F1829LIN/LBUS))
    (pad 1 thru_hole circle (at 2.5 -3.5) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 4 /PIC16F1829LIN/LBUS))
    (pad 1 thru_hole circle (at 2.5 3.5) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 4 /PIC16F1829LIN/LBUS))
    (pad 1 thru_hole circle (at -2.5 3.5) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 4 /PIC16F1829LIN/LBUS))
  )
  (module edge-connector-motherboard:TERM_SCREW_M3 (layer F.Cu) (tedit 595A133F)
    (at 156.21 154.94)
    (fp_text reference J3 (at 0 0) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x01 (at 0 5) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.5 -3.5) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 26 GNDPWR))
    (pad 1 thru_hole circle (at 2.5 -3.5) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 26 GNDPWR))
    (pad 1 thru_hole circle (at 2.5 3.5) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 26 GNDPWR))
    (pad 1 thru_hole circle (at -2.5 3.5) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 26 GNDPWR))
  )
  (module edge-connector-motherboard:TERM_SCREW_M3 (layer F.Cu) (tedit 595A133F)
    (at 133.35 35.56)
    (fp_text reference J4 (at 0 0) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x01 (at 0 5) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.5 -3.5) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 1 thru_hole circle (at 2.5 -3.5) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 1 thru_hole circle (at 2.5 3.5) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 1 thru_hole circle (at -2.5 3.5) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 1 +12V))
  )
  (module edge-connector-motherboard:TERM_SCREW_M3 (layer F.Cu) (tedit 595A133F)
    (at 144.78 35.56)
    (fp_text reference J5 (at 0 0) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x01 (at 0 5) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.5 -3.5) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 4 /PIC16F1829LIN/LBUS))
    (pad 1 thru_hole circle (at 2.5 -3.5) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 4 /PIC16F1829LIN/LBUS))
    (pad 1 thru_hole circle (at 2.5 3.5) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 4 /PIC16F1829LIN/LBUS))
    (pad 1 thru_hole circle (at -2.5 3.5) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 4 /PIC16F1829LIN/LBUS))
  )
  (module edge-connector-motherboard:TERM_SCREW_M3 (layer F.Cu) (tedit 595A133F)
    (at 156.21 35.56)
    (fp_text reference J6 (at 0 0) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x01 (at 0 5) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.5 -3.5) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 26 GNDPWR))
    (pad 1 thru_hole circle (at 2.5 -3.5) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 26 GNDPWR))
    (pad 1 thru_hole circle (at 2.5 3.5) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 26 GNDPWR))
    (pad 1 thru_hole circle (at -2.5 3.5) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 26 GNDPWR))
  )
  (module Pin_Headers:Pin_Header_Angled_2x32_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC7)
    (at 140.97 49.53)
    (descr "Through hole angled pin header, 2x32, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x32 2.54mm double row")
    (fp_text reference J7 (at 5.585 -2.27) (layer F.SilkS))
    (fp_text value CONN_02X32 (at 5.585 81.01) (layer F.Fab))
    (fp_text user %R (at 5.585 -2.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 GNDPWR))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 GNDPWR))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /D1))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /E1))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /E1))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 GNDPWR))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 GNDPWR))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /D2))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /E2))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /E2))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 GNDPWR))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 GNDPWR))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /D3))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 22 thru_hole oval (at 2.54 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 23 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /E3))
    (pad 24 thru_hole oval (at 2.54 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /E3))
    (pad 25 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 GNDPWR))
    (pad 26 thru_hole oval (at 2.54 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 GNDPWR))
    (pad 27 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /D4))
    (pad 28 thru_hole oval (at 2.54 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 29 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 30 thru_hole oval (at 2.54 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 31 thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /E4))
    (pad 32 thru_hole oval (at 2.54 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /E4))
    (pad 33 thru_hole oval (at 0 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 GNDPWR))
    (pad 34 thru_hole oval (at 2.54 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 GNDPWR))
    (pad 35 thru_hole oval (at 0 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /D5))
    (pad 36 thru_hole oval (at 2.54 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 37 thru_hole oval (at 0 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 38 thru_hole oval (at 2.54 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 39 thru_hole oval (at 0 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /E5))
    (pad 40 thru_hole oval (at 2.54 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /E5))
    (pad 41 thru_hole oval (at 0 50.8) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 GNDPWR))
    (pad 42 thru_hole oval (at 2.54 50.8) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 GNDPWR))
    (pad 43 thru_hole oval (at 0 53.34) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /D6))
    (pad 44 thru_hole oval (at 2.54 53.34) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 45 thru_hole oval (at 0 55.88) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 46 thru_hole oval (at 2.54 55.88) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 47 thru_hole oval (at 0 58.42) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /E6))
    (pad 48 thru_hole oval (at 2.54 58.42) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /E6))
    (pad 49 thru_hole oval (at 0 60.96) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 GNDPWR))
    (pad 50 thru_hole oval (at 2.54 60.96) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 GNDPWR))
    (pad 51 thru_hole oval (at 0 63.5) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /D7))
    (pad 52 thru_hole oval (at 2.54 63.5) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 53 thru_hole oval (at 0 66.04) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 54 thru_hole oval (at 2.54 66.04) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 55 thru_hole oval (at 0 68.58) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /E7))
    (pad 56 thru_hole oval (at 2.54 68.58) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /E7))
    (pad 57 thru_hole oval (at 0 71.12) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 GNDPWR))
    (pad 58 thru_hole oval (at 2.54 71.12) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 GNDPWR))
    (pad 59 thru_hole oval (at 0 73.66) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /D8))
    (pad 60 thru_hole oval (at 2.54 73.66) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 61 thru_hole oval (at 0 76.2) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 62 thru_hole oval (at 2.54 76.2) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 63 thru_hole oval (at 0 78.74) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /E8))
    (pad 64 thru_hole oval (at 2.54 78.74) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /E8))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_2x32_Pitch2.54mm.wrl
      (at (xyz 0.05 -1.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module edge-connector-motherboard:TERM_SCREW_M3 (layer F.Cu) (tedit 595A133F)
    (at 133.35 49.53 90)
    (fp_text reference J8 (at 0 0 90) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x01 (at 0 5 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.5 -3.5 90) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 6 /E1))
    (pad 1 thru_hole circle (at 2.5 -3.5 90) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 6 /E1))
    (pad 1 thru_hole circle (at 2.5 3.5 90) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 6 /E1))
    (pad 1 thru_hole circle (at -2.5 3.5 90) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 6 /E1))
  )
  (module edge-connector-motherboard:TERM_SCREW_M3 (layer F.Cu) (tedit 595A133F)
    (at 133.35 60.96 90)
    (fp_text reference J9 (at 0 0 90) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x01 (at 0 5 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.5 -3.5 90) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 8 /E2))
    (pad 1 thru_hole circle (at 2.5 -3.5 90) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 8 /E2))
    (pad 1 thru_hole circle (at 2.5 3.5 90) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 8 /E2))
    (pad 1 thru_hole circle (at -2.5 3.5 90) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 8 /E2))
  )
  (module edge-connector-motherboard:TERM_SCREW_M3 (layer F.Cu) (tedit 595A133F)
    (at 133.35 72.39 90)
    (fp_text reference J10 (at 0 0 90) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x01 (at 0 5 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.5 -3.5 90) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 10 /E3))
    (pad 1 thru_hole circle (at 2.5 -3.5 90) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 10 /E3))
    (pad 1 thru_hole circle (at 2.5 3.5 90) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 10 /E3))
    (pad 1 thru_hole circle (at -2.5 3.5 90) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 10 /E3))
  )
  (module edge-connector-motherboard:TERM_SCREW_M3 (layer F.Cu) (tedit 595A133F)
    (at 133.31 83.82 90)
    (fp_text reference J11 (at 0 0.04 90) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x01 (at 0 5 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.5 -3.5 90) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 12 /E4))
    (pad 1 thru_hole circle (at 2.5 -3.5 90) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 12 /E4))
    (pad 1 thru_hole circle (at 2.5 3.5 90) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 12 /E4))
    (pad 1 thru_hole circle (at -2.5 3.5 90) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 12 /E4))
  )
  (module edge-connector-motherboard:TERM_SCREW_M3 (layer F.Cu) (tedit 595A133F)
    (at 133.35 95.25 90)
    (fp_text reference J12 (at 0 0 90) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x01 (at 0 5 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.5 -3.5 90) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 14 /E5))
    (pad 1 thru_hole circle (at 2.5 -3.5 90) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 14 /E5))
    (pad 1 thru_hole circle (at 2.5 3.5 90) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 14 /E5))
    (pad 1 thru_hole circle (at -2.5 3.5 90) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 14 /E5))
  )
  (module edge-connector-motherboard:TERM_SCREW_M3 (layer F.Cu) (tedit 595A133F)
    (at 133.35 106.68 90)
    (fp_text reference J13 (at 0 0 90) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x01 (at 0 5 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.5 -3.5 90) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 16 /E6))
    (pad 1 thru_hole circle (at 2.5 -3.5 90) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 16 /E6))
    (pad 1 thru_hole circle (at 2.5 3.5 90) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 16 /E6))
    (pad 1 thru_hole circle (at -2.5 3.5 90) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 16 /E6))
  )
  (module edge-connector-motherboard:TERM_SCREW_M3 (layer F.Cu) (tedit 595A133F)
    (at 133.35 118.11 90)
    (fp_text reference J14 (at 0 0 90) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x01 (at 0 5 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.5 -3.5 90) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 18 /E7))
    (pad 1 thru_hole circle (at 2.5 -3.5 90) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 18 /E7))
    (pad 1 thru_hole circle (at 2.5 3.5 90) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 18 /E7))
    (pad 1 thru_hole circle (at -2.5 3.5 90) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 18 /E7))
  )
  (module edge-connector-motherboard:TERM_SCREW_M3 (layer F.Cu) (tedit 595A133F)
    (at 133.35 129.54 90)
    (fp_text reference J15 (at 0 0 90) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x01 (at 0 5 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.5 -3.5 90) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 20 /E8))
    (pad 1 thru_hole circle (at 2.5 -3.5 90) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 20 /E8))
    (pad 1 thru_hole circle (at 2.5 3.5 90) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 20 /E8))
    (pad 1 thru_hole circle (at -2.5 3.5 90) (size 3 3) (drill 1.85) (layers *.Cu *.Mask)
      (net 20 /E8))
  )
  (module Housings_SSOP:SSOP-20_5.3x7.2mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 145.923 139.065 180)
    (descr "20-Lead Plastic Shrink Small Outline (SS)-5.30 mm Body [SSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at 0 -4.75 180) (layer F.SilkS))
    (fp_text value PIC16F1829LIN (at 0 4.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -3.6 -2.925 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at -3.6 -2.275 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 /D1))
    (pad 3 smd rect (at -3.6 -1.625 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 7 /D2))
    (pad 4 smd rect (at -3.6 -0.975 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 21 /PIC16F1829LIN//MCLR))
    (pad 5 smd rect (at -3.6 -0.325 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 9 /D3))
    (pad 6 smd rect (at -3.6 0.325 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 11 /D4))
    (pad 7 smd rect (at -3.6 0.975 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 13 /D5))
    (pad 8 smd rect (at -3.6 1.625 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at -3.6 2.275 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 /PIC16F1829LIN/LBUS))
    (pad 10 smd rect (at -3.6 2.925 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 11 smd rect (at 3.6 2.925 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C1-Pad1)"))
    (pad 12 smd rect (at 3.6 2.275 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U1-Pad12)"))
    (pad 13 smd rect (at 3.6 1.625 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U1-Pad12)"))
    (pad 14 smd rect (at 3.6 0.975 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 15 /D6))
    (pad 15 smd rect (at 3.6 0.325 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 17 /D7))
    (pad 16 smd rect (at 3.6 -0.325 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 19 /D8))
    (pad 17 smd rect (at 3.6 -0.975 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at 3.6 -1.625 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 23 /PIC16F1829LIN/ICSPCLK))
    (pad 19 smd rect (at 3.6 -2.275 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 24 /PIC16F1829LIN/ICSPDAT))
    (pad 20 smd rect (at 3.6 -2.925 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/SSOP-20_5.3x7.2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x05_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 130.81 147.32 180)
    (descr "Through hole angled pin header, 1x05, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x05 2.54mm single row")
    (fp_text reference P3 (at -2.54 -7.62 180) (layer F.SilkS))
    (fp_text value MOLEX-22-28-6050 (at 4.315 12.43 180) (layer F.Fab))
    (fp_text user %R (at 4.315 -2.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /PIC16F1829LIN//MCLR))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /PIC16F1829LIN/ICSPDAT))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /PIC16F1829LIN/ICSPCLK))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_1x05_Pitch2.54mm.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_line (start 127 29.21) (end 127 161.29) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 162.56 29.21) (end 127 29.21) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 162.56 161.29) (end 162.56 29.21) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127 161.29) (end 162.56 161.29) (layer Edge.Cuts) (width 0.15))
)
