(kicad_pcb (version 20171130) (host pcbnew 5.1.7-a382d34a8~87~ubuntu20.04.1)
  (general
    (thickness 1.6)
    (drawings 15)
    (tracks 317)
    (zones 0)
    (modules 8)
    (nets 31)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.18)
    (user_trace_width 0.2032)
    (user_trace_width 0.3048)
    (trace_clearance 0.1524)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.4064)
    (via_drill 0.254)
    (via_min_size 0.4064)
    (via_min_drill 0.254)
    (uvia_size 0.4064)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.4064)
    (uvia_min_drill 0.254)
    (edge_width 0.01)
    (segment_width 0.2032)
    (pcb_text_width 0.254)
    (pcb_text_size 1.2192 1.2192)
    (mod_edge_width 0.1)
    (mod_text_size 0.4572 0.4572)
    (mod_text_width 0.0254)
    (pad_size 1.2 1.2)
    (pad_drill 0.75)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 147.2184 99.187)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Teeprom_GERBER"))
  )
  (net 0 "")
  (net 1 /D3)
  (net 2 /A10)
  (net 3 /D4)
  (net 4 /A7)
  (net 5 /D5)
  (net 6 /A6)
  (net 7 /D6)
  (net 8 /A5)
  (net 9 /D7)
  (net 10 /A4)
  (net 11 /A11)
  (net 12 /A3)
  (net 13 /~OE)
  (net 14 /A2)
  (net 15 /A13)
  (net 16 /A1)
  (net 17 /A0)
  (net 18 /A12)
  (net 19 /D0)
  (net 20 /A9)
  (net 21 /D1)
  (net 22 /A8)
  (net 23 /D2)
  (net 24 /~CE)
  (net 25 /A14)
  (net 26 /~WE)
  (net 27 VCC)
  (net 28 GND)
  (net 29 /A15)
  (net 30 /A16)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.4064)
    (via_drill 0.254)
    (uvia_dia 0.4064)
    (uvia_drill 0.254)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.1524)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A16)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /~CE)
    (add_net /~OE)
    (add_net /~WE)
    (add_net GND)
    (add_net VCC)
  )
  (module 000_LOCAL:SW_DS05-127-2-02BK-SMT-TR (layer Top) (tedit 5FA904DD)
    (at 147.2184 84.187)
    (attr smd)
    (fp_text reference S1 (at 0 0) (layer F.SilkS))
    (fp_text value 2xSPST (at 12.175 3.065) (layer F.Fab))
    (fp_text user 2 (at -1.905 0.635 -90) (layer F.SilkS))
    (fp_text user 1 (at -1.905 -0.635 -90) (layer F.SilkS))
    (fp_text user ON (at 1.905 0 -90) (layer F.SilkS))
    (pad 1B smd roundrect (at 3.81 -0.635) (size 1.27 0.76) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /A15))
    (pad 2B smd roundrect (at 3.81 0.635) (size 1.27 0.76) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 /A16))
    (pad 2A smd roundrect (at -3.81 0.635) (size 1.27 0.76) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 VCC))
    (pad 1A smd roundrect (at -3.81 -0.635) (size 1.27 0.76) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 VCC))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/CUI_DEVICES_DS05-127-2-02BK-SMT-TR.step
      (offset (xyz 9.66 1.1024 -1.5011))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module 000_LOCAL:FlashOpt100_PRG_4x7_female_offset (layer Top) (tedit 5FA8E5A5)
    (at 147.2184 99.187 270)
    (descr "Through hole straight pin header, 2x07, 2.00mm pitch, double rows")
    (tags "Through hole pin header THT 2x07 2.00mm double row")
    (fp_text reference J2 (at 0 6.06 270 unlocked) (layer F.SilkS) hide)
    (fp_text value FlashOpt100_PRG_4x7 (at 0 8 90) (layer F.Fab))
    (fp_text user %R (at 0 6.06 90) (layer F.Fab))
    (pad 21 thru_hole circle (at 9 -0.06 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 /D3))
    (pad 28 thru_hole circle (at 11 -5.94 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 13 /~OE))
    (pad 25 thru_hole circle (at 9 -4.06 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 9 /D7))
    (pad 26 thru_hole circle (at 11 -4.06 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 24 /~CE))
    (pad 23 thru_hole circle (at 9 -1.94 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 /D5))
    (pad 24 thru_hole circle (at 11 -1.94 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 7 /D6))
    (pad 15 thru_hole circle (at 9 6.06 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 16 /A1))
    (pad 22 thru_hole circle (at 11 -0.06 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 /D4))
    (pad 16 thru_hole circle (at 11 6.06 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 17 /A0))
    (pad 27 thru_hole circle (at 9 -5.94 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 /A10))
    (pad 19 thru_hole circle (at 9 2.06 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 23 /D2))
    (pad 20 thru_hole circle (at 11 2.06 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 28 GND))
    (pad 17 thru_hole circle (at 9 3.94 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 19 /D0))
    (pad 18 thru_hole circle (at 11 3.94 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 21 /D1))
    (pad 13 thru_hole circle (at -9 6.06 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 12 /A3))
    (pad 14 thru_hole circle (at -11 6.06 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 14 /A2))
    (pad 11 thru_hole circle (at -9 3.94 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 8 /A5))
    (pad 12 thru_hole circle (at -11 3.94 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 10 /A4))
    (pad 9 thru_hole circle (at -9 2.06 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 /A7))
    (pad 10 thru_hole circle (at -11 2.06 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 6 /A6))
    (pad 7 thru_hole circle (at -9 -0.06 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 27 VCC))
    (pad 8 thru_hole circle (at -11 -0.06 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 18 /A12))
    (pad 5 thru_hole circle (at -9 -1.94 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 25 /A14))
    (pad 6 thru_hole circle (at -11 -1.94 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 26 /~WE))
    (pad 3 thru_hole circle (at -9 -4.06 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 22 /A8))
    (pad 4 thru_hole circle (at -11 -4.06 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 15 /A13))
    (pad 1 thru_hole circle (at -8 -5.94 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 11 /A11))
    (pad 2 thru_hole circle (at -10 -5.94 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 20 /A9))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/PinHeader_2x07_P2.00mm_Vertical.step
      (offset (xyz 9 6 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/PinHeader_2x06_P2.00mm_Vertical.step
      (offset (xyz -11 4 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/PinHeader_2x01_P2.00mm_Vertical.step
      (offset (xyz -10 6 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:TSOP32-14mm (layer Top) (tedit 5F926D8B)
    (at 147.2184 99.187 180)
    (descr "Module CMS TSOP 32 pins")
    (tags "CMS TSOP")
    (attr smd)
    (fp_text reference U1 (at -2.2352 0 270) (layer F.SilkS) hide)
    (fp_text value "29F010 TSOP" (at 0 0 -90) (layer F.SilkS))
    (pad 1 smd roundrect (at -3.75 6.75 180) (size 0.3 1) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /A11))
    (pad 2 smd roundrect (at -3.25 6.75 180) (size 0.3 1) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /A9))
    (pad 3 smd roundrect (at -2.75 6.75 180) (size 0.3 1) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /A8))
    (pad 4 smd roundrect (at -2.25 6.75 180) (size 0.3 1) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /A13))
    (pad 5 smd roundrect (at -1.75 6.75 180) (size 0.3 1) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 /A14))
    (pad 6 smd roundrect (at -1.25 6.75 180) (size 0.3 1) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at -0.75 6.75 180) (size 0.3 1) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 /~WE))
    (pad 8 smd roundrect (at -0.25 6.75 180) (size 0.3 1) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 VCC))
    (pad 9 smd roundrect (at 0.25 6.75 180) (size 0.3 1) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 10 smd roundrect (at 0.75 6.75 180) (size 0.3 1) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 /A16))
    (pad 11 smd roundrect (at 1.25 6.75 180) (size 0.3 1) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /A15))
    (pad 12 smd roundrect (at 1.75 6.75 180) (size 0.3 1) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /A12))
    (pad 13 smd roundrect (at 2.25 6.75 180) (size 0.3 1) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /A7))
    (pad 14 smd roundrect (at 2.75 6.75 180) (size 0.3 1) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /A6))
    (pad 15 smd roundrect (at 3.25 6.75 180) (size 0.3 1) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /A5))
    (pad 16 smd roundrect (at 3.75 6.75 180) (size 0.3 1) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /A4))
    (pad 17 smd roundrect (at 3.75 -6.75 180) (size 0.3 1) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /A3))
    (pad 18 smd roundrect (at 3.25 -6.75 180) (size 0.3 1) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /A2))
    (pad 19 smd roundrect (at 2.75 -6.75 180) (size 0.3 1) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 /A1))
    (pad 20 smd roundrect (at 2.25 -6.75 180) (size 0.3 1) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 /A0))
    (pad 21 smd roundrect (at 1.75 -6.75 180) (size 0.3 1) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /D0))
    (pad 22 smd roundrect (at 1.25 -6.75 180) (size 0.3 1) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /D1))
    (pad 23 smd roundrect (at 0.75 -6.75 180) (size 0.3 1) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 /D2))
    (pad 24 smd roundrect (at 0.25 -6.75 180) (size 0.3 1) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 GND))
    (pad 25 smd roundrect (at -0.25 -6.75 180) (size 0.3 1) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /D3))
    (pad 26 smd roundrect (at -0.75 -6.75 180) (size 0.3 1) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /D4))
    (pad 27 smd roundrect (at -1.25 -6.75 180) (size 0.3 1) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /D5))
    (pad 28 smd roundrect (at -1.75 -6.75 180) (size 0.3 1) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /D6))
    (pad 29 smd roundrect (at -2.25 -6.75 180) (size 0.3 1) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /D7))
    (pad 30 smd roundrect (at -2.75 -6.75 180) (size 0.3 1) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /~CE))
    (pad 31 smd roundrect (at -3.25 -6.75 180) (size 0.3 1) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /A10))
    (pad 32 smd roundrect (at -3.75 -6.75 180) (size 0.3 1) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /~OE))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/TSOP32_8x14.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module 000_LOCAL:pcb2molex8878_chamfer (layer Top) (tedit 5F934572)
    (at 147.2184 99.187)
    (descr "Castellated edge contacts to fit Molex 8878 Socket")
    (solder_mask_margin -0.28)
    (attr virtual)
    (fp_text reference carrier? (at -1.5 0 -90) (layer Dwgs.User) hide)
    (fp_text value pcb2molex8878_chamfer (at 2.23 -9.45 -90) (layer F.Fab) hide)
    (fp_text user "10.0 x 1.0 retainer wedges on top surface" (at -0.24 -17.41) (layer Dwgs.User))
    (fp_text user "36.6 x 14.4 x 1.4 - backside pocket" (at -2.29 -16.93) (layer Dwgs.User))
    (fp_text user "Eco2.User is Edge.Cuts for use with \"pcb2molex8878_chamfer\" carrier." (at -0.05 13.65) (layer Eco2.User))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/pcb2molex8878_chamfer.step
      (offset (xyz 0 0 -0.2))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module 000_LOCAL:pcb2molex8878 (layer Top) (tedit 5F934421)
    (at 147.2184 99.187)
    (descr "Castellated edge contacts to fit Molex 8878 Socket")
    (solder_mask_margin -0.28)
    (attr virtual)
    (fp_text reference J1 (at -0.9906 -0.9906 -90) (layer Dwgs.User) hide)
    (fp_text value Tandy_100_102_200_option_rom (at 2.0701 -8.8773 -90) (layer F.Fab) hide)
    (fp_text user "Eco1.User is Edge.Cuts for use without carrier." (at -0.0298 12.25) (layer Eco1.User))
    (pad 28 thru_hole roundrect (at 8.6 -16.51 180) (size 1.8 1.6) (drill 1.6 (offset 0.1 0)) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 25 /A14) (solder_mask_margin -0.19))
    (pad 14 thru_hole roundrect (at -8.6 16.51) (size 1.8 1.6) (drill 1.6 (offset 0.1 0)) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 28 GND) (solder_mask_margin -0.19))
    (pad 27 thru_hole roundrect (at 8.6 -13.97 180) (size 1.8 1.6) (drill 1.6 (offset 0.1 0)) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 24 /~CE) (solder_mask_margin -0.19))
    (pad 13 thru_hole roundrect (at -8.6 13.97) (size 1.8 1.6) (drill 1.6 (offset 0.1 0)) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 23 /D2) (solder_mask_margin -0.19))
    (pad 26 thru_hole roundrect (at 8.6 -11.43 180) (size 1.8 1.6) (drill 1.6 (offset 0.1 0)) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 22 /A8) (solder_mask_margin -0.19))
    (pad 12 thru_hole roundrect (at -8.6 11.43) (size 1.8 1.6) (drill 1.6 (offset 0.1 0)) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 21 /D1) (solder_mask_margin -0.19))
    (pad 25 thru_hole roundrect (at 8.6 -8.89 180) (size 1.8 1.6) (drill 1.6 (offset 0.1 0)) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 20 /A9) (solder_mask_margin -0.19))
    (pad 11 thru_hole roundrect (at -8.6 8.89) (size 1.8 1.6) (drill 1.6 (offset 0.1 0)) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 19 /D0) (solder_mask_margin -0.19))
    (pad 24 thru_hole roundrect (at 8.6 -6.35 180) (size 1.8 1.6) (drill 1.6 (offset 0.1 0)) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 18 /A12) (solder_mask_margin -0.19))
    (pad 10 thru_hole roundrect (at -8.6 6.35) (size 1.8 1.6) (drill 1.6 (offset 0.1 0)) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 17 /A0) (solder_mask_margin -0.19))
    (pad 23 thru_hole roundrect (at 8.6 -3.81 180) (size 1.8 1.6) (drill 1.6 (offset 0.1 0)) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (solder_mask_margin -0.19))
    (pad 9 thru_hole roundrect (at -8.6 3.81) (size 1.8 1.6) (drill 1.6 (offset 0.1 0)) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 16 /A1) (solder_mask_margin -0.19))
    (pad 22 thru_hole roundrect (at 8.6 -1.27 180) (size 1.8 1.6) (drill 1.6 (offset 0.1 0)) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 15 /A13) (solder_mask_margin -0.19))
    (pad 8 thru_hole roundrect (at -8.6 1.27) (size 1.8 1.6) (drill 1.6 (offset 0.1 0)) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 14 /A2) (solder_mask_margin -0.19))
    (pad 21 thru_hole roundrect (at 8.6 1.27 180) (size 1.8 1.6) (drill 1.6 (offset 0.1 0)) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 13 /~OE) (solder_mask_margin -0.19))
    (pad 7 thru_hole roundrect (at -8.6 -1.27) (size 1.8 1.6) (drill 1.6 (offset 0.1 0)) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 12 /A3) (solder_mask_margin -0.19))
    (pad 20 thru_hole roundrect (at 8.6 3.81 180) (size 1.8 1.6) (drill 1.6 (offset 0.1 0)) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 11 /A11) (solder_mask_margin -0.19))
    (pad 6 thru_hole roundrect (at -8.6 -3.81) (size 1.8 1.6) (drill 1.6 (offset 0.1 0)) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 10 /A4) (solder_mask_margin -0.19))
    (pad 19 thru_hole roundrect (at 8.6 6.35 180) (size 1.8 1.6) (drill 1.6 (offset 0.1 0)) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 9 /D7) (solder_mask_margin -0.19))
    (pad 5 thru_hole roundrect (at -8.6 -6.35) (size 1.8 1.6) (drill 1.6 (offset 0.1 0)) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 8 /A5) (solder_mask_margin -0.19))
    (pad 18 thru_hole roundrect (at 8.6 8.89 180) (size 1.8 1.6) (drill 1.6 (offset 0.1 0)) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 7 /D6) (solder_mask_margin -0.19))
    (pad 4 thru_hole roundrect (at -8.6 -8.89) (size 1.8 1.6) (drill 1.6 (offset 0.1 0)) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 6 /A6) (solder_mask_margin -0.19))
    (pad 17 thru_hole roundrect (at 8.6 11.43 180) (size 1.8 1.6) (drill 1.6 (offset 0.1 0)) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 5 /D5) (solder_mask_margin -0.19))
    (pad 3 thru_hole roundrect (at -8.6 -11.43) (size 1.8 1.6) (drill 1.6 (offset 0.1 0)) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 4 /A7) (solder_mask_margin -0.19))
    (pad 16 thru_hole roundrect (at 8.6 13.97 180) (size 1.8 1.6) (drill 1.6 (offset 0.1 0)) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 3 /D4) (solder_mask_margin -0.19))
    (pad 2 thru_hole roundrect (at -8.6 -13.97) (size 1.8 1.6) (drill 1.6 (offset 0.1 0)) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 2 /A10) (solder_mask_margin -0.19))
    (pad 15 thru_hole roundrect (at 8.6 16.51 180) (size 1.8 1.6) (drill 1.6 (offset 0.1 0)) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 1 /D3) (solder_mask_margin -0.19))
    (pad 1 thru_hole roundrect (at -8.6 -16.51) (size 1.8 1.6) (drill 1.6 (offset 0.1 0)) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 27 VCC) (solder_mask_margin -0.19))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/pcb2molex8878_chamfer.step_x
      (offset (xyz 0 0 -0.23))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module 000_LOCAL:R_0805_2012Metric (layer Top) (tedit 5FA8AD18)
    (at 151.9684 86.187 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 0 -90 unlocked) (layer F.SilkS))
    (fp_text value 47k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 30 /A16))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 28 GND))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/R_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:R_0805_2012Metric (layer Top) (tedit 5FA8AE89)
    (at 151.9684 82.187 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 0 -90 unlocked) (layer F.SilkS))
    (fp_text value 47k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 29 /A15))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 28 GND))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/R_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:R_0805_2012Metric (layer Top) (tedit 5F92312E)
    (at 152.4684 94.437 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 0 unlocked) (layer F.SilkS))
    (fp_text value 47k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 26 /~WE))
    (pad 1 smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 27 VCC))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/R_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 1 (at 140.2184 82.687) (layer F.SilkS))
  (gr_text FlashOpt100 (at 152.7184 101.687 -90) (layer F.SilkS))
  (gr_text ROM (at 143.9684 113.437 -90) (layer F.SilkS))
  (gr_text Select (at 142.4684 113.437 -90) (layer F.SilkS))
  (gr_text Select (at 141.9684 84.187 -90) (layer F.SilkS))
  (gr_text "1 [ ][ ]\n2 [ ][x]\n3 [x][ ]\n4 [x][x]" (at 147.2184 113.437 -90) (layer F.SilkS))
  (gr_text "4 x Option Rom" (at 140.7184 99.187 -90) (layer F.SilkS))
  (gr_line (start 141.1184 80.187) (end 155.2184 80.187) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 155.2184 118.187) (end 139.2184 118.187) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 155.2184 80.187) (end 155.2184 118.187) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 139.2184 82.087) (end 141.1184 80.187) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 139.2184 118.187) (end 139.2184 82.087) (layer Edge.Cuts) (width 0.01))
  (gr_text tandy.wiki/Teeprom (at 147.2184 116.437) (layer F.SilkS))
  (gr_text "Tandy 100/102/200" (at 142.2184 99.187 -90) (layer F.SilkS))
  (gr_text "R1,R2,R3: 47k" (at 140.7184 114.187 -270) (layer B.SilkS))
)
