(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 4.69)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (1 "In1.Cu" signal)
    (2 "In2.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In1.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 2" (type "prepreg") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In2.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 3" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 87.72 61.7)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "+5V")
  (net 2 "/AO0")
  (net 3 "/AI0")
  (net 4 "/AO1")
  (net 5 "/AI1")
  (net 6 "GNDA")
  (net 7 "/AI2")
  (net 8 "GND")
  (net 9 "/AI3")
  (net 10 "/UART_RX")
  (net 11 "/DIO0{slash}PWM0")
  (net 12 "/DIO1{slash}PWM1")
  (net 13 "/UART_TX")
  (net 14 "/DIO2{slash}PWM2")
  (net 15 "/DIO3{slash}PWM3")
  (net 16 "/DIO11{slash}PWM7")
  (net 17 "/DIO4{slash}SPI_CS")
  (net 18 "/DIO5{slash}SPI_CLK")
  (net 19 "/DIO12{slash}PWM8")
  (net 20 "/DIO6{slash}SPI_MISO")
  (net 21 "/DIO7{slash}SPI_MOSI")
  (net 22 "/DIO13{slash}PWM9")
  (net 23 "/DIO8{slash}PWM4")
  (net 24 "/DIO9{slash}PWM5")
  (net 25 "/DIO10{slash}PWM6")
  (net 26 "/DIO14{slash}I2C_SCL")
  (net 27 "+3.3V")
  (net 28 "/DIO15{slash}I2C_SDA")
  (net 29 "Net-(D1-Pad1)")
  (net 30 "Net-(D1-Pad2)")
  (net 31 "Net-(D2-Pad1)")
  (net 32 "Net-(D2-Pad2)")
  (net 33 "Net-(D3-Pad1)")
  (net 34 "Net-(D3-Pad2)")
  (net 35 "Net-(D4-Pad1)")
  (net 36 "Net-(D4-Pad2)")
  (net 37 "Net-(D5-Pad1)")
  (net 38 "Net-(D5-Pad2)")
  (net 39 "Net-(D6-Pad1)")
  (net 40 "Net-(D6-Pad2)")
  (net 41 "Net-(D7-Pad1)")
  (net 42 "Net-(D7-Pad2)")
  (net 43 "Net-(D8-Pad1)")
  (net 44 "Net-(D8-Pad2)")
  (net 45 "Net-(D9-Pad1)")
  (net 46 "Net-(D9-Pad2)")
  (net 47 "Net-(D10-Pad1)")
  (net 48 "Net-(D10-Pad2)")
  (net 49 "Net-(D11-Pad1)")
  (net 50 "Net-(D11-Pad2)")
  (net 51 "Net-(D12-Pad1)")
  (net 52 "Net-(D12-Pad2)")
  (net 53 "Net-(D19-Pad1)")
  (net 54 "Net-(D19-Pad2)")
  (net 55 "Net-(D20-Pad1)")
  (net 56 "Net-(D20-Pad2)")
  (net 57 "Net-(D21-Pad1)")
  (net 58 "Net-(D21-Pad2)")
  (net 59 "Net-(D22-Pad1)")
  (net 60 "Net-(D22-Pad2)")
  (net 61 "Net-(P1-Pad2)")
  (net 62 "Net-(P2-Pad2)")
  (net 63 "Net-(P3-Pad2)")
  (net 64 "Net-(P4-Pad2)")
  (net 65 "Net-(P5-Pad2)")
  (net 66 "Net-(P6-Pad2)")
  (net 67 "Net-(P7-Pad2)")
  (net 68 "Net-(P8-Pad2)")
  (net 69 "Net-(P9-Pad2)")
  (net 70 "Net-(P10-Pad2)")
  (net 71 "Net-(P11-Pad2)")
  (net 72 "Net-(P12-Pad2)")
  (net 73 "Net-(P13-Pad2)")
  (net 74 "Net-(P14-Pad2)")
  (net 75 "Net-(P15-Pad2)")
  (net 76 "Net-(P16-Pad2)")
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (tedit 587A3A7B)
    (at 97.3328 126.4412 -90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D22" (at 4.572 -0.508 180) (layer "F.SilkS"))
    (fp_text value "Red" (at 1.27 2.96 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 59 "Net-(D22-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 60 "Net-(D22-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (tedit 587A3A7B)
    (at 171.2468 39.9796 -90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D7" (at -1.8288 -0.0508 180) (layer "F.SilkS"))
    (fp_text value "Green" (at 1.27 2.96 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 41 "Net-(D7-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 42 "Net-(D7-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library Loader:705550037" (layer "F.Cu")
    (tedit 0)
    (at 111.252 99.7204 180)
    (descr "70555-0037-1")
    (tags "Connector")
    (property "Description" "2.54mm Pitch SL Wire-to-Board Header, Low Profile, Surface Mount, Single Row, Right-Angle, 3.05mm Pocket, Shrouded, with Press-fit Plastic Peg,  Circuits, Tin (Sn) Plating, Embossed Tape Packaging")
    (property "Height" "7.38")
    (property "Manufacturer_Name" "Molex")
    (property "Manufacturer_Part_Number" "15-91-7030")
    (property "Mouser Part Number" "538-15-91-7030")
    (property "Mouser Price/Stock" "https://www.mouser.com/Search/Refine.aspx?Keyword=538-15-91-7030")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P16" (at -2.54 6.061) (layer "F.SilkS"))
    (fp_text value "70555-0037" (at -2.54 6.061) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at -2.54 6.061) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 1.4 8.64 180) (size 3.4 3.4) (drill 3.4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -6.48 8.64 180) (size 3.4 3.4) (drill 3.4) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 6 "GNDA") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -2.54 0 180) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 76 "Net-(P16-Pad2)") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -5.08 0 180) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 9 "/AI3") (pintype "passive"))
    (model "C:\\Users\\Don Koch\\Documents\\KiCad\\6.0\\SamacSys_Parts.3dshapes\\70555-0037.stp"
      (offset (xyz -2.539999924 -7.139999759 2.400000059))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Library Loader:705550037" (layer "F.Cu")
    (tedit 0)
    (at 176.8693 81.9404 90)
    (descr "70555-0037-1")
    (tags "Connector")
    (property "Description" "2.54mm Pitch SL Wire-to-Board Header, Low Profile, Surface Mount, Single Row, Right-Angle, 3.05mm Pocket, Shrouded, with Press-fit Plastic Peg,  Circuits, Tin (Sn) Plating, Embossed Tape Packaging")
    (property "Height" "7.38")
    (property "Manufacturer_Name" "Molex")
    (property "Manufacturer_Part_Number" "15-91-7030")
    (property "Mouser Part Number" "538-15-91-7030")
    (property "Mouser Price/Stock" "https://www.mouser.com/Search/Refine.aspx?Keyword=538-15-91-7030")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P4" (at -2.54 6.061 90) (layer "F.SilkS"))
    (fp_text value "70555-0037" (at -2.54 6.061 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at -2.54 6.061 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 1.4 8.64 90) (size 3.4 3.4) (drill 3.4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -6.48 8.64 90) (size 3.4 3.4) (drill 3.4) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 8 "GND") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -2.54 0 90) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 64 "Net-(P4-Pad2)") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -5.08 0 90) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 15 "/DIO3{slash}PWM3") (pintype "passive"))
    (model "C:\\Users\\Don Koch\\Documents\\KiCad\\6.0\\SamacSys_Parts.3dshapes\\70555-0037.stp"
      (offset (xyz -2.539999924 -7.139999759 2.400000059))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Library Loader:705550037" (layer "F.Cu")
    (tedit 0)
    (at 176.911 125.1712 90)
    (descr "70555-0037-1")
    (tags "Connector")
    (property "Description" "2.54mm Pitch SL Wire-to-Board Header, Low Profile, Surface Mount, Single Row, Right-Angle, 3.05mm Pocket, Shrouded, with Press-fit Plastic Peg,  Circuits, Tin (Sn) Plating, Embossed Tape Packaging")
    (property "Height" "7.38")
    (property "Manufacturer_Name" "Molex")
    (property "Manufacturer_Part_Number" "15-91-7030")
    (property "Mouser Part Number" "538-15-91-7030")
    (property "Mouser Price/Stock" "https://www.mouser.com/Search/Refine.aspx?Keyword=538-15-91-7030")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P1" (at -2.54 6.061 90) (layer "F.SilkS"))
    (fp_text value "70555-0037" (at -2.54 6.061 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at -2.54 6.061 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -6.48 8.64 90) (size 3.4 3.4) (drill 3.4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 1.4 8.64 90) (size 3.4 3.4) (drill 3.4) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 8 "GND") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -2.54 0 90) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 61 "Net-(P1-Pad2)") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -5.08 0 90) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 11 "/DIO0{slash}PWM0") (pintype "passive"))
    (model "C:\\Users\\Don Koch\\Documents\\KiCad\\6.0\\SamacSys_Parts.3dshapes\\70555-0037.stp"
      (offset (xyz -2.539999924 -7.139999759 2.400000059))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Library Loader:705550037" (layer "F.Cu")
    (tedit 0)
    (at 176.8693 53.2384 90)
    (descr "70555-0037-1")
    (tags "Connector")
    (property "Description" "2.54mm Pitch SL Wire-to-Board Header, Low Profile, Surface Mount, Single Row, Right-Angle, 3.05mm Pocket, Shrouded, with Press-fit Plastic Peg,  Circuits, Tin (Sn) Plating, Embossed Tape Packaging")
    (property "Height" "7.38")
    (property "Manufacturer_Name" "Molex")
    (property "Manufacturer_Part_Number" "15-91-7030")
    (property "Mouser Part Number" "538-15-91-7030")
    (property "Mouser Price/Stock" "https://www.mouser.com/Search/Refine.aspx?Keyword=538-15-91-7030")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P6" (at -2.54 6.061 90) (layer "F.SilkS"))
    (fp_text value "70555-0037" (at -2.54 6.061 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at -2.54 6.061 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -6.48 8.64 90) (size 3.4 3.4) (drill 3.4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 1.4 8.64 90) (size 3.4 3.4) (drill 3.4) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 8 "GND") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -2.54 0 90) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 66 "Net-(P6-Pad2)") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -5.08 0 90) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 18 "/DIO5{slash}SPI_CLK") (pintype "passive"))
    (model "C:\\Users\\Don Koch\\Documents\\KiCad\\6.0\\SamacSys_Parts.3dshapes\\70555-0037.stp"
      (offset (xyz -2.539999924 -7.139999759 2.400000059))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "" locked (layer "F.Cu")
    (tedit 0)
    (at 159.0676 38.648 180)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle locked (at -0.125806 0.207518 180) (size 3.81 3.81) (drill 3.81) (layers F&B.Cu *.Mask))
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (tedit 587A3A7B)
    (at 171.704 126.3904 -90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D1" (at -1.9812 0 180) (layer "F.SilkS"))
    (fp_text value "Green" (at 1.27 2.96 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 29 "Net-(D1-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 30 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library Loader:705550038" locked (layer "F.Cu")
    (tedit 0)
    (at 92.3584 129.42 -90)
    (descr "70555-0038-2")
    (tags "Connector")
    (property "Description" "2.54mm Pitch SL Wire-to-Board Header, Low Profile, Surface Mount, Single Row, Right-Angle, 3.05mm Pocket, Shrouded, with Press-fit Plastic Peg,  Circuits, Tin (Sn) Plating, Embossed Tape Packaging")
    (property "Height" "7.38")
    (property "Manufacturer_Name" "Molex")
    (property "Manufacturer_Part_Number" "15-91-7030")
    (property "Mouser Part Number" "538-15-91-7030")
    (property "Mouser Price/Stock" "https://www.mouser.com/Search/Refine.aspx?Keyword=538-15-91-7030")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P12" (at -1.8796 5.1674 90) (layer "F.SilkS"))
    (fp_text value "70555-0038" (at -3.81 6.031 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at -3.81 6.031 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 1.39 8.64 270) (size 3.45 3.45) (drill 3.45) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -9.01 8.64 270) (size 3.45 3.45) (drill 3.45) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.755 1.755) (drill 1.17) (layers *.Cu *.Mask)
      (net 8 "GND") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -2.54 0 270) (size 1.755 1.755) (drill 1.17) (layers *.Cu *.Mask)
      (net 72 "Net-(P12-Pad2)") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -5.08 0 270) (size 1.755 1.755) (drill 1.17) (layers *.Cu *.Mask)
      (net 28 "/DIO15{slash}I2C_SDA") (pintype "passive"))
    (pad "4" thru_hole circle locked (at -7.62 0 270) (size 1.755 1.755) (drill 1.17) (layers *.Cu *.Mask)
      (net 26 "/DIO14{slash}I2C_SCL") (pintype "passive"))
    (model "C:\\Users\\Don Koch\\Documents\\KiCad\\6.0\\SamacSys_Parts.3dshapes\\70555-0038.stp"
      (offset (xyz -3.809999886 -7.110000027 2.79999991))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (tedit 587A3A7B)
    (at 97.3988 76.7126 -90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D19" (at 4.4658 -0.5944 180) (layer "F.SilkS"))
    (fp_text value "Red" (at 1.27 2.96 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 53 "Net-(D19-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 54 "Net-(D19-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library Loader:705550037" (layer "F.Cu")
    (tedit 0)
    (at 125.222 99.7204 180)
    (descr "70555-0037-1")
    (tags "Connector")
    (property "Description" "2.54mm Pitch SL Wire-to-Board Header, Low Profile, Surface Mount, Single Row, Right-Angle, 3.05mm Pocket, Shrouded, with Press-fit Plastic Peg,  Circuits, Tin (Sn) Plating, Embossed Tape Packaging")
    (property "Height" "7.38")
    (property "Manufacturer_Name" "Molex")
    (property "Manufacturer_Part_Number" "15-91-7030")
    (property "Mouser Part Number" "538-15-91-7030")
    (property "Mouser Price/Stock" "https://www.mouser.com/Search/Refine.aspx?Keyword=538-15-91-7030")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P15" (at -2.54 6.061) (layer "F.SilkS"))
    (fp_text value "70555-0037" (at -2.54 6.061) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at -2.54 6.061) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -6.48 8.64 180) (size 3.4 3.4) (drill 3.4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 1.4 8.64 180) (size 3.4 3.4) (drill 3.4) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 6 "GNDA") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -2.54 0 180) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 75 "Net-(P15-Pad2)") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -5.08 0 180) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 7 "/AI2") (pintype "passive"))
    (model "C:\\Users\\Don Koch\\Documents\\KiCad\\6.0\\SamacSys_Parts.3dshapes\\70555-0037.stp"
      (offset (xyz -2.539999924 -7.139999759 2.400000059))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (tedit 587A3A7B)
    (at 98.1964 104.5414 -90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D11" (at -1.8238 0 180) (layer "F.SilkS"))
    (fp_text value "Green" (at 1.27 2.96 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 49 "Net-(D11-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 50 "Net-(D11-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library Loader:705550038" locked (layer "F.Cu")
    (tedit 0)
    (at 92.3584 79.1788 -90)
    (descr "70555-0038-2")
    (tags "Connector")
    (property "Description" "2.54mm Pitch SL Wire-to-Board Header, Low Profile, Surface Mount, Single Row, Right-Angle, 3.05mm Pocket, Shrouded, with Press-fit Plastic Peg,  Circuits, Tin (Sn) Plating, Embossed Tape Packaging")
    (property "Height" "7.38")
    (property "Manufacturer_Name" "Molex")
    (property "Manufacturer_Part_Number" "15-91-7030")
    (property "Mouser Part Number" "538-15-91-7030")
    (property "Mouser Price/Stock" "https://www.mouser.com/Search/Refine.aspx?Keyword=538-15-91-7030")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P9" (at -3.81 6.031 90) (layer "F.SilkS"))
    (fp_text value "70555-0038" (at -3.81 6.031 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at -3.81 6.031 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -9.01 8.64 270) (size 3.45 3.45) (drill 3.45) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 1.39 8.64 270) (size 3.45 3.45) (drill 3.45) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.755 1.755) (drill 1.17) (layers *.Cu *.Mask)
      (net 8 "GND") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -2.54 0 270) (size 1.755 1.755) (drill 1.17) (layers *.Cu *.Mask)
      (net 69 "Net-(P9-Pad2)") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -5.08 0 270) (size 1.755 1.755) (drill 1.17) (layers *.Cu *.Mask)
      (net 24 "/DIO9{slash}PWM5") (pintype "passive"))
    (pad "4" thru_hole circle locked (at -7.62 0 270) (size 1.755 1.755) (drill 1.17) (layers *.Cu *.Mask)
      (net 23 "/DIO8{slash}PWM4") (pintype "passive"))
    (model "C:\\Users\\Don Koch\\Documents\\KiCad\\6.0\\SamacSys_Parts.3dshapes\\70555-0038.stp"
      (offset (xyz -3.809999886 -7.110000027 2.79999991))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Library Loader:705550037" (layer "F.Cu")
    (tedit 0)
    (at 139.192 99.7204 180)
    (descr "70555-0037-1")
    (tags "Connector")
    (property "Description" "2.54mm Pitch SL Wire-to-Board Header, Low Profile, Surface Mount, Single Row, Right-Angle, 3.05mm Pocket, Shrouded, with Press-fit Plastic Peg,  Circuits, Tin (Sn) Plating, Embossed Tape Packaging")
    (property "Height" "7.38")
    (property "Manufacturer_Name" "Molex")
    (property "Manufacturer_Part_Number" "15-91-7030")
    (property "Mouser Part Number" "538-15-91-7030")
    (property "Mouser Price/Stock" "https://www.mouser.com/Search/Refine.aspx?Keyword=538-15-91-7030")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P14" (at -2.54 6.061) (layer "F.SilkS"))
    (fp_text value "70555-0037" (at -2.54 6.061) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at -2.54 6.061) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -6.48 8.64 180) (size 3.4 3.4) (drill 3.4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 1.4 8.64 180) (size 3.4 3.4) (drill 3.4) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 6 "GNDA") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -2.54 0 180) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 74 "Net-(P14-Pad2)") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -5.08 0 180) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 5 "/AI1") (pintype "passive"))
    (model "C:\\Users\\Don Koch\\Documents\\KiCad\\6.0\\SamacSys_Parts.3dshapes\\70555-0037.stp"
      (offset (xyz -2.539999924 -7.139999759 2.400000059))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (tedit 587A3A7B)
    (at 97.536 51.7144 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D8" (at 4.4704 -0.1524 180) (layer "F.SilkS"))
    (fp_text value "Green" (at 1.27 2.96 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 43 "Net-(D8-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 44 "Net-(D8-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (tedit 587A3A7B)
    (at 171.3992 83.2612 -90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D4" (at -1.8796 -0.1016 180) (layer "F.SilkS"))
    (fp_text value "Green" (at 1.27 2.96 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 35 "Net-(D4-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 36 "Net-(D4-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (tedit 587A3A7B)
    (at 171.1452 69.1388 -90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D5" (at -1.9812 -0.0508 180) (layer "F.SilkS"))
    (fp_text value "Green" (at 1.27 2.96 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 37 "Net-(D5-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 38 "Net-(D5-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (tedit 587A3A7B)
    (at 97.1296 87.9856 -90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D10" (at -1.8288 0.0508 180) (layer "F.SilkS"))
    (fp_text value "Green" (at 1.27 2.96 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 47 "Net-(D10-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 48 "Net-(D10-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (tedit 587A3A7B)
    (at 171.3484 54.2036 -90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D6" (at -1.8796 -0.0508 180) (layer "F.SilkS"))
    (fp_text value "Green" (at 1.27 2.96 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 39 "Net-(D6-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 40 "Net-(D6-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library Loader:705550037" (layer "F.Cu")
    (tedit 0)
    (at 92.7263 52.5272 -90)
    (descr "70555-0037-1")
    (tags "Connector")
    (property "Description" "2.54mm Pitch SL Wire-to-Board Header, Low Profile, Surface Mount, Single Row, Right-Angle, 3.05mm Pocket, Shrouded, with Press-fit Plastic Peg,  Circuits, Tin (Sn) Plating, Embossed Tape Packaging")
    (property "Height" "7.38")
    (property "Manufacturer_Name" "Molex")
    (property "Manufacturer_Part_Number" "15-91-7030")
    (property "Mouser Part Number" "538-15-91-7030")
    (property "Mouser Price/Stock" "https://www.mouser.com/Search/Refine.aspx?Keyword=538-15-91-7030")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P8" (at -2.54 6.061 90) (layer "F.SilkS"))
    (fp_text value "70555-0037" (at -2.54 6.061 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at -2.54 6.061 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -6.48 8.64 270) (size 3.4 3.4) (drill 3.4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 1.4 8.64 270) (size 3.4 3.4) (drill 3.4) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 8 "GND") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -2.54 0 270) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 68 "Net-(P8-Pad2)") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -5.08 0 270) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 21 "/DIO7{slash}SPI_MOSI") (pintype "passive"))
    (model "C:\\Users\\Don Koch\\Documents\\KiCad\\6.0\\SamacSys_Parts.3dshapes\\70555-0037.stp"
      (offset (xyz -2.539999924 -7.139999759 2.400000059))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (tedit 587A3A7B)
    (at 98.1964 110.0278 -90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D21" (at 4.3738 0.0508 180) (layer "F.SilkS"))
    (fp_text value "Red" (at 1.27 2.96 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 57 "Net-(D21-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 58 "Net-(D21-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "" locked (layer "F.Cu")
    (tedit 0)
    (at 109.8042 38.6334 180)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" np_thru_hole circle locked (at 0.242392 0.192918 180) (size 3.81 3.81) (drill 3.81) (layers F&B.Cu *.Mask))
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (tedit 587A3A7B)
    (at 97.3328 120.8532 -90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D12" (at -1.9304 0.0508 180) (layer "F.SilkS"))
    (fp_text value "Green" (at 1.27 2.96 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 51 "Net-(D12-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 52 "Net-(D12-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library Loader:705550037" (layer "F.Cu")
    (tedit 0)
    (at 176.8693 67.7164 90)
    (descr "70555-0037-1")
    (tags "Connector")
    (property "Description" "2.54mm Pitch SL Wire-to-Board Header, Low Profile, Surface Mount, Single Row, Right-Angle, 3.05mm Pocket, Shrouded, with Press-fit Plastic Peg,  Circuits, Tin (Sn) Plating, Embossed Tape Packaging")
    (property "Height" "7.38")
    (property "Manufacturer_Name" "Molex")
    (property "Manufacturer_Part_Number" "15-91-7030")
    (property "Mouser Part Number" "538-15-91-7030")
    (property "Mouser Price/Stock" "https://www.mouser.com/Search/Refine.aspx?Keyword=538-15-91-7030")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P5" (at -2.54 6.061 90) (layer "F.SilkS"))
    (fp_text value "70555-0037" (at -2.54 6.061 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at -2.54 6.061 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -6.48 8.64 90) (size 3.4 3.4) (drill 3.4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 1.4 8.64 90) (size 3.4 3.4) (drill 3.4) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 8 "GND") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -2.54 0 90) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 65 "Net-(P5-Pad2)") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -5.08 0 90) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 17 "/DIO4{slash}SPI_CS") (pintype "passive"))
    (model "C:\\Users\\Don Koch\\Documents\\KiCad\\6.0\\SamacSys_Parts.3dshapes\\70555-0037.stp"
      (offset (xyz -2.539999924 -7.139999759 2.400000059))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Library Loader:705550037" (layer "F.Cu")
    (tedit 0)
    (at 176.8693 38.7604 90)
    (descr "70555-0037-1")
    (tags "Connector")
    (property "Description" "2.54mm Pitch SL Wire-to-Board Header, Low Profile, Surface Mount, Single Row, Right-Angle, 3.05mm Pocket, Shrouded, with Press-fit Plastic Peg,  Circuits, Tin (Sn) Plating, Embossed Tape Packaging")
    (property "Height" "7.38")
    (property "Manufacturer_Name" "Molex")
    (property "Manufacturer_Part_Number" "15-91-7030")
    (property "Mouser Part Number" "538-15-91-7030")
    (property "Mouser Price/Stock" "https://www.mouser.com/Search/Refine.aspx?Keyword=538-15-91-7030")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P7" (at -2.54 6.061 90) (layer "F.SilkS"))
    (fp_text value "70555-0037" (at -2.54 6.061 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at -2.54 6.061 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -6.48 8.64 90) (size 3.4 3.4) (drill 3.4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 1.4 8.64 90) (size 3.4 3.4) (drill 3.4) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 8 "GND") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -2.54 0 90) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 67 "Net-(P7-Pad2)") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -5.08 0 90) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 20 "/DIO6{slash}SPI_MISO") (pintype "passive"))
    (model "C:\\Users\\Don Koch\\Documents\\KiCad\\6.0\\SamacSys_Parts.3dshapes\\70555-0037.stp"
      (offset (xyz -2.539999924 -7.139999759 2.400000059))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (tedit 587A3A7B)
    (at 97.3836 71.12 -90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D9" (at -1.778 0.1016 180) (layer "F.SilkS"))
    (fp_text value "Green" (at 1.27 2.96 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 45 "Net-(D9-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 46 "Net-(D9-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (tedit 587A3A7B)
    (at 171.2976 97.3836 -90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D3" (at -1.8796 -0.0508 180) (layer "F.SilkS"))
    (fp_text value "Green" (at 1.27 2.96 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 33 "Net-(D3-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 34 "Net-(D3-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library Loader:705550037" (layer "F.Cu")
    (tedit 0)
    (at 176.8693 96.4184 90)
    (descr "70555-0037-1")
    (tags "Connector")
    (property "Description" "2.54mm Pitch SL Wire-to-Board Header, Low Profile, Surface Mount, Single Row, Right-Angle, 3.05mm Pocket, Shrouded, with Press-fit Plastic Peg,  Circuits, Tin (Sn) Plating, Embossed Tape Packaging")
    (property "Height" "7.38")
    (property "Manufacturer_Name" "Molex")
    (property "Manufacturer_Part_Number" "15-91-7030")
    (property "Mouser Part Number" "538-15-91-7030")
    (property "Mouser Price/Stock" "https://www.mouser.com/Search/Refine.aspx?Keyword=538-15-91-7030")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P3" (at -2.54 6.061 90) (layer "F.SilkS"))
    (fp_text value "70555-0037" (at -2.54 6.061 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at -2.54 6.061 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -6.48 8.64 90) (size 3.4 3.4) (drill 3.4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 1.4 8.64 90) (size 3.4 3.4) (drill 3.4) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 8 "GND") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -2.54 0 90) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 63 "Net-(P3-Pad2)") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -5.08 0 90) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 14 "/DIO2{slash}PWM2") (pintype "passive"))
    (model "C:\\Users\\Don Koch\\Documents\\KiCad\\6.0\\SamacSys_Parts.3dshapes\\70555-0037.stp"
      (offset (xyz -2.539999924 -7.139999759 2.400000059))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Library Loader:705550038" locked (layer "F.Cu")
    (tedit 0)
    (at 92.3076 96.0444 -90)
    (descr "70555-0038-2")
    (tags "Connector")
    (property "Description" "2.54mm Pitch SL Wire-to-Board Header, Low Profile, Surface Mount, Single Row, Right-Angle, 3.05mm Pocket, Shrouded, with Press-fit Plastic Peg,  Circuits, Tin (Sn) Plating, Embossed Tape Packaging")
    (property "Height" "7.38")
    (property "Manufacturer_Name" "Molex")
    (property "Manufacturer_Part_Number" "15-91-7030")
    (property "Mouser Part Number" "538-15-91-7030")
    (property "Mouser Price/Stock" "https://www.mouser.com/Search/Refine.aspx?Keyword=538-15-91-7030")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P10" (at -3.81 6.031 90) (layer "F.SilkS"))
    (fp_text value "70555-0038" (at -3.81 6.031 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at -3.81 6.031 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -9.01 8.64 270) (size 3.45 3.45) (drill 3.45) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 1.39 8.64 270) (size 3.45 3.45) (drill 3.45) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.755 1.755) (drill 1.17) (layers *.Cu *.Mask)
      (net 8 "GND") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -2.54 0 270) (size 1.755 1.755) (drill 1.17) (layers *.Cu *.Mask)
      (net 70 "Net-(P10-Pad2)") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -5.08 0 270) (size 1.755 1.755) (drill 1.17) (layers *.Cu *.Mask)
      (net 16 "/DIO11{slash}PWM7") (pintype "passive"))
    (pad "4" thru_hole circle locked (at -7.62 0 270) (size 1.755 1.755) (drill 1.17) (layers *.Cu *.Mask)
      (net 25 "/DIO10{slash}PWM6") (pintype "passive"))
    (model "C:\\Users\\Don Koch\\Documents\\KiCad\\6.0\\SamacSys_Parts.3dshapes\\70555-0038.stp"
      (offset (xyz -3.809999886 -7.110000027 2.79999991))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Library Loader:705550037" (layer "F.Cu")
    (tedit 0)
    (at 153.032 99.7672 180)
    (descr "70555-0037-1")
    (tags "Connector")
    (property "Description" "2.54mm Pitch SL Wire-to-Board Header, Low Profile, Surface Mount, Single Row, Right-Angle, 3.05mm Pocket, Shrouded, with Press-fit Plastic Peg,  Circuits, Tin (Sn) Plating, Embossed Tape Packaging")
    (property "Height" "7.38")
    (property "Manufacturer_Name" "Molex")
    (property "Manufacturer_Part_Number" "15-91-7030")
    (property "Mouser Part Number" "538-15-91-7030")
    (property "Mouser Price/Stock" "https://www.mouser.com/Search/Refine.aspx?Keyword=538-15-91-7030")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P13" (at -2.54 6.061) (layer "F.SilkS"))
    (fp_text value "70555-0037" (at -2.54 6.061) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at -2.54 6.061) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -6.48 8.64 180) (size 3.4 3.4) (drill 3.4) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 1.4 8.64 180) (size 3.4 3.4) (drill 3.4) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 6 "GNDA") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -2.54 0 180) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 73 "Net-(P13-Pad2)") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -5.08 0 180) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 3 "/AI0") (pintype "passive"))
    (model "C:\\Users\\Don Koch\\Documents\\KiCad\\6.0\\SamacSys_Parts.3dshapes\\70555-0037.stp"
      (offset (xyz -2.539999924 -7.139999759 2.400000059))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (tedit 587A3A7B)
    (at 171.5008 112.0648 -90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D2" (at -1.9812 -0.1016 180) (layer "F.SilkS"))
    (fp_text value "Green" (at 1.27 2.96 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 31 "Net-(D2-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 32 "Net-(D2-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library Loader:705550038" locked (layer "F.Cu")
    (tedit 0)
    (at 92.3584 112.656 -90)
    (descr "70555-0038-2")
    (tags "Connector")
    (property "Description" "2.54mm Pitch SL Wire-to-Board Header, Low Profile, Surface Mount, Single Row, Right-Angle, 3.05mm Pocket, Shrouded, with Press-fit Plastic Peg,  Circuits, Tin (Sn) Plating, Embossed Tape Packaging")
    (property "Height" "7.38")
    (property "Manufacturer_Name" "Molex")
    (property "Manufacturer_Part_Number" "15-91-7030")
    (property "Mouser Part Number" "538-15-91-7030")
    (property "Mouser Price/Stock" "https://www.mouser.com/Search/Refine.aspx?Keyword=538-15-91-7030")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P11" (at -3.81 6.031 90) (layer "F.SilkS"))
    (fp_text value "70555-0038" (at -3.81 6.031 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at -3.81 6.031 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 1.39 8.64 270) (size 3.45 3.45) (drill 3.45) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -9.01 8.64 270) (size 3.45 3.45) (drill 3.45) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.755 1.755) (drill 1.17) (layers *.Cu *.Mask)
      (net 8 "GND") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -2.54 0 270) (size 1.755 1.755) (drill 1.17) (layers *.Cu *.Mask)
      (net 71 "Net-(P11-Pad2)") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -5.08 0 270) (size 1.755 1.755) (drill 1.17) (layers *.Cu *.Mask)
      (net 22 "/DIO13{slash}PWM9") (pintype "passive"))
    (pad "4" thru_hole circle locked (at -7.62 0 270) (size 1.755 1.755) (drill 1.17) (layers *.Cu *.Mask)
      (net 19 "/DIO12{slash}PWM8") (pintype "passive"))
    (model "C:\\Users\\Don Koch\\Documents\\KiCad\\6.0\\SamacSys_Parts.3dshapes\\70555-0038.stp"
      (offset (xyz -3.809999886 -7.110000027 2.79999991))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (tedit 587A3A7B)
    (at 97.1296 93.3196 -90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D20" (at 4.4704 -0.6604 180) (layer "F.SilkS"))
    (fp_text value "Red" (at 1.27 2.96 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 55 "Net-(D20-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 56 "Net-(D20-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library Loader:705550037" (layer "F.Cu")
    (tedit 0)
    (at 176.8693 110.8964 90)
    (descr "70555-0037-1")
    (tags "Connector")
    (property "Description" "2.54mm Pitch SL Wire-to-Board Header, Low Profile, Surface Mount, Single Row, Right-Angle, 3.05mm Pocket, Shrouded, with Press-fit Plastic Peg,  Circuits, Tin (Sn) Plating, Embossed Tape Packaging")
    (property "Height" "7.38")
    (property "Manufacturer_Name" "Molex")
    (property "Manufacturer_Part_Number" "15-91-7030")
    (property "Mouser Part Number" "538-15-91-7030")
    (property "Mouser Price/Stock" "https://www.mouser.com/Search/Refine.aspx?Keyword=538-15-91-7030")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P2" (at -2.54 6.061 90) (layer "F.SilkS"))
    (fp_text value "70555-0037" (at -2.54 6.061 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at -2.54 6.061 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 1.4 8.64 90) (size 3.4 3.4) (drill 3.4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -6.48 8.64 90) (size 3.4 3.4) (drill 3.4) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 8 "GND") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -2.54 0 90) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 62 "Net-(P2-Pad2)") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -5.08 0 90) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 12 "/DIO1{slash}PWM1") (pintype "passive"))
    (model "C:\\Users\\Don Koch\\Documents\\KiCad\\6.0\\SamacSys_Parts.3dshapes\\70555-0037.stp"
      (offset (xyz -2.539999924 -7.139999759 2.400000059))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (tedit 5FA16958)
    (at 103.3272 94.9175 -90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q20" (at 2.9741 -1.524 180) (layer "B.SilkS"))
    (fp_text value "DMP200K" (at 0 -2.4 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9375 0.95 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 16 "/DIO11{slash}PWM7") (pinfunction "G") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 -0.95 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 27 "+3.3V") (pinfunction "S") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 56 "Net-(D20-Pad2)") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 90.0176 75.676 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R59" (at -2.8796 0.508 180) (layer "B.SilkS"))
    (fp_text value "0" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 69 "Net-(P9-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (tedit 5FA16958)
    (at 98.5289 46.1416 180)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q8" (at 0 2.4) (layer "B.SilkS"))
    (fp_text value "DMP200K" (at 0 -2.4) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9375 0.95 180) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 21 "/DIO7{slash}SPI_MOSI") (pinfunction "G") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 -0.95 180) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 27 "+3.3V") (pinfunction "S") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 180) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(D8-Pad2)") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 154.4027 97.1296)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Manufacturer" "TDK")
    (property "Part #" "C2012X5R1A476M125AC")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C10" (at 3.3821 0.1016 180) (layer "B.SilkS"))
    (fp_text value "47uF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 6 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 73 "Net-(P13-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 112.7037 97.028)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Manufacturer" "TDK")
    (property "Part #" "C2012X5R1A476M125AC")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C13" (at 3.4251 0.1016) (layer "B.SilkS"))
    (fp_text value "47uF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 6 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 76 "Net-(P16-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 172.4171 109.9312)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at -0.0019 -1.2192) (layer "B.SilkS"))
    (fp_text value "681" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(D2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 100.6856 123.3932 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R12" (at -2.286 0.508 180) (layer "B.SilkS"))
    (fp_text value "681" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 51 "Net-(D12-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 141.732 83.1088 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R64" (at 2.4892 0 180) (layer "B.SilkS"))
    (fp_text value "0" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 74 "Net-(P14-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 1 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 89.916 125.778 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R62" (at -2.7912 0.508 180) (layer "B.SilkS"))
    (fp_text value "0" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 72 "Net-(P12-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 126.5213 96.774)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Manufacturer" "TDK")
    (property "Part #" "C2012X5R1A476M125AC")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C12" (at 3.4759 0) (layer "B.SilkS"))
    (fp_text value "47uF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 6 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 75 "Net-(P15-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (tedit 5FA16958)
    (at 103.3272 89.5881 -90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q10" (at -2.6693 -1.1684 180) (layer "B.SilkS"))
    (fp_text value "DMP200K" (at 0 -2.4 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9375 0.95 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 25 "/DIO10{slash}PWM6") (pinfunction "G") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 -0.95 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 27 "+3.3V") (pinfunction "S") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 48 "Net-(D10-Pad2)") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (tedit 5FA16958)
    (at 171.0667 45.5016)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q7" (at 0 2.4) (layer "B.SilkS"))
    (fp_text value "DMP200K" (at 0 -2.4) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9375 0.95) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 20 "/DIO6{slash}SPI_MISO") (pinfunction "G") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 -0.95) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 27 "+3.3V") (pinfunction "S") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(D7-Pad2)") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (tedit 5FA16958)
    (at 171.2237 74.676)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q5" (at 0 2.4) (layer "B.SilkS"))
    (fp_text value "DMP200K" (at 0 -2.4) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9375 0.95) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 17 "/DIO4{slash}SPI_CS") (pinfunction "G") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 -0.95) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 27 "+3.3V") (pinfunction "S") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(D5-Pad2)") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 100.9396 73.6092 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at -2.3876 1.016 180) (layer "B.SilkS"))
    (fp_text value "681" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "Net-(D9-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 180.1876 42.3512 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R37" (at 4.2324 -0.1016 180) (layer "B.SilkS"))
    (fp_text value "0" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 67 "Net-(P7-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 27 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 140.8016 84.0072 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R44" (at 3.6924 0.0348 90) (layer "B.SilkS"))
    (fp_text value "0" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 74 "Net-(P14-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 27 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (tedit 5FA16958)
    (at 171.4223 103.058)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q3" (at 0 2.4) (layer "B.SilkS"))
    (fp_text value "DMP200K" (at 0 -2.4) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9375 0.95) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 14 "/DIO2{slash}PWM2") (pinfunction "G") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 -0.95) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 27 "+3.3V") (pinfunction "S") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 34 "Net-(D3-Pad2)") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 90.0364 108.9632 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R61" (at -2.588 0.6284 180) (layer "B.SilkS"))
    (fp_text value "0" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 71 "Net-(P11-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 180.2892 56.7596 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R36" (at 3.8448 0.1016 180) (layer "B.SilkS"))
    (fp_text value "0" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 66 "Net-(P6-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 27 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (tedit 5FA16958)
    (at 103.9876 111.6584 -90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q21" (at 2.7432 -1.3208 180) (layer "B.SilkS"))
    (fp_text value "DMP200K" (at 0 -2.4 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9375 0.95 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 22 "/DIO13{slash}PWM9") (pinfunction "G") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 -0.95 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 27 "+3.3V") (pinfunction "S") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(D21-Pad2)") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 180.6448 85.4804 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R34" (at 4.1308 0.2032 180) (layer "B.SilkS"))
    (fp_text value "0" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 64 "Net-(P4-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 27 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 180.5432 112.3348 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R52" (at 2.556 0.254 180) (layer "B.SilkS"))
    (fp_text value "0" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 62 "Net-(P2-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 1 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (tedit 5FA16958)
    (at 103.5152 122.4557 -90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q12" (at -2.7201 -2.1996 180) (layer "B.SilkS"))
    (fp_text value "DMP200K" (at 0 -2.4 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9375 0.95 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 26 "/DIO14{slash}I2C_SCL") (pinfunction "G") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 -0.95 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 27 "+3.3V") (pinfunction "S") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 52 "Net-(D12-Pad2)") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 89.916 127.778 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R42" (at -3.794 -0.254 180) (layer "B.SilkS"))
    (fp_text value "0" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 27 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 72 "Net-(P12-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (tedit 5FA16958)
    (at 104.5464 78.3105 -90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q19" (at 2.7155 -1.2192 180) (layer "B.SilkS"))
    (fp_text value "DMP200K" (at 0 -2.4 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9375 0.95 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 24 "/DIO9{slash}PWM5") (pinfunction "G") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 -0.95 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 27 "+3.3V") (pinfunction "S") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 54 "Net-(D19-Pad2)") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 101.346 107.0864 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R11" (at -2.3876 0.5588 180) (layer "B.SilkS"))
    (fp_text value "681" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(D11-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 180.4924 99.9904 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R33" (at 3.9972 -0.254 180) (layer "B.SilkS"))
    (fp_text value "0" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 63 "Net-(P3-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 27 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 90.0176 110.9632 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R41" (at -4.0988 -0.6096 180) (layer "B.SilkS"))
    (fp_text value "0" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 27 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 71 "Net-(P11-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 180.1876 40.3192 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R57" (at 2.5748 0.2032 180) (layer "B.SilkS"))
    (fp_text value "0" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 67 "Net-(P7-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 1 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 180.2892 126.762 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R51" (at 2.8608 0.0508 180) (layer "B.SilkS"))
    (fp_text value "0" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 61 "Net-(P1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 1 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (tedit 5FA16958)
    (at 171.3761 88.7476)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q4" (at 0 2.4) (layer "B.SilkS"))
    (fp_text value "DMP200K" (at 0 -2.4) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9375 0.95) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 15 "/DIO3{slash}PWM3") (pinfunction "G") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 -0.95) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 27 "+3.3V") (pinfunction "S") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(D4-Pad2)") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 172.6165 124.3076)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.524) (layer "B.SilkS"))
    (fp_text value "681" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(D1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 101.3968 112.5728 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R21" (at 2.5908 1.7272 180) (layer "B.SilkS"))
    (fp_text value "681" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 57 "Net-(D21-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 172.2101 95.25)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 0.1035 -1.3716) (layer "B.SilkS"))
    (fp_text value "681" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(D3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 100.5332 90.5275 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R10" (at -2.2879 0.7112 180) (layer "B.SilkS"))
    (fp_text value "681" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 47 "Net-(D10-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 126.6096 84.0232 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R45" (at 4.7404 0.1524 90) (layer "B.SilkS"))
    (fp_text value "0" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 75 "Net-(P15-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 27 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 113.792 83.1248 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R66" (at 2.7592 0.1524 180) (layer "B.SilkS"))
    (fp_text value "0" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 76 "Net-(P16-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 1 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (tedit 5FA16958)
    (at 171.4223 117.6172)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q2" (at 0 2.4) (layer "B.SilkS"))
    (fp_text value "DMP200K" (at 0 -2.4) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9375 0.95) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 12 "/DIO1{slash}PWM1") (pinfunction "G") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 -0.95) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 27 "+3.3V") (pinfunction "S") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(D2-Pad2)") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 90.0176 77.6064 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R39" (at -4.1308 -0.4064 180) (layer "B.SilkS"))
    (fp_text value "0" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 27 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 69 "Net-(P9-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 140.6359 97.2312)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Manufacturer" "TDK")
    (property "Part #" "C2012X5R1A476M125AC")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C11" (at 3.3313 0.0508) (layer "B.SilkS"))
    (fp_text value "47uF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 6 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 74 "Net-(P14-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (tedit 5FA16958)
    (at 103.5152 128.0391 -90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q22" (at 2.9233 -1.5392 180) (layer "B.SilkS"))
    (fp_text value "DMP200K" (at 0 -2.4 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9375 0.95 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 28 "/DIO15{slash}I2C_SDA") (pinfunction "G") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 -0.95 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 27 "+3.3V") (pinfunction "S") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 60 "Net-(D22-Pad2)") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 180.2892 69.2564 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R55" (at 2.7084 0.2032 180) (layer "B.SilkS"))
    (fp_text value "0" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 65 "Net-(P5-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 1 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_2x17_P2.54mm_Vertical" locked (layer "B.Cu")
    (tedit 5A19A431)
    (at 154.6976 106.448 90)
    (descr "Through hole straight socket strip, 2x17, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x17 2.54mm double row")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 2.2064 -18.5028) (layer "B.SilkS"))
    (fp_text value "Conn_02x17_Odd_Even" (at -1.27 -43.41 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at -1.27 -20.32) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "+5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at -2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "/AO0") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "/AI0") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at -2.54 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/AO1") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "/AI1") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at -2.54 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "GNDA") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "/AI2") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at -2.54 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "GND") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval locked (at 0 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "/AI3") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval locked (at -2.54 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "/UART_RX") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval locked (at 0 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/DIO0{slash}PWM0") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval locked (at -2.54 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "GND") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval locked (at 0 -15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "/DIO1{slash}PWM1") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval locked (at -2.54 -15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "/UART_TX") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval locked (at 0 -17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "/DIO2{slash}PWM2") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval locked (at -2.54 -17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "GND") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval locked (at 0 -20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "/DIO3{slash}PWM3") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval locked (at -2.54 -20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "/DIO11{slash}PWM7") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval locked (at 0 -22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "/DIO4{slash}SPI_CS") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval locked (at -2.54 -22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "GND") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" thru_hole oval locked (at 0 -25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "/DIO5{slash}SPI_CLK") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" thru_hole oval locked (at -2.54 -25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "/DIO12{slash}PWM8") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" thru_hole oval locked (at 0 -27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "/DIO6{slash}SPI_MISO") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" thru_hole oval locked (at -2.54 -27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "GND") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" thru_hole oval locked (at 0 -30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "/DIO7{slash}SPI_MOSI") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" thru_hole oval locked (at -2.54 -30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "/DIO13{slash}PWM9") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" thru_hole oval locked (at 0 -33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "/DIO8{slash}PWM4") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" thru_hole oval locked (at -2.54 -33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "GND") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" thru_hole oval locked (at 0 -35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "/DIO9{slash}PWM5") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" thru_hole oval locked (at -2.54 -35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "GND") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" thru_hole oval locked (at 0 -38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "/DIO10{slash}PWM6") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" thru_hole oval locked (at -2.54 -38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "/DIO14{slash}I2C_SCL") (pinfunction "Pin_32") (pintype "passive"))
    (pad "33" thru_hole oval locked (at 0 -40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "+3.3V") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" thru_hole oval locked (at -2.54 -40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "/DIO15{slash}I2C_SDA") (pinfunction "Pin_34") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x17_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (tedit 5FA16958)
    (at 171.3253 59.7408)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q6" (at 0 2.4) (layer "B.SilkS"))
    (fp_text value "DMP200K" (at 0 -2.4) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9375 0.95) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "/DIO5{slash}SPI_CLK") (pinfunction "G") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 -0.95) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 27 "+3.3V") (pinfunction "S") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(D6-Pad2)") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 90.0176 49.1076 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R58" (at 2.6256 -0.3556 180) (layer "B.SilkS"))
    (fp_text value "0" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 68 "Net-(P8-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 1 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 96.6705 53.7972 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at -0.0527 -1.6764) (layer "B.SilkS"))
    (fp_text value "681" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(D8-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 89.9804 94.4532 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R40" (at -3.8448 -0.2676 180) (layer "B.SilkS"))
    (fp_text value "0" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 27 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 70 "Net-(P10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 89.9804 92.4024 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R60" (at -2.6896 0.3692 180) (layer "B.SilkS"))
    (fp_text value "0" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 70 "Net-(P10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 127.54 83.1436 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R65" (at 2.6764 0.1712) (layer "B.SilkS"))
    (fp_text value "0" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 75 "Net-(P15-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 1 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (tedit 5FA16958)
    (at 104.3432 72.6717 -90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q9" (at -2.8725 -0.8128 180) (layer "B.SilkS"))
    (fp_text value "DMP200K" (at 0 -2.4 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9375 0.95 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 23 "/DIO8{slash}PWM4") (pinfunction "G") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 -0.95 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 27 "+3.3V") (pinfunction "S") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 46 "Net-(D9-Pad2)") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 180.5432 114.3508 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R32" (at 4.2672 -0.0508 180) (layer "B.SilkS"))
    (fp_text value "0" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 62 "Net-(P2-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 27 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 90.0176 51.0888 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R38" (at 3.9276 0.3048 180) (layer "B.SilkS"))
    (fp_text value "0" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 68 "Net-(P8-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 27 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 100.5332 95.9085 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R20" (at 2.4911 1.27 180) (layer "B.SilkS"))
    (fp_text value "681" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 55 "Net-(D20-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 100.6856 128.9304 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R22" (at 2.4384 1.2192 180) (layer "B.SilkS"))
    (fp_text value "681" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 59 "Net-(D22-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 112.9124 84.0044 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R46" (at 4.3528 0.1844 90) (layer "B.SilkS"))
    (fp_text value "0" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 76 "Net-(P16-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 27 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 101.158 79.2526 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R19" (at 2.4338 1.1328 180) (layer "B.SilkS"))
    (fp_text value "681" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 53 "Net-(D19-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 172.0069 67.056)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 0.0527 -1.3716) (layer "B.SilkS"))
    (fp_text value "681" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(D5-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 180.2892 128.7432 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R31" (at 3.5908 -0.2032 180) (layer "B.SilkS"))
    (fp_text value "0" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 61 "Net-(P1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 27 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (tedit 5FA16958)
    (at 171.704 132.2555)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q1" (at 2.8956 1.0945) (layer "B.SilkS"))
    (fp_text value "DMP200K" (at 0 -2.4) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9375 0.95) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 11 "/DIO0{slash}PWM0") (pinfunction "G") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 -0.95) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 27 "+3.3V") (pinfunction "S") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(D1-Pad2)") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 172.2101 37.846)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 0.1035 -1.4224) (layer "B.SilkS"))
    (fp_text value "681" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(D7-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (tedit 5FA16958)
    (at 103.9876 106.172 -90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q11" (at -2.6416 -2.1336 180) (layer "B.SilkS"))
    (fp_text value "DMP200K" (at 0 -2.4 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9375 0.95 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 19 "/DIO12{slash}PWM8") (pinfunction "G") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 -0.95 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 27 "+3.3V") (pinfunction "S") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(D11-Pad2)") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 180.2892 54.7784 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R56" (at 2.6068 0.0508 180) (layer "B.SilkS"))
    (fp_text value "0" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 66 "Net-(P6-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 1 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 154.5844 84.0232 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R43" (at 3.9116 0.1016 90) (layer "B.SilkS"))
    (fp_text value "0" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 73 "Net-(P13-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 27 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 172.2609 51.9684)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 0 -1.4732) (layer "B.SilkS"))
    (fp_text value "681" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(D6-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 180.4924 97.9772 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R53" (at 2.7272 0.254 180) (layer "B.SilkS"))
    (fp_text value "0" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 63 "Net-(P3-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 1 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 180.6448 83.4804 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R54" (at 2.5052 0 180) (layer "B.SilkS"))
    (fp_text value "0" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 64 "Net-(P4-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 1 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 172.3117 81.0768)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 0.0527 -1.3716) (layer "B.SilkS"))
    (fp_text value "681" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 35 "Net-(D4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 180.2892 71.2564 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R35" (at 3.9784 -0.0508 180) (layer "B.SilkS"))
    (fp_text value "0" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 65 "Net-(P5-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 27 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 155.5148 83.1088 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272MXPBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R63" (at 2.6924 -0.1176 180) (layer "B.SilkS"))
    (fp_text value "0" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 73 "Net-(P13-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 1 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc locked (start 81.685524 134.468476) (mid 78.74 133.2484) (end 77.519924 130.302876) (layer "Edge.Cuts") (width 0.1))
  (gr_line locked (start 187.452876 34.136724) (end 81.685524 34.136724) (layer "Edge.Cuts") (width 0.1))
  (gr_arc locked (start 191.6176 130.302) (mid 190.397524 133.247524) (end 187.452 134.4676) (layer "Edge.Cuts") (width 0.1))
  (gr_arc locked (start 77.519924 38.302324) (mid 78.74 35.3568) (end 81.685524 34.136724) (layer "Edge.Cuts") (width 0.1))
  (gr_arc locked (start 187.452876 34.136724) (mid 190.3984 35.3568) (end 191.618476 38.302324) (layer "Edge.Cuts") (width 0.1))
  (gr_line locked (start 191.6176 130.302) (end 191.618476 38.302324) (layer "Edge.Cuts") (width 0.1))
  (gr_line locked (start 77.519924 38.302324) (end 77.519924 130.302876) (layer "Edge.Cuts") (width 0.1))
  (gr_line locked (start 81.685524 134.468476) (end 187.452 134.4676) (layer "Edge.Cuts") (width 0.1))
  (gr_text "+5V" (at 87.1728 108.1532) (layer "B.SilkS"))
  (gr_text "+3.3V" (at 86.7664 128.4732) (layer "B.SilkS"))
  (gr_text "+5V" (at 87.1728 74.7268) (layer "B.SilkS"))
  (gr_text "+3.3V" (at 183.4896 128.8796) (layer "B.SilkS"))
  (gr_text "+3.3V" (at 86.7156 111.6584) (layer "B.SilkS"))
  (gr_text "+3.3V" (at 183.4896 57.2516) (layer "B.SilkS"))
  (gr_text "+3.3V" (at 183.6928 85.8012) (layer "B.SilkS"))
  (gr_text "1" (at 157.48 106.5784) (layer "B.SilkS"))
  (gr_text "+3.3V" (at 183.5404 100.33) (layer "B.SilkS"))
  (gr_text "+5V" (at 183.1848 82.3468) (layer "B.SilkS"))
  (gr_text "+3.3V" (at 183.6928 42.8244) (layer "B.SilkS"))
  (gr_text "2\n" (at 157.48 109.2708) (layer "B.SilkS"))
  (gr_text "+5V" (at 183.0324 96.8756) (layer "B.SilkS"))
  (gr_text "+3.3V" (at 183.5404 71.7804) (layer "B.SilkS"))
  (gr_text "+3.3V" (at 86.868 51.6636) (layer "B.SilkS"))
  (gr_text "+5V" (at 183.0324 68.326) (layer "B.SilkS"))
  (gr_text "+5V" (at 87.2744 91.5924) (layer "B.SilkS"))
  (gr_text "34" (at 111.506 108.9152) (layer "B.SilkS"))
  (gr_text "+3.3V" (at 86.8172 95.0976) (layer "B.SilkS"))
  (gr_text "+5V" (at 183.2356 111.252) (layer "B.SilkS"))
  (gr_text "+5V" (at 183.1848 39.37) (layer "B.SilkS"))
  (gr_text "+5V" (at 87.2236 124.968) (layer "B.SilkS"))
  (gr_text "33" (at 111.3536 106.3244) (layer "B.SilkS"))
  (gr_text "+3.3V" (at 183.7436 114.7064) (layer "B.SilkS"))
  (gr_text "+3.3V" (at 86.7156 78.232) (layer "B.SilkS"))
  (gr_text "+5V" (at 87.3252 48.1584) (layer "B.SilkS"))
  (gr_text "+5V" (at 182.9816 53.7972) (layer "B.SilkS"))
  (gr_text "+5V" (at 183.0324 125.8824) (layer "B.SilkS"))
  (gr_text "DIO12" (at 101.9048 104.8004 270) (layer "F.SilkS"))
  (gr_text "DIO15" (at 100.7364 128.4224 270) (layer "F.SilkS"))
  (gr_text "DIO6" (at 167.1828 40.9956 90) (layer "F.SilkS"))
  (gr_text "BLD Date 2023" (at 91.0844 38.6588) (layer "F.SilkS"))
  (gr_text "DIO2" (at 167.2336 98.7552 90) (layer "F.SilkS"))
  (gr_text "34" (at 111.0488 109.1692) (layer "F.SilkS"))
  (gr_text "DIO8" (at 100.8888 71.9328 270) (layer "F.SilkS"))
  (gr_text "AI1" (at 142.0368 102.8192) (layer "F.SilkS"))
  (gr_text "1" (at 157.3276 106.426) (layer "F.SilkS"))
  (gr_text "DIO0" (at 167.132 127.8128 90) (layer "F.SilkS"))
  (gr_text "DIO4" (at 167.0812 70.2564 90) (layer "F.SilkS"))
  (gr_text "DIO14" (at 100.838 121.3104 270) (layer "F.SilkS"))
  (gr_text "AI2" (at 128.0668 102.9716) (layer "F.SilkS"))
  (gr_text "DIO11" (at 100.4824 95.8596 270) (layer "F.SilkS"))
  (gr_text "2" (at 157.226 108.966) (layer "F.SilkS"))
  (gr_text "DIO7" (at 101.6508 50.6984 270) (layer "F.SilkS"))
  (gr_text "DIO13" (at 101.7524 112.0648 270) (layer "F.SilkS"))
  (gr_text "DIO9" (at 100.9396 78.3336 270) (layer "F.SilkS"))
  (gr_text "AI0\n" (at 155.956 102.87) (layer "F.SilkS"))
  (gr_text "DIO3" (at 167.1828 84.4296 90) (layer "F.SilkS"))
  (gr_text "DIO10" (at 100.6856 88.9 270) (layer "F.SilkS"))
  (gr_text "AI3" (at 113.9444 102.9208) (layer "F.SilkS"))
  (gr_text "33" (at 111.0488 106.6292) (layer "F.SilkS"))
  (gr_text "4272" (at 135.4836 119.2276) (layer "F.SilkS"))
  (gr_text "DIO1" (at 167.1828 113.284 90) (layer "F.SilkS"))
  (gr_text "DIO5" (at 167.386 55.0164 90) (layer "F.SilkS"))
  (gr_text "Maverick Robotics" (at 135.0772 129.9972) (layer "F.SilkS"))
  (dimension (type aligned) (layer "User.2")
    (pts (xy 159.0676 38.648) (xy 159.2072 106.6292))
    (height -10.098834)
    (gr_text "2676.4308 mils" (at 170.386211 72.6155 270.1176572) (layer "User.2"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.2")
    (pts (xy 159.4176 38.648) (xy 109.8042 38.6842))
    (height 5.685376)
    (gr_text "1953.2840 mils" (at 134.605913 31.830726 0.04180537617) (layer "User.2"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.2")
    (pts (xy 159.2176 106.348) (xy 154.7176 106.348))
    (height -6.2)
    (gr_text "177.1654 mils" (at 156.9676 111.398) (layer "User.2"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.9")
    (pts (xy 77.5462 134.4422) (xy 77.5462 34.1122))
    (height 0)
    (gr_text "3950.0000 mils" (at 76.3962 84.2772 90) (layer "User.9"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.9")
    (pts (xy 191.6176 134.4422) (xy 77.5462 134.4422))
    (height 0)
    (gr_text "4491.0000 mils" (at 134.5819 133.2922) (layer "User.9"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 8) (net_name "GND") (layer "In1.Cu") (name "+3.3V") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.4352 133.858)
        (xy 79.1972 35.4584)
        (xy 190.754 34.7472)
        (xy 190.8556 133.9088)
      )
    )
  )
  (zone (net 6) (net_name "GNDA") (layer "In2.Cu") (name "GNDA") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148.2852 107.5944)
        (xy 145.8468 107.6452)
        (xy 143.2052 107.5436)
        (xy 143.1544 105.0544)
        (xy 109.3724 105.0036)
        (xy 109.524335 98.041077)
        (xy 159.765535 97.990277)
        (xy 159.4612 104.5464)
        (xy 153.5684 104.8512)
        (xy 153.3144 107.5944)
        (xy 151.0284 107.696)
        (xy 150.876 110.1852)
        (xy 148.1836 110.236)
      )
    )
  )
  (zone (net 27) (net_name "+3.3V") (layer "In2.Cu") (name "GND") (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.232 34.6456)
        (xy 190.8048 34.5948)
        (xy 190.8556 133.6548)
        (xy 131.050624 133.9088)
        (xy 133.347428 105.238355)
        (xy 143.000509 105.289155)
        (xy 143.002 107.6452)
        (xy 148.1328 107.696)
        (xy 147.9804 110.3884)
        (xy 150.9776 110.3884)
        (xy 151.13 107.8484)
        (xy 153.416 107.7976)
        (xy 153.7208 105.0036)
        (xy 159.6644 104.7496)
        (xy 160.02 97.8916)
        (xy 109.4232 97.9424)
        (xy 109.22 105.1052)
        (xy 133.1976 105.1052)
        (xy 131.0132 133.9088)
        (xy 78.3844 133.9596)
      )
    )
  )
  (zone (net 1) (net_name "+5V") (layer "B.Cu") (name "+3.3V") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.0336 34.594381)
        (xy 90.932 133.247981)
        (xy 79.248 133.0452)
        (xy 78.6892 34.4424)
      )
    )
  )
  (zone (net 1) (net_name "+5V") (layer "B.Cu") (hatch none 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.998 82.9564)
        (xy 110.9472 80.1116)
        (xy 156.6164 80.264)
        (xy 168.1988 76.5048)
        (xy 180.574809 76.520265)
        (xy 183.134 76.454)
        (xy 183.061278 79.163701)
        (xy 167.845623 79.198229)
        (xy 156.6672 83.058)
        (xy 156.6672 83.0072)
      )
    )
  )
  (zone (net 1) (net_name "+5V") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.368915 82.949778)
        (xy 100.2792 85.598)
        (xy 87.5792 85.5472)
        (xy 87.5792 82.4484)
        (xy 100.1776 82.4992)
        (xy 111.318115 80.104978)
      )
    )
  )
  (zone (net 1) (net_name "+5V") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 179.0192 35.2044)
        (xy 190.246 35.2044)
        (xy 190.246 121.3104)
        (xy 190.246 133.4008)
        (xy 179.3748 133.35)
      )
    )
  )
)
