<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<hole x="69.2404" y="118.7704" drill="3.175"/>
<hole x="49.4792" y="84.709" drill="3.175"/>
<hole x="119.7864" y="68.1736" drill="3.175"/>
<hole x="85.6234" y="48.4124" drill="3.175"/>
<hole x="98.8822" y="-0.9652" drill="3.175"/>
<hole x="138.2522" y="-0.9652" drill="3.175"/>
<wire x1="94.0816" y1="-3.6068" x2="143.0274" y2="-3.6068" width="0" layer="20"/>
<wire x1="94.0816" y1="-3.6068" x2="47.879" y2="80.3148" width="0" layer="20" curve="64"/>
<wire x1="143.0274" y1="-3.6068" x2="48.514" y2="133.5024" width="0" layer="20" curve="71"/>
<text>J007944A PEZ POWER</text>
<text>20191112</text>
<text>S</text>
<text>S</text>
<text>RED</text>
<text>IR</text>
<text>TEM</text>
<text>SPARE
LED</text>
<text>PHOTO-
DIODE</text>
<text>FAN</text>
<text>FAN</text>
<text>FROM CONTROL MODULE</text>
<text>+15V</text>
<text>GND</text>
<text>GND</text>
<wire x1="46.355" y1="131.9784" x2="46.3804" y2="83.4136" width="0" layer="20"/>
<wire x1="46.355" y1="131.9784" x2="48.514" y2="133.5024" width="0" layer="20" curve="-115.391065"/>
<wire x1="46.3804" y1="83.4136" x2="47.879" y2="80.3148" width="0" layer="20" curve="60.087498"/>
<text>IR</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>GND</text>
<text>SCLK</text>
<text>MOSI</text>
<text>CS</text>
<text>ENABLE</text>
<text>PELTIER</text>
</plain>
<libraries>
<library name="STEVES_BU">
<packages>
<package name="1206S">
</package>
<package name="TE-MATE-N-LOK-2">
</package>
<package name="TO252_HS">
</package>
<package name="0805S">
</package>
<package name="AMPMODU-2">
</package>
<package name="MSOP10">
</package>
<package name="0603S">
</package>
<package name="AMPMODU6">
</package>
<package name="LOGO_BMP_OP">
</package>
<package name="SRU8043">
</package>
<package name="1210S">
</package>
<package name="PWRDI-123">
</package>
<package name="SOIC8-EP">
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO220-IGO">
</package>
<package name="POWER_JACK_PTH">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="153CLV-0605">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
</packages>
</library>
<library name="2pinheader2.54mm">
<packages>
<package name="2PINHEADER2.5MM">
</package>
</packages>
</library>
<library name="heatsink">
<description>&lt;b&gt;Heatsinks&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="D03PA-PAD">
<description>&lt;b&gt;HEATSINK&lt;/b&gt;&lt;p&gt;
distributor Schukat</description>
</package>
</packages>
</library>
<library name="STEVES">
<packages>
<package name="0603S">
</package>
<package name="SOT23-3">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J4" library="STEVES_BU" package="TE-MATE-N-LOK-2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="STEVES_BU" package="TO252_HS" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="STEVES_BU" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="STEVES_BU" package="AMPMODU-2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="STEVES_BU" package="AMPMODU-2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="STEVES_BU" package="AMPMODU-2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="adafruit" package="153CLV-0605" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="2pinheader2.54mm" package="2PINHEADER2.5MM" value="2PINHEADER2.54MM">
<attribute name="NAME"/>
</element>
<element name="JP2" library="2pinheader2.54mm" package="2PINHEADER2.5MM" value="2PINHEADER2.54MM">
<attribute name="NAME"/>
</element>
<element name="HS1" library="heatsink" package="D03PA-PAD" value="HEATSINK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="SparkFun" package="TO220-IGO" value="7812">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="STEVES_BU" package="1206S" value="10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="STEVES_BU" package="1206S" value="10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="STEVES_BU" package="MSOP10" value="AD5624R-3 ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="STEVES_BU" package="0603S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="STEVES_BU" package="0603S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="STEVES_BU" package="0805S" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="STEVES" package="0603S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="STEVES" package="SOT23-3" value="LM34880-5V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="2pinheader2.54mm" package="2PINHEADER2.5MM" value="2PINHEADER2.54MM">
<attribute name="NAME"/>
</element>
<element name="J6" library="STEVES_BU" package="AMPMODU6" value="CON6AMPMODU6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun" package="POWER_JACK_PTH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="adafruit" package="153CLV-0605" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="STEVES" package="0603S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$4" library="STEVES_BU" package="LOGO_BMP_OP" value="JFRC-LOGOLOGO_OP"/>
<element name="L1" library="STEVES_BU" package="SRU8043" value="68uH/1A"/>
<element name="C10" library="STEVES_BU" package="1206S" value="2.2@50"/>
<element name="C11" library="STEVES_BU" package="1210S" value="10@50"/>
<element name="R3" library="STEVES_BU" package="1206S" value="1R00"/>
<element name="D1" library="STEVES_BU" package="PWRDI-123" value="DLFS240L"/>
<element name="R4" library="STEVES_BU" package="0805S" value="4.99K"/>
<element name="U4" library="STEVES_BU" package="SOIC8-EP" value="AL8862SP-13"/>
<element name="R5" library="STEVES_BU" package="0805S" value="4.99K"/>
<element name="L2" library="STEVES_BU" package="SRU8043" value="68uH/1A"/>
<element name="C12" library="STEVES_BU" package="1206S" value="2.2@50"/>
<element name="C13" library="STEVES_BU" package="1210S" value="10@50"/>
<element name="R6" library="STEVES_BU" package="1206S" value="1R00"/>
<element name="D2" library="STEVES_BU" package="PWRDI-123" value="DLFS240L"/>
<element name="R7" library="STEVES_BU" package="0805S" value="4.99K"/>
<element name="U5" library="STEVES_BU" package="SOIC8-EP" value="AL8862SP-13"/>
<element name="R8" library="STEVES_BU" package="0805S" value="4.99K"/>
<element name="L3" library="STEVES_BU" package="SRU8043" value="68uH/1A"/>
<element name="C14" library="STEVES_BU" package="1206S" value="2.2@50"/>
<element name="C15" library="STEVES_BU" package="1210S" value="10@50"/>
<element name="R9" library="STEVES_BU" package="1206S" value="1R00"/>
<element name="D3" library="STEVES_BU" package="PWRDI-123" value="DLFS240L"/>
<element name="R10" library="STEVES_BU" package="0805S" value="4.99K"/>
<element name="U6" library="STEVES_BU" package="SOIC8-EP" value="AL8862SP-13"/>
<element name="R11" library="STEVES_BU" package="0805S" value="4.99K"/>
<element name="R12" library="STEVES_BU" package="0805S" value="1 ohm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="STEVES_BU" package="1210S" value="10@50"/>
</elements>
<signals>
<signal name="GND">
<contactref element="Q1" pad="2"/>
<contactref element="C3" pad="-"/>
<contactref element="U3" pad="GND"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="J1" pad="GNDBREAK"/>
<contactref element="J1" pad="GND"/>
<contactref element="C1" pad="-"/>
<contactref element="C11" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="U4" pad="EP"/>
<contactref element="U4" pad="7"/>
<contactref element="U4" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="U5" pad="EP"/>
<contactref element="U5" pad="7"/>
<contactref element="U5" pad="2"/>
<contactref element="R10" pad="1"/>
<contactref element="U6" pad="EP"/>
<contactref element="U6" pad="7"/>
<contactref element="U6" pad="2"/>
<contactref element="U2" pad="3"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="J6" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="R1" pad="2"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="TE_D">
<contactref element="Q1" pad="3"/>
<contactref element="Q1" pad="3S"/>
<contactref element="Q1" pad="P$1"/>
<contactref element="Q1" pad="P$2"/>
<contactref element="Q1" pad="P$3"/>
<contactref element="Q1" pad="P$4"/>
<contactref element="Q1" pad="P$5"/>
<contactref element="Q1" pad="P$6"/>
<contactref element="Q1" pad="P$7"/>
<contactref element="Q1" pad="P$8"/>
<contactref element="Q1" pad="P$9"/>
<contactref element="Q1" pad="P$10"/>
<contactref element="Q1" pad="P$11"/>
<contactref element="Q1" pad="P$12"/>
<contactref element="J4" pad="P$2"/>
</signal>
<signal name="+15V">
<contactref element="J4" pad="P$1"/>
<contactref element="C3" pad="+"/>
<contactref element="U3" pad="IN"/>
<contactref element="C8" pad="1"/>
<contactref element="J1" pad="PWR"/>
<contactref element="C1" pad="+"/>
<contactref element="U1" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="U4" pad="4"/>
<contactref element="D1" pad="K"/>
<contactref element="R6" pad="2"/>
<contactref element="C13" pad="1"/>
<contactref element="U5" pad="4"/>
<contactref element="D2" pad="K"/>
<contactref element="R9" pad="2"/>
<contactref element="C15" pad="1"/>
<contactref element="U6" pad="4"/>
<contactref element="D3" pad="K"/>
</signal>
<signal name="PELTIER">
<contactref element="R1" pad="1"/>
<contactref element="J6" pad="6"/>
</signal>
<signal name="FANS">
<contactref element="JP3" pad="2"/>
<contactref element="JP2" pad="2"/>
<contactref element="U3" pad="OUT"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="SCLK">
<contactref element="U2" pad="7"/>
<contactref element="J6" pad="2"/>
</signal>
<signal name="CS">
<contactref element="U2" pad="6"/>
<contactref element="J6" pad="4"/>
</signal>
<signal name="IR">
<contactref element="U2" pad="2"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="U2" pad="8"/>
<contactref element="J6" pad="3"/>
</signal>
<signal name="RED">
<contactref element="U2" pad="1"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="+5VA">
<contactref element="U1" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$71">
<contactref element="U2" pad="10"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="R-">
<contactref element="J3" pad="2"/>
<contactref element="L1" pad="1"/>
<contactref element="C10" pad="2"/>
</signal>
<signal name="I-">
<contactref element="J2" pad="2"/>
<contactref element="L2" pad="1"/>
<contactref element="C12" pad="2"/>
</signal>
<signal name="AGND">
<contactref element="JP1" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$190">
<contactref element="L1" pad="2"/>
<contactref element="U4" pad="5"/>
<contactref element="U4" pad="6"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="SCNT">
<contactref element="R11" pad="2"/>
<contactref element="U6" pad="8"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="L2" pad="2"/>
<contactref element="U5" pad="5"/>
<contactref element="U5" pad="6"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="SPARE">
<contactref element="U2" pad="4"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="R+">
<contactref element="R3" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="U4" pad="1"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="I+">
<contactref element="R6" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="U5" pad="1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="L3" pad="2"/>
<contactref element="U6" pad="5"/>
<contactref element="U6" pad="6"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="S+">
<contactref element="R9" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="U6" pad="1"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="S-">
<contactref element="L3" pad="1"/>
<contactref element="C14" pad="2"/>
<contactref element="J5" pad="2"/>
</signal>
<signal name="N$3">
</signal>
<signal name="RCNT">
<contactref element="R5" pad="2"/>
<contactref element="U4" pad="8"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="ICNT">
<contactref element="R8" pad="2"/>
<contactref element="U5" pad="8"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="+3V3">
<contactref element="U2" pad="9"/>
<contactref element="C7" pad="1"/>
<contactref element="R12" pad="2"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="ENABLE">
<contactref element="R12" pad="1"/>
<contactref element="J6" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
