(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 40)
    (no_connects 0)
    (area 134.544999 79.991428 152.475001 134.695001)
    (thickness 1.6)
    (drawings 17)
    (tracks 141)
    (zones 0)
    (modules 3)
    (nets 41)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.5 0.5)
    (mod_text_width 0.1)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFF75F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers))
  )
  (net 0 "")
  (net 1 /A40)
  (net 2 /A20)
  (net 3 /A37)
  (net 4 /A38)
  (net 5 /A19)
  (net 6 /A39)
  (net 7 /A17)
  (net 8 /A31)
  (net 9 /A11)
  (net 10 /A12)
  (net 11 /A32)
  (net 12 /A13)
  (net 13 /A33)
  (net 14 /A35)
  (net 15 /A15)
  (net 16 /A34)
  (net 17 /A14)
  (net 18 /A16)
  (net 19 /A36)
  (net 20 /A30)
  (net 21 /A10)
  (net 22 /A8)
  (net 23 /A28)
  (net 24 /A9)
  (net 25 /A29)
  (net 26 /A27)
  (net 27 /A7)
  (net 28 /A26)
  (net 29 /A6)
  (net 30 /A1)
  (net 31 /A21)
  (net 32 /A2)
  (net 33 /A22)
  (net 34 /A3)
  (net 35 /A23)
  (net 36 /A4)
  (net 37 /A24)
  (net 38 /A5)
  (net 39 /A25)
  (net 40 /A18)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A16)
    (add_net /A17)
    (add_net /A18)
    (add_net /A19)
    (add_net /A2)
    (add_net /A20)
    (add_net /A21)
    (add_net /A22)
    (add_net /A23)
    (add_net /A24)
    (add_net /A25)
    (add_net /A26)
    (add_net /A27)
    (add_net /A28)
    (add_net /A29)
    (add_net /A3)
    (add_net /A30)
    (add_net /A31)
    (add_net /A32)
    (add_net /A33)
    (add_net /A34)
    (add_net /A35)
    (add_net /A36)
    (add_net /A37)
    (add_net /A38)
    (add_net /A39)
    (add_net /A4)
    (add_net /A40)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
  )
  (module OLIMEX_Connectors-FP:HN1x20 (layer F.Cu) (tedit 59C29A91)
    (at 149.86 107.95 270)
    (solder_mask_margin 0.0508)
    (solder_paste_margin -0.0508)
    (attr smd)
    (fp_text reference J2 (at -26.67 0 270) (layer F.SilkS))
    (fp_text value CONN_01X20 (at -13.97 2.54 270) (layer F.Fab))
    (pad 17 thru_hole circle (at 16.51 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 3 /A37))
    (pad 18 thru_hole circle (at 19.05 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 4 /A38))
    (pad 20 thru_hole circle (at 24.13 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 1 /A40))
    (pad 19 thru_hole circle (at 21.59 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 6 /A39))
    (pad 15 thru_hole circle (at 11.43 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 14 /A35))
    (pad 16 thru_hole circle (at 13.97 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 19 /A36))
    (pad 14 thru_hole circle (at 8.89 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 16 /A34))
    (pad 13 thru_hole circle (at 6.35 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 13 /A33))
    (pad 11 thru_hole circle (at 1.27 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 8 /A31))
    (pad 12 thru_hole circle (at 3.81 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 11 /A32))
    (pad 10 thru_hole circle (at -1.27 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 20 /A30))
    (pad 9 thru_hole circle (at -3.81 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 25 /A29))
    (pad 7 thru_hole circle (at -8.89 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 26 /A27))
    (pad 8 thru_hole circle (at -6.35 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 23 /A28))
    (pad 6 thru_hole circle (at -11.43 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 28 /A26))
    (pad 5 thru_hole circle (at -13.97 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 39 /A25))
    (pad 1 thru_hole rect (at -24.13 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 31 /A21))
    (pad 2 thru_hole circle (at -21.59 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 33 /A22))
    (pad 3 thru_hole circle (at -19.05 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 35 /A23))
    (pad 4 thru_hole circle (at -16.51 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 37 /A24))
  )
  (module OLIMEX_Connectors-FP:HN1x20 (layer F.Cu) (tedit 59C29A8B)
    (at 137.16 107.95 270)
    (solder_mask_margin 0.0508)
    (solder_paste_margin -0.0508)
    (attr smd)
    (fp_text reference J3 (at -26.67 0 270) (layer F.SilkS))
    (fp_text value CONN_01X20 (at -13.97 -2.54 270) (layer F.Fab))
    (pad 17 thru_hole circle (at 16.51 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 7 /A17))
    (pad 18 thru_hole circle (at 19.05 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 40 /A18))
    (pad 20 thru_hole circle (at 24.13 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 2 /A20))
    (pad 19 thru_hole circle (at 21.59 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 5 /A19))
    (pad 15 thru_hole circle (at 11.43 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 15 /A15))
    (pad 16 thru_hole circle (at 13.97 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 18 /A16))
    (pad 14 thru_hole circle (at 8.89 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 17 /A14))
    (pad 13 thru_hole circle (at 6.35 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 12 /A13))
    (pad 11 thru_hole circle (at 1.27 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 9 /A11))
    (pad 12 thru_hole circle (at 3.81 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 10 /A12))
    (pad 10 thru_hole circle (at -1.27 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 21 /A10))
    (pad 9 thru_hole circle (at -3.81 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 24 /A9))
    (pad 7 thru_hole circle (at -8.89 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 27 /A7))
    (pad 8 thru_hole circle (at -6.35 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 22 /A8))
    (pad 6 thru_hole circle (at -11.43 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 29 /A6))
    (pad 5 thru_hole circle (at -13.97 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 38 /A5))
    (pad 1 thru_hole rect (at -24.13 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 30 /A1))
    (pad 2 thru_hole circle (at -21.59 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 32 /A2))
    (pad 3 thru_hole circle (at -19.05 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 34 /A3))
    (pad 4 thru_hole circle (at -16.51 0 270) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 36 /A4))
  )
  (module "OLIMEX_Connectors-FP:GPH127SMT-02X20(PA-V16X-2X20-LF)" (layer F.Cu) (tedit 57D7DAC1)
    (at 143.51 106.68 270)
    (attr smd)
    (fp_text reference J1 (at -10.668 4.0005 270) (layer F.SilkS))
    (fp_text value CONN_02X20 (at 0 -4.445 270) (layer F.Fab))
    (fp_text user 40 (at 13.8 -0.7 270) (layer F.SilkS))
    (fp_text user 39 (at 13.8 0.7 270) (layer F.SilkS))
    (fp_text user 1 (at -13.7 0.7 270) (layer F.SilkS))
    (fp_text user 2 (at -13.7 -0.7 270) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 11.43 0) (size 0.7 0.7) (drill 0.7) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 40 smd rect (at 12.065 -2.032) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 /A40) (solder_mask_margin 0.0508))
    (pad 39 smd rect (at 12.065 2.032) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 /A20) (solder_mask_margin 0.0508))
    (pad 38 smd rect (at 10.795 -2.032) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 6 /A39) (solder_mask_margin 0.0508))
    (pad 37 smd rect (at 10.795 2.032) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 5 /A19) (solder_mask_margin 0.0508))
    (pad 36 smd rect (at 9.525 -2.032) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 4 /A38) (solder_mask_margin 0.0508))
    (pad 35 smd rect (at 9.525 2.032) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 40 /A18) (solder_mask_margin 0.0508))
    (pad 34 smd rect (at 8.255 -2.032) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 3 /A37) (solder_mask_margin 0.0508))
    (pad 33 smd rect (at 8.255 2.032) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 7 /A17) (solder_mask_margin 0.0508))
    (pad 32 smd rect (at 6.985 -2.032 180) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 19 /A36) (solder_mask_margin 0.0508))
    (pad 31 smd rect (at 6.985 2.032 180) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 18 /A16) (solder_mask_margin 0.0508))
    (pad 30 smd rect (at 5.715 -2.032 180) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 14 /A35) (solder_mask_margin 0.0508))
    (pad 29 smd rect (at 5.715 2.032 180) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 15 /A15) (solder_mask_margin 0.0508))
    (pad 28 smd rect (at 4.445 -2.032 180) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 16 /A34) (solder_mask_margin 0.0508))
    (pad 27 smd rect (at 4.445 2.032 180) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 17 /A14) (solder_mask_margin 0.0508))
    (pad 26 smd rect (at 3.175 -2.032 180) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 13 /A33) (solder_mask_margin 0.0508))
    (pad 25 smd rect (at 3.175 2.032 180) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 12 /A13) (solder_mask_margin 0.0508))
    (pad 24 smd rect (at 1.905 -2.032 180) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 11 /A32) (solder_mask_margin 0.0508))
    (pad 23 smd rect (at 1.905 2.032 180) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 10 /A12) (solder_mask_margin 0.0508))
    (pad 22 smd rect (at 0.635 -2.032 180) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 8 /A31) (solder_mask_margin 0.0508))
    (pad 21 smd rect (at 0.635 2.032 180) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 9 /A11) (solder_mask_margin 0.0508))
    (pad 1 smd rect (at -12.065 2.032 180) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 30 /A1) (solder_mask_margin 0.0508))
    (pad 2 smd rect (at -12.065 -2.032 180) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 31 /A21) (solder_mask_margin 0.0508))
    (pad 3 smd rect (at -10.795 2.032 180) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 32 /A2) (solder_mask_margin 0.0508))
    (pad 4 smd rect (at -10.795 -2.032 180) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 33 /A22) (solder_mask_margin 0.0508))
    (pad 5 smd rect (at -9.525 2.032 180) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 34 /A3) (solder_mask_margin 0.0508))
    (pad 6 smd rect (at -9.525 -2.032 180) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 35 /A23) (solder_mask_margin 0.0508))
    (pad 7 smd rect (at -8.255 2.032 180) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 36 /A4) (solder_mask_margin 0.0508))
    (pad 8 smd rect (at -8.255 -2.032 180) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 37 /A24) (solder_mask_margin 0.0508))
    (pad 9 smd rect (at -6.985 2.032 180) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 38 /A5) (solder_mask_margin 0.0508))
    (pad 10 smd rect (at -6.985 -2.032 180) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 39 /A25) (solder_mask_margin 0.0508))
    (pad 11 smd rect (at -5.715 2.032 180) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 29 /A6) (solder_mask_margin 0.0508))
    (pad 12 smd rect (at -5.715 -2.032 180) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 28 /A26) (solder_mask_margin 0.0508))
    (pad 13 smd rect (at -4.445 2.032) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 27 /A7) (solder_mask_margin 0.0508))
    (pad 14 smd rect (at -4.445 -2.032) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 26 /A27) (solder_mask_margin 0.0508))
    (pad 15 smd rect (at -3.175 2.032) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 22 /A8) (solder_mask_margin 0.0508))
    (pad 16 smd rect (at -3.175 -2.032) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 23 /A28) (solder_mask_margin 0.0508))
    (pad 17 smd rect (at -1.905 2.032) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 24 /A9) (solder_mask_margin 0.0508))
    (pad 18 smd rect (at -1.905 -2.032) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 25 /A29) (solder_mask_margin 0.0508))
    (pad 19 smd rect (at -0.635 2.032) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 21 /A10) (solder_mask_margin 0.0508))
    (pad 20 smd rect (at -0.635 -2.032) (size 1.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 20 /A30) (solder_mask_margin 0.0508))
    (pad "" np_thru_hole circle (at -11.43 0) (size 0.7 0.7) (drill 0.7) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
  )
  (gr_text "0.039\" / 1mm\npitch\nbreakout" (at 143.51 87.63) (layer F.SilkS))
  (gr_text 20 (at 147.828 106.68) (layer F.SilkS))
  (gr_text 19 (at 139.192 106.68) (layer F.SilkS))
  (gr_line (start 134.62 134.62) (end 134.62 81.28) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.4 134.62) (end 134.62 134.62) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.4 81.28) (end 152.4 134.62) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.62 81.28) (end 152.4 81.28) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text 29 (at 139.065 119.38) (layer F.SilkS))
  (gr_text 30 (at 147.955 119.38) (layer F.SilkS))
  (gr_text "1.27mm/0.05\" to 2.54mm/0.1\"\nbreakout board\nbrianredbeard.com" (at 142.24 107.95 90) (layer B.SilkS))
  (gr_text 10 (at 147.955 93.98) (layer F.SilkS))
  (gr_text 9 (at 139.065 93.98) (layer F.SilkS))
  (gr_text 40 (at 147.955 132.08) (layer F.SilkS))
  (gr_text 39 (at 139.065 132.08) (layer F.SilkS))
  (gr_text 2 (at 147.955 83.82) (layer F.SilkS))
  (gr_text 1 (at 139.065 83.82) (layer F.SilkS))
  (gr_text 1 (at 135.89 83.82) (layer Eco2.User))
)
