(kicad_pcb (version 4) (host pcbnew no-vcs-found-product)
  (general
    (links 397)
    (no_connects 5)
    (area 87.5254 24.4348 194.335401 88.54212)
    (thickness 1.6)
    (drawings 41)
    (tracks 690)
    (zones 0)
    (modules 268)
    (nets 87)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (user_trace_width 1.2)
    (trace_clearance 0.1)
    (zone_clearance 0.1)
    (zone_45_only yes)
    (trace_min 0.16)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.3)
    (via_min_drill 0.3)
    (user_via 0.6 0.3)
    (user_via 0.8 0.4)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.6 0.6)
    (pad_drill 0.3)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 96.5454 75.4888)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory /home/nristow/Dropbox/freelance/penguiconbadge/gerberfinal/))
  )
  (net 0 "")
  (net 1 +BATT)
  (net 2 GND)
  (net 3 /VIN)
  (net 4 /VDD)
  (net 5 "Net-(C3-Pad2)")
  (net 6 RESET)
  (net 7 +3V3)
  (net 8 "Net-(D1-Pad2)")
  (net 9 "Net-(D1-Pad1)")
  (net 10 "Net-(P3-Pad2)")
  (net 11 "Net-(P3-Pad3)")
  (net 12 "Net-(P3-Pad6)")
  (net 13 /TXD)
  (net 14 /RXD)
  (net 15 BATT_CHECK)
  (net 16 "Net-(Q1-Pad3)")
  (net 17 ADC)
  (net 18 /RST)
  (net 19 /D-)
  (net 20 /D+)
  (net 21 "Net-(R9-Pad1)")
  (net 22 "Net-(R12-Pad1)")
  (net 23 "Net-(SW2-Pad1)")
  (net 24 /GPIO16)
  (net 25 /GPIO14)
  (net 26 /GPIO12)
  (net 27 /GPIO13)
  (net 28 /GPIO5)
  (net 29 "Net-(U10-Pad1)")
  (net 30 "Net-(U6-Pad4)")
  (net 31 "Net-(U7-Pad4)")
  (net 32 "Net-(U8-Pad4)")
  (net 33 "Net-(U10-Pad4)")
  (net 34 "Net-(U11-Pad4)")
  (net 35 "Net-(U12-Pad4)")
  (net 36 "Net-(U13-Pad4)")
  (net 37 "Net-(U14-Pad4)")
  (net 38 "Net-(U15-Pad4)")
  (net 39 "Net-(U16-Pad4)")
  (net 40 "Net-(U17-Pad4)")
  (net 41 "Net-(U18-Pad4)")
  (net 42 "Net-(U19-Pad4)")
  (net 43 "Net-(U20-Pad4)")
  (net 44 "Net-(U21-Pad4)")
  (net 45 "Net-(U22-Pad4)")
  (net 46 "Net-(U23-Pad4)")
  (net 47 "Net-(U24-Pad4)")
  (net 48 "Net-(U25-Pad4)")
  (net 49 "Net-(U26-Pad4)")
  (net 50 "Net-(U27-Pad4)")
  (net 51 "Net-(U28-Pad4)")
  (net 52 "Net-(U29-Pad4)")
  (net 53 "Net-(D2-Pad2)")
  (net 54 "Net-(U30-Pad4)")
  (net 55 "Net-(C5-Pad2)")
  (net 56 "Net-(P7-Pad1)")
  (net 57 "Net-(P4-Pad1)")
  (net 58 "Net-(P4-Pad3)")
  (net 59 "Net-(P4-Pad4)")
  (net 60 "Net-(P4-Pad5)")
  (net 61 "Net-(P4-Pad6)")
  (net 62 "Net-(P4-Pad7)")
  (net 63 "Net-(P4-Pad8)")
  (net 64 "Net-(P5-Pad6)")
  (net 65 "Net-(P8-Pad2)")
  (net 66 "Net-(P8-Pad3)")
  (net 67 "Net-(P8-Pad4)")
  (net 68 "Net-(P8-Pad5)")
  (net 69 "Net-(P8-Pad6)")
  (net 70 "Net-(P6-Pad4)")
  (net 71 "Net-(P6-Pad5)")
  (net 72 "Net-(U1-Pad1)")
  (net 73 "Net-(U1-Pad2)")
  (net 74 "Net-(U1-Pad11)")
  (net 75 "Net-(U1-Pad12)")
  (net 76 "Net-(U1-Pad23)")
  (net 77 "Net-(U1-Pad24)")
  (net 78 "Net-(U1-Pad27)")
  (net 79 "Net-(U2-Pad9)")
  (net 80 "Net-(U2-Pad10)")
  (net 81 "Net-(U2-Pad11)")
  (net 82 "Net-(U2-Pad12)")
  (net 83 "Net-(U2-Pad13)")
  (net 84 "Net-(U2-Pad14)")
  (net 85 "Net-(P3-Pad4)")
  (net 86 "Net-(C10-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1)
    (trace_width 0.3)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +BATT)
    (add_net /D+)
    (add_net /D-)
    (add_net /GPIO12)
    (add_net /GPIO13)
    (add_net /GPIO14)
    (add_net /GPIO16)
    (add_net /GPIO5)
    (add_net /RST)
    (add_net /RXD)
    (add_net /TXD)
    (add_net /VDD)
    (add_net /VIN)
    (add_net ADC)
    (add_net BATT_CHECK)
    (add_net GND)
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(P3-Pad3)")
    (add_net "Net-(P3-Pad4)")
    (add_net "Net-(P3-Pad6)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P4-Pad3)")
    (add_net "Net-(P4-Pad4)")
    (add_net "Net-(P4-Pad5)")
    (add_net "Net-(P4-Pad6)")
    (add_net "Net-(P4-Pad7)")
    (add_net "Net-(P4-Pad8)")
    (add_net "Net-(P5-Pad6)")
    (add_net "Net-(P6-Pad4)")
    (add_net "Net-(P6-Pad5)")
    (add_net "Net-(P7-Pad1)")
    (add_net "Net-(P8-Pad2)")
    (add_net "Net-(P8-Pad3)")
    (add_net "Net-(P8-Pad4)")
    (add_net "Net-(P8-Pad5)")
    (add_net "Net-(P8-Pad6)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R9-Pad1)")
    (add_net "Net-(SW2-Pad1)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad24)")
    (add_net "Net-(U1-Pad27)")
    (add_net "Net-(U10-Pad1)")
    (add_net "Net-(U10-Pad4)")
    (add_net "Net-(U11-Pad4)")
    (add_net "Net-(U12-Pad4)")
    (add_net "Net-(U13-Pad4)")
    (add_net "Net-(U14-Pad4)")
    (add_net "Net-(U15-Pad4)")
    (add_net "Net-(U16-Pad4)")
    (add_net "Net-(U17-Pad4)")
    (add_net "Net-(U18-Pad4)")
    (add_net "Net-(U19-Pad4)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad9)")
    (add_net "Net-(U20-Pad4)")
    (add_net "Net-(U21-Pad4)")
    (add_net "Net-(U22-Pad4)")
    (add_net "Net-(U23-Pad4)")
    (add_net "Net-(U24-Pad4)")
    (add_net "Net-(U25-Pad4)")
    (add_net "Net-(U26-Pad4)")
    (add_net "Net-(U27-Pad4)")
    (add_net "Net-(U28-Pad4)")
    (add_net "Net-(U29-Pad4)")
    (add_net "Net-(U30-Pad4)")
    (add_net "Net-(U6-Pad4)")
    (add_net "Net-(U7-Pad4)")
    (add_net "Net-(U8-Pad4)")
    (add_net RESET)
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 147.8454 61.4888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 148.2454 57.6888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 147.9454 54.0888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 147.9454 51.1888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 148.1454 48.1888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 147.2454 45.7888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 148.1454 41.9888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 147.1454 38.9888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 149.4454 37.1888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 148.3454 34.4888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 152.0454 34.7888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 155.0454 33.6888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 158.3454 34.7888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 164.9454 34.2888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 172.9454 34.4888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 180.4454 34.4888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 187.9454 40.3888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 181.2454 40.5888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 174.1454 40.9888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 166.3454 40.9888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 151.8454 40.5888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 157.5454 41.3888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 151.8454 48.4888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 187.5454 48.0888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 181.3454 48.6888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 173.5454 48.5888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 165.6454 49.1888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 157.8454 49.3888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 151.7454 55.8888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 158.3454 56.8888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 165.5454 56.9888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 173.9454 57.3888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 180.7454 56.6888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 188.2454 56.1888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 188.1454 62.8888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 180.3454 64.2888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 172.6454 64.2888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 165.0454 64.3888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 157.5454 64.2888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 116.9454 37.6888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 105.7454 33.9888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 112.8454 33.5888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 114.4454 34.3888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 117.5454 34.2888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 117.5454 34.2888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 140.6454 33.2888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 138.6454 36.6888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 140.8454 38.8888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 139.3454 41.5888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 141.3454 44.9888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 138.8454 53.3888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 142.1454 55.9888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 137.5454 58.8888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 137.8454 62.3888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 141.9454 63.8888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 140.9454 62.2888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 138.1454 63.6888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 139.0454 66.4888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 142.1454 66.5888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 136.8454 67.5888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 132.9454 64.4888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 130.8454 62.7888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 120.6454 62.1888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 126.2454 63.3888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 126.1454 67.3888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 121.8454 67.6888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 119.5454 73.5888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 118.1454 73.5888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 126.3454 73.0888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 129.0454 69.9888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 130.1454 73.7888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 131.2454 73.8888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 136.6454 74.2888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 133.5454 74.0888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 134.3454 72.0888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 133.7454 69.1888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 142.2454 74.6888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 139.4454 74.4888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 138.7454 71.4888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 140.5454 69.6888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 148.8454 65.6888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 148.8454 67.6888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 147.8454 72.0888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 151.8454 71.0888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 159.1454 70.8888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 167.1454 71.1888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 181.6454 70.7888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 174.4454 70.9888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 172.9454 73.0888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 172.9454 73.0888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 188.2454 70.1888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 187.6454 73.2888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 180.3454 73.4888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 187.2454 78.4888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 185.1454 82.1888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 181.9454 78.7888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 178.7454 81.8888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 175.4454 78.0888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 171.9454 81.5888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 167.4454 78.2888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 167.4454 78.2888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 166.5454 82.1888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 159.8454 78.2888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 159.8454 78.2888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 158.2454 83.4888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 152.5454 77.9888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 151.5454 83.1888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 148.1454 79.1888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 146.5454 83.1888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 141.7454 79.9888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 139.9454 81.1888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 139.9454 81.1888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 138.3454 83.0888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 136.8454 80.3888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 134.0454 83.5888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 130.8454 80.3888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 128.7454 81.4888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 126.2454 80.3888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 124.2454 80.9888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 122.1454 78.8888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 121.8454 76.6888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 117.2454 78.6888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 114.9454 78.2888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 110.3454 77.0888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 109.0454 78.9888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 107.5454 80.9888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 99.7454 74.6888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 103.5454 75.0888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 105.8454 75.3888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 108.6454 75.2888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 108.6454 75.2888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 109.5454 72.1888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 108.4454 69.4888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 113.5454 72.5888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 112.4454 72.1888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 111.7454 69.6888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 113.4454 70.4888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 120.6454 68.6888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 118.2454 68.2888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 120.2454 65.5888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 118.9454 61.9888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 113.4454 61.0888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 114.7454 56.7888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 112.7454 54.7888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 116.0454 53.0888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 106.8454 53.1888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 103.9454 52.2888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 107.6454 50.2888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 103.5454 46.0888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 99.3454 45.1888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 103.7454 42.4888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 102.1454 40.8888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 101.0454 37.9888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 101.7454 35.1888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 98.3454 34.9888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 94.0454 36.0888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 91.1454 39.5888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 92.4454 42.5888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 91.1454 44.3888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 92.6454 45.4888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 91.5454 48.0888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 92.8454 50.5888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 91.2454 52.7888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 92.6454 54.9888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 91.6454 57.7888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 92.5454 60.0888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 91.5454 62.3888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 92.4454 64.7888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 90.4454 66.9888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 92.3454 69.8888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 91.6454 73.2888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 91.3454 77.1888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 93.4454 80.5888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 104.4454 81.7888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module penguiconbadge:SOT223-6 (layer F.Cu) (tedit 570B03D0)
    (at 114.8854 65.5828 270)
    (fp_text reference U4 (at 0 5.3 270) (layer F.SilkS))
    (fp_text value TPS73733DCQR (at 0 -0.5 270) (layer F.Fab))
    (pad 6 smd rect (at 0 -3.1 270) (size 3.45 2.15) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 3.1 270) (size 0.55 2.15) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1.27 3.1 270) (size 0.55 2.15) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 1 smd rect (at -2.54 3.1 270) (size 0.55 2.15) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 4 smd rect (at 1.27 3.1 270) (size 0.55 2.15) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(C10-Pad1)"))
    (pad 5 smd rect (at 2.54 3.1 270) (size 0.55 2.15) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
  )
  (module ESP8266:ESP-12E (layer F.Cu) (tedit 559F8D21)
    (at 119.89 41.91)
    (descr "Module, ESP-8266, ESP-12, 16 pad, SMD")
    (tags "Module ESP-8266 ESP8266")
    (fp_text reference U2 (at -2 -2) (layer F.SilkS))
    (fp_text value ESP-12E (at 8 1) (layer F.Fab))
    (fp_text user "No Copper" (at 8.38 -5.4) (layer F.CrtYd))
    (pad 9 smd oval (at 2.99 15.75 90) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(U2-Pad9)"))
    (pad 10 smd oval (at 4.99 15.75 90) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(U2-Pad10)"))
    (pad 11 smd oval (at 6.99 15.75 90) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(U2-Pad11)"))
    (pad 12 smd oval (at 8.99 15.75 90) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(U2-Pad12)"))
    (pad 13 smd oval (at 10.99 15.75 90) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(U2-Pad13)"))
    (pad 14 smd oval (at 12.99 15.75 90) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(U2-Pad14)"))
    (pad 1 smd rect (at 0 0) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(C5-Pad2)"))
    (pad 2 smd oval (at 0 2) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 17 ADC))
    (pad 3 smd oval (at 0 4) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R9-Pad1)"))
    (pad 4 smd oval (at 0 6) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 24 /GPIO16))
    (pad 5 smd oval (at 0 8) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 25 /GPIO14))
    (pad 6 smd oval (at 0 10) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 26 /GPIO12))
    (pad 7 smd oval (at 0 12) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 27 /GPIO13))
    (pad 8 smd oval (at 0 14) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 15 smd oval (at 16 14) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 16 smd oval (at 16 12) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 17 smd oval (at 16 10) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 18 smd oval (at 16 8) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(SW2-Pad1)"))
    (pad 19 smd oval (at 16 6) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 28 /GPIO5))
    (pad 20 smd oval (at 16 4) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 15 BATT_CHECK))
    (pad 21 smd oval (at 16 2) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 14 /RXD))
    (pad 22 smd oval (at 16 0) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 13 /TXD))
    (model ${ESPLIB}/ESP8266.3dshapes/ESP-12.wrl
      (at (xyz 0.04 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
    (model /home/nristow/Dropbox/kicad/kicad-ESP8266/ESP8266.3dshapes/ESP-12.wrl
      (at (xyz 0.04 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 56CB8B3D)
    (at 96.5454 40.1828 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference BT1 (at 0.0508 5.0038 180) (layer F.SilkS))
    (fp_text value "LiPO 1S" (at 2.5908 1.2446 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +BATT))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 125 73 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -2.4888 0.0442 90) (layer F.SilkS))
    (fp_text value 0.1u (at -1.676 1.238 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 /VIN))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 123 73 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -2.438 0.063 90) (layer F.SilkS))
    (fp_text value 1.0u (at -0.0758 -1.4356 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 /VIN))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 124 68)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 /VDD))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeA_EIA-3216_Wave (layer F.Cu) (tedit 0)
    (at 124 64 90)
    (descr "Tantal Cap. , Size A, EIA-3216, Wave,")
    (tags "Tantal Cap. , Size A, EIA-3216, Wave,")
    (attr smd)
    (fp_text reference C4 (at 0.5 -1.9276 90) (layer F.SilkS))
    (fp_text value 4.7u (at -0.09906 3.0988 90) (layer F.Fab))
    (fp_text user + (at -3.6148 -1.8006 90) (layer F.SilkS))
    (pad 2 smd rect (at 1.50114 0 90) (size 2.14884 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (pad 1 smd rect (at -1.50114 0 90) (size 2.14884 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 4 /VDD))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeA_EIA-3216_Wave.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 103.5454 48.0568 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at -2.413 0 180) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 RESET))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(C5-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 104 65)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 4.7UF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 /VIN))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 99 69 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 2.5282 0.1108 90) (layer F.SilkS))
    (fp_text value 4.7UF (at 3.8744 -0.0924 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 108.8644 64.3128 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 1u (at -2.8174 -0.0438 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 111.7854 60.9988 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at 2.431 0.1002 90) (layer F.SilkS))
    (fp_text value 1u (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 108.9914 66.8528 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at 2.8374 0.056 180) (layer F.SilkS))
    (fp_text value 1u (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210 (layer F.Cu) (tedit 5415D85D)
    (at 149 75)
    (descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C12 (at 0 -2.7) (layer F.SilkS))
    (fp_text value 100uf (at 0 2.7) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 186.4614 35.3568 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C13 (at 0.9398 -2.4638 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 157.48 37.465 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at 2.3622 -0.0508 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 165.1 37.465 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at 2.3368 -0.0254 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 172.72 37.35 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C16 (at 2.3488 -0.1016 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 180.34 37.465 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C17 (at 2.2098 -0.0254 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 187.2234 43.7388 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C18 (at 2.2352 -0.762 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 157.48 45.085 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C19 (at 2.2606 -0.1524 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 165.1 45.085 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C20 (at 2.2352 -0.0762 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 172.72 45.085 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C21 (at 2.3114 -0.127 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 180.34 45.085 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C22 (at 2.2098 -0.0762 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 186.9694 51.3588 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C23 (at 2.5146 -0.4826 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 157.48 52.705 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C24 (at 2.1336 -0.1778 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 165.1 52.82 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C25 (at 2.3502 -0.1524 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 172.72 52.705 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C26 (at 2.3876 -0.127 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 180.34 52.705 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C27 (at 2.3114 -0.1778 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 186.9694 58.9788 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C28 (at 2.4892 -0.4064 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 157.48 60.325 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C29 (at 2.3368 -0.0508 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 165.1 60.325 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C30 (at 2.1082 -0.2794 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 172.72 60.325 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C31 (at 2.2098 -0.0762 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 180.34 60.325 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C32 (at 2.3114 -0.1016 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 186.9694 66.5988 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C33 (at 2.5908 -0.3302 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 157.48 67.945 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C34 (at 2.3622 -0.2032 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 165.1 68.06 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C35 (at 2.274 0 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 172.72 67.945 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C36 (at 2.3368 -0.0254 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 180.34 67.945 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C37 (at 2.2098 -0.0508 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-1206 (layer F.Cu) (tedit 56CC45C5)
    (at 102 73)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D1 (at -3.1432 0.0758 90) (layer F.SilkS))
    (fp_text value CHARGE (at 0 2) (layer F.SilkS))
    (pad 2 smd rect (at 1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D1-Pad1)"))
  )
  (module Connect:USB_Micro-B (layer F.Cu) (tedit 5543E447)
    (at 116 77)
    (descr "Micro USB Type B Receptacle")
    (tags "USB USB_B USB_micro USB_OTG")
    (attr smd)
    (fp_text reference P3 (at -2.1064 -3.3146) (layer F.SilkS))
    (fp_text value USB_OTG (at 0 4.8) (layer F.Fab))
    (pad 1 smd rect (at -1.3009 -1.56254 90) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 /VIN))
    (pad 2 smd rect (at -0.6509 -1.56254 90) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(P3-Pad2)"))
    (pad 3 smd rect (at -0.0009 -1.56254 90) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(P3-Pad3)"))
    (pad 4 smd rect (at 0.6491 -1.56254 90) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(P3-Pad4)"))
    (pad 5 smd rect (at 1.2991 -1.56254 90) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at -2.5009 -1.56254 90) (size 0.95 1.25) (drill oval 0.55 0.85) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P3-Pad6)"))
    (pad 6 thru_hole oval (at 2.4991 -1.56254 90) (size 0.95 1.25) (drill oval 0.55 0.85) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P3-Pad6)"))
    (pad 6 thru_hole oval (at -3.5009 1.13746 90) (size 1.55 1) (drill oval 1.15 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P3-Pad6)"))
    (pad 6 thru_hole oval (at 3.4991 1.13746 90) (size 1.55 1) (drill oval 1.15 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P3-Pad6)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 0)
    (at 144.8054 35.8648)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at -3.0226 -0.1524) (layer F.SilkS))
    (fp_text value CONN_01X08 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(P4-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 58 "Net-(P4-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 59 "Net-(P4-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(P4-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 61 "Net-(P4-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 62 "Net-(P4-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 63 "Net-(P4-Pad8)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 570A87BE)
    (at 96.5454 45.2628)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at 0 -5.1) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 RESET))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 +3V3))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 /VIN))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 64 "Net-(P5-Pad6)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 0)
    (at 137.62 78 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P6 (at -2.5366 -0.1496 360) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 RESET))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /TXD))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /RXD))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(P6-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 71 "Net-(P6-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 0)
    (at 144.8054 57.7088)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P7 (at 2.4638 -0.3048 90) (layer F.SilkS))
    (fp_text value CONN_01X08 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 56 "Net-(P7-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /GPIO16))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /GPIO14))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /GPIO13))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /GPIO12))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /GPIO5))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /TXD))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /RXD))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 0)
    (at 96.5454 62.7888)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P8 (at 0 -19.812) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 ADC))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 65 "Net-(P8-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 66 "Net-(P8-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 67 "Net-(P8-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 68 "Net-(P8-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(P8-Pad6)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 101.89 44.44 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0.0408 1.7674 90) (layer F.SilkS))
    (fp_text value 2.4k (at -0.3402 2.9612 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 ADC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 128 75)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 2.3782 0.0316) (layer F.SilkS))
    (fp_text value 4.7K (at 1.921 -1.213 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 /VIN))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 /RST))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 101.89 48 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0.0448 1.7166 90) (layer F.SilkS))
    (fp_text value 750 (at 0.0194 3.0882 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(Q1-Pad3)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 ADC))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 116.5454 48.3108 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -2.2606 -0.0508 180) (layer F.SilkS))
    (fp_text value 10K (at -0.0762 3.4036 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(C5-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 105.7 53.33 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 1.4546 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 BATT_CHECK))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 118 70)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -2.3792 0.0786) (layer F.SilkS))
    (fp_text value 27 (at 2.4214 -0.023) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(P3-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 /D-))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 118 72)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -2.4808 0.1868) (layer F.SilkS))
    (fp_text value 27 (at 2.3452 0.0344) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(P3-Pad3)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 /D+))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 116.5454 46.5328)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 2.2606 0.254) (layer F.SilkS))
    (fp_text value 10k (at -2.6924 1.8034) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R9-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 107 73 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 470 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 /VIN))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 101 65)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 2K (at -0.1366 1.5988) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R12-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-28-1EP_5x5mm_Pitch0.5mm (layer F.Cu) (tedit 54130A77)
    (at 129 70)
    (descr "28-Lead Plastic Quad Flat, No Lead Package (MQ) - 5x5x0.9 mm Body [QFN or VQFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U1 (at 0 -3.875) (layer F.SilkS))
    (fp_text value CP2102 (at 4.0198 0.3072 90) (layer F.Fab))
    (pad 1 smd oval (at -2.45 -1.5) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(U1-Pad1)"))
    (pad 2 smd oval (at -2.45 -1) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(U1-Pad2)"))
    (pad 3 smd oval (at -2.45 -0.5) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (pad 4 smd oval (at -2.45 0) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 20 /D+))
    (pad 5 smd oval (at -2.45 0.5) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 /D-))
    (pad 6 smd oval (at -2.45 1) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 /VDD))
    (pad 7 smd oval (at -2.45 1.5) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 /VIN))
    (pad 8 smd oval (at -1.5 2.45 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 /VIN))
    (pad 9 smd oval (at -1 2.45 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 /RST))
    (pad 10 smd oval (at -0.5 2.45 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd oval (at 0 2.45 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(U1-Pad11)"))
    (pad 12 smd oval (at 0.5 2.45 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(U1-Pad12)"))
    (pad 13 smd oval (at 1 2.45 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd oval (at 1.5 2.45 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd oval (at 2.45 1.5) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd oval (at 2.45 1) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd oval (at 2.45 0.5) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd oval (at 2.45 0) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd oval (at 2.45 -0.5) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd oval (at 2.45 -1) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd oval (at 2.45 -1.5) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd oval (at 1.5 -2.45 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd oval (at 1 -2.45 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(U1-Pad23)"))
    (pad 24 smd oval (at 0.5 -2.45 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U1-Pad24)"))
    (pad 25 smd oval (at 0 -2.45 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 13 /TXD))
    (pad 26 smd oval (at -0.5 -2.45 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /RXD))
    (pad 27 smd oval (at -1 -2.45 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U1-Pad27)"))
    (pad 28 smd oval (at -1.5 -2.45 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 RESET))
    (pad 29 smd rect (at 0.8375 0.8375) (size 1.675 1.675) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 29 smd rect (at 0.8375 -0.8375) (size 1.675 1.675) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 29 smd rect (at -0.8375 0.8375) (size 1.675 1.675) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 29 smd rect (at -0.8375 -0.8375) (size 1.675 1.675) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/QFN-28-1EP_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 55360473)
    (at 102 68.9)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U3 (at 2.8004 -0.1676) (layer F.SilkS))
    (fp_text value MCP73831T (at -0.1714 2.347) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 /VIN))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R12-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-1206 (layer F.Cu) (tedit 56CB8AD4)
    (at 102 77)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D2 (at -3.067 0.0128 90) (layer F.SilkS))
    (fp_text value POWER (at 0 2) (layer F.SilkS))
    (pad 2 smd rect (at 1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 106.75 77 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 390 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(D2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 117.1194 56.6928 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C38 (at 0.0508 1.4986 180) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeA_EIA-3216_Wave (layer F.Cu) (tedit 0)
    (at 115.8494 59.2328 180)
    (descr "Tantal Cap. , Size A, EIA-3216, Wave,")
    (tags "Tantal Cap. , Size A, EIA-3216, Wave,")
    (attr smd)
    (fp_text reference C39 (at -0.0254 -1.9812 180) (layer F.SilkS))
    (fp_text value 10uf (at -2.032 -3.3274 180) (layer F.Fab))
    (fp_text user + (at -3.59918 -1.80086 180) (layer F.SilkS))
    (pad 2 smd rect (at 1.50114 0 180) (size 2.14884 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.50114 0 180) (size 2.14884 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeA_EIA-3216_Wave.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module penguiconbadge:rgb_led_pth_spaced_leads (layer F.Cu) (tedit 56FA3C17)
    (at 153.67 38.1)
    (descr "5mm common cathode RGB LED")
    (tags "RGB LED 5mm Common Cathode")
    (fp_text reference U6 (at 0 -2.25) (layer F.SilkS))
    (fp_text value WS8212-TH (at 0 6.25) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 -0.3) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 27 /GPIO13))
    (pad 2 thru_hole rect (at 0 1.2) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 +3V3))
    (pad 3 thru_hole oval (at 0 2.6) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 4.1) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(U6-Pad4)"))
  )
  (module penguiconbadge:rgb_led_pth_spaced_leads (layer F.Cu) (tedit 56FA3C17)
    (at 161.29 38.1)
    (descr "5mm common cathode RGB LED")
    (tags "RGB LED 5mm Common Cathode")
    (fp_text reference U7 (at 0 -2.25) (layer F.SilkS))
    (fp_text value WS8212-TH (at 0 6.25) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 -0.3) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(U6-Pad4)"))
    (pad 2 thru_hole rect (at 0 1.2) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 +3V3))
    (pad 3 thru_hole oval (at 0 2.6) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 4.1) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(U7-Pad4)"))
  )
  (module penguiconbadge:rgb_led_pth_spaced_leads (layer F.Cu) (tedit 56FA3C17)
    (at 168.91 38.1)
    (descr "5mm common cathode RGB LED")
    (tags "RGB LED 5mm Common Cathode")
    (fp_text reference U8 (at 0 -2.25) (layer F.SilkS))
    (fp_text value WS8212-TH (at 0 6.25) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 -0.3) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(U7-Pad4)"))
    (pad 2 thru_hole rect (at 0 1.2) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 +3V3))
    (pad 3 thru_hole oval (at 0 2.6) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 4.1) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(U8-Pad4)"))
  )
  (module penguiconbadge:rgb_led_pth_spaced_leads (layer F.Cu) (tedit 56FA3C17)
    (at 176.53 38.1)
    (descr "5mm common cathode RGB LED")
    (tags "RGB LED 5mm Common Cathode")
    (fp_text reference U9 (at 0 -2.25) (layer F.SilkS))
    (fp_text value WS8212-TH (at 0 6.25) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 -0.3) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(U8-Pad4)"))
    (pad 2 thru_hole rect (at 0 1.2) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 +3V3))
    (pad 3 thru_hole oval (at 0 2.6) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 4.1) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(U10-Pad1)"))
  )
  (module penguiconbadge:rgb_led_pth_spaced_leads (layer F.Cu) (tedit 56FA3C17)
    (at 184.15 38.1)
    (descr "5mm common cathode RGB LED")
    (tags "RGB LED 5mm Common Cathode")
    (fp_text reference U10 (at 0 -2.25) (layer F.SilkS))
    (fp_text value WS8212-TH (at 0 6.25) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 -0.3) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(U10-Pad1)"))
    (pad 2 thru_hole rect (at 0 1.2) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 +3V3))
    (pad 3 thru_hole oval (at 0 2.6) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 4.1) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(U10-Pad4)"))
  )
  (module penguiconbadge:rgb_led_pth_spaced_leads (layer F.Cu) (tedit 56FA3C17)
    (at 153.67 45.72)
    (descr "5mm common cathode RGB LED")
    (tags "RGB LED 5mm Common Cathode")
    (fp_text reference U11 (at 0 -2.25) (layer F.SilkS))
    (fp_text value WS8212-TH (at 0 6.25) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 -0.3) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(U10-Pad4)"))
    (pad 2 thru_hole rect (at 0 1.2) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 +3V3))
    (pad 3 thru_hole oval (at 0 2.6) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 4.1) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(U11-Pad4)"))
  )
  (module penguiconbadge:rgb_led_pth_spaced_leads (layer F.Cu) (tedit 56FA3C17)
    (at 161.29 45.72)
    (descr "5mm common cathode RGB LED")
    (tags "RGB LED 5mm Common Cathode")
    (fp_text reference U12 (at 0 -2.25) (layer F.SilkS))
    (fp_text value WS8212-TH (at 0 6.25) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 -0.3) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(U11-Pad4)"))
    (pad 2 thru_hole rect (at 0 1.2) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 +3V3))
    (pad 3 thru_hole oval (at 0 2.6) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 4.1) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(U12-Pad4)"))
  )
  (module penguiconbadge:rgb_led_pth_spaced_leads (layer F.Cu) (tedit 56FA3C17)
    (at 168.91 45.72)
    (descr "5mm common cathode RGB LED")
    (tags "RGB LED 5mm Common Cathode")
    (fp_text reference U13 (at 0 -2.25) (layer F.SilkS))
    (fp_text value WS8212-TH (at 0 6.25) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 -0.3) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(U12-Pad4)"))
    (pad 2 thru_hole rect (at 0 1.2) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 +3V3))
    (pad 3 thru_hole oval (at 0 2.6) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 4.1) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(U13-Pad4)"))
  )
  (module penguiconbadge:rgb_led_pth_spaced_leads (layer F.Cu) (tedit 56FA3C17)
    (at 176.53 45.72)
    (descr "5mm common cathode RGB LED")
    (tags "RGB LED 5mm Common Cathode")
    (fp_text reference U14 (at 0 -2.25) (layer F.SilkS))
    (fp_text value WS8212-TH (at 0 6.25) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 -0.3) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(U13-Pad4)"))
    (pad 2 thru_hole rect (at 0 1.2) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 +3V3))
    (pad 3 thru_hole oval (at 0 2.6) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 4.1) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(U14-Pad4)"))
  )
  (module penguiconbadge:rgb_led_pth_spaced_leads (layer F.Cu) (tedit 56FA3C17)
    (at 184.15 45.72)
    (descr "5mm common cathode RGB LED")
    (tags "RGB LED 5mm Common Cathode")
    (fp_text reference U15 (at 0 -2.25) (layer F.SilkS))
    (fp_text value WS8212-TH (at 0 6.25) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 -0.3) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(U14-Pad4)"))
    (pad 2 thru_hole rect (at 0 1.2) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 +3V3))
    (pad 3 thru_hole oval (at 0 2.6) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 4.1) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(U15-Pad4)"))
  )
  (module penguiconbadge:rgb_led_pth_spaced_leads (layer F.Cu) (tedit 56FA3C17)
    (at 153.67 53.34)
    (descr "5mm common cathode RGB LED")
    (tags "RGB LED 5mm Common Cathode")
    (fp_text reference U16 (at 0 -2.25) (layer F.SilkS))
    (fp_text value WS8212-TH (at 0 6.25) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 -0.3) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(U15-Pad4)"))
    (pad 2 thru_hole rect (at 0 1.2) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 +3V3))
    (pad 3 thru_hole oval (at 0 2.6) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 4.1) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(U16-Pad4)"))
  )
  (module penguiconbadge:rgb_led_pth_spaced_leads (layer F.Cu) (tedit 56FA3C17)
    (at 161.29 53.34)
    (descr "5mm common cathode RGB LED")
    (tags "RGB LED 5mm Common Cathode")
    (fp_text reference U17 (at 0 -2.25) (layer F.SilkS))
    (fp_text value WS8212-TH (at 0 6.25) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 -0.3) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(U16-Pad4)"))
    (pad 2 thru_hole rect (at 0 1.2) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 +3V3))
    (pad 3 thru_hole oval (at 0 2.6) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 4.1) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(U17-Pad4)"))
  )
  (module penguiconbadge:rgb_led_pth_spaced_leads (layer F.Cu) (tedit 56FA3C17)
    (at 168.91 53.34)
    (descr "5mm common cathode RGB LED")
    (tags "RGB LED 5mm Common Cathode")
    (fp_text reference U18 (at 0 -2.25) (layer F.SilkS))
    (fp_text value WS8212-TH (at 0 6.25) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 -0.3) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(U17-Pad4)"))
    (pad 2 thru_hole rect (at 0 1.2) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 +3V3))
    (pad 3 thru_hole oval (at 0 2.6) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 4.1) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(U18-Pad4)"))
  )
  (module penguiconbadge:rgb_led_pth_spaced_leads (layer F.Cu) (tedit 56FA3C17)
    (at 176.53 53.34)
    (descr "5mm common cathode RGB LED")
    (tags "RGB LED 5mm Common Cathode")
    (fp_text reference U19 (at 0 -2.25) (layer F.SilkS))
    (fp_text value WS8212-TH (at 0 6.25) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 -0.3) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(U18-Pad4)"))
    (pad 2 thru_hole rect (at 0 1.2) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 +3V3))
    (pad 3 thru_hole oval (at 0 2.6) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 4.1) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(U19-Pad4)"))
  )
  (module penguiconbadge:rgb_led_pth_spaced_leads (layer F.Cu) (tedit 56FA3C17)
    (at 184.15 53.34)
    (descr "5mm common cathode RGB LED")
    (tags "RGB LED 5mm Common Cathode")
    (fp_text reference U20 (at 0 -2.25) (layer F.SilkS))
    (fp_text value WS8212-TH (at 0 6.25) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 -0.3) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(U19-Pad4)"))
    (pad 2 thru_hole rect (at 0 1.2) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 +3V3))
    (pad 3 thru_hole oval (at 0 2.6) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 4.1) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(U20-Pad4)"))
  )
  (module penguiconbadge:rgb_led_pth_spaced_leads (layer F.Cu) (tedit 56FA3C17)
    (at 153.67 60.96)
    (descr "5mm common cathode RGB LED")
    (tags "RGB LED 5mm Common Cathode")
    (fp_text reference U21 (at 0 -2.25) (layer F.SilkS))
    (fp_text value WS8212-TH (at 0 6.25) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 -0.3) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(U20-Pad4)"))
    (pad 2 thru_hole rect (at 0 1.2) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 +3V3))
    (pad 3 thru_hole oval (at 0 2.6) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 4.1) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(U21-Pad4)"))
  )
  (module penguiconbadge:rgb_led_pth_spaced_leads (layer F.Cu) (tedit 56FA3C17)
    (at 161.29 60.96)
    (descr "5mm common cathode RGB LED")
    (tags "RGB LED 5mm Common Cathode")
    (fp_text reference U22 (at 0 -2.25) (layer F.SilkS))
    (fp_text value WS8212-TH (at 0 6.25) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 -0.3) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(U21-Pad4)"))
    (pad 2 thru_hole rect (at 0 1.2) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 +3V3))
    (pad 3 thru_hole oval (at 0 2.6) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 4.1) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(U22-Pad4)"))
  )
  (module penguiconbadge:rgb_led_pth_spaced_leads (layer F.Cu) (tedit 56FA3C17)
    (at 168.91 60.96)
    (descr "5mm common cathode RGB LED")
    (tags "RGB LED 5mm Common Cathode")
    (fp_text reference U23 (at 0 -2.25) (layer F.SilkS))
    (fp_text value WS8212-TH (at 0 6.25) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 -0.3) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(U22-Pad4)"))
    (pad 2 thru_hole rect (at 0 1.2) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 +3V3))
    (pad 3 thru_hole oval (at 0 2.6) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 4.1) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(U23-Pad4)"))
  )
  (module penguiconbadge:rgb_led_pth_spaced_leads (layer F.Cu) (tedit 56FA3C17)
    (at 176.53 60.96)
    (descr "5mm common cathode RGB LED")
    (tags "RGB LED 5mm Common Cathode")
    (fp_text reference U24 (at 0 -2.25) (layer F.SilkS))
    (fp_text value WS8212-TH (at 0 6.25) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 -0.3) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(U23-Pad4)"))
    (pad 2 thru_hole rect (at 0 1.2) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 +3V3))
    (pad 3 thru_hole oval (at 0 2.6) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 4.1) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(U24-Pad4)"))
  )
  (module penguiconbadge:rgb_led_pth_spaced_leads (layer F.Cu) (tedit 56FA3C17)
    (at 184.15 60.96)
    (descr "5mm common cathode RGB LED")
    (tags "RGB LED 5mm Common Cathode")
    (fp_text reference U25 (at 0 -2.25) (layer F.SilkS))
    (fp_text value WS8212-TH (at 0 6.25) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 -0.3) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(U24-Pad4)"))
    (pad 2 thru_hole rect (at 0 1.2) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 +3V3))
    (pad 3 thru_hole oval (at 0 2.6) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 4.1) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(U25-Pad4)"))
  )
  (module penguiconbadge:rgb_led_pth_spaced_leads (layer F.Cu) (tedit 56FA3C17)
    (at 153.67 68.58)
    (descr "5mm common cathode RGB LED")
    (tags "RGB LED 5mm Common Cathode")
    (fp_text reference U26 (at 0 -2.25) (layer F.SilkS))
    (fp_text value WS8212-TH (at 0 6.25) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 -0.3) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(U25-Pad4)"))
    (pad 2 thru_hole rect (at 0 1.2) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 +3V3))
    (pad 3 thru_hole oval (at 0 2.6) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 4.1) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(U26-Pad4)"))
  )
  (module penguiconbadge:rgb_led_pth_spaced_leads (layer F.Cu) (tedit 56FA3C17)
    (at 161.29 68.58)
    (descr "5mm common cathode RGB LED")
    (tags "RGB LED 5mm Common Cathode")
    (fp_text reference U27 (at 0 -2.25) (layer F.SilkS))
    (fp_text value WS8212-TH (at 0 6.25) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 -0.3) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(U26-Pad4)"))
    (pad 2 thru_hole rect (at 0 1.2) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 +3V3))
    (pad 3 thru_hole oval (at 0 2.6) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 4.1) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(U27-Pad4)"))
  )
  (module penguiconbadge:rgb_led_pth_spaced_leads (layer F.Cu) (tedit 56FA3C17)
    (at 168.91 68.58)
    (descr "5mm common cathode RGB LED")
    (tags "RGB LED 5mm Common Cathode")
    (fp_text reference U28 (at 0 -2.25) (layer F.SilkS))
    (fp_text value WS8212-TH (at 0 6.25) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 -0.3) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(U27-Pad4)"))
    (pad 2 thru_hole rect (at 0 1.2) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 +3V3))
    (pad 3 thru_hole oval (at 0 2.6) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 4.1) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(U28-Pad4)"))
  )
  (module penguiconbadge:rgb_led_pth_spaced_leads (layer F.Cu) (tedit 56FA3C17)
    (at 176.53 68.58)
    (descr "5mm common cathode RGB LED")
    (tags "RGB LED 5mm Common Cathode")
    (fp_text reference U29 (at 0 -2.25) (layer F.SilkS))
    (fp_text value WS8212-TH (at 0 6.25) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 -0.3) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(U28-Pad4)"))
    (pad 2 thru_hole rect (at 0 1.2) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 +3V3))
    (pad 3 thru_hole oval (at 0 2.6) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 4.1) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(U29-Pad4)"))
  )
  (module penguiconbadge:rgb_led_pth_spaced_leads (layer F.Cu) (tedit 56FA3C17)
    (at 184.15 68.58)
    (descr "5mm common cathode RGB LED")
    (tags "RGB LED 5mm Common Cathode")
    (fp_text reference U30 (at 0 -2.25) (layer F.SilkS))
    (fp_text value WS8212-TH (at 0 6.25) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 -0.3) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(U29-Pad4)"))
    (pad 2 thru_hole rect (at 0 1.2) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 +3V3))
    (pad 3 thru_hole oval (at 0 2.6) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 4.1) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(U30-Pad4)"))
  )
  (module TO_SOT_Packages_SMD:SOT-323 (layer F.Cu) (tedit 0)
    (at 102.0454 52.0888 180)
    (tags "SMD SOT")
    (attr smd)
    (fp_text reference Q1 (at 0.127 -2.032 180) (layer F.SilkS))
    (fp_text value RUU002N05 (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at -0.65024 -0.94996 180) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 15 BATT_CHECK))
    (pad 1 smd rect (at 0.65024 -0.94996 180) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 0.94996 180) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(Q1-Pad3)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-323.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module penguiconbadge:SW_SPST_B3S-1100 (layer F.Cu) (tedit 57102E24)
    (at 110.1 40.15 180)
    (descr "Surface Mount Tactile Switch for High-Density Packaging with Ground Terminal")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference PROGRAM (at 0 4.5612 180) (layer F.SilkS))
    (fp_text value PROGRAM (at 0 4.6612 180) (layer F.SilkS))
    (pad 1 smd rect (at -3.975 -2.25 180) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(SW2-Pad1)"))
    (pad 1 smd rect (at 3.975 -2.25 180) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(SW2-Pad1)"))
    (pad 2 smd rect (at -3.975 2.25 180) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 3.975 2.25 180) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 3.9 0 180) (size 1.7 1.3) (layers F.Cu F.Paste F.Mask))
  )
  (module penguiconbadge:SW_SPST_B3S-1100 (layer F.Cu) (tedit 57102E29)
    (at 110.0454 48.15 180)
    (descr "Surface Mount Tactile Switch for High-Density Packaging with Ground Terminal")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference RESET (at -0.1 -4.4388 180) (layer F.SilkS))
    (fp_text value RESET (at 0 -4.3388 180) (layer F.SilkS))
    (pad 1 smd rect (at -3.975 -2.25 180) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 3.975 -2.25 180) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -3.975 2.25 180) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(C5-Pad2)"))
    (pad 2 smd rect (at 3.975 2.25 180) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(C5-Pad2)"))
    (pad 3 smd rect (at 3.9 0 180) (size 1.7 1.3) (layers F.Cu F.Paste F.Mask))
  )
  (module kicadmade:KiCad-Logo_Copper_11mmx5mm (layer F.Cu) (tedit 56780A65)
    (at 105.1454 58.3888)
    (fp_text reference G*** (at -0.8 -1.6) (layer Cmts.User))
    (fp_text value "KiCad Logo" (at 2.8 -1) (layer F.SilkS) hide)
    (fp_text user "DESIGNED WITH" (at 0 2.6) (layer F.SilkS))
    (pad 1 smd circle (at -2.17 -1.49) (size 0.9 0.9) (layers F.Cu F.Mask)
      (solder_mask_margin -0.01))
  )
  (module Symbols:Symbol_OSHW-Logo_SilkScreen (layer B.Cu) (tedit 5710277E)
    (at 156.3454 80.9888 180)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference REF** (at -3.9 1.6 180) (layer B.Fab))
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 0.30988 -6.56082 180) (layer B.Fab))
  )
  (module penguiconbadge:AHA-SILK (layer B.Cu) (tedit 0)
    (at 120.6454 45.9888 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module penguiconbadge:via (layer F.Cu) (tedit 57102814)
    (at 99.0454 82.4888)
    (fp_text reference REF** (at 0.1 -3.9) (layer F.SilkS) hide)
    (fp_text value via (at 0.1 3.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (gr_line (start 189.5454 84.4888) (end 188.5454 85.4888) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.5454 85.4888) (end 89.5454 84.4888) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 189.5454 32.9888) (end 188.0454 32.9888) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.5454 32.4888) (end 92.9454 32.4888) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 189.5454 84.4888) (end 189.5454 32.9888) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.5454 32.4888) (end 89.5454 84.4888) (layer Edge.Cuts) (width 0.1))
  (gr_text 3V3 (at 99.5934 47.8028) (layer F.SilkS))
  (gr_line (start 100.4054 32.3088) (end 179.6034 32.3088) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 187.2234 32.3088) (end 188.0454 32.9888) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 183.4134 32.3088) (end 179.6034 32.3088) (angle 180) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 96.6724 32.3088) (end 92.9454 32.4888) (angle 182.7650209) (layer Edge.Cuts) (width 0.1))
  (gr_circle (center 183.5404 32.3088) (end 181.6354 32.5628) (layer Edge.Cuts) (width 0.1))
  (gr_circle (center 96.5454 32.3088) (end 94.6404 32.5628) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.5454 85.4888) (end 188.5454 85.4888) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120.8024 79.9338) (end 125.5454 85.4888) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.4044 79.9338) (end 120.8024 79.9338) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 106.5454 85.4888) (end 111.4044 79.9338) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.5454 85.4888) (end 106.5454 85.4888) (layer Edge.Cuts) (width 0.1))
  (gr_text "ALLHANDSACTIVE.ORG\n501(c)3 NON PROFIT MAKERSPACE\nLOCATED IN DOWNTOWN ANN ARBOR, MI\n\n734-436-4924" (at 120.4214 60.2488) (layer B.SilkS))
  (gr_text RST (at 99.3394 45.1358) (layer F.SilkS))
  (gr_text "GND\n" (at 141.4526 38.481) (layer F.SilkS))
  (gr_text 16 (at 142.3416 57.785) (layer F.SilkS))
  (gr_text 14 (at 142.3924 60.2996) (layer F.SilkS))
  (gr_text 13 (at 142.4454 62.7888) (layer F.SilkS))
  (gr_text 12 (at 142.3454 65.4558) (layer F.SilkS))
  (gr_text 10 (at 142.3162 67.945) (layer F.SilkS))
  (gr_text 5 (at 142.3454 70.2888) (layer F.SilkS))
  (gr_text TX (at 142.2654 73.025) (layer F.SilkS))
  (gr_text RX (at 142.24 75.7936) (layer F.SilkS))
  (gr_text A0 (at 94.0816 62.8904) (layer F.SilkS))
  (gr_text "GND\n" (at 99.7204 52.8828) (layer F.SilkS))
  (gr_text GND (at 99.7204 55.4228) (layer F.SilkS))
  (gr_text 5V (at 99.2124 50.3428) (layer F.SilkS))
  (gr_text "FTDI " (at 134.9756 75.0062) (layer F.SilkS))
  (gr_text GND (at 124.8664 73.7108 270) (layer B.SilkS))
  (gr_text RX (at 132.6134 74.5236 270) (layer B.SilkS))
  (gr_text TX (at 135.3058 74.5744 270) (layer B.SilkS))
  (gr_text "DCR\n" (at 137.668 73.787 270) (layer B.SilkS))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 87.6554 30.4588) (xy 87.6554 85.0688) (xy 194.3354 86.1568) (xy 194.3354 25.8318) (xy 91.5924 26.7208)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 87.5254 30.5288) (xy 87.7794 86.4088) (xy 194.0814 86.4108) (xy 194.0814 24.4348) (xy 91.5924 26.4668)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.3)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.5454 32.4888) (xy 119.5454 39.4888) (xy 136.5454 39.4888) (xy 136.5454 32.4888)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.3)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.5454 32.4888) (xy 119.5454 39.4888) (xy 136.5454 39.4888) (xy 136.5454 32.4888)
      )
    )
  )
  (zone (net 1) (net_name +BATT) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.4204 63.2968) (xy 112.1664 63.0428) (xy 112.1664 61.7728) (xy 109.7534 61.7728) (xy 108.9914 62.2808)
        (xy 108.9914 63.2968)
      )
    )
  )
  (zone (net 7) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.5634 64.4398) (xy 113.5634 62.9158) (xy 117.2464 59.4868) (xy 118.0084 59.4868) (xy 118.0084 61.7728)
        (xy 114.9604 64.4398)
      )
    )
  )
)
