(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 38)
    (zones 0)
    (modules 12)
    (nets 3)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1 2)
    (pad_drill 0)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (grid_origin 104.14 52.07)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x3fff3_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber_DMG_Audio/"))
  )
  (net 0 "")
  (net 1 /GND)
  (net 2 /PWR)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /GND)
    (add_net /PWR)
  )
  (net_class GND ""
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_1x2mm (layer F.Cu) (tedit 60F5DB02)
    (at 110.49 57.15 90)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_1x01_SMD_1x2mm (at 0 2.54 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 4 smd roundrect (at 0 0 90) (size 1 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_1x2mm (layer F.Cu) (tedit 60F5DAFC)
    (at 110.49 55.5 90)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_1x01_SMD_1x2mm (at 0 2.54 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd roundrect (at 0 0 90) (size 1 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_1x2mm (layer F.Cu) (tedit 60F5DAED)
    (at 110.49 52.27 270)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_1x01_SMD_1x2mm (at 0 2.54 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0 270) (size 1 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /PWR))
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_1x2mm (layer F.Cu) (tedit 60F5DAF6)
    (at 110.49 53.94 90)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_1x01_SMD_1x2mm (at 0 2.54 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0 0 90) (size 1 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module ASJ-99H-R-HT-T_R:R (layer B.Cu) (tedit 60F5C18A)
    (at 118.11 60.96 90)
    (fp_text reference J1 (at 2.54 0 180) (layer B.SilkS))
    (fp_text value ADAM_TECH_ASJ-99H-R-HT-T/R (at 13.01 -5.915 90) (layer B.Fab))
    (pad 5 thru_hole oval (at 7 4.5 90) (size 2.4 1.2) (drill oval 1.2 0.6) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 4 thru_hole oval (at 5 3.1 90) (size 2.4 1.2) (drill oval 1.2 0.6) (layers *.Cu *.Mask)
      (net 2 /PWR))
    (pad 3 thru_hole oval (at 7 1.6 90) (size 2.4 1.2) (drill oval 1.2 0.6) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 7 -1.6 90) (size 2.4 1.2) (drill oval 1.2 0.6) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 3.9 -3.6 90) (size 2.4 1.2) (drill oval 1.2 0.6) (layers *.Cu *.Mask))
    (pad None np_thru_hole circle (at 0 -3 90) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad None np_thru_hole circle (at 0 3.5 90) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -1.1 0 90) (size 1.2 2.4) (drill oval 0.6 1.2) (layers *.Cu *.Mask)
      (net 1 /GND))
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 118.11 53.34 270)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference I2 (at 0 0) (layer F.SilkS))
    (fp_text value L_0603_1608Metric (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 126 60.96)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference M2 (at 2.54 2.54) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-3216-10_Kemet-I (layer F.Cu) (tedit 5B301BBE)
    (at 119.38 58.5 90)
    (descr "Tantalum Capacitor SMD Kemet-I (3216-10 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C2 (at -0.08 0) (layer F.SilkS))
    (fp_text value CP_EIA-3216-10_Kemet-I (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.35 0 90) (size 1.4 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185))
    (pad 2 smd roundrect (at 1.35 0 90) (size 1.4 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3216-10_Kemet-I.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-3216-10_Kemet-I (layer F.Cu) (tedit 5B301BBE)
    (at 116.84 58.5 90)
    (descr "Tantalum Capacitor SMD Kemet-I (3216-10 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C1 (at -0.08 0) (layer F.SilkS))
    (fp_text value CP_EIA-3216-10_Kemet-I (at 0 6.35 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.35 0 90) (size 1.4 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185))
    (pad 1 smd roundrect (at -1.35 0 90) (size 1.4 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3216-10_Kemet-I.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 109.82 60.97)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference M1 (at -2.54 2.54) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 123.19 59.69 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference I3 (at 0 1.27 180) (layer F.SilkS))
    (fp_text value L_0603_1608Metric (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 113.03 59.69 270)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference I1 (at 0 1.27) (layer F.SilkS))
    (fp_text value L_0603_1608Metric (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "By Z Ali" (at 125.93 55.38 90) (layer F.Mask))
  (gr_arc (start 125.73 53.34) (end 127.87 53.34) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 126.4 62.23) (end 126.4 63.7) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 109.72 62.23) (end 109.72 63.7) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_text "DMG Audio" (at 124.76 55.38 90) (layer F.Mask))
  (gr_line (start 108.25 62.23) (end 108.25 51.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 126.4 63.7) (end 109.72 63.7) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 127.87 53.34) (end 127.87 62.23) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 108.25 51.2) (end 125.73 51.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 129.54 64.77) (end 129.54 64.77) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.27 64.77) (xy 107.95 64.77) (xy 107.95 50.8) (xy 128.27 50.8)
      )
    )
  )
  (zone (net 1) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.27 64.77) (xy 107.95 64.77) (xy 107.95 50.8) (xy 128.27 50.8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.27 64.77) (xy 107.95 64.77) (xy 107.95 50.8) (xy 128.27 50.8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.27 64.77) (xy 107.95 64.77) (xy 107.95 50.8) (xy 128.27 50.8)
      )
    )
  )
)
