<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.5.2">
<drawing>
<board>
<plain>
<wire x1="0.01" y1="1.895" x2="1.905" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1.905" y1="0" x2="49.53" y2="0" width="0" layer="20"/>
<wire x1="49.53" y1="0" x2="51.435" y2="1.905" width="0" layer="20" curve="90"/>
<wire x1="51.435" y1="1.905" x2="51.435" y2="19.685" width="0" layer="20"/>
<wire x1="51.435" y1="19.685" x2="49.53" y2="21.59" width="0" layer="20" curve="90"/>
<wire x1="49.53" y1="21.59" x2="1.905" y2="21.59" width="0" layer="20"/>
<wire x1="1.905" y1="21.59" x2="0.01" y2="19.695" width="0" layer="20" curve="90"/>
<wire x1="0.01" y1="19.695" x2="0.01" y2="1.895" width="0" layer="20"/>
<text>+5V</text>
<text>GND</text>
<text>GND</text>
<text>+5V</text>
<text>.1uf</text>
<text>.1uf</text>
<text>LM7805</text>
<text>1N4001</text>
<text>+9V
Center
Positive</text>
<text>220uf</text>
<text>GND</text>
<text>VIDEO</text>
<text>Power/Video v1.3</text>
<text>voltage
test</text>
</plain>
<libraries>
<library name="v-reg">
<packages>
<package name="78XXS">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="AVR_ICSP">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RCA">
</package>
<package name="1X02">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALLEZ">
<description>This is the "EZ" version of the .1" spaced ceramic thru-hole cap.&lt;br&gt;
It has reduced top mask to make it harder to put the component on the wrong side of the board.</description>
</package>
<package name="CPOL-RADIAL-100UF-25V">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED5MM-KIT">
<description>&lt;h3&gt;LED5MM-KIT&lt;/h3&gt;
5MM Through-hole LED&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3-KIT">
<description>&lt;h3&gt;AXIAL-0.3-KIT&lt;/h3&gt;

Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of the AXIAL-0.3 package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="DCJACK_2MM_PTH">
<description>DJ Jack 2.0mm PTH Right-Angle</description>
</package>
</packages>
</library>
<library name="pot">
<description>&lt;b&gt;Potentiometers&lt;/b&gt;&lt;p&gt;
Beckman, Copal, Piher, Spectrol, Schukat&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="CA6V">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
distributor Schukat</description>
</package>
</packages>
</library>
<library name="solpad">
<description>&lt;b&gt;Solder Pads/Test Points&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="LSP11">
<description>&lt;b&gt;SOLDER PAD&lt;/b&gt;&lt;p&gt;
drill 1.1 mm</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO41-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="v-reg" package="78XXS" value="LM7805">
<attribute name="VALUE"/>
</element>
<element name="D1" library="diode" package="DO41-10" value="1N4001">
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun" package="AVR_ICSP" value="M05X2PTH"/>
<element name="JP2" library="SparkFun" package="AVR_ICSP" value="M05X2PTH"/>
<element name="JP3" library="SparkFun-Connectors" package="RCA" value="RCA"/>
<element name="C4" library="SparkFun-Capacitors" package="CAP-PTH-SMALLEZ" value="0.1uf">
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="CAP-PTH-SMALLEZ" value="0.1uf">
<attribute name="VALUE"/>
</element>
<element name="LED1" library="SparkFun-LED" package="LED5MM-KIT" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3-KIT" value="1k"/>
<element name="C2" library="SparkFun-Capacitors" package="CPOL-RADIAL-100UF-25V" value=""/>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3-KIT" value="75R"/>
<element name="JP4" library="SparkFun-Connectors" package="1X02" value="M02PTH">
<attribute name="VALUE"/>
</element>
<element name="CN1" library="adafruit" package="DCJACK_2MM_PTH" value="">
<attribute name="VALUE"/>
</element>
<element name="R3" library="pot" package="CA6V" value="">
<attribute name="VALUE"/>
</element>
<element name="LSP1" library="solpad" package="LSP11" value="LSP11">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="GND"/>
<contactref element="JP1" pad="7"/>
<contactref element="JP1" pad="5"/>
<contactref element="JP1" pad="3"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP1" pad="9"/>
<contactref element="JP2" pad="7"/>
<contactref element="JP2" pad="5"/>
<contactref element="JP2" pad="3"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP2" pad="9"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="JP3" pad="SHELL"/>
<contactref element="LED1" pad="K"/>
<contactref element="JP4" pad="2"/>
<contactref element="CN1" pad="GND"/>
<contactref element="R3" pad="A"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="OUT"/>
<contactref element="JP1" pad="8"/>
<contactref element="JP1" pad="6"/>
<contactref element="JP1" pad="4"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP1" pad="10"/>
<contactref element="JP2" pad="8"/>
<contactref element="JP2" pad="6"/>
<contactref element="JP2" pad="4"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP2" pad="10"/>
<contactref element="C4" pad="1"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="N$44">
<contactref element="D1" pad="A"/>
<contactref element="CN1" pad="PWR"/>
</signal>
<signal name="N$46">
<contactref element="IC1" pad="IN"/>
<contactref element="D1" pad="C"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="LED1" pad="A"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="N$2">
<contactref element="C2" pad="2"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="N$3">
<contactref element="JP3" pad="PIN"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="GNDBREAK">
<contactref element="CN1" pad="GNDBREAK"/>
</signal>
<signal name="N$5">
<contactref element="C2" pad="1"/>
<contactref element="LSP1" pad="MP"/>
<contactref element="R3" pad="S"/>
</signal>
<signal name="N$4">
<contactref element="R3" pad="E"/>
<contactref element="JP4" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
