(kicad_pcb (version 20171130) (host pcbnew "(5.1.0)-1")
  (general
    (thickness 1.6)
    (drawings 7)
    (tracks 98)
    (zones 0)
    (modules 14)
    (nets 40)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 1.5)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "REV1 Gerbers/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +12V)
  (net 3 +5V)
  (net 4 "Net-(R1-Pad2)")
  (net 5 "Net-(R1-Pad1)")
  (net 6 "Net-(R2-Pad2)")
  (net 7 "Net-(R2-Pad1)")
  (net 8 "Net-(R3-Pad2)")
  (net 9 "Net-(R3-Pad1)")
  (net 10 "Net-(U2-Pad16)")
  (net 11 "Net-(U2-Pad17)")
  (net 12 "Net-(U2-Pad15)")
  (net 13 "Net-(U2-Pad18)")
  (net 14 "Net-(U2-Pad14)")
  (net 15 "Net-(U2-Pad13)")
  (net 16 "Net-(U2-Pad12)")
  (net 17 "Net-(U2-Pad11)")
  (net 18 "Net-(U2-Pad22)")
  (net 19 "Net-(U2-Pad10)")
  (net 20 "Net-(U2-Pad23)")
  (net 21 "Net-(U2-Pad9)")
  (net 22 "Net-(U2-Pad24)")
  (net 23 "Net-(U2-Pad8)")
  (net 24 "Net-(U2-Pad25)")
  (net 25 "Net-(U2-Pad7)")
  (net 26 "Net-(U2-Pad6)")
  (net 27 "Net-(U2-Pad27)")
  (net 28 "Net-(U2-Pad5)")
  (net 29 "Net-(U2-Pad28)")
  (net 30 "Net-(U2-Pad3)")
  (net 31 "Net-(U2-Pad2)")
  (net 32 "Net-(U2-Pad1)")
  (net 33 "Net-(U3-Pad3)")
  (net 34 "Net-(U4-Pad3)")
  (net 35 "Net-(U5-Pad3)")
  (net 36 "Net-(J1-Pad6)")
  (net 37 "Net-(J1-Pad5)")
  (net 38 "Net-(J1-Pad4)")
  (net 39 "Net-(J1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad18)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad22)")
    (add_net "Net-(U2-Pad23)")
    (add_net "Net-(U2-Pad24)")
    (add_net "Net-(U2-Pad25)")
    (add_net "Net-(U2-Pad27)")
    (add_net "Net-(U2-Pad28)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U2-Pad9)")
    (add_net "Net-(U3-Pad3)")
    (add_net "Net-(U4-Pad3)")
    (add_net "Net-(U5-Pad3)")
  )
  (module *Kyles_Drawings:PARTICLE_BORON (layer F.Cu) (tedit 5E0BBCB9)
    (at 154.2473 93.5062)
    (fp_text reference U2 (at -24.3771 9.3765 180) (layer F.SilkS))
    (fp_text value PARTICLE_BORON (at 0 0) (layer F.Fab))
    (pad 16 thru_hole oval (at 19.05 8.89) (size 1.25 2) (drill 0.92) (layers *.Cu *.Mask)
      (net 10 "Net-(U2-Pad16)"))
    (pad 17 thru_hole oval (at 19.05 -8.89) (size 1.25 2) (drill 0.92) (layers *.Cu *.Mask)
      (net 11 "Net-(U2-Pad17)"))
    (pad 15 thru_hole oval (at 16.51 8.89) (size 1.25 2) (drill 0.92) (layers *.Cu *.Mask)
      (net 12 "Net-(U2-Pad15)"))
    (pad 18 thru_hole oval (at 16.51 -8.89) (size 1.25 2) (drill 0.92) (layers *.Cu *.Mask)
      (net 13 "Net-(U2-Pad18)"))
    (pad 14 thru_hole oval (at 13.97 8.89) (size 1.25 2) (drill 0.92) (layers *.Cu *.Mask)
      (net 14 "Net-(U2-Pad14)"))
    (pad 19 thru_hole oval (at 13.97 -8.89) (size 1.25 2) (drill 0.92) (layers *.Cu *.Mask)
      (net 8 "Net-(R3-Pad2)"))
    (pad 13 thru_hole oval (at 11.43 8.89) (size 1.25 2) (drill 0.92) (layers *.Cu *.Mask)
      (net 15 "Net-(U2-Pad13)"))
    (pad 20 thru_hole oval (at 11.43 -8.89) (size 1.25 2) (drill 0.92) (layers *.Cu *.Mask)
      (net 6 "Net-(R2-Pad2)"))
    (pad 12 thru_hole oval (at 8.89 8.89) (size 1.25 2) (drill 0.92) (layers *.Cu *.Mask)
      (net 16 "Net-(U2-Pad12)"))
    (pad 21 thru_hole oval (at 8.89 -8.89) (size 1.25 2) (drill 0.92) (layers *.Cu *.Mask)
      (net 4 "Net-(R1-Pad2)"))
    (pad 11 thru_hole oval (at 6.35 8.89) (size 1.25 2) (drill 0.92) (layers *.Cu *.Mask)
      (net 17 "Net-(U2-Pad11)"))
    (pad 22 thru_hole oval (at 6.35 -8.89) (size 1.25 2) (drill 0.92) (layers *.Cu *.Mask)
      (net 18 "Net-(U2-Pad22)"))
    (pad 10 thru_hole oval (at 3.81 8.89) (size 1.25 2) (drill 0.92) (layers *.Cu *.Mask)
      (net 19 "Net-(U2-Pad10)"))
    (pad 23 thru_hole oval (at 3.81 -8.89) (size 1.25 2) (drill 0.92) (layers *.Cu *.Mask)
      (net 20 "Net-(U2-Pad23)"))
    (pad 9 thru_hole oval (at 1.27 8.89) (size 1.25 2) (drill 0.92) (layers *.Cu *.Mask)
      (net 21 "Net-(U2-Pad9)"))
    (pad 24 thru_hole oval (at 1.27 -8.89) (size 1.25 2) (drill 0.92) (layers *.Cu *.Mask)
      (net 22 "Net-(U2-Pad24)"))
    (pad 8 thru_hole oval (at -1.27 8.89) (size 1.25 2) (drill 0.92) (layers *.Cu *.Mask)
      (net 23 "Net-(U2-Pad8)"))
    (pad 25 thru_hole oval (at -1.27 -8.89) (size 1.25 2) (drill 0.92) (layers *.Cu *.Mask)
      (net 24 "Net-(U2-Pad25)"))
    (pad 7 thru_hole oval (at -3.81 8.89) (size 1.25 2) (drill 0.92) (layers *.Cu *.Mask)
      (net 25 "Net-(U2-Pad7)"))
    (pad 26 thru_hole oval (at -3.81 -8.89) (size 1.25 2) (drill 0.92) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 6 thru_hole oval (at -6.35 8.89) (size 1.25 2) (drill 0.92) (layers *.Cu *.Mask)
      (net 26 "Net-(U2-Pad6)"))
    (pad 27 thru_hole oval (at -6.35 -8.89) (size 1.25 2) (drill 0.92) (layers *.Cu *.Mask)
      (net 27 "Net-(U2-Pad27)"))
    (pad 5 thru_hole oval (at -8.89 8.89) (size 1.25 2) (drill 0.92) (layers *.Cu *.Mask)
      (net 28 "Net-(U2-Pad5)"))
    (pad 28 thru_hole oval (at -8.89 -8.89) (size 1.25 2) (drill 0.92) (layers *.Cu *.Mask)
      (net 29 "Net-(U2-Pad28)"))
    (pad 4 thru_hole oval (at -11.43 8.89) (size 1.25 2) (drill 0.92) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at -13.97 8.89) (size 1.25 2) (drill 0.92) (layers *.Cu *.Mask)
      (net 30 "Net-(U2-Pad3)"))
    (pad 2 thru_hole oval (at -16.51 8.89) (size 1.25 2) (drill 0.92) (layers *.Cu *.Mask)
      (net 31 "Net-(U2-Pad2)"))
    (pad 1 thru_hole oval (at -19.05 8.89) (size 1.25 2) (drill 0.92) (layers *.Cu *.Mask)
      (net 32 "Net-(U2-Pad1)"))
  )
  (module Connector_Molex:Molex_Nano-Fit_105314-xx06_2x03_P2.50mm_Horizontal (layer F.Cu) (tedit 5B782416)
    (at 115.951 96.3549 180)
    (descr "Molex Nano-Fit Power Connectors, 105314-xx06, 3 Pins per row (http://www.molex.com/pdm_docs/sd/1053141208_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Nano-Fit top entry")
    (fp_text reference J1 (at 8.65 -2.92 180) (layer F.SilkS))
    (fp_text value Conn_02x03_Top_Bottom (at 8.65 7.92 180) (layer F.Fab))
    (fp_text user %R (at 8.65 6.02 180) (layer F.Fab))
    (pad "" np_thru_hole circle (at 9.68 5 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 9.68 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 2.5 5 180) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 36 "Net-(J1-Pad6)"))
    (pad 5 thru_hole circle (at 2.5 2.5 180) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 37 "Net-(J1-Pad5)"))
    (pad 4 thru_hole circle (at 2.5 0 180) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 38 "Net-(J1-Pad4)"))
    (pad 3 thru_hole circle (at 0 5 180) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 39 "Net-(J1-Pad3)"))
    (pad 2 thru_hole circle (at 0 2.5 180) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 2 +12V))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_Nano-Fit_105314-xx06_2x03_P2.50mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:DIP-6_W7.62mm (layer F.Cu) (tedit 5AFEF30B)
    (at 168.9227 96.647 90)
    (descr http://optoelectronics.liteon.com/upload/download/DS70-2001-026/MOC306X%20series%20201606.pdf)
    (fp_text reference U5 (at -1.9685 -0.1778 180) (layer F.SilkS))
    (fp_text value H11L1M (at 4.1 8.1 90) (layer F.Fab))
    (fp_text user REF** (at 3.94 3.1 90) (layer F.Fab))
    (pad 6 thru_hole circle (at 7.62 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 5 thru_hole circle (at 7.62 2.54 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at 7.62 5.08 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J1-Pad4)"))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(U5-Pad3)"))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(R3-Pad1)"))
  )
  (module digikey-footprints:DIP-6_W7.62mm (layer F.Cu) (tedit 5AFEF30B)
    (at 152.4508 96.6343 90)
    (descr http://optoelectronics.liteon.com/upload/download/DS70-2001-026/MOC306X%20series%20201606.pdf)
    (fp_text reference U4 (at -1.9304 0.1397 180) (layer F.SilkS))
    (fp_text value H11L1M (at 4.1 8.1 90) (layer F.Fab))
    (fp_text user REF** (at 3.94 3.1 90) (layer F.Fab))
    (pad 6 thru_hole circle (at 7.62 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 5 thru_hole circle (at 7.62 2.54 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at 7.62 5.08 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J1-Pad5)"))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(U4-Pad3)"))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(R2-Pad1)"))
  )
  (module digikey-footprints:DIP-6_W7.62mm (layer F.Cu) (tedit 5AFEF30B)
    (at 134.9375 96.6851 90)
    (descr http://optoelectronics.liteon.com/upload/download/DS70-2001-026/MOC306X%20series%20201606.pdf)
    (fp_text reference U3 (at -1.7526 -0.2159 180) (layer F.SilkS))
    (fp_text value H11L1M (at 4.1 8.1 90) (layer F.Fab))
    (fp_text user REF** (at 3.94 3.1 90) (layer F.Fab))
    (pad 6 thru_hole circle (at 7.62 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 5 thru_hole circle (at 7.62 2.54 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at 7.62 5.08 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J1-Pad6)"))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(U3-Pad3)"))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(R1-Pad1)"))
  )
  (module *Kyles_Drawings:V7805-2000 (layer F.Cu) (tedit 5E0BC827)
    (at 125.6665 93.9038 270)
    (tags 102-2175-ND)
    (fp_text reference U1 (at 0 2.5 270) (layer F.SilkS))
    (fp_text value V7805-2000 (at 0 -3.048 270) (layer F.Fab))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 1.2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 2 thru_hole oval (at 0 0 270) (size 1.2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at -2.54 0 270) (size 1.2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 +12V))
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 176.8729 89.0143 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R6 (at 3.81 -1.92 270) (layer F.SilkS))
    (fp_text value 270Ω (at 3.7592 -0.0381 270) (layer F.SilkS))
    (fp_text user %R (at 3.81 0 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 38 "Net-(J1-Pad4)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 160.5661 89.1413 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R5 (at 3.81 -1.92 270) (layer F.SilkS))
    (fp_text value 270Ω (at 3.7338 0.0508 270) (layer F.SilkS))
    (fp_text user %R (at 3.81 0 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 37 "Net-(J1-Pad5)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 143.0147 89.0143 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R4 (at 3.81 -1.92 270) (layer F.SilkS))
    (fp_text value 270Ω (at 3.7592 -0.0635 270) (layer F.SilkS))
    (fp_text user %R (at 3.81 0 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 36 "Net-(J1-Pad6)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 165.9509 96.6978 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R3 (at 3.81 -1.92 90) (layer F.SilkS))
    (fp_text value 56Ω (at 3.8354 0 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 "Net-(R3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 148.9329 96.7105 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at 3.81 -1.92 90) (layer F.SilkS))
    (fp_text value 56Ω (at 3.937 -0.0127 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "Net-(R2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 131.953 96.6851 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at 3.81 -1.92 90) (layer F.SilkS))
    (fp_text value 56Ω (at 3.6449 0.0635 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(R1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 126.5682 102.4509 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C2 (at 6.2992 0.9017 180) (layer F.SilkS))
    (fp_text value 22µF (at 6.0706 -0.6858 180) (layer F.SilkS))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 126.4158 86.0679 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C1 (at 5.0292 -0.0381 180) (layer F.SilkS))
    (fp_text value 10µF (at 1.1176 2.5781 180) (layer F.SilkS))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +12V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "-\n+" (at 118.8339 95.1484) (layer B.SilkS))
  (gr_text "L\nUL\nST" (at 109.6645 93.8276) (layer B.SilkS))
  (gr_text "KM 2019\nCellular Remote Start\nParticle Boron\nREV 1" (at 112.1156 84.2899) (layer F.SilkS))
  (gr_line (start 179.75 104.75) (end 179.75 80.25) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 102.5 104.75) (end 179.75 104.75) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 102.5 80.25) (end 102.5 104.75) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 179.75 80.25) (end 102.5 80.25) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.1268 75.3618) (xy 185.8137 75.4253) (xy 185.9407 111.252) (xy 99.949 111.1885)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 180.1114 79.5909) (xy 180.1114 104.9401) (xy 101.6635 104.4956) (xy 102.2477 80.2386)
      )
    )
  )
)
