(kicad_pcb (version 20171130) (host pcbnew 5.1.6-c6e7f7d~87~ubuntu20.04.1)
  (general
    (thickness 1.6)
    (drawings 25)
    (tracks 4)
    (zones 0)
    (modules 2)
    (nets 4)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.5)
    (trace_clearance 0.16)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.16)
    (via_size 0.42)
    (via_drill 0.26)
    (via_min_size 0.42)
    (via_min_drill 0.26)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.025)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.1016)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.6 1.6)
    (pad_drill 0.8)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 127 95.758)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /+5V)
  (net 2 /GND)
  (net 3 "Net-(CN2-PadSH)")
  (net_class Default "This is the default net class."
    (clearance 0.16)
    (trace_width 0.16)
    (via_dia 0.42)
    (via_drill 0.26)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /+5V)
    (add_net /GND)
    (add_net "Net-(CN2-PadSH)")
  )
  (module 0_LOCAL:TE-5207826_cut (layer B.Cu) (tedit 5F2A163C)
    (at 121.475 94.333 180)
    (descr "9-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 25mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "9-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 25mm")
    (fp_text reference CN1 (at -5.5372 1.7018 180) (layer B.SilkS) hide)
    (fp_text value DB9_Female (at -5.54 -4.53 180) (layer B.Fab))
    (fp_text user %R (at -5.54 -1.42 180) (layer B.Fab))
    (pad 9 thru_hole circle (at -9.695 -2.84 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /+5V))
    (pad 8 thru_hole circle (at -6.925 -2.84 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at -4.155 -2.84 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /GND))
    (pad 6 thru_hole circle (at -1.385 -2.84 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -11.08 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -8.31 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -5.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -2.77 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/3dmodels/TE-5207826_cut.step
      (offset (xyz -5.528 -1.42 11.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0_LOCAL:USB_A_Female_UE27AC54100_cut (layer F.Cu) (tedit 5F266A81)
    (at 135.55 95.758 270)
    (fp_text reference CN2 (at 0 -0.889 270 unlocked) (layer F.SilkS) hide)
    (fp_text value UE27AC54100 (at 0 11.35 270) (layer F.Fab))
    (fp_text user %R (at -0.025 0.975 270) (layer F.Fab))
    (pad SH smd oval (at 6.8 0 270) (size 4.8 2.2) (drill (offset -1.5 0)) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(CN2-PadSH)"))
    (pad SH smd oval (at -6.8 0 270) (size 4.8 2.2) (drill (offset 1.5 0)) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(CN2-PadSH)"))
    (pad 4 thru_hole circle (at 3.5 -2.71 270) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 /GND))
    (pad 3 thru_hole circle (at 1 -2.71 270) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -1 -2.71 270) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at -3.5 -2.71 270) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 /+5V))
    (pad SH thru_hole circle (at 7.4 0 270) (size 4 4) (drill 3) (layers *.Cu *.Mask)
      (net 3 "Net-(CN2-PadSH)"))
    (pad SH thru_hole circle (at -7.4 0 270) (size 4 4) (drill 3) (layers *.Cu *.Mask)
      (net 3 "Net-(CN2-PadSH)"))
    (model ${KIPRJMOD}/3dmodels/USB-A_female_horiz_thru.step
      (offset (xyz 0 3.5 6.9))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 137.225 100.383) (end 137.225 102.383) (angle -90) (layer Edge.Cuts) (width 0.025))
  (gr_arc (start 137.225 91.133) (end 139.225 91.133) (angle -90) (layer Edge.Cuts) (width 0.025))
  (gr_arc (start 119.5 91.133) (end 119.5 89.133) (angle -90) (layer Edge.Cuts) (width 0.025))
  (gr_arc (start 119.5 100.383) (end 117.5 100.383) (angle -90) (layer Edge.Cuts) (width 0.025))
  (gr_text - (at 138.2 100.708 90) (layer F.SilkS))
  (gr_text + (at 138.2 90.808 90) (layer F.SilkS))
  (gr_text - (at 138.2 100.708 90) (layer B.SilkS))
  (gr_text + (at 138.2 90.808 90) (layer B.SilkS))
  (gr_line (start 117.5 100.383) (end 117.5 91.133) (layer Edge.Cuts) (width 0.025))
  (gr_line (start 137.225 89.133) (end 119.5 89.133) (layer Edge.Cuts) (width 0.025))
  (gr_line (start 137.225 102.383) (end 119.5 102.383) (layer Edge.Cuts) (width 0.025))
  (gr_line (start 139.225 100.383) (end 139.225 91.133) (layer Edge.Cuts) (width 0.025))
  (gr_text "TE 5207826" (at 127 95.783) (layer B.SilkS))
  (gr_text SS-52100-001 (at 131.56 99.528) (layer F.SilkS))
  (gr_text github.com/bkw777/BCR_Breakout (at 126.3 100.683) (layer B.SilkS))
  (gr_text "BCR to USB 5v" (at 126 90.458) (layer B.SilkS))
  (gr_text "BCR 5V" (at 119.1 95.758 90) (layer F.SilkS))
  (gr_text "DE9F SIDE" (at 127 93.058) (layer B.SilkS))
  (gr_text "USB SIDE" (at 131.425 92.058) (layer F.SilkS))
)
