(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.6)
    (drawings 27)
    (tracks 67)
    (zones 0)
    (modules 6)
    (nets 21)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 1)
    (trace_clearance 0.127)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /RST)
  (net 2 /TDI)
  (net 3 /TDO)
  (net 4 /TCK)
  (net 5 /TMS)
  (net 6 /VTref)
  (net 7 /GND9)
  (net 8 /GND7)
  (net 9 /GND5)
  (net 10 /GND3)
  (net 11 /1)
  (net 12 /2)
  (net 13 /3)
  (net 14 /4)
  (net 15 /5)
  (net 16 /6)
  (net 17 /7)
  (net 18 /8)
  (net 19 /9)
  (net 20 /10)
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (add_net /1)
    (add_net /10)
    (add_net /2)
    (add_net /3)
    (add_net /4)
    (add_net /5)
    (add_net /6)
    (add_net /7)
    (add_net /8)
    (add_net /9)
    (add_net /GND3)
    (add_net /GND5)
    (add_net /GND7)
    (add_net /GND9)
    (add_net /RST)
    (add_net /TCK)
    (add_net /TDI)
    (add_net /TDO)
    (add_net /TMS)
    (add_net /VTref)
  )
  (module JohnAdriaan:Mandel_tiny (layer B.Cu) (tedit 0)
    (at 146.4 80.9 90)
    (fp_text reference G*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (module JohnAdriaan:Mandel_nano (layer F.Cu) (tedit 0)
    (at 142.6 76.6 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module JohnAdriaan:Mandel_nano (layer F.Cu) (tedit 0)
    (at 134 76.6 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module JohnAdriaan:CS10_POGO_0.7 (layer F.Cu) (tedit 5F475AD8)
    (at 133.9 80.5)
    (descr "Through hole straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 1.27mm double row")
    (fp_text reference Pogo2 (at 0.01 -4.8) (layer F.SilkS) hide)
    (fp_text value CS10 (at 0 4.8) (layer F.Fab))
    (fp_text user %R (at 0.01 0 90) (layer F.Fab))
    (pad 1 thru_hole oval (at -0.635 -2.54 300) (size 2 0.85) (drill 0.7 (offset -0.585 0)) (layers *.Cu *.Mask)
      (net 11 /1))
    (pad 2 thru_hole oval (at 0.635 -2.54 60) (size 2 0.85) (drill 0.7 (offset 0.585 0)) (layers *.Cu *.Mask)
      (net 12 /2))
    (pad 3 thru_hole oval (at -0.635 -1.27 340) (size 2 0.85) (drill 0.7 (offset -0.585 0)) (layers *.Cu *.Mask)
      (net 13 /3))
    (pad 4 thru_hole oval (at 0.635 -1.27 20) (size 2 0.85) (drill 0.7 (offset 0.585 0)) (layers *.Cu *.Mask)
      (net 14 /4))
    (pad 5 thru_hole oval (at -0.635 0) (size 2 0.85) (drill 0.7 (offset -0.585 0)) (layers *.Cu *.Mask)
      (net 15 /5))
    (pad 6 thru_hole oval (at 0.635 0) (size 2 0.85) (drill 0.7 (offset 0.585 0)) (layers *.Cu *.Mask)
      (net 16 /6))
    (pad 7 thru_hole oval (at -0.635 1.27 20) (size 2 0.85) (drill 0.7 (offset -0.585 0)) (layers *.Cu *.Mask)
      (net 17 /7))
    (pad 8 thru_hole oval (at 0.635 1.27 340) (size 2 0.85) (drill 0.7 (offset 0.585 0)) (layers *.Cu *.Mask)
      (net 18 /8))
    (pad 9 thru_hole oval (at -0.635 2.54 60) (size 2 0.85) (drill 0.7 (offset -0.585 0)) (layers *.Cu *.Mask)
      (net 19 /9))
    (pad 10 thru_hole oval (at 0.635 2.54 300) (size 2 0.85) (drill 0.7 (offset 0.585 0)) (layers *.Cu *.Mask)
      (net 20 /10))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module JohnAdriaan:CS10_POGO_0.7 (layer F.Cu) (tedit 5F475AD8)
    (at 142.5 80.5)
    (descr "Through hole straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 1.27mm double row")
    (fp_text reference Pogo1 (at 0.01 -4.8) (layer F.SilkS) hide)
    (fp_text value CS10 (at 0 4.8) (layer F.Fab))
    (fp_text user %R (at 0.01 0 90) (layer F.Fab))
    (pad 1 thru_hole oval (at -0.635 -2.54 300) (size 2 0.85) (drill 0.7 (offset -0.585 0)) (layers *.Cu *.Mask)
      (net 6 /VTref))
    (pad 2 thru_hole oval (at 0.635 -2.54 60) (size 2 0.85) (drill 0.7 (offset 0.585 0)) (layers *.Cu *.Mask)
      (net 5 /TMS))
    (pad 3 thru_hole oval (at -0.635 -1.27 340) (size 2 0.85) (drill 0.7 (offset -0.585 0)) (layers *.Cu *.Mask)
      (net 10 /GND3))
    (pad 4 thru_hole oval (at 0.635 -1.27 20) (size 2 0.85) (drill 0.7 (offset 0.585 0)) (layers *.Cu *.Mask)
      (net 4 /TCK))
    (pad 5 thru_hole oval (at -0.635 0) (size 2 0.85) (drill 0.7 (offset -0.585 0)) (layers *.Cu *.Mask)
      (net 9 /GND5))
    (pad 6 thru_hole oval (at 0.635 0) (size 2 0.85) (drill 0.7 (offset 0.585 0)) (layers *.Cu *.Mask)
      (net 3 /TDO))
    (pad 7 thru_hole oval (at -0.635 1.27 20) (size 2 0.85) (drill 0.7 (offset -0.585 0)) (layers *.Cu *.Mask)
      (net 8 /GND7))
    (pad 8 thru_hole oval (at 0.635 1.27 340) (size 2 0.85) (drill 0.7 (offset 0.585 0)) (layers *.Cu *.Mask)
      (net 2 /TDI))
    (pad 9 thru_hole oval (at -0.635 2.54 60) (size 2 0.85) (drill 0.7 (offset -0.585 0)) (layers *.Cu *.Mask)
      (net 7 /GND9))
    (pad 10 thru_hole oval (at 0.635 2.54 300) (size 2 0.85) (drill 0.7 (offset 0.585 0)) (layers *.Cu *.Mask)
      (net 1 /RST))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module JohnAdriaan:CS10 (layer F.Cu) (tedit 5F2FD7DA)
    (at 149.45 80.5)
    (descr "Pogo Straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Pogo pin header THT SMD 2x05 1.27mm double row")
    (attr smd)
    (fp_text reference J1 (at 0 -6) (layer F.SilkS) hide)
    (fp_text value CS10 (at 0 6.5) (layer F.Fab))
    (fp_text user %R (at 0.01 0 90) (layer F.Fab))
    (pad 10 smd custom (at 1.95 2.54) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 1 /RST) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center -1.315 0) (end -0.815 0) (width 0))
      ))
    (pad 10 thru_hole oval (at 0.635 2.54) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 /RST))
    (pad 9 smd custom (at -1.95 2.54) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 7 /GND9) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 1.315 0) (end 1.815 0) (width 0))
      ))
    (pad 9 thru_hole oval (at -0.635 2.54) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 7 /GND9))
    (pad 8 smd custom (at 1.95 1.27) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 2 /TDI) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center -1.315 0) (end -0.815 0) (width 0))
      ))
    (pad 8 thru_hole oval (at 0.635 1.27) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 /TDI))
    (pad 7 smd custom (at -1.95 1.27) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 8 /GND7) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 1.315 0) (end 1.815 0) (width 0))
      ))
    (pad 7 thru_hole oval (at -0.635 1.27) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 8 /GND7))
    (pad 6 smd custom (at 1.95 0) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 3 /TDO) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center -1.315 0) (end -0.815 0) (width 0))
      ))
    (pad 6 thru_hole oval (at 0.635 0) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 /TDO))
    (pad 5 smd custom (at -1.95 0) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 9 /GND5) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 1.315 0) (end 1.815 0) (width 0))
      ))
    (pad 5 thru_hole oval (at -0.635 0) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 9 /GND5))
    (pad 4 smd custom (at 1.95 -1.27) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 4 /TCK) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center -1.315 0) (end -0.815 0) (width 0))
      ))
    (pad 4 thru_hole oval (at 0.635 -1.27) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 /TCK))
    (pad 3 smd custom (at -1.95 -1.27) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 10 /GND3) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 1.315 0) (end 1.815 0) (width 0))
      ))
    (pad 3 thru_hole oval (at -0.635 -1.27) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 10 /GND3))
    (pad 2 smd custom (at 1.95 -2.54) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 5 /TMS) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center -1.315 0) (end -0.815 0) (width 0))
      ))
    (pad 2 thru_hole oval (at 0.635 -2.54) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 5 /TMS))
    (pad 1 smd custom (at -1.95 -2.54) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 6 /VTref) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.815 -0.5) (xy 1.815 -0.5) (xy 1.815 0.5) (xy 0.815 0.5)) (width 0))
      ))
    (pad 1 thru_hole rect (at -0.635 -2.54) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 6 /VTref))
  )
  (gr_text CS10 (at 133.9 85.3) (layer F.SilkS))
  (gr_arc (start 139.7 81.05) (end 140 81.05) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 137.7 81.05) (end 137.7 80.75) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 137.7 79.95) (end 137.4 79.95) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 139.7 79.95) (end 139.7 80.25) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 139.7 80.75) (end 137.7 80.75) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 137.7 80.25) (end 139.7 80.25) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 140 79.95) (end 140 75.25) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 140 85.75) (end 140 81.05) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 137.4 81.05) (end 137.4 85.75) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 137.4 75.25) (end 137.4 79.95) (layer Edge.Cuts) (width 0.05))
  (gr_text Pogo (at 136.5 82 90) (layer F.SilkS))
  (gr_arc (start 131.65 75.25) (end 131.65 75) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 137.15 75.25) (end 137.4 75.25) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 131.65 85.75) (end 131.4 85.75) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 131.65 75) (end 137.15 75) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 131.4 85.75) (end 131.4 75.25) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 137.15 85.75) (end 137.15 86) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 137.15 86) (end 131.65 86) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 153.75 85.75) (end 153.75 86) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 140.25 85.75) (end 140 85.75) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 140.25 75.25) (end 140.25 75) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 153.75 75.25) (end 154 75.25) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text "CS10 Pogo" (at 149.7 85) (layer F.SilkS))
  (gr_line (start 153.75 86) (end 140.25 86) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 154 75.25) (end 154 85.75) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 140.25 75) (end 153.75 75) (layer Edge.Cuts) (width 0.05))
)
