(kicad_pcb (version 20170123) (host pcbnew "(2017-06-10 revision 1f14389)-master")
  (general
    (links 196)
    (no_connects 0)
    (area 69.749999 36.801666 231.805001 89.1825)
    (thickness 1.6002)
    (drawings 17)
    (tracks 879)
    (zones 0)
    (modules 69)
    (nets 77)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.8128)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed yes)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(BZ1-Pad1)")
  (net 3 +5V)
  (net 4 "Net-(C4-Pad2)")
  (net 5 "Net-(C5-Pad2)")
  (net 6 "Net-(D1-Pad2)")
  (net 7 "Net-(D1-Pad1)")
  (net 8 "Net-(E1-Pad2)")
  (net 9 "Net-(E1-PadA)")
  (net 10 "Net-(E1-PadB)")
  (net 11 "Net-(F1-Pad2)")
  (net 12 "Net-(J1-Pad1)")
  (net 13 USB_D-)
  (net 14 USB_D+)
  (net 15 USB_ID)
  (net 16 /MISO)
  (net 17 /SCK)
  (net 18 /MOSI)
  (net 19 /RST)
  (net 20 OLED_SCL)
  (net 21 OLED_SDA)
  (net 22 PB0)
  (net 23 PB1)
  (net 24 PB2)
  (net 25 PC2)
  (net 26 PC3)
  (net 27 PE0)
  (net 28 PE1)
  (net 29 SER_DTR)
  (net 30 SER_CTS)
  (net 31 SER_RXD)
  (net 32 SER_TXD)
  (net 33 SER_VCC)
  (net 34 LED_DIN)
  (net 35 LED_DOUT)
  (net 36 LED_CIN)
  (net 37 LED_COUT)
  (net 38 "Net-(R1-Pad1)")
  (net 39 RESET)
  (net 40 "Net-(R3-Pad1)")
  (net 41 "Net-(R6-Pad1)")
  (net 42 "Net-(S1-Pad1)")
  (net 43 "Net-(S2-Pad1)")
  (net 44 "Net-(S4-Pad3)")
  (net 45 "Net-(U1-Pad5)")
  (net 46 "Net-(U1-Pad6)")
  (net 47 "Net-(U2-Pad5)")
  (net 48 "Net-(U2-Pad6)")
  (net 49 "Net-(U3-Pad5)")
  (net 50 "Net-(U3-Pad6)")
  (net 51 "Net-(U4-Pad5)")
  (net 52 "Net-(U4-Pad6)")
  (net 53 "Net-(U5-Pad5)")
  (net 54 "Net-(U5-Pad6)")
  (net 55 "Net-(U6-Pad5)")
  (net 56 "Net-(U6-Pad6)")
  (net 57 "Net-(U7-Pad5)")
  (net 58 "Net-(U7-Pad6)")
  (net 59 LED_CMID)
  (net 60 LED_DMID)
  (net 61 "Net-(U10-Pad2)")
  (net 62 "Net-(U10-Pad1)")
  (net 63 "Net-(U10-Pad5)")
  (net 64 "Net-(U10-Pad6)")
  (net 65 "Net-(U11-Pad5)")
  (net 66 "Net-(U11-Pad6)")
  (net 67 "Net-(U12-Pad5)")
  (net 68 "Net-(U12-Pad6)")
  (net 69 "Net-(U13-Pad5)")
  (net 70 "Net-(U13-Pad6)")
  (net 71 "Net-(U14-Pad5)")
  (net 72 "Net-(U14-Pad6)")
  (net 73 "Net-(U15-Pad5)")
  (net 74 "Net-(U15-Pad6)")
  (net 75 "Net-(S3-Pad3)")
  (net 76 "Net-(S5-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RST)
    (add_net /SCK)
    (add_net LED_CIN)
    (add_net LED_CMID)
    (add_net LED_COUT)
    (add_net LED_DIN)
    (add_net LED_DMID)
    (add_net LED_DOUT)
    (add_net "Net-(BZ1-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(E1-Pad2)")
    (add_net "Net-(E1-PadA)")
    (add_net "Net-(E1-PadB)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(S1-Pad1)")
    (add_net "Net-(S2-Pad1)")
    (add_net "Net-(S3-Pad3)")
    (add_net "Net-(S4-Pad3)")
    (add_net "Net-(S5-Pad2)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U10-Pad1)")
    (add_net "Net-(U10-Pad2)")
    (add_net "Net-(U10-Pad5)")
    (add_net "Net-(U10-Pad6)")
    (add_net "Net-(U11-Pad5)")
    (add_net "Net-(U11-Pad6)")
    (add_net "Net-(U12-Pad5)")
    (add_net "Net-(U12-Pad6)")
    (add_net "Net-(U13-Pad5)")
    (add_net "Net-(U13-Pad6)")
    (add_net "Net-(U14-Pad5)")
    (add_net "Net-(U14-Pad6)")
    (add_net "Net-(U15-Pad5)")
    (add_net "Net-(U15-Pad6)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U3-Pad6)")
    (add_net "Net-(U4-Pad5)")
    (add_net "Net-(U4-Pad6)")
    (add_net "Net-(U5-Pad5)")
    (add_net "Net-(U5-Pad6)")
    (add_net "Net-(U6-Pad5)")
    (add_net "Net-(U6-Pad6)")
    (add_net "Net-(U7-Pad5)")
    (add_net "Net-(U7-Pad6)")
    (add_net OLED_SCL)
    (add_net OLED_SDA)
    (add_net PB0)
    (add_net PB1)
    (add_net PB2)
    (add_net PC2)
    (add_net PC3)
    (add_net PE0)
    (add_net PE1)
    (add_net RESET)
    (add_net SER_CTS)
    (add_net SER_DTR)
    (add_net SER_RXD)
    (add_net SER_TXD)
    (add_net USB_D+)
    (add_net USB_D-)
    (add_net USB_ID)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.508)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net SER_VCC)
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 593DB4AD)
    (at 200.66 63.5 90)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U17 (at 0 -6.05 90) (layer F.SilkS))
    (fp_text value ATMEGA328PB-AU (at 0 6.05 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -4.25 -2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(E1-PadB)"))
    (pad 2 smd rect (at -4.25 -2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(E1-Pad2)"))
    (pad 3 smd rect (at -4.25 -1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 27 PE0))
    (pad 4 smd rect (at -4.25 -0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 5 smd rect (at -4.25 0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -4.25 1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 28 PE1))
    (pad 7 smd rect (at -4.25 2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad2)"))
    (pad 8 smd rect (at -4.25 2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C5-Pad2)"))
    (pad 9 smd rect (at -2.8 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(S3-Pad3)"))
    (pad 10 smd rect (at -2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(S4-Pad3)"))
    (pad 11 smd rect (at -1.2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(S5-Pad2)"))
    (pad 12 smd rect (at -0.4 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 22 PB0))
    (pad 13 smd rect (at 0.4 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 PB1))
    (pad 14 smd rect (at 1.2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 24 PB2))
    (pad 15 smd rect (at 2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R6-Pad1)"))
    (pad 16 smd rect (at 2.8 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R3-Pad1)"))
    (pad 17 smd rect (at 4.25 2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad2)"))
    (pad 18 smd rect (at 4.25 2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 19 smd rect (at 4.25 1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(S1-Pad1)"))
    (pad 20 smd rect (at 4.25 0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 21 smd rect (at 4.25 -0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 22 smd rect (at 4.25 -1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(S2-Pad1)"))
    (pad 23 smd rect (at 4.25 -2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 34 LED_DIN))
    (pad 24 smd rect (at 4.25 -2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 36 LED_CIN))
    (pad 25 smd rect (at 2.8 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 25 PC2))
    (pad 26 smd rect (at 2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 26 PC3))
    (pad 27 smd rect (at 1.2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 21 OLED_SDA))
    (pad 28 smd rect (at 0.4 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 20 OLED_SCL))
    (pad 29 smd rect (at -0.4 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 39 RESET))
    (pad 30 smd rect (at -1.2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 32 SER_TXD))
    (pad 31 smd rect (at -2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 31 SER_RXD))
    (pad 32 smd rect (at -2.8 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(E1-PadA)"))
    (model Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:USB_Micro-B (layer F.Cu) (tedit 5543E447)
    (at 225.552 50.546 90)
    (descr "Micro USB Type B Receptacle")
    (tags "USB USB_B USB_micro USB_OTG")
    (attr smd)
    (fp_text reference J1 (at 0 -3.24 90) (layer F.SilkS))
    (fp_text value USB_OTG (at 0 5.01 90) (layer F.Fab))
    (pad 1 smd rect (at -1.3 -1.35 180) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at -0.65 -1.35 180) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 13 USB_D-))
    (pad 3 smd rect (at 0 -1.35 180) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 14 USB_D+))
    (pad 4 smd rect (at 0.65 -1.35 180) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 15 USB_ID))
    (pad 5 smd rect (at 1.3 -1.35 180) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at -2.5 -1.35 180) (size 0.95 1.25) (drill oval 0.55 0.85) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 2.5 -1.35 180) (size 0.95 1.25) (drill oval 0.55 0.85) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at -3.5 1.35 180) (size 1.55 1) (drill oval 1.15 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 3.5 1.35 180) (size 1.55 1) (drill oval 1.15 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 593D9770)
    (at 217.17 52.07 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference JP1 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value Jumper_NC_Dual (at 0 7.41 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(F1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 SER_VCC))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connectors:1pin (layer F.Cu) (tedit 593DAD8B)
    (at 224.79 41.91)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Fuse_Holders_and_Fuses:Fuse_SMD1206_HandSoldering (layer F.Cu) (tedit 0)
    (at 213.36 49.98 270)
    (descr "Fuse, Sicherung, SMD1206, Littlefuse-Wickmann 433 Series, Hand Soldering,")
    (tags "Fuse Sicherung SMD1206 Littlefuse-Wickmann 433 Series Hand Soldering ")
    (attr smd)
    (fp_text reference F1 (at 4.63 0) (layer F.SilkS))
    (fp_text value 500mA (at -0.15 2.5 270) (layer F.Fab))
    (pad 1 smd rect (at -2.09 0) (size 2.03 2.65) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 2.09 0) (size 2.03 2.65) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(F1-Pad2)"))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 593DAD96)
    (at 143.51 85.09)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 593DAD92)
    (at 224.79 85.09)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 2.54 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 593DAD82)
    (at 143.51 41.91)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 593DAD78)
    (at 73.66 85.09)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 593DAD7F)
    (at 73.66 41.91)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module pec11r:pec11r (layer F.Cu) (tedit 593DAFC7)
    (at 127 63.5)
    (fp_text reference E1 (at 0 -4.45) (layer F.SilkS))
    (fp_text value PEC11R (at 0 4.4) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.5 -7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 -7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(E1-Pad2)"))
    (pad C thru_hole circle (at 0 7.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad A thru_hole circle (at -2.5 7.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(E1-PadA)"))
    (pad B thru_hole circle (at 2.5 7.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(E1-PadB)"))
    (pad "" thru_hole circle (at 6.2 0) (size 3 3) (drill 2.6) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -6.2 0) (size 3 3) (drill 2.6) (layers *.Cu *.Mask F.SilkS))
  )
  (module Pin_Headers:Pin_Header_Straight_1x16_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC2)
    (at 148.59 83.82 90)
    (descr "Through hole straight pin header, 1x16, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x16 2.54mm single row")
    (fp_text reference J4 (at 2.54 1.778 180) (layer F.SilkS))
    (fp_text value CONN_01X16 (at 0 40.43 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 PB2))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 PB1))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 PB0))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 PC2))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 PC3))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 PE0))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 PE1))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 SER_DTR))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 SER_CTS))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 USB_D+))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 USB_D-))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 USB_ID))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x16_Pitch2.54mm.wrl
      (at (xyz 0 -0.75 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CrumpPrints:APA102 (layer F.Cu) (tedit 593DB00D)
    (at 110.153956 74.862799 34)
    (fp_text reference U3 (at -3.632747 0.081775 124) (layer F.SilkS))
    (fp_text value APA102 (at 0.2 0 34) (layer F.SilkS))
    (pad 3 smd rect (at 1.6 2.2 124) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.6 -2.2 124) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 5 smd rect (at 0.000001 -2.2 124) (size 1.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(U3-Pad5)"))
    (pad 2 smd rect (at -0.000001 2.2 124) (size 1.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U2-Pad5)"))
    (pad 1 smd rect (at -1.6 2.2 124) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U2-Pad6)"))
    (pad 6 smd rect (at -1.6 -2.2 124) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(U3-Pad6)"))
  )
  (module Buzzers_Beepers:BUZZER (layer F.Cu) (tedit 0)
    (at 219.71 63.5)
    (fp_text reference BZ1 (at 0.24892 -1.75006) (layer F.SilkS))
    (fp_text value Buzzer (at 0 1.50114) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -5.08 0) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 2 "Net-(BZ1-Pad1)"))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 204.49 54.61 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 200.68 73.66)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -1.75) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 199.41 54.61 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 193.04 81.3 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 3.536 0) (layer F.SilkS))
    (fp_text value 22pF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 208.28 81.26 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at -3.576 0 180) (layer F.SilkS))
    (fp_text value 22pF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C5-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 593DAF29)
    (at 124.09207 78.459998 169)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 0 -1.75 169) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75 169) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 169) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 169) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 169) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 593DAF25)
    (at 118.58848 76.208419 146.5)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 -1.75 146.5) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75 146.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 146.5) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 146.5) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 146.5) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 593DAF2E)
    (at 114.365467 72.022099 124)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 0 -1.75 124) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75 124) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 124) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 124) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 124) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 593DAF4E)
    (at 112.065947 66.538367 101.5)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 0 -1.75 101.5) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75 101.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 101.5) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 101.5) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 101.5) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 593DAF77)
    (at 112.040001 60.59207 79)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 0 -1.75 79) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75 79) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 79) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 79) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 79) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 593DAF81)
    (at 114.29158 55.08848 56.5)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at 0 -1.75 56.5) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75 56.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 56.5) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 56.5) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 56.5) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 593DAF85)
    (at 118.4779 50.865467 34)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at 0 -1.75 34) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75 34) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 34) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 34) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 34) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 593DAF8B)
    (at 123.961632 48.565947 11.5)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C13 (at 0 -1.75 11.5) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75 11.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 11.5) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 11.5) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 11.5) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 593DAF8E)
    (at 129.907929 48.540001 349)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C14 (at 0 -1.75 349) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75 349) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 349) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 349) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 349) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 593DAF91)
    (at 135.411519 50.79158 326.5)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C15 (at 0 -1.75 326.5) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75 326.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 326.5) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 326.5) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 326.5) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 593DAF94)
    (at 139.634532 54.9779 304)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C16 (at 0 -1.75 304) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75 304) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 304) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 304) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 304) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 593DAF99)
    (at 141.934052 60.461632 281.5)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C17 (at 0 -1.75 281.5) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75 281.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 281.5) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 281.5) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 281.5) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 593DAF9C)
    (at 141.959998 66.407929 259)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C18 (at 0 -1.75 259) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75 259) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 259) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 259) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 259) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 593DAFA0)
    (at 139.708419 71.911519 236.5)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C19 (at 0 -1.75 236.5) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75 236.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 236.5) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 236.5) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 236.5) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 593DAFA4)
    (at 135.522099 76.134532 214)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C20 (at 0 -1.75 214) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75 214) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 214) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 214) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 214) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 593DAFAA)
    (at 130.038367 78.434052 191.5)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C21 (at 0 -1.75 191.5) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75 191.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 191.5) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 191.5) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 191.5) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 86.36 63.5 90)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC5)
    (at 201.93 50.8 180)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J2 (at 1.27 -2.33 180) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 1.27 7.41 180) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.33 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /MISO))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /SCK))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /MOSI))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /RST))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 168.91 44.45 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 OLED_SCL))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 OLED_SDA))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 194.31 41.91 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 0 15.03 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 SER_DTR))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 SER_RXD))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 SER_TXD))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 SER_VCC))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 SER_CTS))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x04_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC5)
    (at 107.95 81.28 270)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (fp_text reference J6 (at 1.27 -2.33 270) (layer F.SilkS))
    (fp_text value CONN_02X04 (at 1.27 9.95 270) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.33 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 LED_DIN))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 LED_DOUT))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 LED_CIN))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 LED_COUT))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x04_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 593DB1D2)
    (at 220.98 80.01 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 3.175 0) (layer F.SilkS))
    (fp_text value 10K (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 196.85 76.12 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 39 RESET))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 207.01 50.8 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -3.556 0 180) (layer F.SilkS))
    (fp_text value 330 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /MISO))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 207.01 48.26)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 3.556 0) (layer F.SilkS))
    (fp_text value 330 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /SCK))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 206.93 45.72)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 3.636 0) (layer F.SilkS))
    (fp_text value 330 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 /RST))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 39 RESET))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 195.58 48.34 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 3.382 0 180) (layer F.SilkS))
    (fp_text value 330 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R6-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 /MOSI))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 83.82 63.5 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 1K (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_TH_Tactile_Omron_B3F-10xx (layer F.Cu) (tedit 5928351D)
    (at 74.018 52.07)
    (descr SW_TH_Tactile_Omron_B3F-10xx_https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "Omron B3F-10xx")
    (fp_text reference S1 (at 3.25 -2.05) (layer F.SilkS))
    (fp_text value 10-XX (at 3.2 6.5) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 4 thru_hole circle (at 6.5 4.5) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 0 4.5) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 6.5 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(S1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(S1-Pad1)"))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_TH_Tactile_Omron_B3F-10xx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_TH_Tactile_Omron_B3F-10xx (layer F.Cu) (tedit 5928351D)
    (at 74.168 71.12)
    (descr SW_TH_Tactile_Omron_B3F-10xx_https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "Omron B3F-10xx")
    (fp_text reference S2 (at 3.25 -2.05) (layer F.SilkS))
    (fp_text value 10-XX (at 3.2 6.5) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 4 thru_hole circle (at 6.5 4.5) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 0 4.5) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 6.5 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(S2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(S2-Pad1)"))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_TH_Tactile_Omron_B3F-10xx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_TH_Tactile_Omron_B3F-10xx (layer F.Cu) (tedit 5928351D)
    (at 90.17 71.12)
    (descr SW_TH_Tactile_Omron_B3F-10xx_https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "Omron B3F-10xx")
    (fp_text reference S4 (at 3.25 -2.05) (layer F.SilkS))
    (fp_text value 10-XX (at 3.2 6.5) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 4 thru_hole circle (at 6.5 4.5) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(S4-Pad3)"))
    (pad 3 thru_hole circle (at 0 4.5) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(S4-Pad3)"))
    (pad 2 thru_hole circle (at 6.5 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_TH_Tactile_Omron_B3F-10xx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CrumpPrints:APA102 (layer F.Cu) (tedit 593DAFF6)
    (at 123.122761 83.446664 79)
    (fp_text reference U1 (at -3.491043 -0.029175 169) (layer F.SilkS))
    (fp_text value APA102 (at 0.2 0 79) (layer F.SilkS))
    (pad 3 smd rect (at 1.6 2.2 169) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.6 -2.2 169) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 5 smd rect (at 0 -2.2 169) (size 1.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(U1-Pad5)"))
    (pad 2 smd rect (at 0 2.2 169) (size 1.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 36 LED_CIN))
    (pad 1 smd rect (at -1.6 2.2 169) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 34 LED_DIN))
    (pad 6 smd rect (at -1.6 -2.2 169) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U1-Pad6)"))
  )
  (module CrumpPrints:APA102 (layer F.Cu) (tedit 593DB003)
    (at 115.78464 80.444559 56.5)
    (fp_text reference U2 (at -3.49093 -0.078988 146.5) (layer F.SilkS))
    (fp_text value APA102 (at 0.2 0 56.5) (layer F.SilkS))
    (pad 3 smd rect (at 1.6 2.2 146.5) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.6 -2.2 146.5) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 5 smd rect (at 0 -2.2 146.5) (size 1.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U2-Pad5)"))
    (pad 2 smd rect (at 0 2.2 146.5) (size 1.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(U1-Pad5)"))
    (pad 1 smd rect (at -1.6 2.2 146.5) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U1-Pad6)"))
    (pad 6 smd rect (at -1.6 -2.2 146.5) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U2-Pad6)"))
  )
  (module CrumpPrints:APA102 (layer F.Cu) (tedit 593DB024)
    (at 107.08793 67.551156 11.5)
    (fp_text reference U4 (at -3.54103 0.070287 101.5) (layer F.SilkS))
    (fp_text value APA102 (at 0.2 0 11.5) (layer F.SilkS))
    (pad 3 smd rect (at 1.6 2.2 101.5) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.6 -2.2 101.5) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 5 smd rect (at 0 -2.2 101.5) (size 1.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U4-Pad5)"))
    (pad 2 smd rect (at 0 2.2 101.5) (size 1.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(U3-Pad5)"))
    (pad 1 smd rect (at -1.6 2.2 101.5) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(U3-Pad6)"))
    (pad 6 smd rect (at -1.6 -2.2 101.5) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U4-Pad6)"))
  )
  (module CrumpPrints:APA102 (layer F.Cu) (tedit 54BDEC7B)
    (at 107.053335 59.622761 349)
    (fp_text reference U5 (at -3.241709 -0.07764 79) (layer F.SilkS))
    (fp_text value APA102 (at 0.2 0 349) (layer F.SilkS))
    (pad 3 smd rect (at 1.6 2.2 79) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.6 -2.2 79) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 5 smd rect (at 0 -2.2 79) (size 1.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(U5-Pad5)"))
    (pad 2 smd rect (at 0 2.2 79) (size 1.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U4-Pad5)"))
    (pad 1 smd rect (at -1.6 2.2 79) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U4-Pad6)"))
    (pad 6 smd rect (at -1.6 -2.2 79) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(U5-Pad6)"))
  )
  (module CrumpPrints:APA102 (layer F.Cu) (tedit 54BDEC7B)
    (at 110.05544 52.28464 326.5)
    (fp_text reference U6 (at -3.350737 0.132819 56.5) (layer F.SilkS))
    (fp_text value APA102 (at 0.2 0 326.5) (layer F.SilkS))
    (pad 3 smd rect (at 1.6 2.2 56.5) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.6 -2.2 56.5) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 5 smd rect (at 0 -2.2 56.5) (size 1.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(U6-Pad5)"))
    (pad 2 smd rect (at 0 2.2 56.5) (size 1.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(U5-Pad5)"))
    (pad 1 smd rect (at -1.6 2.2 56.5) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(U5-Pad6)"))
    (pad 6 smd rect (at -1.6 -2.2 56.5) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U6-Pad6)"))
  )
  (module CrumpPrints:APA102 (layer F.Cu) (tedit 54BDEC7B)
    (at 115.6372 46.653956 304)
    (fp_text reference U7 (at -3.280136 0.013234 34) (layer F.SilkS))
    (fp_text value APA102 (at 0.2 0 304) (layer F.SilkS))
    (pad 3 smd rect (at 1.6 2.2 34) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.6 -2.2 34) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 5 smd rect (at 0.000001 -2.2 34) (size 1.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(U7-Pad5)"))
    (pad 2 smd rect (at -0.000001 2.2 34) (size 1.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(U6-Pad5)"))
    (pad 1 smd rect (at -1.6 2.2 34) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U6-Pad6)"))
    (pad 6 smd rect (at -1.6 -2.2 34) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(U7-Pad6)"))
  )
  (module CrumpPrints:APA102 (layer F.Cu) (tedit 54BDEC7B)
    (at 122.948843 43.58793 281.5)
    (fp_text reference U8 (at -2.992589 -0.077336 11.5) (layer F.SilkS))
    (fp_text value APA102 (at 0.2 0 281.5) (layer F.SilkS))
    (pad 3 smd rect (at 1.6 2.2 11.5) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.6 -2.2 11.5) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 5 smd rect (at 0 -2.2 11.5) (size 1.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 59 LED_CMID))
    (pad 2 smd rect (at 0 2.2 11.5) (size 1.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(U7-Pad5)"))
    (pad 1 smd rect (at -1.6 2.2 11.5) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(U7-Pad6)"))
    (pad 6 smd rect (at -1.6 -2.2 11.5) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 60 LED_DMID))
  )
  (module CrumpPrints:APA102 (layer F.Cu) (tedit 54BDEC7B)
    (at 130.877238 43.553335 259)
    (fp_text reference U9 (at -2.94391 0.123227 349) (layer F.SilkS))
    (fp_text value APA102 (at 0.2 0 259) (layer F.SilkS))
    (pad 3 smd rect (at 1.6 2.2 349) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.6 -2.2 349) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 5 smd rect (at 0 -2.2 349) (size 1.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(U10-Pad2)"))
    (pad 2 smd rect (at 0 2.2 349) (size 1.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 59 LED_CMID))
    (pad 1 smd rect (at -1.6 2.2 349) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 60 LED_DMID))
    (pad 6 smd rect (at -1.6 -2.2 349) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(U10-Pad1)"))
  )
  (module CrumpPrints:APA102 (layer F.Cu) (tedit 54BDEC7B)
    (at 138.215359 46.55544 236.5)
    (fp_text reference U10 (at -3.350738 0.132818 326.5) (layer F.SilkS))
    (fp_text value APA102 (at 0.2 0 236.5) (layer F.SilkS))
    (pad 3 smd rect (at 1.6 2.2 326.5) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.6 -2.2 326.5) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 5 smd rect (at 0 -2.2 326.5) (size 1.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(U10-Pad5)"))
    (pad 2 smd rect (at 0 2.2 326.5) (size 1.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(U10-Pad2)"))
    (pad 1 smd rect (at -1.6 2.2 326.5) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(U10-Pad1)"))
    (pad 6 smd rect (at -1.6 -2.2 326.5) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(U10-Pad6)"))
  )
  (module CrumpPrints:APA102 (layer F.Cu) (tedit 54BDEC7B)
    (at 143.846043 52.1372 214)
    (fp_text reference U11 (at -3.138102 -0.197343 304) (layer F.SilkS))
    (fp_text value APA102 (at 0.2 0 214) (layer F.SilkS))
    (pad 3 smd rect (at 1.6 2.2 304) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.6 -2.2 304) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 5 smd rect (at 0.000001 -2.2 304) (size 1.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(U11-Pad5)"))
    (pad 2 smd rect (at -0.000001 2.2 304) (size 1.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(U10-Pad5)"))
    (pad 1 smd rect (at -1.6 2.2 304) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(U10-Pad6)"))
    (pad 6 smd rect (at -1.6 -2.2 304) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(U11-Pad6)"))
  )
  (module CrumpPrints:APA102 (layer F.Cu) (tedit 54BDEC7B)
    (at 146.912069 59.448843 191.5)
    (fp_text reference U12 (at -3.241491 -0.127975 281.5) (layer F.SilkS))
    (fp_text value APA102 (at 0.2 0 191.5) (layer F.SilkS))
    (pad 3 smd rect (at 1.6 2.2 281.5) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.6 -2.2 281.5) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 5 smd rect (at 0 -2.2 281.5) (size 1.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(U12-Pad5)"))
    (pad 2 smd rect (at 0 2.2 281.5) (size 1.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(U11-Pad5)"))
    (pad 1 smd rect (at -1.6 2.2 281.5) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(U11-Pad6)"))
    (pad 6 smd rect (at -1.6 -2.2 281.5) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(U12-Pad6)"))
  )
  (module CrumpPrints:APA102 (layer F.Cu) (tedit 54BDEC7B)
    (at 146.946664 67.377238 169)
    (fp_text reference U13 (at -3.24171 -0.077641 259) (layer F.SilkS))
    (fp_text value APA102 (at 0.2 0 169) (layer F.SilkS))
    (pad 3 smd rect (at 1.6 2.2 259) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.6 -2.2 259) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 5 smd rect (at 0 -2.2 259) (size 1.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(U13-Pad5)"))
    (pad 2 smd rect (at 0 2.2 259) (size 1.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(U12-Pad5)"))
    (pad 1 smd rect (at -1.6 2.2 259) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(U12-Pad6)"))
    (pad 6 smd rect (at -1.6 -2.2 259) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(U13-Pad6)"))
  )
  (module CrumpPrints:APA102 (layer F.Cu) (tedit 54BDEC7B)
    (at 143.944559 74.715359 146.5)
    (fp_text reference U14 (at -3.490931 -0.078988 236.5) (layer F.SilkS))
    (fp_text value APA102 (at 0.2 0 146.5) (layer F.SilkS))
    (pad 3 smd rect (at 1.6 2.2 236.5) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.6 -2.2 236.5) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 5 smd rect (at 0 -2.2 236.5) (size 1.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(U14-Pad5)"))
    (pad 2 smd rect (at 0 2.2 236.5) (size 1.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(U13-Pad5)"))
    (pad 1 smd rect (at -1.6 2.2 236.5) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(U13-Pad6)"))
    (pad 6 smd rect (at -1.6 -2.2 236.5) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(U14-Pad6)"))
  )
  (module CrumpPrints:APA102 (layer F.Cu) (tedit 54BDEC7B)
    (at 138.362799 80.346043 124)
    (fp_text reference U15 (at -3.385425 -0.057784 214) (layer F.SilkS))
    (fp_text value APA102 (at 0.2 0 124) (layer F.SilkS))
    (pad 3 smd rect (at 1.6 2.2 214) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.6 -2.2 214) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 5 smd rect (at 0.000001 -2.2 214) (size 1.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(U15-Pad5)"))
    (pad 2 smd rect (at -0.000001 2.2 214) (size 1.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(U14-Pad5)"))
    (pad 1 smd rect (at -1.6 2.2 214) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(U14-Pad6)"))
    (pad 6 smd rect (at -1.6 -2.2 214) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(U15-Pad6)"))
  )
  (module CrumpPrints:APA102 (layer F.Cu) (tedit 54BDEC7B)
    (at 131.051156 83.412069 101.5)
    (fp_text reference U16 (at -3.241491 -0.127974 191.5) (layer F.SilkS))
    (fp_text value APA102 (at 0.2 0 101.5) (layer F.SilkS))
    (pad 3 smd rect (at 1.6 2.2 191.5) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.6 -2.2 191.5) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 5 smd rect (at 0 -2.2 191.5) (size 1.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 37 LED_COUT))
    (pad 2 smd rect (at 0 2.2 191.5) (size 1.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(U15-Pad5)"))
    (pad 1 smd rect (at -1.6 2.2 191.5) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(U15-Pad6)"))
    (pad 6 smd rect (at -1.6 -2.2 191.5) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 35 LED_DOUT))
  )
  (module Crystals:Crystal_HC49-U_Vertical (layer F.Cu) (tedit 58CD2E9C)
    (at 198.12 82.55)
    (descr "Crystal THT HC-49/U http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-49/U")
    (fp_text reference Y1 (at 2.44 -3.525) (layer F.SilkS))
    (fp_text value 16MHz (at 2.44 3.525) (layer F.Fab))
    (fp_text user %R (at 2.44 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad2)"))
    (pad 2 thru_hole circle (at 4.88 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C5-Pad2)"))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_HC49-U_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_PTS645 (layer F.Cu) (tedit 58724A80)
    (at 213.36 80.01 270)
    (descr "C&K Components SPST SMD PTS645 Series 6mm Tact Switch")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference S6 (at 0 -4.05 270) (layer F.SilkS))
    (fp_text value SW_SPST (at 0 4.15 270) (layer F.Fab))
    (fp_text user %R (at 0 -4.05 270) (layer F.Fab))
    (pad 2 smd rect (at -3.98 2.25 270) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -3.98 -2.25 270) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 39 RESET))
    (pad 1 smd rect (at 3.98 -2.25 270) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 39 RESET))
    (pad 2 smd rect (at 3.98 2.25 270) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Buttons_Switches_SMD.3dshapes/SW_SPST_PTS645.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_TH_Tactile_Omron_B3F-10xx (layer F.Cu) (tedit 5928351D)
    (at 90.17 52.07)
    (descr SW_TH_Tactile_Omron_B3F-10xx_https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "Omron B3F-10xx")
    (fp_text reference S3 (at 3.25 -2.05) (layer F.SilkS))
    (fp_text value 10-XX (at 3.2 6.5) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 4 thru_hole circle (at 6.5 4.5) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 "Net-(S3-Pad3)"))
    (pad 3 thru_hole circle (at 0 4.5) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 "Net-(S3-Pad3)"))
    (pad 2 thru_hole circle (at 6.5 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_TH_Tactile_Omron_B3F-10xx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPDT_CK-JS102011SAQN (layer F.Cu) (tedit 593D9A8A)
    (at 227.33 77.47 90)
    (descr http://www.ckswitches.com/media/1422/js.pdf)
    (tags "switch spdt")
    (attr smd)
    (fp_text reference S5 (at 4.064 -2.794 180) (layer F.SilkS))
    (fp_text value SPDT (at 0 -2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.5 -2.75 90) (size 1.25 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0 -2.75 90) (size 1.25 2.5) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(S5-Pad2)"))
    (pad 3 smd rect (at 2.5 -2.75 90) (size 1.25 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(BZ1-Pad1)"))
    (pad "" np_thru_hole circle (at -3.4 0 90) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 3.4 0 90) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPDT_CK-JS102011SAQN.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "sit/stand - v1\nDavid Riley\ndriley@moonfall.com" (at 86.36 85.09) (layer B.SilkS))
  (gr_text "sit/stand - v1\nDavid Riley\ndriley@moonfall.com" (at 78.74 44.45) (layer F.SilkS))
  (gr_line (start 228.6 86.36) (end 228.6 86.36) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 228.6 40.64) (end 228.6 86.36) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 226.06 38.1) (end 226.06 38.1) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 72.39 38.1) (end 226.06 38.1) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 226.06 88.9) (end 72.39 88.9) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 226.06 86.36) (end 226.06 88.9) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 226.06 40.64) (end 228.6 40.64) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 69.85 40.64) (end 69.85 40.64) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 69.85 86.36) (end 69.85 40.64) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 72.39 40.64) (end 72.39 38.1) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 72.39 86.36) (end 69.85 86.36) (angle -90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 71.12 40.64) (xy 71.12 86.36) (xy 72.39 87.63) (xy 227.33 87.63) (xy 227.33 86.36)
        (xy 227.33 40.64) (xy 226.06 39.37) (xy 72.39 39.37)
      )
    )
  )
  (zone (net 3) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 71.12 39.37) (xy 71.12 87.63) (xy 227.33 87.63) (xy 227.33 39.37)
      )
    )
  )
)
