(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 42)
    (no_connects 0)
    (area 130.734999 29.134999 177.875001 106.755001)
    (thickness 1.6)
    (drawings 18)
    (tracks 123)
    (zones 0)
    (modules 26)
    (nets 26)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 177.8 29.21)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C2-Pad2)")
  (net 5 2)
  (net 6 input_gnd)
  (net 7 8)
  (net 8 "Net-(C5-Pad1)")
  (net 9 "Net-(C5-Pad2)")
  (net 10 "Net-(C6-Pad1)")
  (net 11 "Net-(C6-Pad2)")
  (net 12 "Net-(C8-Pad1)")
  (net 13 "Net-(C9-Pad1)")
  (net 14 output_gnd)
  (net 15 "Net-(C10-Pad1)")
  (net 16 "Net-(D1-Pad2)")
  (net 17 "Net-(J3-Pad1)")
  (net 18 "Net-(J3-Pad2)")
  (net 19 "Net-(J3-Pad3)")
  (net 20 "Net-(J3-Pad4)")
  (net 21 "Net-(R1-Pad1)")
  (net 22 "Net-(R3-Pad1)")
  (net 23 "Net-(R4-Pad2)")
  (net 24 R-O)
  (net 25 L-O)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 2)
    (add_net 8)
    (add_net L-O)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad2)")
    (add_net R-O)
    (add_net input_gnd)
    (add_net output_gnd)
  )
  (module Potentiometers:Potentiometer_Alps_RK163_Double_Vertical (layer F.Cu) (tedit 58826D39)
    (at 166.37 34.29 90)
    (descr "Potentiometer, vertically mounted, Omeg PC16PU, Omeg PC16PU, Omeg PC16PU, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GH/249GH Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148A/149A Single with mounting plates, Vishay/Spectrol 148/149 Double, Vishay/Spectrol 148A/149A Double with mounting plates, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16SV Single, Piher PC-16 Double, Piher PC-16 Triple, Piher T16H Single, Piher T16L Single, Piher T16H Double, Alps RK163 Single, Alps RK163 Double, http://www.alps.com/prod/info/E/PDF/Potentiometer/MetalShaft/RK163/RK163.PDF")
    (tags "Potentiometer vertical  Omeg PC16PU  Omeg PC16PU  Omeg PC16PU  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GH/249GH Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148A/149A Single with mounting plates  Vishay/Spectrol 148/149 Double  Vishay/Spectrol 148A/149A Double with mounting plates  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16SV Single  Piher PC-16 Double  Piher PC-16 Triple  Piher T16H Single  Piher T16L Single  Piher T16H Double  Alps RK163 Single  Alps RK163 Double")
    (fp_text reference RV1 (at 0 -15.2 90) (layer F.SilkS))
    (fp_text value POT_Dual_Separate (at 0 5.2 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 -10 90) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 24 R-O))
    (pad 2 thru_hole circle (at 0 -5 90) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 14 output_gnd))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 9 "Net-(C5-Pad2)"))
    (pad 6 thru_hole circle (at -5 -10 90) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 25 L-O))
    (pad 5 thru_hole circle (at -5 -5 90) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 14 output_gnd))
    (pad 4 thru_hole circle (at -5 0 90) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Potentiometers.3dshapes/Potentiometer_Alps_RK163_Double_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT2:SW_CuK_OS102011MA1QN1_SPDT_Angled (layer F.Cu) (tedit 59AFFC74)
    (at 175.26 44.45 90)
    (descr "CuK miniature slide switch, OS series, SPDT, right angle, http://www.ckswitches.com/media/1428/os.pdf")
    (tags "switch SPDT")
    (fp_text reference SW1 (at 1.4 -3.6 90) (layer F.SilkS))
    (fp_text value SW_SPST (at 1.7 7.7 90) (layer F.Fab))
    (fp_text user %R (at 2.3 1.7 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.5 2.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 2))
    (pad 2 thru_hole oval (at 2 0 90) (size 1.5 2.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 input_gnd))
    (pad 3 thru_hole oval (at 4 0 90) (size 1.5 2.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at -2.1 0 90) (size 2.2 3.5) (drill 1.5) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 6.1 0 90) (size 2.2 3.5) (drill 1.5) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_CuK_OS102011MA1QN1_SPDT_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_capacitors:CP_5x11mm (layer F.Cu) (tedit 0)
    (at 165.1 48.26)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C1 (at 0 -4.2) (layer F.SilkS))
    (fp_text value CP (at 0 4.2) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 0 -1) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad2)"))
    (model walter/capacitors/cp_5x11mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_capacitors:CP_4x7mm (layer F.Cu) (tedit 0)
    (at 152.4 86.36 180)
    (descr "Capacitor, pol, cyl 4x7mm")
    (fp_text reference C2 (at 0 -3.6 180) (layer F.SilkS))
    (fp_text value CP (at 0 3.6 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0.75 180) (size 1.2 1.2) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 0 -0.75 180) (size 1.2 1.2) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C2-Pad2)"))
    (model walter/capacitors/cp_4x7mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_capacitors:CP_5x7mm (layer F.Cu) (tedit 0)
    (at 166.37 85.09 270)
    (descr "Capacitor, pol, cyl 5x7mm")
    (fp_text reference C3 (at 0 -4.2 270) (layer F.SilkS))
    (fp_text value CP (at 0 4.2 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 5 2))
    (pad 2 thru_hole circle (at 0 -1 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 6 input_gnd))
    (model walter/capacitors/cp_5x7mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_capacitors:CP_5x11mm (layer F.Cu) (tedit 0)
    (at 167.64 73.66 90)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C4 (at 0 -4.2 90) (layer F.SilkS))
    (fp_text value CP (at 0 4.2 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1 90) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 7 8))
    (pad 2 thru_hole circle (at 0 -1 90) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 6 input_gnd))
    (model walter/capacitors/cp_5x11mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_capacitors:CP_5x11mm (layer F.Cu) (tedit 0)
    (at 158.75 48.26)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C5 (at 0 -4.2) (layer F.SilkS))
    (fp_text value CP (at 0 4.2) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C5-Pad1)"))
    (pad 2 thru_hole circle (at 0 -1) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C5-Pad2)"))
    (model walter/capacitors/cp_5x11mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_capacitors:CP_4x7mm (layer F.Cu) (tedit 0)
    (at 160.02 86.36 180)
    (descr "Capacitor, pol, cyl 4x7mm")
    (fp_text reference C6 (at 0 -3.6 180) (layer F.SilkS))
    (fp_text value CP (at 0 3.6 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0.75 180) (size 1.2 1.2) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at 0 -0.75 180) (size 1.2 1.2) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C6-Pad2)"))
    (model walter/capacitors/cp_4x7mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 166.37 55.88 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C7 (at 1.25 -2.56 270) (layer F.SilkS))
    (fp_text value C_Small (at 1.25 2.56 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 8))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 input_gnd))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_capacitors:CP_5x11mm (layer F.Cu) (tedit 0)
    (at 166.37 63.5 270)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C8 (at 0 -4.2 270) (layer F.SilkS))
    (fp_text value CP (at 0 4.2 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(C8-Pad1)"))
    (pad 2 thru_hole circle (at 0 -1 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 6 input_gnd))
    (model walter/capacitors/cp_5x11mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_capacitors:CP_4x7mm (layer F.Cu) (tedit 0)
    (at 135.89 48.26 270)
    (descr "Capacitor, pol, cyl 4x7mm")
    (fp_text reference C9 (at 0 -3.6 270) (layer F.SilkS))
    (fp_text value CP (at 0 3.6 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0.75 270) (size 1.2 1.2) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C9-Pad1)"))
    (pad 2 thru_hole circle (at 0 -0.75 270) (size 1.2 1.2) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 14 output_gnd))
    (model walter/capacitors/cp_4x7mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_capacitors2:CP_4x7mm (layer F.Cu) (tedit 526424B7)
    (at 146.05 46.99 90)
    (descr "Capacitor, pol, cyl 4x7mm")
    (fp_text reference C10 (at 0 -3.6 90) (layer F.SilkS))
    (fp_text value CP (at 0 3.6 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0.75 90) (size 1.2 1.2) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(C10-Pad1)"))
    (pad 2 thru_hole circle (at 0 -0.75 90) (size 1.2 1.2) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 14 output_gnd))
    (model walter/capacitors/cp_4x7mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 173.99 50.8 270)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -3.96 270) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 input_gnd))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_pc:conn_usb_B_micro_smd-3 (layer F.Cu) (tedit 5AD5C42C)
    (at 147.32 104.14)
    (descr "USB B micro SMD connector with retention pins")
    (fp_text reference J3 (at 0 2.60096) (layer F.SilkS))
    (fp_text value USB_OTG (at 0 -4.0005) (layer F.SilkS))
    (pad "" smd rect (at -1.19888 0) (size 1.89738 1.89738) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 1.19888 0) (size 1.89738 1.89738) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 3.9497 0) (size 1.89738 1.89738) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -3.9497 0) (size 1.89738 1.89738) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.30048 -2.67462) (size 0.39878 1.34874) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J3-Pad1)"))
    (pad 2 smd rect (at -0.6477 -2.67462) (size 0.39878 1.3462) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J3-Pad2)"))
    (pad 3 smd rect (at 0 -2.67462) (size 0.39878 1.3462) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J3-Pad3)"))
    (pad 4 smd rect (at 0.6477 -2.67462) (size 0.39878 1.3462) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J3-Pad4)"))
    (pad 5 smd rect (at 1.30048 -2.67462) (size 0.39878 1.3462) (layers F.Cu F.Paste F.Mask)
      (net 14 output_gnd))
    (pad "" np_thru_hole circle (at 1.89738 -2.1463) (size 0.79756 0.79756) (drill 0.79756) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -1.89992 -2.14884) (size 0.79756 0.79756) (drill 0.79756) (layers *.Cu *.Mask F.SilkS))
    (model walter/conn_pc/usb_B_micro_smd-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:Pin_d1.4mm_L8.5mm_W2.8mm_FlatFork (layer F.Cu) (tedit 59B3E075)
    (at 148.59 40.64)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference J4 (at 0 2.25) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 14 output_gnd))
    (model ${KISYS3DMOD}/Connectors.3dshapes/Pin_d1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:Pin_d1.4mm_L8.5mm_W2.8mm_FlatFork (layer F.Cu) (tedit 59B3E075)
    (at 153.67 50.8)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference J5 (at 0 2.25) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 15 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Connectors.3dshapes/Pin_d1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 152.4 69.85 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 -2.31 270) (layer F.SilkS))
    (fp_text value R (at 5.08 2.31 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(R1-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 173.99 95.25 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.08 -2.31 90) (layer F.SilkS))
    (fp_text value R (at 5.08 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 2))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 8))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 160.02 69.85 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 5.08 -2.31 270) (layer F.SilkS))
    (fp_text value R (at 5.08 2.31 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(R3-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 173.99 57.15 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 5.08 -2.31 270) (layer F.SilkS))
    (fp_text value R (at 5.08 2.31 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(D1-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 173.99 81.28 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 5.08 -2.31 90) (layer F.SilkS))
    (fp_text value R (at 5.08 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 8))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:Switch_Slide_11.6x4mm_EG1218 (layer F.Cu) (tedit 5A1EC915)
    (at 134.62 69.85 90)
    (descr http://spec_sheets.e-switch.com/specs/P040040.pdf)
    (fp_text reference SW2 (at 2.49 -3.02 90) (layer F.SilkS))
    (fp_text value SW_SPDT_MSM (at 2.11 3.14 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 17 "Net-(J3-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 23 "Net-(R4-Pad2)"))
    (pad 3 thru_hole circle (at 5 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 "Net-(C9-Pad1)"))
  )
  (module w_pth_circuits:dil_8-300_socket (layer F.Cu) (tedit 0)
    (at 156.21 59.69 270)
    (descr "IC, DIL8 x 0,3\", with socket")
    (tags DIL)
    (fp_text reference U1 (at 0 -6.35 270) (layer F.SilkS))
    (fp_text value SSM2165 (at 0 6.604 270) (layer F.SilkS))
    (pad 1 thru_hole oval (at -3.81 3.81 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at -1.27 3.81 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 5 2))
    (pad 3 thru_hole oval (at 1.27 3.81 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(R1-Pad1)"))
    (pad 4 thru_hole oval (at 3.81 3.81 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 6 input_gnd))
    (pad 5 thru_hole oval (at 3.81 -3.81 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(R3-Pad1)"))
    (pad 6 thru_hole oval (at 1.27 -3.81 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(C8-Pad1)"))
    (pad 7 thru_hole oval (at -1.27 -3.81 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C5-Pad1)"))
    (pad 8 thru_hole oval (at -3.81 -3.81 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 7 8))
    (model walter/pth_circuits/dil_8-300_socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Horizontal (layer F.Cu) (tedit 58CE52AD)
    (at 147.32 53.34 180)
    (descr "TO-220-3, Horizontal, RM 2.54mm")
    (tags "TO-220-3 Horizontal RM 2.54mm")
    (fp_text reference U2 (at 2.54 -20.58 180) (layer F.SilkS))
    (fp_text value LM7805_TO220 (at 2.54 1.9 180) (layer F.Fab))
    (fp_text user %R (at 2.54 -20.58 180) (layer F.Fab))
    (pad 0 np_thru_hole oval (at 2.54 -16.66 180) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(C10-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 14 output_gnd))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Horizontal.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad-lib:fml-Tayda_3.5mm_stereo_TRS_jack_A-853 (layer F.Cu) (tedit 5B442B6F)
    (at 138.43 36.83)
    (fp_text reference J1 (at -4.318 7.112) (layer F.SilkS))
    (fp_text value Audio-Jack-3 (at 0 0.508) (layer F.SilkS))
    (pad 3 thru_hole rect (at 0 -1.596) (size 3.5 2.5) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 14 output_gnd))
    (pad 2 thru_hole oval (at 5 3.41) (size 1.75 3.5) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 24 R-O))
    (pad 1 thru_hole oval (at -5 3.41) (size 1.75 3.5) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 25 L-O))
    (pad 4 thru_hole oval (at 2.5 3.41) (size 1.75 3.5) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole oval (at -2.5 3.41) (size 1.75 3.5) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module kicad-lib:fml-Tayda_3.5mm_stereo_TRS_jack_A-853 (layer F.Cu) (tedit 5B442B6F)
    (at 160.02 100.33 180)
    (fp_text reference J2 (at -4.318 7.112 180) (layer F.SilkS))
    (fp_text value Audio-Jack-3 (at 0 0.508 180) (layer F.SilkS))
    (pad 3 thru_hole rect (at 0 -1.596 180) (size 3.5 2.5) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 6 input_gnd))
    (pad 2 thru_hole oval (at 5 3.41 180) (size 1.75 3.5) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C2-Pad2)"))
    (pad 1 thru_hole oval (at -5 3.41 180) (size 1.75 3.5) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C6-Pad2)"))
    (pad 4 thru_hole oval (at 2.5 3.41 180) (size 1.75 3.5) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole oval (at -2.5 3.41 180) (size 1.75 3.5) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  )
  (gr_text "APA3541\nPORTABLE \nAUDIO AMP" (at 140.97 92.71) (layer B.SilkS))
  (gr_text "APA3541\nPORTABLE \nAUDIO AMP" (at 139.7 92.71) (layer F.SilkS))
  (gr_line (start 177.8 101.6) (end 177.8 33.02) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.62 106.68) (end 173.99 106.68) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.81 102.87) (end 130.81 33.02) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.62 29.21) (end 173.99 29.21) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 134.62 33.02) (end 130.81 33.02) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.8 102.87) (end 177.8 101.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 173.99 33.02) (end 173.99 29.21) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 173.99 102.87) (end 177.8 102.87) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 134.62 102.87) (end 134.62 106.68) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 134.62 102.87) (end 135.89 101.6) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 173.99 102.87) (end 175.26 101.6) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 173.99 33.02) (end 175.26 31.75) (layer Edge.Cuts) (width 0.15))
  (gr_text 9V+ (at 153.67 46.99) (layer B.SilkS))
  (gr_text 9V+ (at 153.67 46.99) (layer F.SilkS))
  (gr_text GND (at 148.59 36.83) (layer F.SilkS))
  (gr_text GND (at 148.59 36.83) (layer B.SilkS))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 177.8 106.68) (xy 130.81 106.68) (xy 130.81 29.21) (xy 177.8 29.21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 177.8 106.68) (xy 130.81 106.68) (xy 130.81 29.21) (xy 177.8 29.21)
      )
    )
  )
)
