(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 0)
    (no_connects 10)
    (area 132.016499 87.566499 165.163501 121.348501)
    (thickness 1.6002)
    (drawings 21)
    (tracks 125)
    (zones 0)
    (modules 8)
    (nets 18)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.254)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.127)
    (edge_width 0.127)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (grid_origin 160.02 119.38)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x3ffff_80000001)
      (usegerberextensions true)
      (usegerberattributes true)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory CAM/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(JL1-Pad3)")
  (net 4 "Net-(JL1-Pad4)")
  (net 5 "Net-(JN1-Pad1)")
  (net 6 "Net-(JN1-Pad2)")
  (net 7 "Net-(JN1-Pad3)")
  (net 8 "Net-(JN1-Pad4)")
  (net 9 "Net-(JN1-Pad5)")
  (net 10 "Net-(JN1-Pad6)")
  (net 11 "Net-(JN1-Pad7)")
  (net 12 "Net-(JN1-Pad8)")
  (net 13 "Net-(JN1-Pad9)")
  (net 14 "Net-(JN1-Pad10)")
  (net 15 "Net-(JN1-Pad11)")
  (net 16 "Net-(JN1-Pad12)")
  (net 17 "Net-(JR1-Pad1)")
  (net_class Default "Imperial - this is the standard class"
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(JL1-Pad3)")
    (add_net "Net-(JL1-Pad4)")
    (add_net "Net-(JN1-Pad1)")
    (add_net "Net-(JN1-Pad10)")
    (add_net "Net-(JN1-Pad11)")
    (add_net "Net-(JN1-Pad12)")
    (add_net "Net-(JN1-Pad2)")
    (add_net "Net-(JN1-Pad3)")
    (add_net "Net-(JN1-Pad4)")
    (add_net "Net-(JN1-Pad5)")
    (add_net "Net-(JN1-Pad6)")
    (add_net "Net-(JN1-Pad7)")
    (add_net "Net-(JN1-Pad8)")
    (add_net "Net-(JN1-Pad9)")
    (add_net "Net-(JR1-Pad1)")
  )
  (net_class 0.2mm ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class Minimal ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 592C9D89)
    (at 148.5011 110.49 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 152.4 90.17 270)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference JL1 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value led (at 0 9.95 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(JL1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(JL1-Pad4)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC2)
    (at 162.56 120.015 270)
    (descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x12 2.54mm single row")
    (fp_text reference JN1 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value nixie (at 0 30.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(JN1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(JN1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(JN1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(JN1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(JN1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(JN1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(JN1-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(JN1-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(JN1-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(JN1-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(JN1-Pad11)"))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(JN1-Pad12)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 160.02 114.3 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JR1 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value jumper (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(JR1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(JN1-Pad12)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module adafruit:adafruit-WS2812B (layer F.Cu) (tedit 592C8129)
    (at 148.5011 105.0036 90)
    (attr smd)
    (fp_text reference LED1 (at 3.8989 0.4445 360) (layer F.SilkS))
    (fp_text value WS2812B5050 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1-VD smd rect (at 2.44856 1.64846 270) (size 1.4986 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2-DO smd rect (at 2.44856 -1.64846 270) (size 1.4986 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(JL1-Pad4)"))
    (pad 3-GN smd rect (at -2.44856 -1.64846 270) (size 1.4986 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 4-DI smd rect (at -2.44856 1.64846 270) (size 1.4986 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(JL1-Pad3)"))
  )
  (module mynixies:mynixies-5991-D-SUB (layer F.Cu) (tedit 592C814C)
    (at 148.5011 105.0036)
    (attr virtual)
    (fp_text reference NX1 (at 10.795 0.635 270) (layer F.SilkS))
    (fp_text value 5991 (at -10.795 0 90) (layer F.SilkS))
    (fp_text user TOP (at 0.635 -5.715) (layer F.SilkS))
    (pad 0 thru_hole circle (at 5.588 4.318) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 15 "Net-(JN1-Pad11)"))
    (pad 1 thru_hole circle (at -3.7846 7.7597) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 6 "Net-(JN1-Pad2)"))
    (pad 2 thru_hole circle (at -5.588 4.318) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 7 "Net-(JN1-Pad3)"))
    (pad 3 thru_hole circle (at -5.588 0) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 8 "Net-(JN1-Pad4)"))
    (pad 4 thru_hole circle (at -5.588 -4.318) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 9 "Net-(JN1-Pad5)"))
    (pad 5 thru_hole circle (at -3.7846 -7.7597) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 10 "Net-(JN1-Pad6)"))
    (pad 6 thru_hole circle (at 0 -8.636) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 11 "Net-(JN1-Pad7)"))
    (pad 7 thru_hole circle (at 3.7846 -7.7597) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 12 "Net-(JN1-Pad8)"))
    (pad 8 thru_hole circle (at 5.588 -4.318) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 13 "Net-(JN1-Pad9)"))
    (pad 9 thru_hole circle (at 5.588 0) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 14 "Net-(JN1-Pad10)"))
    (pad A thru_hole circle (at 3.7846 7.7597) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 17 "Net-(JR1-Pad1)"))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 161.29 110.49)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -1.7) (layer F.SilkS))
    (fp_text value R (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(JR1-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(JN1-Pad12)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module logos:mermaid_l (layer F.Cu) (tedit 0)
    (at 135.255 92.71)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (gr_text Dout (at 144.78 88.265) (layer F.SilkS))
  (gr_text Din (at 147.32 88.265) (layer F.SilkS))
  (gr_text Vcc (at 149.86 88.265) (layer F.SilkS))
  (gr_text Gnd (at 152.4 88.265) (layer F.SilkS))
  (gr_text NC (at 162.56 117.475) (layer F.SilkS))
  (gr_text 1 (at 160.02 117.475) (layer F.SilkS))
  (gr_text 2 (at 157.48 117.475) (layer F.SilkS))
  (gr_text 3 (at 154.94 117.475) (layer F.SilkS))
  (gr_text 4 (at 152.4 117.475) (layer F.SilkS))
  (gr_text 5 (at 149.86 117.475) (layer F.SilkS))
  (gr_text 6 (at 147.32 117.475) (layer F.SilkS))
  (gr_text 7 (at 144.78 117.475) (layer F.SilkS))
  (gr_text 8 (at 142.24 117.475) (layer F.SilkS))
  (gr_text 9 (at 139.7 117.475) (layer F.SilkS))
  (gr_text 0 (at 137.16 117.475) (layer F.SilkS))
  (gr_text A (at 134.62 117.475) (layer F.SilkS))
  (gr_line (start 132.08 121.92) (end 132.08 87.63) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 165.1 87.63) (end 165.1 121.92) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 132.08 87.63) (end 165.1 87.63) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 165.1 121.92) (end 132.08 121.92) (layer Edge.Cuts) (width 0.127))
  (gr_text nixies.us (at 138.43 92.71 90) (layer F.Mask))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.715 88.265) (xy 132.715 97.155) (xy 139.7 97.155) (xy 139.7 88.265)
      )
    )
  )
)
