(kicad_pcb (version 20171130) (host pcbnew 5.1.6-c6e7f7d~86~ubuntu16.04.1)
  (general
    (thickness 1.6)
    (drawings 12)
    (tracks 336)
    (zones 0)
    (modules 21)
    (nets 54)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.999999 2.999999)
    (pad_drill 2.29)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad2)")
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C2-Pad2)")
  (net 4 "Net-(C2-Pad1)")
  (net 5 VCC)
  (net 6 GND)
  (net 7 "Net-(C5-Pad2)")
  (net 8 "Net-(C5-Pad1)")
  (net 9 "Net-(C6-Pad2)")
  (net 10 "Net-(C6-Pad1)")
  (net 11 "Net-(C7-Pad2)")
  (net 12 "Net-(C8-Pad2)")
  (net 13 "Net-(C9-Pad2)")
  (net 14 "Net-(C10-Pad2)")
  (net 15 /PS2_CLK)
  (net 16 "Net-(J1-Pad6)")
  (net 17 /PS2_DATA)
  (net 18 "Net-(J1-Pad2)")
  (net 19 "Net-(J2-Pad7)")
  (net 20 /TX3)
  (net 21 /RX3)
  (net 22 "Net-(J2-Pad4)")
  (net 23 "Net-(J3-Pad9)")
  (net 24 "Net-(J3-Pad6)")
  (net 25 "Net-(J3-Pad4)")
  (net 26 /TX_PRT)
  (net 27 "Net-(J3-Pad1)")
  (net 28 "Net-(J4-Pad9)")
  (net 29 /RTS_COMP)
  (net 30 /CTS_COMP)
  (net 31 "Net-(J4-Pad6)")
  (net 32 "Net-(J4-Pad4)")
  (net 33 /TX_COMP)
  (net 34 /RX_COMP)
  (net 35 "Net-(J4-Pad1)")
  (net 36 /RX1)
  (net 37 /TX1)
  (net 38 /RTS1)
  (net 39 "Net-(U1-Pad5)")
  (net 40 "Net-(U1-Pad8)")
  (net 41 /RX2)
  (net 42 /TX2)
  (net 43 /RTS2)
  (net 44 "Net-(U1-Pad32)")
  (net 45 "Net-(U1-Pad31)")
  (net 46 /CTS2)
  (net 47 "Net-(U1-Pad29)")
  (net 48 "Net-(U1-Pad28)")
  (net 49 /CTS1)
  (net 50 "Net-(U1-Pad20)")
  (net 51 /CTS_PRT)
  (net 52 /RTS_PRT)
  (net 53 /RX_PRT)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CTS1)
    (add_net /CTS2)
    (add_net /CTS_COMP)
    (add_net /CTS_PRT)
    (add_net /PS2_CLK)
    (add_net /PS2_DATA)
    (add_net /RTS1)
    (add_net /RTS2)
    (add_net /RTS_COMP)
    (add_net /RTS_PRT)
    (add_net /RX1)
    (add_net /RX2)
    (add_net /RX3)
    (add_net /RX_COMP)
    (add_net /RX_PRT)
    (add_net /TX1)
    (add_net /TX2)
    (add_net /TX3)
    (add_net /TX_COMP)
    (add_net /TX_PRT)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(J3-Pad9)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad4)")
    (add_net "Net-(J4-Pad6)")
    (add_net "Net-(J4-Pad9)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad31)")
    (add_net "Net-(U1-Pad32)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad8)")
    (add_net VCC)
  )
  (module ps2-serial-printer-terminal:DSUB-9_Female_Horizontal_4UCON_09956 (layer F.Cu) (tedit 5EFD15B2)
    (at 219.71 124.46 270)
    (fp_text reference J3 (at 0 14 90) (layer F.SilkS))
    (fp_text value DB9_Female (at 0 16 90) (layer F.Fab))
    (pad 11 thru_hole circle (at 12.495 9.52 270) (size 4.2 4.2) (drill 3.2) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 10 thru_hole circle (at -12.495 9.52 270) (size 4.2 4.2) (drill 3.2) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 9 thru_hole circle (at 4.155 8.1 270) (size 1.7 1.7) (drill 1.09) (layers *.Cu *.Mask)
      (net 23 "Net-(J3-Pad9)"))
    (pad 8 thru_hole circle (at 1.385 8.1 270) (size 1.7 1.7) (drill 1.09) (layers *.Cu *.Mask)
      (net 52 /RTS_PRT))
    (pad 7 thru_hole circle (at -1.385 8.1 270) (size 1.7 1.7) (drill 1.09) (layers *.Cu *.Mask)
      (net 51 /CTS_PRT))
    (pad 6 thru_hole circle (at -4.155 8.1 270) (size 1.7 1.7) (drill 1.09) (layers *.Cu *.Mask)
      (net 24 "Net-(J3-Pad6)"))
    (pad 5 thru_hole circle (at 5.54 10.94 270) (size 1.7 1.7) (drill 1.09) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 4 thru_hole circle (at 2.77 10.94 270) (size 1.7 1.7) (drill 1.09) (layers *.Cu *.Mask)
      (net 25 "Net-(J3-Pad4)"))
    (pad 3 thru_hole circle (at 0 10.94 270) (size 1.7 1.7) (drill 1.09) (layers *.Cu *.Mask)
      (net 53 /RX_PRT))
    (pad 2 thru_hole circle (at -2.77 10.94 270) (size 1.7 1.7) (drill 1.09) (layers *.Cu *.Mask)
      (net 26 /TX_PRT))
    (pad 1 thru_hole circle (at -5.54 10.94 270) (size 1.7 1.7) (drill 1.09) (layers *.Cu *.Mask)
      (net 27 "Net-(J3-Pad1)"))
  )
  (module ps2-serial-printer-terminal:DSUB-9_Female_Horizontal_4UCON_09956 (layer F.Cu) (tedit 5EFD15B2)
    (at 127 124.46 90)
    (fp_text reference J4 (at 0 14 90) (layer F.SilkS))
    (fp_text value DB9_Female (at 0 16 90) (layer F.Fab))
    (pad 11 thru_hole circle (at 12.495 9.52 90) (size 4.2 4.2) (drill 3.2) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 10 thru_hole circle (at -12.495 9.52 90) (size 4.2 4.2) (drill 3.2) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 9 thru_hole circle (at 4.155 8.1 90) (size 1.7 1.7) (drill 1.09) (layers *.Cu *.Mask)
      (net 28 "Net-(J4-Pad9)"))
    (pad 8 thru_hole circle (at 1.385 8.1 90) (size 1.7 1.7) (drill 1.09) (layers *.Cu *.Mask)
      (net 29 /RTS_COMP))
    (pad 7 thru_hole circle (at -1.385 8.1 90) (size 1.7 1.7) (drill 1.09) (layers *.Cu *.Mask)
      (net 30 /CTS_COMP))
    (pad 6 thru_hole circle (at -4.155 8.1 90) (size 1.7 1.7) (drill 1.09) (layers *.Cu *.Mask)
      (net 31 "Net-(J4-Pad6)"))
    (pad 5 thru_hole circle (at 5.54 10.94 90) (size 1.7 1.7) (drill 1.09) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 4 thru_hole circle (at 2.77 10.94 90) (size 1.7 1.7) (drill 1.09) (layers *.Cu *.Mask)
      (net 32 "Net-(J4-Pad4)"))
    (pad 3 thru_hole circle (at 0 10.94 90) (size 1.7 1.7) (drill 1.09) (layers *.Cu *.Mask)
      (net 34 /RX_COMP))
    (pad 2 thru_hole circle (at -2.77 10.94 90) (size 1.7 1.7) (drill 1.09) (layers *.Cu *.Mask)
      (net 33 /TX_COMP))
    (pad 1 thru_hole circle (at -5.54 10.94 90) (size 1.7 1.7) (drill 1.09) (layers *.Cu *.Mask)
      (net 35 "Net-(J4-Pad1)"))
  )
  (module Package_SO:SOIC-16_3.9x9.9mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 154.239 115.509 180)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U3 (at 2.855 -6.157) (layer F.SilkS))
    (fp_text value MAX3232 (at 0 5.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 16 smd roundrect (at 2.475 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 VCC))
    (pad 15 smd roundrect (at 2.475 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 GND))
    (pad 14 smd roundrect (at 2.475 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 /TX_COMP))
    (pad 13 smd roundrect (at 2.475 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 /RX_COMP))
    (pad 12 smd roundrect (at 2.475 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 /RX2))
    (pad 11 smd roundrect (at 2.475 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 /TX2))
    (pad 10 smd roundrect (at 2.475 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 /RTS2))
    (pad 9 smd roundrect (at 2.475 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 /CTS2))
    (pad 8 smd roundrect (at -2.475 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 /CTS_COMP))
    (pad 7 smd roundrect (at -2.475 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /RTS_COMP))
    (pad 6 smd roundrect (at -2.475 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C10-Pad2)"))
    (pad 5 smd roundrect (at -2.475 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C6-Pad2)"))
    (pad 4 smd roundrect (at -2.475 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C6-Pad1)"))
    (pad 3 smd roundrect (at -2.475 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(C2-Pad2)"))
    (pad 2 smd roundrect (at -2.475 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(C9-Pad2)"))
    (pad 1 smd roundrect (at -2.475 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-16_3.9x9.9mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 189.659 115.959 180)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U2 (at 2.8674 -6.0626) (layer F.SilkS))
    (fp_text value MAX3232 (at 0 5.9) (layer F.Fab))
    (fp_text user %R (at 0.81 -1.77) (layer F.Fab))
    (pad 16 smd roundrect (at 2.475 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 VCC))
    (pad 15 smd roundrect (at 2.475 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 GND))
    (pad 14 smd roundrect (at 2.475 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 /TX_PRT))
    (pad 13 smd roundrect (at 2.475 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 /RX_PRT))
    (pad 12 smd roundrect (at 2.475 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 /RX1))
    (pad 11 smd roundrect (at 2.475 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 /TX1))
    (pad 10 smd roundrect (at 2.475 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 /RTS1))
    (pad 9 smd roundrect (at 2.475 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 /CTS1))
    (pad 8 smd roundrect (at -2.475 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 /CTS_PRT))
    (pad 7 smd roundrect (at -2.475 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 /RTS_PRT))
    (pad 6 smd roundrect (at -2.475 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C8-Pad2)"))
    (pad 5 smd roundrect (at -2.475 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C5-Pad2)"))
    (pad 4 smd roundrect (at -2.475 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(C5-Pad1)"))
    (pad 3 smd roundrect (at -2.475 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad2)"))
    (pad 2 smd roundrect (at -2.475 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(C7-Pad2)"))
    (pad 1 smd roundrect (at -2.475 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module teensy:Teensy30_31_32_LC_minus (layer F.Cu) (tedit 5EEEDB4F)
    (at 174.244 124.714 90)
    (fp_text reference U1 (at 0 -10.16 90) (layer F.SilkS))
    (fp_text value Teensy3.2 (at 0 10.16 90) (layer F.Fab))
    (fp_text user T3.1 (at -6.35 -2.54) (layer F.SilkS))
    (fp_text user T3.2 (at -10.16 -2.54) (layer F.SilkS))
    (pad 1 thru_hole rect (at -16.51 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 2 thru_hole circle (at -13.97 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 36 /RX1))
    (pad 3 thru_hole circle (at -11.43 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 37 /TX1))
    (pad 4 thru_hole circle (at -8.89 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 38 /RTS1))
    (pad 5 thru_hole circle (at -6.35 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(U1-Pad5)"))
    (pad 6 thru_hole circle (at -3.81 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 15 /PS2_CLK))
    (pad 7 thru_hole circle (at -1.27 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 17 /PS2_DATA))
    (pad 8 thru_hole circle (at 1.27 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(U1-Pad8)"))
    (pad 9 thru_hole circle (at 3.81 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 21 /RX3))
    (pad 10 thru_hole circle (at 6.35 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 20 /TX3))
    (pad 11 thru_hole circle (at 8.89 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 41 /RX2))
    (pad 12 thru_hole circle (at 11.43 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 42 /TX2))
    (pad 13 thru_hole circle (at 13.97 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 43 /RTS2))
    (pad 33 thru_hole circle (at -16.51 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 5 VCC))
    (pad 32 thru_hole circle (at -13.97 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(U1-Pad32)"))
    (pad 31 thru_hole circle (at -11.43 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(U1-Pad31)"))
    (pad 30 thru_hole circle (at -8.89 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 46 /CTS2))
    (pad 29 thru_hole circle (at -6.35 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(U1-Pad29)"))
    (pad 28 thru_hole circle (at -3.81 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(U1-Pad28)"))
    (pad 27 thru_hole circle (at -1.27 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 49 /CTS1))
    (pad 20 thru_hole circle (at 16.51 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(U1-Pad20)"))
  )
  (module ps2-serial-printer-terminal:MD-80SM (layer F.Cu) (tedit 5EF0796D)
    (at 191.77 142.494 180)
    (fp_text reference J2 (at 0 13.4112) (layer F.SilkS))
    (fp_text value Mini-DIN-8 (at 0 14) (layer F.Fab))
    (pad 11 thru_hole oval (at 6.75 5.5 180) (size 1.3 2.8) (drill oval 0.7 2.2) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 10 thru_hole oval (at -6.75 5.5 180) (size 1.3 2.8) (drill oval 0.7 2.2) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 9 thru_hole oval (at 0 4.7 180) (size 2.8 1.3) (drill oval 2.2 0.7) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 8 thru_hole circle (at 3.4 11 180) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 7 thru_hole circle (at 0.9 11 180) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad7)"))
    (pad 6 thru_hole circle (at -3.4 11 180) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 21 /RX3))
    (pad 5 thru_hole circle (at 3.4 8.5 180) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 20 /TX3))
    (pad 4 thru_hole circle (at -1.3 11 180) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad4)"))
    (pad 3 thru_hole circle (at -3.4 8.5 180) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 2 thru_hole circle (at 1.3 8.5 180) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at -1.3 8.5 180) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 GND))
  )
  (module ps2-serial-printer-terminal:5749231-1 (layer F.Cu) (tedit 5EF076CE)
    (at 156.464 142.368 180)
    (fp_text reference J1 (at -8 11 90) (layer F.SilkS))
    (fp_text value Mini-DIN-6 (at 0 14) (layer F.Fab))
    (pad 9 thru_hole roundrect (at 6.76 5.51 180) (size 3 3) (drill 2.29) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 6 GND))
    (pad 8 thru_hole roundrect (at -6.76 5.51 180) (size 3 3) (drill 2.29) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 6 GND))
    (pad 7 thru_hole roundrect (at 0 4.7 180) (size 3 3) (drill 2.29) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 6 GND))
    (pad 5 thru_hole circle (at -3.35 11 180) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 15 /PS2_CLK))
    (pad 6 thru_hole circle (at 3.35 11 180) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad6)"))
    (pad 3 thru_hole circle (at -3.35 8.51 180) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 4 thru_hole circle (at 3.35 8.51 180) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 1 thru_hole circle (at -1.3 8.51 180) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 17 /PS2_DATA))
    (pad 2 thru_hole circle (at 1.3 8.51 180) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad2)"))
  )
  (module MountingHole:MountingHole_3mm_Pad_Via (layer F.Cu) (tedit 56DDBED4)
    (at 203.2 138.43)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (attr virtual)
    (fp_text reference H4 (at 0 -4) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.59099 -1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 0 -2.25) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at -1.59099 -1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at -2.25 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at -1.59099 1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 0 2.25) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 1.59099 1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 2.25 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Mask)
      (net 6 GND))
  )
  (module MountingHole:MountingHole_3mm_Pad_Via (layer F.Cu) (tedit 56DDBED4)
    (at 143.51 138.43)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (attr virtual)
    (fp_text reference H3 (at -3.5052 -2.8956) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.59099 -1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 0 -2.25) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at -1.59099 -1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at -2.25 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at -1.59099 1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 0 2.25) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 1.59099 1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 2.25 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Mask)
      (net 6 GND))
  )
  (module MountingHole:MountingHole_3mm_Pad_Via (layer F.Cu) (tedit 56DDBED4)
    (at 203.2 113.03 180)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (attr virtual)
    (fp_text reference H2 (at -3.0988 3.302) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.59099 -1.59099 180) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 0 -2.25 180) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at -1.59099 -1.59099 180) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at -2.25 0 180) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at -1.59099 1.59099 180) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 0 2.25 180) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 1.59099 1.59099 180) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 2.25 0 180) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 6 6) (drill 3) (layers *.Cu *.Mask)
      (net 6 GND))
  )
  (module MountingHole:MountingHole_3mm_Pad_Via (layer F.Cu) (tedit 56DDBED4)
    (at 143.51 113.03)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (attr virtual)
    (fp_text reference H1 (at -3.4544 -2.9972) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.59099 -1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 0 -2.25) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at -1.59099 -1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at -2.25 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at -1.59099 1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 0 2.25) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 1.59099 1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 2.25 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Mask)
      (net 6 GND))
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 159.7152 112.014 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C10 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value C (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 14 "Net-(C10-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 159.258 120.142 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C9 (at -0.9144 1.524 90) (layer F.SilkS))
    (fp_text value C (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 13 "Net-(C9-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 194.564 112.522 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C8 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value C (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 12 "Net-(C8-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 194.564 120.65 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C7 (at 0.4064 1.5748 90) (layer F.SilkS))
    (fp_text value C (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 11 "Net-(C7-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 159.258 116.078 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C6 (at 0 1.524 90) (layer F.SilkS))
    (fp_text value C (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 9 "Net-(C6-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 10 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 194.564 116.586 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at 0 1.524 90) (layer F.SilkS))
    (fp_text value C (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 "Net-(C5-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 149.352 118.872 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at -2.54 -0.2032 180) (layer F.SilkS))
    (fp_text value C (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 VCC))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 184.658 119.634 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value C (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 VCC))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 155.702 122.174 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 0 -1.65) (layer F.SilkS))
    (fp_text value C (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 "Net-(C2-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 191.262 122.428 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 -1.65) (layer F.SilkS))
    (fp_text value C (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 "Net-(C1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text SP3232EB (at 189.992 115.824 90) (layer F.SilkS))
  (gr_text SP3232EB (at 154.432 115.824 90) (layer F.SilkS))
  (gr_text "PS/2 Serial Printer Terminal v2" (at 171.45 107.95 90) (layer B.SilkS))
  (gr_text github.com/RussellSenior/lqp02-teletype/ (at 173.99 107.95 90) (layer B.SilkS))
  (gr_text "SUN KBD" (at 191.516 140.716) (layer B.SilkS))
  (gr_text "PS/2 KBD" (at 156.464 140.716) (layer B.SilkS))
  (gr_text COMPUTER (at 129.54 124.46 270) (layer B.SilkS))
  (gr_text PRINTER (at 217.17 124.46 90) (layer B.SilkS))
  (gr_line (start 127 142.24) (end 127 106.68) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 219.71 142.24) (end 219.71 106.68) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 219.71 142.24) (end 127 142.24) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 127 106.68) (end 219.71 106.68) (layer Edge.Cuts) (width 0.1))
  (zone (net 5) (net_name VCC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 219.71 142.24) (xy 127 142.24) (xy 127 106.68) (xy 219.71 106.68)
      )
    )
  )
  (zone (net 6) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 219.71 142.24) (xy 127 142.24) (xy 127 106.68) (xy 219.71 106.68)
      )
    )
  )
)
