(kicad_pcb (version 20171130) (host pcbnew 5.1.5)
  (general
    (thickness 1.6)
    (drawings 65)
    (tracks 201)
    (zones 0)
    (modules 9)
    (nets 42)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010e0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 /GND)
  (net 2 "Net-(G1-Pad14)")
  (net 3 "Net-(G1-Pad16)")
  (net 4 "Net-(G1-Pad20)")
  (net 5 "Net-(G1-Pad18)")
  (net 6 "Net-(G1-Pad12)")
  (net 7 "Net-(G2-Pad14)")
  (net 8 "Net-(G2-Pad16)")
  (net 9 "Net-(G2-Pad20)")
  (net 10 "Net-(G2-Pad18)")
  (net 11 "Net-(G2-Pad12)")
  (net 12 "Net-(G3-Pad14)")
  (net 13 "Net-(G3-Pad16)")
  (net 14 "Net-(G3-Pad20)")
  (net 15 "Net-(G3-Pad18)")
  (net 16 "Net-(G3-Pad12)")
  (net 17 "Net-(G4-Pad14)")
  (net 18 "Net-(G4-Pad16)")
  (net 19 "Net-(G4-Pad20)")
  (net 20 "Net-(G4-Pad18)")
  (net 21 "Net-(G4-Pad12)")
  (net 22 "Net-(G1-Pad15)")
  (net 23 "Net-(G1-Pad11)")
  (net 24 "Net-(G1-Pad17)")
  (net 25 "Net-(G1-Pad19)")
  (net 26 "Net-(G1-Pad13)")
  (net 27 "Net-(G2-Pad15)")
  (net 28 "Net-(G2-Pad17)")
  (net 29 "Net-(G2-Pad13)")
  (net 30 "Net-(G2-Pad11)")
  (net 31 "Net-(G2-Pad19)")
  (net 32 "Net-(G3-Pad15)")
  (net 33 "Net-(G3-Pad11)")
  (net 34 "Net-(G3-Pad17)")
  (net 35 "Net-(G3-Pad19)")
  (net 36 "Net-(G3-Pad13)")
  (net 37 "Net-(G4-Pad15)")
  (net 38 "Net-(G4-Pad17)")
  (net 39 "Net-(G4-Pad13)")
  (net 40 "Net-(G4-Pad11)")
  (net 41 "Net-(G4-Pad19)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /GND)
    (add_net "Net-(G1-Pad11)")
    (add_net "Net-(G1-Pad12)")
    (add_net "Net-(G1-Pad13)")
    (add_net "Net-(G1-Pad14)")
    (add_net "Net-(G1-Pad15)")
    (add_net "Net-(G1-Pad16)")
    (add_net "Net-(G1-Pad17)")
    (add_net "Net-(G1-Pad18)")
    (add_net "Net-(G1-Pad19)")
    (add_net "Net-(G1-Pad20)")
    (add_net "Net-(G2-Pad11)")
    (add_net "Net-(G2-Pad12)")
    (add_net "Net-(G2-Pad13)")
    (add_net "Net-(G2-Pad14)")
    (add_net "Net-(G2-Pad15)")
    (add_net "Net-(G2-Pad16)")
    (add_net "Net-(G2-Pad17)")
    (add_net "Net-(G2-Pad18)")
    (add_net "Net-(G2-Pad19)")
    (add_net "Net-(G2-Pad20)")
    (add_net "Net-(G3-Pad11)")
    (add_net "Net-(G3-Pad12)")
    (add_net "Net-(G3-Pad13)")
    (add_net "Net-(G3-Pad14)")
    (add_net "Net-(G3-Pad15)")
    (add_net "Net-(G3-Pad16)")
    (add_net "Net-(G3-Pad17)")
    (add_net "Net-(G3-Pad18)")
    (add_net "Net-(G3-Pad19)")
    (add_net "Net-(G3-Pad20)")
    (add_net "Net-(G4-Pad11)")
    (add_net "Net-(G4-Pad12)")
    (add_net "Net-(G4-Pad13)")
    (add_net "Net-(G4-Pad14)")
    (add_net "Net-(G4-Pad15)")
    (add_net "Net-(G4-Pad16)")
    (add_net "Net-(G4-Pad17)")
    (add_net "Net-(G4-Pad18)")
    (add_net "Net-(G4-Pad19)")
    (add_net "Net-(G4-Pad20)")
  )
  (module unl_silab:crossed_circle_fiducial (layer F.Cu) (tedit 5DEEB95A)
    (at 124.4092 119.38)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value crossed_circle_fiducial (at 0 0) (layer F.Fab) hide)
  )
  (module unl_silab:crossed_circle_fiducial (layer F.Cu) (tedit 5DEEB95A)
    (at 95.6056 119.38)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value crossed_circle_fiducial (at 0 0) (layer F.Fab) hide)
  )
  (module unl_silab:crossed_circle_fiducial (layer F.Cu) (tedit 5DEEB95A)
    (at 124.4092 40.5892)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value crossed_circle_fiducial (at 0 0) (layer F.Fab) hide)
  )
  (module unl_silab:crossed_circle_fiducial (layer F.Cu) (tedit 5DEEB95A)
    (at 95.6056 40.5892)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value crossed_circle_fiducial (at 0 0) (layer F.Fab) hide)
  )
  (module unl_silab:NLOGO (layer F.Cu) (tedit 5D65A532)
    (at 108.75 115.25)
    (fp_text reference G*** (at 7.112 1.016) (layer F.SilkS) hide)
    (fp_text value LOGO (at 8.128 -2.032) (layer F.SilkS) hide)
  )
  (module unl_silab:2x10_wirebond_pads_and_testpts (layer F.Cu) (tedit 5D659E5A)
    (at 109.25 59)
    (fp_text reference G1 (at -0.25 0) (layer F.SilkS) hide)
    (fp_text value Conn_02x10_Counter_Clockwise (at 0 -10) (layer F.Fab))
    (pad 15 smd rect (at 1 -0.2) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(G1-Pad15)"))
    (pad 14 smd rect (at 1 -0.6) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(G1-Pad14)"))
    (pad 16 smd rect (at 1 0.2) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(G1-Pad16)"))
    (pad 20 smd rect (at 1 1.8) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(G1-Pad20)"))
    (pad 18 smd rect (at 1 1) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(G1-Pad18)"))
    (pad 12 smd rect (at 1 -1.4) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(G1-Pad12)"))
    (pad 17 smd rect (at 1 0.6) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(G1-Pad17)"))
    (pad 13 smd rect (at 1 -1) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(G1-Pad13)"))
    (pad 11 smd rect (at 1 -1.8) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(G1-Pad11)"))
    (pad 19 smd rect (at 1 1.4) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(G1-Pad19)"))
    (pad 10 smd rect (at -1 1.8) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 9 smd rect (at -1 1.4) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 8 smd rect (at -1 1) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 7 smd rect (at -1 0.6) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 6 smd rect (at -1 0.2) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 5 smd rect (at -1 -0.2) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 4 smd rect (at -1 -0.6) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 3 smd rect (at -1 -1) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 2 smd rect (at -1 -1.4) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 20 smd circle (at 10 7.4) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(G1-Pad20)"))
    (pad 13 smd circle (at 10 -3.8) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(G1-Pad13)"))
    (pad 19 smd circle (at 10 5.8) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(G1-Pad19)"))
    (pad 17 smd circle (at 10 2.6) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(G1-Pad17)"))
    (pad 12 smd circle (at 10 -5.4) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(G1-Pad12)"))
    (pad 11 smd circle (at 10 -7) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(G1-Pad11)"))
    (pad 16 smd circle (at 10 1) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(G1-Pad16)"))
    (pad 18 smd circle (at 10 4.2) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(G1-Pad18)"))
    (pad 14 smd circle (at 10 -2.2) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(G1-Pad14)"))
    (pad 15 smd circle (at 10 -0.6) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(G1-Pad15)"))
    (pad 10 smd circle (at -10 7.4) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 9 smd circle (at -10 5.8) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 8 smd circle (at -10 4.2) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 7 smd circle (at -10 2.6) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 6 smd circle (at -10 1) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 5 smd circle (at -10 -0.6) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 4 smd circle (at -10 -2.2) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 3 smd circle (at -10 -3.8) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 2 smd circle (at -10 -5.4) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 1 smd circle (at -10 -7) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 1 smd rect (at -1 -1.8) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
  )
  (module unl_silab:2x10_wirebond_pads_and_testpts (layer F.Cu) (tedit 5D659E5A)
    (at 109.25 110)
    (fp_text reference G4 (at -0.25 0) (layer F.SilkS) hide)
    (fp_text value Conn_02x10_Counter_Clockwise (at 0 -10) (layer F.Fab))
    (pad 15 smd rect (at 1 -0.2) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(G4-Pad15)"))
    (pad 14 smd rect (at 1 -0.6) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(G4-Pad14)"))
    (pad 16 smd rect (at 1 0.2) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(G4-Pad16)"))
    (pad 20 smd rect (at 1 1.8) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(G4-Pad20)"))
    (pad 18 smd rect (at 1 1) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(G4-Pad18)"))
    (pad 12 smd rect (at 1 -1.4) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(G4-Pad12)"))
    (pad 17 smd rect (at 1 0.6) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(G4-Pad17)"))
    (pad 13 smd rect (at 1 -1) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(G4-Pad13)"))
    (pad 11 smd rect (at 1 -1.8) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(G4-Pad11)"))
    (pad 19 smd rect (at 1 1.4) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(G4-Pad19)"))
    (pad 10 smd rect (at -1 1.8) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 9 smd rect (at -1 1.4) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 8 smd rect (at -1 1) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 7 smd rect (at -1 0.6) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 6 smd rect (at -1 0.2) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 5 smd rect (at -1 -0.2) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 4 smd rect (at -1 -0.6) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 3 smd rect (at -1 -1) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 2 smd rect (at -1 -1.4) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 20 smd circle (at 10 7.4) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(G4-Pad20)"))
    (pad 13 smd circle (at 10 -3.8) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(G4-Pad13)"))
    (pad 19 smd circle (at 10 5.8) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(G4-Pad19)"))
    (pad 17 smd circle (at 10 2.6) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(G4-Pad17)"))
    (pad 12 smd circle (at 10 -5.4) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(G4-Pad12)"))
    (pad 11 smd circle (at 10 -7) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(G4-Pad11)"))
    (pad 16 smd circle (at 10 1) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(G4-Pad16)"))
    (pad 18 smd circle (at 10 4.2) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(G4-Pad18)"))
    (pad 14 smd circle (at 10 -2.2) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(G4-Pad14)"))
    (pad 15 smd circle (at 10 -0.6) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(G4-Pad15)"))
    (pad 10 smd circle (at -10 7.4) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 9 smd circle (at -10 5.8) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 8 smd circle (at -10 4.2) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 7 smd circle (at -10 2.6) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 6 smd circle (at -10 1) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 5 smd circle (at -10 -0.6) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 4 smd circle (at -10 -2.2) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 3 smd circle (at -10 -3.8) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 2 smd circle (at -10 -5.4) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 1 smd circle (at -10 -7) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 1 smd rect (at -1 -1.8) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
  )
  (module unl_silab:2x10_wirebond_pads_and_testpts (layer F.Cu) (tedit 5D659E5A)
    (at 109.25 93)
    (fp_text reference G3 (at -0.25 0) (layer F.SilkS) hide)
    (fp_text value Conn_02x10_Counter_Clockwise (at 0 -10) (layer F.Fab))
    (pad 15 smd rect (at 1 -0.2) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(G3-Pad15)"))
    (pad 14 smd rect (at 1 -0.6) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(G3-Pad14)"))
    (pad 16 smd rect (at 1 0.2) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(G3-Pad16)"))
    (pad 20 smd rect (at 1 1.8) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(G3-Pad20)"))
    (pad 18 smd rect (at 1 1) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(G3-Pad18)"))
    (pad 12 smd rect (at 1 -1.4) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(G3-Pad12)"))
    (pad 17 smd rect (at 1 0.6) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(G3-Pad17)"))
    (pad 13 smd rect (at 1 -1) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(G3-Pad13)"))
    (pad 11 smd rect (at 1 -1.8) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(G3-Pad11)"))
    (pad 19 smd rect (at 1 1.4) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(G3-Pad19)"))
    (pad 10 smd rect (at -1 1.8) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 9 smd rect (at -1 1.4) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 8 smd rect (at -1 1) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 7 smd rect (at -1 0.6) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 6 smd rect (at -1 0.2) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 5 smd rect (at -1 -0.2) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 4 smd rect (at -1 -0.6) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 3 smd rect (at -1 -1) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 2 smd rect (at -1 -1.4) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 20 smd circle (at 10 7.4) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(G3-Pad20)"))
    (pad 13 smd circle (at 10 -3.8) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(G3-Pad13)"))
    (pad 19 smd circle (at 10 5.8) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(G3-Pad19)"))
    (pad 17 smd circle (at 10 2.6) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(G3-Pad17)"))
    (pad 12 smd circle (at 10 -5.4) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(G3-Pad12)"))
    (pad 11 smd circle (at 10 -7) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(G3-Pad11)"))
    (pad 16 smd circle (at 10 1) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(G3-Pad16)"))
    (pad 18 smd circle (at 10 4.2) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(G3-Pad18)"))
    (pad 14 smd circle (at 10 -2.2) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(G3-Pad14)"))
    (pad 15 smd circle (at 10 -0.6) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(G3-Pad15)"))
    (pad 10 smd circle (at -10 7.4) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 9 smd circle (at -10 5.8) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 8 smd circle (at -10 4.2) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 7 smd circle (at -10 2.6) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 6 smd circle (at -10 1) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 5 smd circle (at -10 -0.6) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 4 smd circle (at -10 -2.2) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 3 smd circle (at -10 -3.8) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 2 smd circle (at -10 -5.4) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 1 smd circle (at -10 -7) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 1 smd rect (at -1 -1.8) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
  )
  (module unl_silab:2x10_wirebond_pads_and_testpts (layer F.Cu) (tedit 5D659E5A)
    (at 109.25 76)
    (fp_text reference G2 (at -0.25 0) (layer F.SilkS) hide)
    (fp_text value Conn_02x10_Counter_Clockwise (at 0 -10) (layer F.Fab))
    (pad 15 smd rect (at 1 -0.2) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(G2-Pad15)"))
    (pad 14 smd rect (at 1 -0.6) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(G2-Pad14)"))
    (pad 16 smd rect (at 1 0.2) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(G2-Pad16)"))
    (pad 20 smd rect (at 1 1.8) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(G2-Pad20)"))
    (pad 18 smd rect (at 1 1) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(G2-Pad18)"))
    (pad 12 smd rect (at 1 -1.4) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(G2-Pad12)"))
    (pad 17 smd rect (at 1 0.6) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(G2-Pad17)"))
    (pad 13 smd rect (at 1 -1) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(G2-Pad13)"))
    (pad 11 smd rect (at 1 -1.8) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(G2-Pad11)"))
    (pad 19 smd rect (at 1 1.4) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(G2-Pad19)"))
    (pad 10 smd rect (at -1 1.8) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 9 smd rect (at -1 1.4) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 8 smd rect (at -1 1) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 7 smd rect (at -1 0.6) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 6 smd rect (at -1 0.2) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 5 smd rect (at -1 -0.2) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 4 smd rect (at -1 -0.6) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 3 smd rect (at -1 -1) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 2 smd rect (at -1 -1.4) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 20 smd circle (at 10 7.4) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(G2-Pad20)"))
    (pad 13 smd circle (at 10 -3.8) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(G2-Pad13)"))
    (pad 19 smd circle (at 10 5.8) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(G2-Pad19)"))
    (pad 17 smd circle (at 10 2.6) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(G2-Pad17)"))
    (pad 12 smd circle (at 10 -5.4) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(G2-Pad12)"))
    (pad 11 smd circle (at 10 -7) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(G2-Pad11)"))
    (pad 16 smd circle (at 10 1) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(G2-Pad16)"))
    (pad 18 smd circle (at 10 4.2) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(G2-Pad18)"))
    (pad 14 smd circle (at 10 -2.2) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(G2-Pad14)"))
    (pad 15 smd circle (at 10 -0.6) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(G2-Pad15)"))
    (pad 10 smd circle (at -10 7.4) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 9 smd circle (at -10 5.8) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 8 smd circle (at -10 4.2) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 7 smd circle (at -10 2.6) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 6 smd circle (at -10 1) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 5 smd circle (at -10 -0.6) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 4 smd circle (at -10 -2.2) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 3 smd circle (at -10 -3.8) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 2 smd circle (at -10 -5.4) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 1 smd circle (at -10 -7) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 1 smd rect (at -1 -1.8) (size 1.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
  )
  (gr_text D (at 97.5 110) (layer F.SilkS))
  (gr_text C (at 97.5 93) (layer F.SilkS))
  (gr_text A (at 97.5 59) (layer F.SilkS))
  (gr_text B (at 97.5 76) (layer F.SilkS))
  (gr_text 3 (at 121.25 106.2) (layer F.SilkS))
  (gr_text 10 (at 121.25 117.4) (layer F.SilkS))
  (gr_text 4 (at 121.25 107.8) (layer F.SilkS))
  (gr_text 6 (at 121.25 111) (layer F.SilkS))
  (gr_text 8 (at 121.25 114.2) (layer F.SilkS))
  (gr_text 1 (at 121.25 103) (layer F.SilkS))
  (gr_text 7 (at 121.25 112.6) (layer F.SilkS))
  (gr_text 5 (at 121.25 109.4) (layer F.SilkS))
  (gr_text 2 (at 121.25 104.6) (layer F.SilkS))
  (gr_text 9 (at 121.25 115.8) (layer F.SilkS))
  (gr_text 3 (at 121.25 89.2) (layer F.SilkS))
  (gr_text 10 (at 121.25 100.4) (layer F.SilkS))
  (gr_text 4 (at 121.25 90.8) (layer F.SilkS))
  (gr_text 6 (at 121.25 94) (layer F.SilkS))
  (gr_text 8 (at 121.25 97.2) (layer F.SilkS))
  (gr_text 1 (at 121.25 86) (layer F.SilkS))
  (gr_text 7 (at 121.25 95.6) (layer F.SilkS))
  (gr_text 5 (at 121.25 92.4) (layer F.SilkS))
  (gr_text 2 (at 121.25 87.6) (layer F.SilkS))
  (gr_text 9 (at 121.25 98.8) (layer F.SilkS))
  (gr_text 3 (at 121.25 72.2) (layer F.SilkS))
  (gr_text 10 (at 121.25 83.4) (layer F.SilkS))
  (gr_text 4 (at 121.25 73.8) (layer F.SilkS))
  (gr_text 6 (at 121.25 77) (layer F.SilkS))
  (gr_text 8 (at 121.25 80.2) (layer F.SilkS))
  (gr_text 1 (at 121.25 69) (layer F.SilkS))
  (gr_text 7 (at 121.25 78.6) (layer F.SilkS))
  (gr_text 5 (at 121.25 75.4) (layer F.SilkS))
  (gr_text 2 (at 121.25 70.6) (layer F.SilkS))
  (gr_text 9 (at 121.25 81.8) (layer F.SilkS))
  (gr_text 10 (at 121.25 66.4) (layer F.SilkS))
  (gr_text 9 (at 121.25 64.8) (layer F.SilkS))
  (gr_text 8 (at 121.25 63.2) (layer F.SilkS))
  (gr_text 7 (at 121.25 61.6) (layer F.SilkS))
  (gr_text 6 (at 121.25 60) (layer F.SilkS))
  (gr_text 5 (at 121.25 58.4) (layer F.SilkS))
  (gr_text 4 (at 121.25 56.8) (layer F.SilkS))
  (gr_text 3 (at 121.25 55.2) (layer F.SilkS))
  (gr_text 2 (at 121.25 53.6) (layer F.SilkS))
  (gr_text 1 (at 121.25 52) (layer F.SilkS))
  (gr_text "Wirebond Tester V2\nC Fangmeier\n2019" (at 109.5 104.5) (layer F.SilkS))
  (gr_line (start 125 40) (end 95 40) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125 120) (end 125 40) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 95 120) (end 125 120) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 95 40) (end 95 120) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 97.5 41) (xy 122.5 41) (xy 122.5 50) (xy 97.5 50)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.5 41) (xy 122.5 50) (xy 97.5 50) (xy 97.5 41)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.4092 119.38) (xy 95.6056 119.38) (xy 95.6056 40.5892) (xy 124.4092 40.5892)
      )
    )
  )
)
